(footprint "Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F8CEB8)
  (descr "Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package")
  (tags "SMD SMT crystal oscillator")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.45) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1a2003d3-0ecb-484f-a6e3-edd6b7d1ad92)
  )
  (fp_text value "Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm" (at 0 2.45) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 057623fd-d8de-46cb-8cae-158489a0257d)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.7 0.7) (thickness 0.105)))
    (tstamp 9033ad50-f835-4696-9f8b-9a39401414d2)
  )
  (fp_circle (center 0 0) (end 0.133333 0) (layer "F.Adhes") (width 0.083333) (fill none) (tstamp 21c423f4-4b1d-4c4d-9fce-78b90ec2f632))
  (fp_circle (center 0 0) (end 0.25 0) (layer "F.Adhes") (width 0.1) (fill none) (tstamp 67dd5243-8d7d-4528-8653-2c39cb793492))
  (fp_circle (center 0 0) (end 0.058333 0) (layer "F.Adhes") (width 0.116667) (fill none) (tstamp 878c7dec-a3c0-4cc0-8930-66aea7f548ca))
  (fp_circle (center 0 0) (end 0.208333 0) (layer "F.Adhes") (width 0.083333) (fill none) (tstamp b7e076a6-5253-489e-8653-5c82d63063a0))
  (fp_line (start -1.9 -1.575) (end -1.9 1.575) (layer "F.SilkS") (width 0.12) (tstamp cc699001-4139-409a-82cd-bc2c4d926cc1))
  (fp_line (start -1.9 1.575) (end 1.9 1.575) (layer "F.SilkS") (width 0.12) (tstamp e039843d-af8e-4bc9-81c4-cf25133f2510))
  (fp_line (start -2 -1.7) (end -2 1.7) (layer "F.CrtYd") (width 0.05) (tstamp 00d2a74e-45c0-4d16-8866-24a940e55164))
  (fp_line (start 2 1.7) (end 2 -1.7) (layer "F.CrtYd") (width 0.05) (tstamp 879dbe23-2911-4bde-a8a5-d3468c0bdfbd))
  (fp_line (start 2 -1.7) (end -2 -1.7) (layer "F.CrtYd") (width 0.05) (tstamp ea19823c-ec6b-4a21-b048-e3110332e888))
  (fp_line (start -2 1.7) (end 2 1.7) (layer "F.CrtYd") (width 0.05) (tstamp eb1b2a56-5779-47c5-8993-ff62c71fdc75))
  (fp_line (start -1.5 1.25) (end -1.6 1.15) (layer "F.Fab") (width 0.1) (tstamp 0bcd0afa-1cf0-4be3-83f1-d6f09cf32f8f))
  (fp_line (start -1.5 -1.25) (end 1.5 -1.25) (layer "F.Fab") (width 0.1) (tstamp 1529b4ce-e927-438e-a954-f2300e63af8e))
  (fp_line (start -1.6 -1.15) (end -1.5 -1.25) (layer "F.Fab") (width 0.1) (tstamp 395725a5-7ad3-4d9f-b20f-2a2c8f9c1dbb))
  (fp_line (start 1.6 1.15) (end 1.5 1.25) (layer "F.Fab") (width 0.1) (tstamp 645875d7-89d2-46a5-b485-5777890ee24e))
  (fp_line (start -1.6 0.25) (end -0.6 1.25) (layer "F.Fab") (width 0.1) (tstamp 67b4e877-ab49-4f2e-a7bf-d5adb204f343))
  (fp_line (start -1.6 1.15) (end -1.6 -1.15) (layer "F.Fab") (width 0.1) (tstamp 6a5cb746-2850-4e73-acf0-9df294c2d60c))
  (fp_line (start 1.6 -1.15) (end 1.6 1.15) (layer "F.Fab") (width 0.1) (tstamp 806e4597-32cd-4d28-9563-41bd14f9708b))
  (fp_line (start 1.5 1.25) (end -1.5 1.25) (layer "F.Fab") (width 0.1) (tstamp acea10c0-b702-430b-9b73-7b2159c7454d))
  (fp_line (start 1.5 -1.25) (end 1.6 -1.15) (layer "F.Fab") (width 0.1) (tstamp b88c5857-ce77-4910-a6d0-59d156eb13b5))
  (pad "1" smd rect (at -1.05 0.825) (size 1.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3b0a0b11-ea3c-44fa-81af-9ff509eb34a2))
  (pad "2" smd rect (at 1.05 0.825) (size 1.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7c514b29-ea71-43e0-a727-fcfea224419d))
  (pad "3" smd rect (at 1.05 -0.825) (size 1.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e676a1c5-1c81-4b1a-adb9-184f9349f17c))
  (pad "4" smd rect (at -1.05 -0.825) (size 1.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 4551a4e8-9e94-4967-b865-f84024360aa5))
  (model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KIPRJMOD}/3d-models/3225 SMD Crystal Oscillator.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 180))
  )
)
