(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "HRO-TYPE-C-31-M-12" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "USB" (id 0) (at -5.08 16.51 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "HRO-TYPE-C-31-M-12" (id 1) (at -10.16 -1.27 90)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "HRO-TYPE-C-31-M-12_0_1"
      (rectangle (start -11.43 15.24) (end -8.89 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 -17.78) (end -8.89 15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "HRO-TYPE-C-31-M-12_1_1"
      (pin input line (at 2.54 13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -8.89 180) (length 2.54)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -16.51 180) (length 2.54)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 8.89 180) (length 2.54)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 6.35 180) (length 2.54)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 3.81 180) (length 2.54)
        (name "DN2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 1.27 180) (length 2.54)
        (name "DP1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -1.27 180) (length 2.54)
        (name "DN1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -3.81 180) (length 2.54)
        (name "DP2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -6.35 180) (length 2.54)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Micro_SD_Card TF015" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -16.51 15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Micro_SD_Card TF015" (id 1) (at 16.51 15.24 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 29.21 7.62 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2112221030_SOFNG-TF-015_C113206.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector SD microsd" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Micro SD Card Socket" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "microSD*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Micro_SD_Card TF015_0_0"
      (pin output line (at -21.59 -12.7 0) (length 2.54)
        (name "CD" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "Micro_SD_Card TF015_0_1"
      (rectangle (start -7.62 -9.525) (end -5.08 -10.795)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 -6.985) (end -5.08 -8.255)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 -4.445) (end -5.08 -5.715)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 -1.905) (end -5.08 -3.175)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 0.635) (end -5.08 -0.635)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 3.175) (end -5.08 1.905)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 5.715) (end -5.08 4.445)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 8.255) (end -5.08 6.985)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 16.51 12.7)
          (xy 16.51 13.97)
          (xy -19.05 13.97)
          (xy -19.05 -16.51)
          (xy 16.51 -16.51)
          (xy 16.51 -11.43)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 -11.43)
          (xy -8.89 8.89)
          (xy -1.27 8.89)
          (xy 2.54 12.7)
          (xy 3.81 12.7)
          (xy 3.81 11.43)
          (xy 6.35 11.43)
          (xy 7.62 12.7)
          (xy 20.32 12.7)
          (xy 20.32 -11.43)
          (xy -8.89 -11.43)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "Micro_SD_Card TF015_1_1"
      (pin bidirectional line (at -22.86 7.62 0) (length 3.81)
        (name "DAT2" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 20.32 -15.24 180) (length 3.81)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 5.08 0) (length 3.81)
        (name "DAT3/CD" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 2.54 0) (length 3.81)
        (name "CMD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 0 0) (length 3.81)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -2.54 0) (length 3.81)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 -5.08 0) (length 3.81)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -7.62 0) (length 3.81)
        (name "DAT0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -10.16 0) (length 3.81)
        (name "DAT1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "UCC5606" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 19.05 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "UCC5606" (id 1) (at 10.16 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm" (id 2) (at 7.62 -36.83 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/slus347a/slus347a.pdf" (id 3) (at 7.62 -34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "UCC5606_0_0"
      (pin output line (at -16.51 -2.54 0) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -12.7 0) (length 2.54)
        (name "~{DISCNCT}" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 12.7 0) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 10.16 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 7.62 0) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 5.08 0) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 1.27 19.05 270) (length 2.54)
        (name "TRMPWR" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 19.05 270) (length 2.54)
        (name "TRMPWR" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 1.27 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 3.81 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.35 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 -5.08 0) (length 2.54)
        (name "D8" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 8.89 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 11.43 180) (length 2.54)
        (name "REG" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 16.51 8.89 180) (length 2.54)
        (name "REG" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 2.54 0) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 0 0) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -16.51 -7.62 0) (length 2.54)
        (name "D9" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 13.97 -13.97 0) (length 2.54)
        (name "N/C" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -11.43 -22.86 90) (length 2.54)
        (name "SGND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -8.89 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -6.35 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -3.81 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "UCC5606_0_1"
      (rectangle (start -13.97 16.51) (end 13.97 -20.32)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
)
