(footprint "TS-1187A-B-A-B" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6e84aa00-de6e-4a35-a845-6d72d806004c)
  )
  (fp_text value "TS-1187A-B-A-B" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c1cbdbe1-9226-4c0e-8a39-1f2891b5383b)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 687f8cc9-85cb-406f-8477-078be481afae)
  )
  (pad "1" smd roundrect (at 3 7) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7fa72276-0f28-4c10-b5b2-d0c179826a6a))
  (pad "1" smd roundrect (at -3 7) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp be05a87b-e03f-47ad-b8bb-f9e49451063a))
  (pad "2" smd roundrect (at 3 10.75) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ac62b500-059c-43f9-8922-0f87f8b072c5))
  (pad "2" smd roundrect (at -3 10.75) (size 1 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b2f741ef-fb71-479b-beba-520f02ae4c65))
)
