(footprint "TF-06_MicroSD" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cd706eb7-c090-49e4-91cf-3acc3fa6a300)
  )
  (fp_text value "TF-06_MicroSD" (at 0 -3.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3c6a4f89-1edd-4407-a48d-5fc255048070)
  )
  (fp_text user "${REFERENCE}" (at 0 -2 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 503598fe-b4af-40b2-8d24-e0144b2d8d44)
  )
  (fp_line (start 6 8) (end 6 7) (layer "F.CrtYd") (width 0.05) (tstamp 0981755a-5827-4a5d-81ba-9b5838fb4a7d))
  (fp_line (start -6 -6) (end -6 8) (layer "F.CrtYd") (width 0.05) (tstamp 4b10ae34-f80d-4d9f-b5b8-02f892d54d29))
  (fp_line (start -6 8) (end 6 8) (layer "F.CrtYd") (width 0.05) (tstamp 4becc26e-9b91-4a2d-b9c4-8eb6fcceda44))
  (fp_line (start 6 7) (end 6 -6) (layer "F.CrtYd") (width 0.05) (tstamp b0898591-cb6b-4705-baac-ae38a45435cd))
  (fp_line (start 6 -6) (end -6 -6) (layer "F.CrtYd") (width 0.05) (tstamp ecd76209-6b90-4e90-9d21-8bf031a344a9))
  (pad "1" smd roundrect (at -3.85 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d28894e9-6ffd-401e-ab89-1a348d634b4e))
  (pad "2" smd roundrect (at -2.75 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ccfb1481-202c-4cad-93cf-1283e99d97eb))
  (pad "3" smd roundrect (at -1.65 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9cd27957-a2e7-47b6-aec7-f44cac8c769e))
  (pad "4" smd roundrect (at -0.9 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f4f528bd-b5ef-4ac5-815c-911bd74bb765))
  (pad "5" smd roundrect (at -0.2 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b8ef65de-bd2a-41ec-a8cc-9f990eca1509))
  (pad "6" smd roundrect (at 0.55 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp efc706b7-bd6f-4cd0-8698-0a1728f66eae))
  (pad "7" smd roundrect (at 1.65 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8babd8aa-6687-41eb-b392-c6d3b88c604b))
  (pad "8" smd roundrect (at 2.75 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4b287319-553e-4667-8ce1-81eb85842c01))
  (pad "9" smd roundrect (at 3.85 0.54) (size 0.5 1.08) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5358995e-87f8-4f79-a3f1-9885f1562dce))
  (pad "10" smd roundrect (at 5.225 6.63) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a515aa6f-d9c2-42b3-853a-e063fbf54b44))
  (pad "10" smd roundrect (at 5.225 2.18) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a7a731ea-fd89-456b-ab33-c96da319d7b9))
  (pad "10" smd roundrect (at -5.225 2.18) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b7c50ad8-e4a2-4911-8c0d-5dc21aeec91d))
  (pad "10" smd roundrect (at -5.225 6.63) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d5cfbe9b-8afd-4544-90b0-d943428038c0))
)
