(footprint "TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F7ED41)
  (descr "TSSOP, 24 Pin (https://www.st.com/resource/en/datasheet/led1642gw.pdf#page=37), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "TSSOP SO")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.85) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f8ab52a8-7f5a-431e-9ce8-269defdc20a0)
  )
  (fp_text value "TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm" (at 0 4.85) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d296fac4-ef23-4024-9fa8-ec46cb37bc04)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e80f338f-9d54-4fca-9ada-8d9120032bec)
  )
  (fp_line (start 0 -4.035) (end 2.2 -4.035) (layer "F.SilkS") (width 0.12) (tstamp 0029328e-9975-4a93-8b32-83d525819a3e))
  (fp_line (start 0 4.035) (end -2.2 4.035) (layer "F.SilkS") (width 0.12) (tstamp 514fd8d6-edac-4cfd-9783-45427f355441))
  (fp_line (start 0 4.035) (end 2.2 4.035) (layer "F.SilkS") (width 0.12) (tstamp c0da16b7-fcca-4774-b0d9-8d2ae07f3f4d))
  (fp_line (start 0 -4.035) (end -3.625 -4.035) (layer "F.SilkS") (width 0.12) (tstamp ced20ce9-4db5-41d6-8e51-e51b61aeaefb))
  (fp_line (start -3.88 -4.15) (end -3.88 4.15) (layer "F.CrtYd") (width 0.05) (tstamp 5917fdef-fb82-4232-a296-990860b97e82))
  (fp_line (start 3.88 4.15) (end 3.88 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp 6224739c-8795-4333-9aaf-e0f4582ab9f4))
  (fp_line (start -3.88 4.15) (end 3.88 4.15) (layer "F.CrtYd") (width 0.05) (tstamp 67106241-6086-45bf-9e4e-f13656ce0143))
  (fp_line (start 3.88 -4.15) (end -3.88 -4.15) (layer "F.CrtYd") (width 0.05) (tstamp c471f107-25f2-4f0e-82b6-fff763aef3f1))
  (fp_line (start -1.2 -3.9) (end 2.2 -3.9) (layer "F.Fab") (width 0.1) (tstamp 2059cc5f-c86c-40f9-a7b7-549f77b9acdf))
  (fp_line (start 2.2 3.9) (end -2.2 3.9) (layer "F.Fab") (width 0.1) (tstamp 34018e51-be5b-41f5-b534-37547a97a3ae))
  (fp_line (start 2.2 -3.9) (end 2.2 3.9) (layer "F.Fab") (width 0.1) (tstamp 3d67bebd-bc5a-4ebd-97bf-25ae9b7ede5e))
  (fp_line (start -2.2 3.9) (end -2.2 -2.9) (layer "F.Fab") (width 0.1) (tstamp 7a466bea-07c9-4db6-b004-4e85694534bd))
  (fp_line (start -2.2 -2.9) (end -1.2 -3.9) (layer "F.Fab") (width 0.1) (tstamp ef73f275-62eb-49da-b7fa-24328d0e6898))
  (pad "" smd roundrect (at 0.8 0) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp 2d933511-50bf-42fd-aec3-10413aa45bd8))
  (pad "" smd roundrect (at -0.8 -1.67) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp 4dbc09d3-a47e-4a55-a9e9-545252ee9498))
  (pad "" smd roundrect (at -0.8 0) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp 5cf85995-e384-4fd2-be5a-3c0cf87ac299))
  (pad "" smd roundrect (at 0.8 -1.67) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp 89467729-272a-40c7-99a4-b768d3c8d33d))
  (pad "" smd roundrect (at -0.8 1.67) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp a44826b2-14e4-4bdc-8fbb-f1980cff5c7f))
  (pad "" smd roundrect (at 0.8 1.67) (size 1.29 1.34) (layers "F.Paste") (roundrect_rratio 0.193798) (tstamp cb9b2a3b-fb4c-4cea-b9a2-d33cc2306e15))
  (pad "1" smd roundrect (at -2.875 -3.575) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a0012f1f-ba2d-42ba-95e1-dfb437efa7b3))
  (pad "2" smd roundrect (at -2.875 -2.925) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e69046c6-f106-4d95-8d17-8aba367c1ef5))
  (pad "3" smd roundrect (at -2.875 -2.275) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ec72f21d-1cfc-4a06-9b1f-f5c3044eda53))
  (pad "4" smd roundrect (at -2.875 -1.625) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0e2081a6-1d78-4395-af4d-4642edb456b7))
  (pad "5" smd roundrect (at -2.875 -0.975) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ef486603-7ea7-4ab3-9f2a-261957825871))
  (pad "6" smd roundrect (at -2.875 -0.325) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f1732772-f066-49f3-ae3d-1f882f6cea00))
  (pad "7" smd roundrect (at -2.875 0.325) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp efffdf08-e911-47be-8236-0cba10e4f29d))
  (pad "8" smd roundrect (at -2.875 0.975) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 94db4731-2b40-42d2-ac29-771e9326137b))
  (pad "9" smd roundrect (at -2.875 1.625) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1c33e064-aaa5-4acf-956b-5e9852193db3))
  (pad "10" smd roundrect (at -2.875 2.275) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5b6b8ff0-01b9-49c9-b9ac-05e9dbb9bf92))
  (pad "11" smd roundrect (at -2.875 2.925) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0b6aa98c-284a-47ff-8bea-fcab813afefa))
  (pad "12" smd roundrect (at -2.875 3.575) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4e017852-e57f-4492-bf12-6edccc479114))
  (pad "13" smd roundrect (at 2.875 3.575) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 186c170a-55f1-4311-9463-c6e196c519b5))
  (pad "14" smd roundrect (at 2.875 2.925) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6dad79d6-1c95-419e-9d3c-c5e0d3faeaa7))
  (pad "15" smd roundrect (at 2.875 2.275) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 806543f6-4e93-47d8-b60e-21772d20204c))
  (pad "16" smd roundrect (at 2.875 1.625) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e1c77eff-573e-4ad4-9093-5a873beb3b41))
  (pad "17" smd roundrect (at 2.875 0.975) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cf284bb4-067d-4583-8b20-22b122f135bd))
  (pad "18" smd roundrect (at 2.875 0.325) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 345fa40a-515e-4c9d-92dd-3759e895e5a9))
  (pad "19" smd roundrect (at 2.875 -0.325) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 230548e7-efef-4d3b-9ce6-890f6f963946))
  (pad "20" smd roundrect (at 2.875 -0.975) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 437da493-5871-4b78-a20a-20dcba1ca6cf))
  (pad "21" smd roundrect (at 2.875 -1.625) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6a8a0842-4574-48f1-ac41-9e7276ede06a))
  (pad "22" smd roundrect (at 2.875 -2.275) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b3fb9e74-8d66-47f1-b26c-2d824a90861b))
  (pad "23" smd roundrect (at 2.875 -2.925) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4b2b1616-a2d8-4eae-92ec-b3dd932ddce6))
  (pad "24" smd roundrect (at 2.875 -3.575) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 04f86b21-294f-41bb-873f-d99a3bd35ef8))
  (pad "25" smd rect (at 0 0) (size 3.2 5) (layers "F.Cu" "F.Mask") (tstamp 0ddeb084-740e-44e4-8367-61fb6db506d0))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
