(footprint "JST_SM04B-SRSS-TB(LF)(SN)" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6502101B)
  (attr smd)
  (fp_text reference "REF**" (at -0.545095 -1.767685) (layer "F.SilkS")
    (effects (font (size 1.001173 1.001173) (thickness 0.15)))
    (tstamp 42d55b90-a512-4a39-b88d-a8faf63f9307)
  )
  (fp_text value "JST_SM04B-SRSS-TB_LF__SN_" (at 0 6.4) (layer "F.Fab")
    (effects (font (size 1.000567 1.000567) (thickness 0.15)))
    (tstamp 04cdf8ef-673c-416a-b8ae-b1679f782b37)
  )
  (fp_text user "https://www.snapeda.com/parts/SM04B-SRSS-TB%28LF%29%28SN%29/JST%20Sales/view-part/" (at 0 10.9 unlocked) (layer "User.1")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0938076e-3982-4816-a6ba-558249dc92b5)
  )
  (fp_text user "License: CC-BY-SA 4.0" (at 0 12.6 unlocked) (layer "User.1")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 37d7e60f-5b81-4d69-ba99-35c8c8d9ca74)
  )
  (fp_text user "This footprint comes from SnapEDA, and SnapEDA holds the copyright:" (at 0 9 unlocked) (layer "User.1")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5aa78423-8e10-4f81-880a-a5e3c87b8759)
  )
  (fp_text user "https://creativecommons.org/licenses/by-sa/4.0/" (at 0 13.9 unlocked) (layer "User.1")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a445b58b-22b9-4891-948e-e8705815f97a)
  )
  (fp_text user "This license contains a warranty disclaimer, please read it in full" (at 0 15.7 unlocked) (layer "User.1")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cc41e7d2-eef6-4113-85ea-9211b00a9520)
  )
  (fp_line (start -1.8 4.575) (end 1.8 4.575) (layer "F.SilkS") (width 0.127) (tstamp 0b35f296-1f2c-45db-aacc-9c452ac2b541))
  (fp_line (start 2.2 0.325) (end 3 0.325) (layer "F.SilkS") (width 0.127) (tstamp 0e34d135-4d0c-46d1-a568-bc0ecd0245b1))
  (fp_line (start 3 0.325) (end 3 2.6) (layer "F.SilkS") (width 0.127) (tstamp 268bb2d5-179a-44d4-9acd-784e1c241a18))
  (fp_line (start -3 0.325) (end -3 2.6) (layer "F.SilkS") (width 0.127) (tstamp 8b6e0f1a-7453-41a0-b633-bc311904533b))
  (fp_line (start -2.2 0.325) (end -3 0.325) (layer "F.SilkS") (width 0.127) (tstamp c2174c4b-5931-4d26-922a-d47df1cf0a2d))
  (fp_circle (center -2.45 -0.385) (end -2.35 -0.385) (layer "F.SilkS") (width 0.3) (fill none) (tstamp 9674240b-2669-4ca5-bb3c-a7b5651f14f9))
  (fp_line (start 3.65 -1.025) (end 3.65 5.025) (layer "F.CrtYd") (width 0.05) (tstamp 6e444cb6-65e6-4718-8401-7527ae45437c))
  (fp_line (start 3.65 5.025) (end -3.65 5.025) (layer "F.CrtYd") (width 0.05) (tstamp bffd0d5d-dbc9-4ce4-a5cf-13bb997b66d9))
  (fp_line (start -3.65 -1.025) (end 3.65 -1.025) (layer "F.CrtYd") (width 0.05) (tstamp dc96eb69-da78-45e0-a48d-5347f3b73526))
  (fp_line (start -3.65 5.025) (end -3.65 -1.025) (layer "F.CrtYd") (width 0.05) (tstamp feaf90f8-d2de-4e5a-a6c8-3aa7ddd8c5a8))
  (fp_line (start 3 4.575) (end -3 4.575) (layer "F.Fab") (width 0.127) (tstamp 1645353f-5b93-40a0-b196-7f64ae9ffb02))
  (fp_line (start -3 4.575) (end -3 0.325) (layer "F.Fab") (width 0.127) (tstamp 8f042f95-3631-450e-9d35-41e5818a0404))
  (fp_line (start 3 0.325) (end 3 4.575) (layer "F.Fab") (width 0.127) (tstamp 990f751a-101a-4066-bb9e-d3585f41746a))
  (fp_line (start -3 0.325) (end 3 0.325) (layer "F.Fab") (width 0.127) (tstamp b671c8ae-09dd-4f6c-b136-956f5130445f))
  (fp_circle (center -2.45 -0.385) (end -2.35 -0.385) (layer "F.Fab") (width 0.3) (fill none) (tstamp 3c9fa0a1-b271-4ea4-9631-bcfed6de2ca6))
  (pad "1" smd rect (at -1.5 0) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 9b026a6b-62a5-44ea-adf9-2ce220ef3ea3))
  (pad "2" smd rect (at -0.5 0) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 533aa292-6810-430f-b18d-d3f972fcb85c))
  (pad "3" smd rect (at 0.5 0) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp df640a41-11a3-4654-b648-c6156529de63))
  (pad "4" smd rect (at 1.5 0) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 7eb87791-1adf-4800-ac7f-050ec0d99787))
  (pad "S1" smd rect (at -2.8 3.875 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 1aaa2f2a-01a8-4e65-a8ef-204eb8e2622d))
  (pad "S2" smd rect (at 2.8 3.875 180) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.102) (tstamp 0b5c2537-9481-4692-afb9-d0ba86f2c08a))
)
