(footprint "Buzzer" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
  (tags "CONN DEV")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "SPK1" (at 3.25 -5.25) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b7d7225b-834e-4a33-aef7-c6e4f0f1d4c3)
  )
  (fp_text value "Speaker" (at 1.27 2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 81bec8a2-16a6-44b4-8784-2cd93e0d6bd7)
  )
  (fp_text user "${REFERENCE}" (at 3.25 -5.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2f0227a7-932f-4bc4-82fc-f278ce7c43b6)
  )
  (fp_line (start -1 -4.5) (end 7.5 -4.5)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 8e0ebf4f-507b-465e-9dfb-787ee94b90bc))
  (fp_line (start -1 0.75) (end -1 -4.5)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp fd60d1d6-465e-4bd3-94fc-a9c6831c1a2b))
  (fp_line (start 7.5 -4.5) (end 7.5 0.75)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp d92b5d8f-97d1-4f42-97e3-a615b2180a3f))
  (fp_line (start -1.3 -4.75) (end -1.3 1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e23042e7-1352-46f9-8aca-590a303663cf))
  (fp_line (start -1.3 1) (end 7.75 1)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 266f9fbe-6b27-4a11-8a13-5019c8cbc91f))
  (fp_line (start 7.75 -4.75) (end -1.3 -4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f160d47a-2533-47c1-9d99-9a3c6d755408))
  (fp_line (start 7.75 1) (end 7.75 -4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 444173b5-234b-4db8-998f-6b8c62469bf9))
  (pad "1" smd rect (at 0 -1.75) (size 1.4 5) (layers "F.Cu" "F.Mask") (tstamp a5bc13e7-4eaa-4486-a92a-c891b4af88d3))
  (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp b85e45f7-94fa-4ff3-8ce1-257b33531605))
  (pad "2" smd rect (at 6.5 -1.75) (size 1.4 5) (layers "F.Cu" "F.Mask") (tstamp 9a8eb963-e854-4a61-be63-7404d2c3fa63))
  (pad "2" thru_hole circle (at 6.5 0) (size 1.4 1.4) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp c59a976e-d63a-4ef6-86bd-629ae1b993d6))
)
