(module USB_A_CONNFLY_DS1095-WNR0 (layer F.Cu) (tedit 6112C909)
  (descr http://www.connfly.com/userfiles/image/UpLoadFile/File/2013/5/6/DS1095.pdf)
  (tags "USB-A receptacle horizontal through-hole")
  (fp_text reference REF** (at -1.95 -2.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_CONNFLY_DS1095-WNR0 (at 3.5 7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.5 -2) (end -0.5 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 -1.5) (end 0.5 -2) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.5 -2) (end 0 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.86 0.86) (end 10.86 -1.12) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.86 -1.12) (end -3.86 0.86) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.86 -1.12) (end 10.86 -1.12) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.86 4.56) (end 10.86 13.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.86 13.1) (end 10.86 13.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.86 4.56) (end -3.86 13.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.32 -1.51) (end 12.32 -1.51) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.32 -1.51) (end 12.32 13.49) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.32 13.49) (end -5.32 13.49) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.32 -1.51) (end -5.32 13.49) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.87 -1.01) (end -3.75 -0.13) (layer F.Fab) (width 0.1))
  (fp_line (start -3.75 12.99) (end 10.75 12.99) (layer F.Fab) (width 0.1))
  (fp_line (start -2.87 -1.01) (end 10.75 -1.01) (layer F.Fab) (width 0.1))
  (fp_line (start 10.75 -1.01) (end 10.75 12.99) (layer F.Fab) (width 0.1))
  (fp_line (start -3.75 -0.13) (end -3.75 12.99) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 3.5 5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 5 thru_hole circle (at 10.07 2.71) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -3.07 2.71) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.5 0) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 4.5 0) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 7 0) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CONNFLY_DS1095-WNR0.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model 3d_models/Connector_USB-A.STEP
    (offset (xyz 3.5 -5.75 4))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 180))
  )
)
