(module "ABC80 keyboard pcb" (layer F.Cu) (tedit 6112B56A)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "ABC80 keyboard pcb" (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -25.5 -4.5) (end -25.5 4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start -25.5 4.5) (end -36 4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start -36 4.5) (end -36 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 25.5 -4.5) (end 25.5 4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 25.5 4.5) (end 36 4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 36 4.5) (end 36 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start -36 -4.5) (end -25.5 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 25.5 -4.5) (end 36 -4.5) (layer Dwgs.User) (width 0.12))
  (pad 1 connect rect (at -22 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 2 connect rect (at -18 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 3 connect rect (at -14 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 4 connect rect (at -10 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 5 connect rect (at -6 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 6 connect rect (at -2 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 7 connect rect (at 2 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 8 connect rect (at 6 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 9 connect rect (at 10 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 10 connect rect (at 14 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 11 connect rect (at 18 -1) (size 3 7) (layers B.Cu B.Mask))
  (pad 12 connect rect (at 22 -1) (size 3 7) (layers B.Cu B.Mask))
)
