(module BarrelJack_Wuerth_6941xx301002 (layer F.Cu) (tedit 613A460B)
  (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
  (tags "connector barrel jack")
  (fp_text reference REF** (at 0 -2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BarrelJack_Wuerth_6941xx301002 (at 0 15.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.6 -1) (end -2.5 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.2 0.5) (end 5 0.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.2 5.5) (end 5 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.2 0.5) (end 6.2 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5 0.5) (end 5 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 14.1) (end 5 14.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5 -1.4) (end -5 14.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5 -1.4) (end -5 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.9 -1.3) (end -4.9 0.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.2 -1.3) (end -4.9 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.6 -1) (end 4.6 0.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 -1) (end 4.6 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.6 13.7) (end -4.6 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.6 13.7) (end -4.6 13.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.5 13.6) (end -4.5 0.1) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 13.6) (end -4.5 13.6) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 -0.9) (end 4.5 13.6) (layer F.Fab) (width 0.1))
  (fp_line (start 4.5 -0.9) (end -3.5 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -4.5 0.1) (end -3.5 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 4.6 5.2) (end 4.6 13.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 5 14.1) (end 5 5.5) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 7.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 3 thru_hole oval (at 4.8 3 90) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 5.8) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 4.4 1.8) (drill oval 3.4 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_6941xx301002.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model 3d_models/DCPowerJack5.5mmx2.1mm.STEP
    (offset (xyz 0 -10.5 6))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 180))
  )
)
