(module ESP32-S2-WROVER (layer F.Cu) (tedit 613A4425)
  (descr "ESP32-S2-WROVER(-I) 2.4 GHz Wi-Fi https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf")
  (tags "ESP32-S2  ESP32  WIFI")
  (attr smd)
  (fp_text reference REF** (at -10.41 10.53 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ESP32-S2-WROVER (at 0.04 13.145 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9 -12.02) (end -9 11.68) (layer F.Fab) (width 0.1))
  (fp_line (start -8.5 -12.52) (end -9 -13.02) (layer F.Fab) (width 0.1))
  (fp_line (start -9 -12.02) (end -8.5 -12.52) (layer F.Fab) (width 0.1))
  (fp_line (start -24.25 -12.77) (end -9.63 -12.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start -24.25 -34.57) (end -24.25 -12.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start 24.25 -34.57) (end -24.25 -34.57) (layer F.CrtYd) (width 0.05))
  (fp_line (start 24.25 -12.77) (end 24.25 -34.57) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.63 -12.77) (end 24.25 -12.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start -21.69 -34.32) (end -23.99 -32.02) (layer Dwgs.User) (width 0.12))
  (fp_line (start -16.69 -34.32) (end -24 -27) (layer Dwgs.User) (width 0.12))
  (fp_line (start -11.69 -34.32) (end -24 -22.01) (layer Dwgs.User) (width 0.12))
  (fp_line (start -6.7 -34.32) (end -24 -17.01) (layer Dwgs.User) (width 0.12))
  (fp_line (start -1.73 -34.32) (end -23 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 3.27 -34.32) (end -18 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 8.26 -34.32) (end -13.01 -13.02) (layer Dwgs.User) (width 0.12))
  (fp_line (start 13.28 -34.32) (end -7.99 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 18.31 -34.32) (end -2.95 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 23.28 -34.32) (end 2 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 24 -30.04) (end 7.01 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 24 -25.02) (end 12 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 24 -20.04) (end 17 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start 24 -15.03) (end 22 -13.03) (layer Dwgs.User) (width 0.12))
  (fp_line (start -24 -34.323) (end -24 -13.023) (layer Dwgs.User) (width 0.12))
  (fp_line (start 24 -34.323) (end 24 -13.023) (layer Dwgs.User) (width 0.12))
  (fp_line (start -24 -34.323) (end 24 -34.323) (layer Dwgs.User) (width 0.12))
  (fp_line (start -24 -13.023) (end 24 -13.023) (layer Dwgs.User) (width 0.12))
  (fp_line (start -9.11 -12.37) (end -9.5 -12.37) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.63 12.47) (end 9.63 12.47) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.63 12.47) (end 9.63 -12.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.63 -12.77) (end -9.63 12.47) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.13 -13.03) (end 9.13 -19.45) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.11 -12.37) (end -9.125 -19.45) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.125 -19.45) (end 9.13 -19.45) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.12 11.54) (end 9.12 11.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.12 11.8) (end 7.46 11.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.12 11.44) (end -9.12 11.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.12 11.8) (end -7.46 11.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -9 11.68) (end 9 11.68) (layer F.Fab) (width 0.1))
  (fp_line (start -9 -19.32) (end -9 -13.02) (layer F.Fab) (width 0.1))
  (fp_line (start -9 -19.323) (end 9 -19.323) (layer F.Fab) (width 0.1))
  (fp_line (start 9 -19.32) (end 9 11.68) (layer F.Fab) (width 0.1))
  (fp_line (start 9 -13.023) (end -9 -13.023) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "KEEP-OUT ZONE" (at 0 -27.09) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.15)))
  )
  (fp_text user ANTENNA (at 0 -16.15) (layer Cmts.User)
    (effects (font (size 1.25 1.25) (thickness 0.15)))
  )
  (pad 43 smd rect (at -1.19 -3.735) (size 4.1 4.1) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at 8.625 -11.675) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at 8.625 -10.275) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 8.625 -8.775) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 8.625 -7.175) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 5.25 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 6.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 8.625 10.825) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 8.625 9.325) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 8.625 7.825) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 8.625 6.325) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 8.625 4.825) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 8.625 3.325) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 8.625 1.825) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 8.625 0.325) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 8.625 -1.175) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 8.625 -2.675) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 8.625 -4.175) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 8.625 -5.675) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -8.625 7.725) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -8.625 6.225) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -8.625 4.725) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -8.625 3.225) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -8.625 1.725) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -8.625 0.225) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -8.625 -1.275) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -8.625 -2.775) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -8.625 -4.275) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -8.625 -5.775) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -8.625 -7.275) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -8.625 -8.775) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -8.625 -10.275) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 3.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 2.25 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 0.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -0.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -2.25 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -3.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -5.25 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -6.75 11.475) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -8.625 10.725 180) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -8.625 9.225 180) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -8.625 -11.775) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-S2-WROVER.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model 3d_models/ESP32-S2-WROVER.STEP
    (offset (xyz 0 3.75 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
