(footprint "PinSocket_2x20_P2.54mm_Vertical_Custom"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
	(tags "Through hole socket strip THT 2x20 2.54mm double row")
	(property "Reference" "P1"
		(at 2.2 -0.06 90)
		(layer "F.SilkS")
		(uuid "07baaad5-b3ff-4f88-aafe-baef5d037ac3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CONN_02X20"
		(at -1.27 51.03 180)
		(layer "F.Fab")
		(uuid "65cfd46e-e75d-4fe5-93ee-7e158a78a1fa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical_Custom"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "b546a082-80ad-4f22-a30b-c37a73e78cb8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "5677ea8a-478a-4f08-a72c-42e584f05539")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "47070f65-d72f-46f4-b406-1d7240cecd69")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -3.87 -1.33)
		(end -3.87 49.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a659a698-90a4-4848-98ae-32ba92d01fbb")
	)
	(fp_line
		(start -3.87 -1.33)
		(end -1.27 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1b6aa434-bf37-4ab4-99cf-921c3eac79e0")
	)
	(fp_line
		(start -3.87 49.59)
		(end 1.33 49.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c08f6dfa-f773-4a4d-b3c4-a4f5278f9157")
	)
	(fp_line
		(start -1.27 -1.33)
		(end -1.27 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "158281b3-0314-45ee-8e14-a979d37b411d")
	)
	(fp_line
		(start -1.27 1.27)
		(end 1.33 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "26b4e64a-8bf2-4b46-8e30-fc7bf0eee9a7")
	)
	(fp_line
		(start 0 -1.33)
		(end 1.33 -1.33)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b1f68ff0-8960-4e0a-af3a-5b1a340476ce")
	)
	(fp_line
		(start 1.33 -1.33)
		(end 1.33 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1a67c14c-7d4b-4c39-bf71-6772dc3630db")
	)
	(fp_line
		(start 1.33 1.27)
		(end 1.33 49.59)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d54f9f0a-e3d0-45b5-9a22-fadbeae0fcac")
	)
	(fp_line
		(start -4.34 -1.8)
		(end 1.76 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ad1a7bb2-f61a-4a04-b53c-1eb7bce530c7")
	)
	(fp_line
		(start -4.34 50)
		(end -4.34 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "68f7b8c7-a00d-4c3a-8fb7-f01f234ec9c1")
	)
	(fp_line
		(start 1.76 -1.8)
		(end 1.76 50)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "97ee21ab-ff94-40ae-b8f6-7c9f096075c8")
	)
	(fp_line
		(start 1.76 50)
		(end -4.34 50)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b0ec0d8c-46fd-4e59-8ab4-5f0c2287ace4")
	)
	(fp_line
		(start -3.81 -1.27)
		(end 0.27 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "37f9ef61-e3b4-4220-9502-4e8990b8e46e")
	)
	(fp_line
		(start -3.81 49.53)
		(end -3.81 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "571dddb7-3616-4b88-a620-0cbf903bd15b")
	)
	(fp_line
		(start 0.27 -1.27)
		(end 1.27 -0.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "94e70cab-bf47-4a53-8da7-864580320eed")
	)
	(fp_line
		(start 1.27 -0.27)
		(end 1.27 49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ce140bdb-c9ec-498d-b325-c36e77b84579")
	)
	(fp_line
		(start 1.27 49.53)
		(end -3.81 49.53)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9e6cc8eb-4341-4135-9e96-66bda9082e59")
	)
	(fp_text user "${REFERENCE}"
		(at -1.27 24.13 90)
		(layer "F.Fab")
		(uuid "0c376928-fbe6-476e-bfec-9b60730fdd79")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "82af5557-b10b-4d73-8e29-1b83e9ba3653")
	)
	(pad "2" thru_hole oval
		(at -2.54 0)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c3083d32-e79a-490c-9f3a-8dadb71c9c6b")
	)
	(pad "3" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9a25cb22-e427-4a9b-a5a7-5d8dc74fbb8f")
	)
	(pad "4" thru_hole oval
		(at -2.54 2.54)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b6af563c-7a75-4e98-8797-3be6c74153c3")
	)
	(pad "5" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a5f03c8-b7ac-4b71-b4b4-a12756fdb1cd")
	)
	(pad "6" thru_hole oval
		(at -2.54 5.08)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1f7c1d96-1783-4bae-a625-1143a8cbfaba")
	)
	(pad "7" thru_hole oval
		(at 0 7.62)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60f8c337-df31-4168-ae24-86c42c01ec2e")
	)
	(pad "8" thru_hole oval
		(at -2.54 7.62)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1f08183a-6962-4ddc-959a-dea440be9343")
	)
	(pad "9" thru_hole oval
		(at 0 10.16)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d74f2a41-ab73-4ed0-9764-d18d376b2f43")
	)
	(pad "10" thru_hole oval
		(at -2.54 10.16)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dfa85483-2ca1-410b-a96b-911c31a406fe")
	)
	(pad "11" thru_hole oval
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a1dfbbf-688b-4dbc-a480-c15d96d5ca88")
	)
	(pad "12" thru_hole oval
		(at -2.54 12.7)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e56286b4-75ca-41a0-9d2b-558f1bcf86a7")
	)
	(pad "13" thru_hole oval
		(at 0 15.24)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c976cdb6-93ac-42dd-8846-369d684b8c65")
	)
	(pad "14" thru_hole oval
		(at -2.54 15.24)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1a3084a1-5a0e-4337-92cc-8c2d847f1116")
	)
	(pad "15" thru_hole oval
		(at 0 17.78)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4122736e-2ac9-4165-b8af-0f0ff48a8973")
	)
	(pad "16" thru_hole oval
		(at -2.54 17.78)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5c78763c-1241-478e-a798-9f1235071428")
	)
	(pad "17" thru_hole oval
		(at 0 20.32)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bd9b5f12-2e57-44de-8e03-83ec205d210d")
	)
	(pad "18" thru_hole oval
		(at -2.54 20.32)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2333de2b-67df-4a07-a377-e627ad161198")
	)
	(pad "19" thru_hole oval
		(at 0 22.86)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c2ddd7d1-28ff-4188-9973-043394866ac0")
	)
	(pad "20" thru_hole oval
		(at -2.54 22.86)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1a5cd3e5-884a-4d8d-ad4d-5fbeb499679a")
	)
	(pad "21" thru_hole oval
		(at 0 25.4)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "73646f05-e862-4ea4-9e59-219023c325d1")
	)
	(pad "22" thru_hole oval
		(at -2.54 25.4)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "277d640b-5320-406e-905e-3fab9daa2962")
	)
	(pad "23" thru_hole oval
		(at 0 27.94)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2219c263-5df5-4609-8f27-22cb2c96ba9b")
	)
	(pad "24" thru_hole oval
		(at -2.54 27.94)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "edd37785-9da4-4fca-ac3c-83044c9452c4")
	)
	(pad "25" thru_hole oval
		(at 0 30.48)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5ffb372a-870b-488c-b969-ccc6a6373bef")
	)
	(pad "26" thru_hole oval
		(at -2.54 30.48)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "620284dc-e09b-44f8-b151-a55667b91bf8")
	)
	(pad "27" thru_hole oval
		(at 0 33.02)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e79a9316-88c5-4524-aa40-cc5857027ed9")
	)
	(pad "28" thru_hole oval
		(at -2.54 33.02)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0b7301cf-5476-451b-ac68-8451eaf3b29c")
	)
	(pad "29" thru_hole oval
		(at 0 35.56)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "83d655a6-00a3-4a13-9907-e56ee5126820")
	)
	(pad "30" thru_hole oval
		(at -2.54 35.56)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "535c17bd-b60b-480d-ae92-822e2a384356")
	)
	(pad "31" thru_hole oval
		(at 0 38.1)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0b7e4c75-9353-4aec-9c82-72f30ee5082c")
	)
	(pad "32" thru_hole oval
		(at -2.54 38.1)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "76f8dcab-2506-4368-b572-2d2b8bc2b465")
	)
	(pad "33" thru_hole oval
		(at 0 40.64)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1ec833ab-549e-4970-b52c-bd3c09a4de19")
	)
	(pad "34" thru_hole oval
		(at -2.54 40.64)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bb6ef723-83b3-4431-b31f-72da440ef8a9")
	)
	(pad "35" thru_hole oval
		(at 0 43.18)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e32adc5a-cbb6-4aea-81c2-1383382757cb")
	)
	(pad "36" thru_hole oval
		(at -2.54 43.18)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "080f87c8-279f-4d46-b79f-cba34a0334f5")
	)
	(pad "37" thru_hole oval
		(at 0 45.72)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a776b95e-0edb-4286-9b26-761eb4e5fffa")
	)
	(pad "38" thru_hole oval
		(at -2.54 45.72)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2d7974da-64d2-4875-85ae-d04675041361")
	)
	(pad "39" thru_hole oval
		(at 0 48.26)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5c781816-43bb-4e2a-8578-bcc1fda17aa6")
	)
	(pad "40" thru_hole oval
		(at -2.54 48.26)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "75f7cda6-4da8-4202-8a88-ca2cfe2bb2a3")
	)
	(model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
