(footprint "RPi_Hat_Mounting_Hole"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
	(tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
	(property "Reference" ""
		(at 0 -4.0005 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "407119d4-660a-4ca5-83e2-425022d4036c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0.09906 3.59918 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "25d0bbfa-f1fa-4b15-abe0-aea98ae399ab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1c7cd95f-c5c9-4fae-b721-5ff0ed0eef72")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "af30536e-3879-4c07-9381-addf55a2fcc8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8aa8b352-b2ca-4711-b84e-ac88bdcf7f06")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 3.1 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "B.CrtYd")
		(uuid "e3a8f2cb-e27f-4332-a92e-34e3d9b0a2b3")
	)
	(fp_circle
		(center 0 0)
		(end 3.1 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "a5d091f1-74fa-4152-a0e0-22e26af97dc2")
	)
	(fp_circle
		(center 0 0)
		(end 1.375 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "B.Fab")
		(uuid "b4493c81-f46b-4c0d-8147-9ca5d0e30fe5")
	)
	(fp_circle
		(center 0 0)
		(end 3.1 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "B.Fab")
		(uuid "6f7f1041-785d-4076-9ff3-531cbed06b2d")
	)
	(fp_circle
		(center 0 0)
		(end 1.375 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "cba0b844-a829-47a0-bfe1-a8e9bf0cedf0")
	)
	(fp_circle
		(center 0 0)
		(end 3.1 0)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "8653cc36-bbb7-44d7-98f7-0aff7821bbc0")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 2.75 2.75)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 1.725)
		(clearance 1.725)
		(uuid "62d3d2fd-84d3-4b4b-b3a3-8e598da1de07")
	)
)
