(module EQFP-144-1EP_20x20mm_P0.5mm_EP6.61x5.615mm_ThermalVias (layer F.Cu) (tedit 601C1BFD)
  (descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00485-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "EQFP QFP")
  (attr smd)
  (fp_text reference REF** (at 0 -12.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value EQFP-144-1EP_20x20mm_P0.5mm_EP6.61x5.615mm_ThermalVias (at 0 12.35) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 11.65 9.15) (end 11.65 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.25 9.15) (end 11.65 9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.25 10.25) (end 10.25 9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 10.25) (end 10.25 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 11.65) (end 9.15 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 11.65) (end 9.15 11.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.65 9.15) (end -11.65 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10.25 9.15) (end -11.65 9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10.25 10.25) (end -10.25 9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.15 10.25) (end -10.25 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.15 11.65) (end -9.15 10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 11.65) (end -9.15 11.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.65 -9.15) (end 11.65 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.25 -9.15) (end 11.65 -9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.25 -10.25) (end 10.25 -9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 -10.25) (end 10.25 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 -11.65) (end 9.15 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -11.65) (end 9.15 -11.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -11.65 -9.15) (end -11.65 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10.25 -9.15) (end -11.65 -9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10.25 -10.25) (end -10.25 -9.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.15 -10.25) (end -10.25 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.15 -11.65) (end -9.15 -10.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0 -11.65) (end -9.15 -11.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10 -9) (end -9 -10) (layer F.Fab) (width 0.1))
  (fp_line (start -10 10) (end -10 -9) (layer F.Fab) (width 0.1))
  (fp_line (start 10 10) (end -10 10) (layer F.Fab) (width 0.1))
  (fp_line (start 10 -10) (end 10 10) (layer F.Fab) (width 0.1))
  (fp_line (start -9 -10) (end 10 -10) (layer F.Fab) (width 0.1))
  (fp_line (start -10.11 -9.16) (end -11.4 -9.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.11 -10.11) (end -10.11 -9.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.16 -10.11) (end -10.11 -10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.11 -10.11) (end 10.11 -9.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.16 -10.11) (end 10.11 -10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.11 10.11) (end -10.11 9.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.16 10.11) (end -10.11 10.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.11 10.11) (end 10.11 9.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 9.16 10.11) (end 10.11 10.11) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd roundrect (at -10.6625 -8.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -10.6625 -8.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -10.6625 -7.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -10.6625 -7.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at -10.6625 -6.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -10.6625 -6.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at -10.6625 -5.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at -10.6625 -5.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at -10.6625 -4.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at -10.6625 -4.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at -10.6625 -3.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at -10.6625 -3.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -10.6625 -2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -10.6625 -2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -10.6625 -1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -10.6625 -1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 17 smd roundrect (at -10.6625 -0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 18 smd roundrect (at -10.6625 -0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 19 smd roundrect (at -10.6625 0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 20 smd roundrect (at -10.6625 0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 21 smd roundrect (at -10.6625 1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 22 smd roundrect (at -10.6625 1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 23 smd roundrect (at -10.6625 2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 24 smd roundrect (at -10.6625 2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 25 smd roundrect (at -10.6625 3.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 26 smd roundrect (at -10.6625 3.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 27 smd roundrect (at -10.6625 4.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 28 smd roundrect (at -10.6625 4.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 29 smd roundrect (at -10.6625 5.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 30 smd roundrect (at -10.6625 5.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 31 smd roundrect (at -10.6625 6.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 32 smd roundrect (at -10.6625 6.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 33 smd roundrect (at -10.6625 7.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 34 smd roundrect (at -10.6625 7.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 35 smd roundrect (at -10.6625 8.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 36 smd roundrect (at -10.6625 8.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 37 smd roundrect (at -8.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 38 smd roundrect (at -8.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 39 smd roundrect (at -7.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 40 smd roundrect (at -7.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 41 smd roundrect (at -6.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 42 smd roundrect (at -6.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 43 smd roundrect (at -5.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 44 smd roundrect (at -5.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 45 smd roundrect (at -4.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 46 smd roundrect (at -4.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 47 smd roundrect (at -3.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 48 smd roundrect (at -3.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 49 smd roundrect (at -2.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 50 smd roundrect (at -2.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 51 smd roundrect (at -1.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 52 smd roundrect (at -1.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 53 smd roundrect (at -0.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 54 smd roundrect (at -0.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 55 smd roundrect (at 0.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 56 smd roundrect (at 0.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 57 smd roundrect (at 1.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 1.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 59 smd roundrect (at 2.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 60 smd roundrect (at 2.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 61 smd roundrect (at 3.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 62 smd roundrect (at 3.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 63 smd roundrect (at 4.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 64 smd roundrect (at 4.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 65 smd roundrect (at 5.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 66 smd roundrect (at 5.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 67 smd roundrect (at 6.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 68 smd roundrect (at 6.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 69 smd roundrect (at 7.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 70 smd roundrect (at 7.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 71 smd roundrect (at 8.25 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 72 smd roundrect (at 8.75 10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 73 smd roundrect (at 10.6625 8.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 74 smd roundrect (at 10.6625 8.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 75 smd roundrect (at 10.6625 7.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 76 smd roundrect (at 10.6625 7.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 77 smd roundrect (at 10.6625 6.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 78 smd roundrect (at 10.6625 6.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 79 smd roundrect (at 10.6625 5.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 80 smd roundrect (at 10.6625 5.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 81 smd roundrect (at 10.6625 4.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 82 smd roundrect (at 10.6625 4.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 83 smd roundrect (at 10.6625 3.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 84 smd roundrect (at 10.6625 3.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 85 smd roundrect (at 10.6625 2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 86 smd roundrect (at 10.6625 2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 87 smd roundrect (at 10.6625 1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 88 smd roundrect (at 10.6625 1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 89 smd roundrect (at 10.6625 0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 90 smd roundrect (at 10.6625 0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 91 smd roundrect (at 10.6625 -0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 92 smd roundrect (at 10.6625 -0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 93 smd roundrect (at 10.6625 -1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 94 smd roundrect (at 10.6625 -1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 95 smd roundrect (at 10.6625 -2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 96 smd roundrect (at 10.6625 -2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 97 smd roundrect (at 10.6625 -3.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 98 smd roundrect (at 10.6625 -3.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 99 smd roundrect (at 10.6625 -4.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 100 smd roundrect (at 10.6625 -4.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 101 smd roundrect (at 10.6625 -5.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 102 smd roundrect (at 10.6625 -5.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 103 smd roundrect (at 10.6625 -6.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 104 smd roundrect (at 10.6625 -6.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 105 smd roundrect (at 10.6625 -7.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 106 smd roundrect (at 10.6625 -7.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 107 smd roundrect (at 10.6625 -8.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 108 smd roundrect (at 10.6625 -8.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 109 smd roundrect (at 8.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 110 smd roundrect (at 8.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 111 smd roundrect (at 7.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 112 smd roundrect (at 7.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 113 smd roundrect (at 6.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 114 smd roundrect (at 6.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 115 smd roundrect (at 5.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 116 smd roundrect (at 5.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 117 smd roundrect (at 4.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 118 smd roundrect (at 4.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 119 smd roundrect (at 3.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 120 smd roundrect (at 3.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 121 smd roundrect (at 2.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 122 smd roundrect (at 2.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 123 smd roundrect (at 1.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 124 smd roundrect (at 1.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 125 smd roundrect (at 0.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 126 smd roundrect (at 0.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 127 smd roundrect (at -0.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 128 smd roundrect (at -0.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 129 smd roundrect (at -1.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 130 smd roundrect (at -1.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 131 smd roundrect (at -2.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 132 smd roundrect (at -2.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 133 smd roundrect (at -3.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 134 smd roundrect (at -3.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 135 smd roundrect (at -4.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 136 smd roundrect (at -4.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 137 smd roundrect (at -5.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 138 smd roundrect (at -5.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 139 smd roundrect (at -6.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 140 smd roundrect (at -6.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 141 smd roundrect (at -7.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 142 smd roundrect (at -7.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 143 smd roundrect (at -8.25 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 144 smd roundrect (at -8.75 -10.6625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 145 smd rect (at 0 0) (size 6.61 5.615) (layers F.Cu F.Mask))
  (pad 145 thru_hole circle (at -2.6 -2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -1.3 -2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 0 -2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 1.3 -2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 2.6 -2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -2.6 -0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -1.3 -0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 0 -0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 1.3 -0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 2.6 -0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -2.6 0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -1.3 0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 0 0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 1.3 0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 2.6 0.7) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -2.6 2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at -1.3 2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 0 2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 1.3 2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 thru_hole circle (at 2.6 2.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu))
  (pad 145 smd rect (at 0 0) (size 5.7 4.7) (layers B.Cu))
  (pad "" smd roundrect (at -1.95 -1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -1.95 0) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -1.95 1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -0.65 -1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -0.65 0) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -0.65 1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 0.65 -1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 0.65 0) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 0.65 1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 1.95 -1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 1.95 0) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at 1.95 1.4) (size 1.048094 1.128716) (layers F.Paste) (roundrect_rratio 0.238528))
  (pad "" smd roundrect (at -2.9525 -1.4) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -2.9525 0) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -2.9525 1.4) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 2.9525 -1.4) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 2.9525 0) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 2.9525 1.4) (size 0.568389 1.128716) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd custom (at -1.95 -2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.222735) (xy 0.46158 -0.222735) (xy 0.46158 0.170986) (xy 0.40983 0.222735) (xy -0.40983 0.222735)
         (xy -0.46158 0.170986)) (width 0.124934))
    ))
  (pad "" smd custom (at -0.65 -2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.222735) (xy 0.46158 -0.222735) (xy 0.46158 0.170986) (xy 0.40983 0.222735) (xy -0.40983 0.222735)
         (xy -0.46158 0.170986)) (width 0.124934))
    ))
  (pad "" smd custom (at 0.65 -2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.222735) (xy 0.46158 -0.222735) (xy 0.46158 0.170986) (xy 0.40983 0.222735) (xy -0.40983 0.222735)
         (xy -0.46158 0.170986)) (width 0.124934))
    ))
  (pad "" smd custom (at 1.95 -2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.222735) (xy 0.46158 -0.222735) (xy 0.46158 0.170986) (xy 0.40983 0.222735) (xy -0.40983 0.222735)
         (xy -0.46158 0.170986)) (width 0.124934))
    ))
  (pad "" smd custom (at -1.95 2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.170986) (xy -0.40983 -0.222735) (xy 0.40983 -0.222735) (xy 0.46158 -0.170986) (xy 0.46158 0.222735)
         (xy -0.46158 0.222735)) (width 0.124934))
    ))
  (pad "" smd custom (at -0.65 2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.170986) (xy -0.40983 -0.222735) (xy 0.40983 -0.222735) (xy 0.46158 -0.170986) (xy 0.46158 0.222735)
         (xy -0.46158 0.222735)) (width 0.124934))
    ))
  (pad "" smd custom (at 0.65 2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.170986) (xy -0.40983 -0.222735) (xy 0.40983 -0.222735) (xy 0.46158 -0.170986) (xy 0.46158 0.222735)
         (xy -0.46158 0.222735)) (width 0.124934))
    ))
  (pad "" smd custom (at 1.95 2.45375) (size 0.507938 0.507938) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.46158 -0.170986) (xy -0.40983 -0.222735) (xy 0.40983 -0.222735) (xy 0.46158 -0.170986) (xy 0.46158 0.222735)
         (xy -0.46158 0.222735)) (width 0.124934))
    ))
  (pad "" smd custom (at -2.9525 -2.45375) (size 0.465159 0.465159) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.180964 -0.181972) (xy 0.180964 -0.181972) (xy 0.180964 0.096453) (xy 0.095446 0.181972) (xy -0.180964 0.181972)
) (width 0.206461))
    ))
  (pad "" smd custom (at -2.9525 2.45375) (size 0.465159 0.465159) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.180964 -0.181972) (xy 0.095446 -0.181972) (xy 0.180964 -0.096453) (xy 0.180964 0.181972) (xy -0.180964 0.181972)
) (width 0.206461))
    ))
  (pad "" smd custom (at 2.9525 -2.45375) (size 0.465159 0.465159) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.180964 -0.181972) (xy 0.180964 -0.181972) (xy 0.180964 0.181972) (xy -0.095446 0.181972) (xy -0.180964 0.096453)
) (width 0.206461))
    ))
  (pad "" smd custom (at 2.9525 2.45375) (size 0.465159 0.465159) (layers F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.180964 -0.096453) (xy -0.095446 -0.181972) (xy 0.180964 -0.181972) (xy 0.180964 0.181972) (xy -0.180964 0.181972)
) (width 0.206461))
    ))
  (model ${KISYS3DMOD}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP6.61x5.615mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model 3d-models/EP4CE6E22C8.STEP
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 180 180))
  )
)
