{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["sheet"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"sheet","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Designator","Comment","Footprint","Quantity"]
["U13","EP4CE15F17C8N","PACKAGE_BGA:BGA-256_17.0X17.0MM_LAYOUT16X16_P1.0MM_BALL0.5MM_PAD0.4MM_NSMD",1]
["R41","25","RESISTOR_SMD:R_0402_1005METRIC",1]
["U11","ESP32-S2-WROVER-I","MAX80:ESP32-S2-WROVER",1]
["U12","DS3231M+","PACKAGE_SO:SOIC-16W_7.5X10.3MM_P1.27MM",1]
["BT1","BATTERY_CELL","MAX80:BATTERYHOLDER_KEYSTONE_103_1X20MM",0]
["J3","MICRO_SD_CARD DM3AT-SF-PEJM5","MAX80:MICROSD_HC_HIROSE_DM3AT-SF-PEJM5",0]
["C8,C10,C11,C12,C13,C14,C15,C9,C1,C17,C18,C19,C20,C21,C22,C23,C24,C27,C26,C30,C29,C31,C32,C42,C41,C43,C28","1UF","CAPACITOR_SMD:C_0402_1005METRIC",0]
["D22,D2","LED-G","LED_SMD:LED_0603_1608METRIC",0]
["DESIGNATOR","COMMENT","FOOTPRINT",0]
["J6","CONN_01X01_MALE","CONNECTOR_PINHEADER_2.54MM:PINHEADER_1X01_P2.54MM_HORIZONTAL",0]
["J4","CONN_02X20_ODD_EVEN","CONNECTOR_IDC:IDC-HEADER_2X20_P2.54MM_HORIZONTAL",0]
["J2","BARREL_JACK_SWITCH","MAX80:BARRELJACK_WUERTH_6941XX301002",0]
["J5","HDMI_C_1.3","MAX80:HDMI_MICRO-D_MOLEX_46765-2X0X",0]
["J1,J7","CONN_01X02_MALE","CONNECTOR_PINHEADER_2.54MM:PINHEADER_1X02_P2.54MM_HORIZONTAL",0]
["J8","CONN_02X5_ODD_EVEN","CONNECTOR_PINHEADER_2.54MM:PINHEADER_2X06_P2.54MM_VERTICAL",0]
["X1","ABC-BUS","MAX80:MAB64B-FAB64Q",0]