 -- Copyright (C) 2020  Intel Corporation. All rights reserved.
 -- Your use of Intel Corporation's design tools, logic functions 
 -- and other software and tools, and any partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Intel Program License 
 -- Subscription Agreement, the Intel Quartus Prime License Agreement,
 -- the Intel FPGA IP License Agreement, or other applicable license
 -- agreement, including, without limitation, that your use is for
 -- the sole purpose of programming logic devices manufactured by
 -- Intel and sold by Intel or its authorized distributors.  Please
 -- refer to the applicable agreement for further details, at
 -- https://fpgasoftware.intel.com/eula.
 -- 
 -- This is a Quartus Prime output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus Prime input file. This file cannot be used
 -- to make Quartus Prime pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus Prime help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.2V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --                  Bank 1:       3.3V
 --                  Bank 2:       3.3V
 --                  Bank 3:       3.3V
 --                  Bank 4:       3.3V
 --                  Bank 5:       2.5V
 --                  Bank 6:       3.3V
 --                  Bank 7:       3.3V
 --                  Bank 8:       3.3V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --                  It can also be used to report unused dedicated pins. The connection
 --                  on the board for unused dedicated pins depends on whether this will
 --                  be used in a future design. One example is device migration. When
 --                  using device migration, refer to the device pin-tables. If it is a
 --                  GND pin in the pin table or if it will not be used in a future design
 --                  for another purpose the it MUST be connected to GND. If it is an unused
 --                  dedicated pin, then it can be connected to a valid signal on the board
 --                  (low, high, or toggling) if that signal is required for a different
 --                  revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --                  This pin should be connected to GND. It may also be connected  to a
 --                  valid signal  on the board  (low, high, or toggling)  if that signal
 --                  is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin. Connect each pin marked GND* directly to GND
 --                  or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus Prime Version 20.1.1 Build 720 11/11/2020 SJ Lite Edition
CHIP  "max80"  ASSIGNED TO AN: EP4CE15F17C8

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
VCCIO8                       : A1        : power  :                   : 3.3V    : 8         :                
abc_int800_x                 : A2        : output : 3.3-V LVTTL       :         : 8         : Y              
abc_nmi_x                    : A3        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_dq[11]                    : A4        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_dq[8]                     : A5        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_a[9]                      : A6        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_a[7]                      : A7        : output : 3.3-V LVTTL       :         : 8         : Y              
abc_a[0]                     : A8        : input  : 3.3-V LVTTL       :         : 8         : Y              
abc_a[2]                     : A9        : input  : 3.3-V LVTTL       :         : 7         : Y              
sr_dq[7]                     : A10       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_dq[5]                     : A11       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_dq[0]                     : A12       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_ba[0]                     : A13       : output : 3.3-V LVTTL       :         : 7         : Y              
sr_a[0]                      : A14       : output : 3.3-V LVTTL       :         : 7         : Y              
sr_a[3]                      : A15       : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : A16       : power  :                   : 3.3V    : 7         :                
abc_xm_x                     : B1        : output : 3.3-V LVTTL       :         : 1         : Y              
GND                          : B2        : gnd    :                   :         :           :                
abc_int80_x                  : B3        : output : 3.3-V LVTTL       :         : 8         : Y              
abc_rdy_x                    : B4        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_dq[10]                    : B5        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_a[12]                     : B6        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_a[8]                      : B7        : output : 3.3-V LVTTL       :         : 8         : Y              
abc_a[1]                     : B8        : input  : 3.3-V LVTTL       :         : 8         : Y              
GND+                         : B9        :        :                   :         : 7         :                
sr_dq[6]                     : B10       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_dq[4]                     : B11       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_ras_n                     : B12       : output : 3.3-V LVTTL       :         : 7         : Y              
sr_ba[1]                     : B13       : output : 3.3-V LVTTL       :         : 7         : Y              
sr_a[1]                      : B14       : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : B15       : gnd    :                   :         :           :                
rtc_int_n                    : B16       : input  : 3.3-V LVTTL       :         : 6         : Y              
flash_io[0]                  : C1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
abc_a_oe                     : C2        : output : 3.3-V LVTTL       :         : 1         : Y              
GND*                         : C3        :        :                   :         : 8         :                
VCCIO8                       : C4        : power  :                   : 3.3V    : 8         :                
GND                          : C5        : gnd    :                   :         :           :                
sr_dq[14]                    : C6        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : C7        : power  :                   : 3.3V    : 8         :                
sr_a[11]                     : C8        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_a[4]                      : C9        : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : C10       : power  :                   : 3.3V    : 7         :                
sr_dq[3]                     : C11       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GND                          : C12       : gnd    :                   :         :           :                
VCCIO7                       : C13       : power  :                   : 3.3V    : 7         :                
sr_a[10]                     : C14       : output : 3.3-V LVTTL       :         : 7         : Y              
i2c_sda                      : C15       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
i2c_scl                      : C16       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
abc_a[3]                     : D1        : input  : 3.3-V LVTTL       :         : 1         : Y              
flash_cs_n                   : D2        : output : 3.3-V LVTTL       :         : 1         : Y              
sr_clk                       : D3        : output : 3.3-V LVTTL       :         : 8         : Y              
VCCD_PLL3                    : D4        : power  :                   : 1.2V    :           :                
sr_dq[15]                    : D5        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_dq[13]                    : D6        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
GND                          : D7        : gnd    :                   :         :           :                
sr_dqm[1]                    : D8        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_a[5]                      : D9        : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : D10       : gnd    :                   :         :           :                
sr_dq[2]                     : D11       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
sr_cs_n                      : D12       : output : 3.3-V LVTTL       :         : 7         : Y              
VCCD_PLL2                    : D13       : power  :                   : 1.2V    :           :                
sr_a[2]                      : D14       : output : 3.3-V LVTTL       :         : 7         : Y              
tty_cts                      : D15       : output : 3.3-V LVTTL       :         : 6         : Y              
tty_rts                      : D16       : input  : 3.3-V LVTTL       :         : 6         : Y              
abc_a[6]                     : E1        : input  : 3.3-V LVTTL       :         : 1         : Y              
GND                          : E2        : gnd    :                   :         :           :                
VCCIO1                       : E3        : power  :                   : 3.3V    : 1         :                
GND                          : E4        : gnd    :                   :         :           :                
GNDA3                        : E5        : gnd    :                   :         :           :                
sr_dq[12]                    : E6        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_dq[9]                     : E7        : bidir  : 3.3-V LVTTL       :         : 8         : Y              
sr_a[6]                      : E8        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_cas_n                     : E9        : output : 3.3-V LVTTL       :         : 7         : Y              
sr_dqm[0]                    : E10       : output : 3.3-V LVTTL       :         : 7         : Y              
sr_dq[1]                     : E11       : bidir  : 3.3-V LVTTL       :         : 7         : Y              
GNDA2                        : E12       : gnd    :                   :         :           :                
GND                          : E13       : gnd    :                   :         :           :                
VCCIO6                       : E14       : power  :                   : 3.3V    : 6         :                
rtc_32khz                    : E15       : input  : 3.3-V LVTTL       :         : 6         : Y              
tty_txd                      : E16       : input  : 3.3-V LVTTL       :         : 6         : Y              
abc_a[7]                     : F1        : input  : 3.3-V LVTTL       :         : 1         : Y              
abc_cs_n                     : F2        : input  : 3.3-V LVTTL       :         : 1         : Y              
abc_a[5]                     : F3        : input  : 3.3-V LVTTL       :         : 1         : Y              
nSTATUS                      : F4        :        :                   :         : 1         :                
VCCA3                        : F5        : power  :                   : 2.5V    :           :                
GND                          : F6        : gnd    :                   :         :           :                
VCCINT                       : F7        : power  :                   : 1.2V    :           :                
sr_cke                       : F8        : output : 3.3-V LVTTL       :         : 8         : Y              
sr_we_n                      : F9        : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : F10       : gnd    :                   :         :           :                
VCCINT                       : F11       : power  :                   : 1.2V    :           :                
VCCA2                        : F12       : power  :                   : 2.5V    :           :                
tty_rxd                      : F13       : output : 3.3-V LVTTL       :         : 6         : Y              
sd_dat[2]                    : F14       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
sd_dat[0]                    : F15       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
sd_dat[3]                    : F16       : bidir  : 3.3-V LVTTL       :         : 6         : Y              
abc_a[8]                     : G1        : input  : 3.3-V LVTTL       :         : 1         : Y              
abc_out_n[0]                 : G2        : input  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : G3        : power  :                   : 3.3V    : 1         :                
GND                          : G4        : gnd    :                   :         :           :                
abc_a[4]                     : G5        : input  : 3.3-V LVTTL       :         : 1         : Y              
VCCINT                       : G6        : power  :                   : 1.2V    :           :                
VCCINT                       : G7        : power  :                   : 1.2V    :           :                
VCCINT                       : G8        : power  :                   : 1.2V    :           :                
VCCINT                       : G9        : power  :                   : 1.2V    :           :                
VCCINT                       : G10       : power  :                   : 1.2V    :           :                
GND*                         : G11       :        :                   :         : 6         :                
MSEL2                        : G12       :        :                   :         : 6         :                
GND                          : G13       : gnd    :                   :         :           :                
VCCIO6                       : G14       : power  :                   : 3.3V    : 6         :                
sd_clk                       : G15       : output : 3.3-V LVTTL       :         : 6         : Y              
sd_cmd                       : G16       : output : 3.3-V LVTTL       :         : 6         : Y              
flash_sck                    : H1        : output : 3.3-V LVTTL       :         : 1         : Y              
flash_io[1]                  : H2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
TCK                          : H3        : input  :                   :         : 1         :                
TDI                          : H4        : input  :                   :         : 1         :                
nCONFIG                      : H5        :        :                   :         : 1         :                
VCCINT                       : H6        : power  :                   : 1.2V    :           :                
GND                          : H7        : gnd    :                   :         :           :                
GND                          : H8        : gnd    :                   :         :           :                
GND                          : H9        : gnd    :                   :         :           :                
GND                          : H10       : gnd    :                   :         :           :                
VCCINT                       : H11       : power  :                   : 1.2V    :           :                
MSEL1                        : H12       :        :                   :         : 6         :                
MSEL0                        : H13       :        :                   :         : 6         :                
CONF_DONE                    : H14       :        :                   :         : 6         :                
GND                          : H15       : gnd    :                   :         :           :                
GND                          : H16       : gnd    :                   :         :           :                
abc_a[9]                     : J1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_out_n[1]                 : J2        : input  : 3.3-V LVTTL       :         : 2         : Y              
nCE                          : J3        :        :                   :         : 1         :                
TDO                          : J4        : output :                   :         : 1         :                
TMS                          : J5        : input  :                   :         : 1         :                
VCCINT                       : J6        : power  :                   : 1.2V    :           :                
GND                          : J7        : gnd    :                   :         :           :                
GND                          : J8        : gnd    :                   :         :           :                
GND                          : J9        : gnd    :                   :         :           :                
GND                          : J10       : gnd    :                   :         :           :                
GND                          : J11       : gnd    :                   :         :           :                
GND*                         : J12       :        :                   :         : 5         :                
GND*                         : J13       :        :                   :         : 5         :                
GND*                         : J14       :        :                   :         : 5         :                
hdmi_clk                     : J15       : output : LVDS              :         : 5         : Y              
hdmi_clk(n)                  : J16       : output : LVDS              :         : 5         : N              
abc_a[11]                    : K1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_out_n[4]                 : K2        : input  : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : K3        : power  :                   : 3.3V    : 2         :                
GND                          : K4        : gnd    :                   :         :           :                
abc_out_n[2]                 : K5        : input  : 3.3-V LVTTL       :         : 2         : Y              
GND*                         : K6        :        :                   :         : 2         :                
VCCINT                       : K7        : power  :                   : 1.2V    :           :                
GND                          : K8        : gnd    :                   :         :           :                
GND*                         : K9        :        :                   :         : 4         :                
GND*                         : K10       :        :                   :         : 4         :                
VCCINT                       : K11       : power  :                   : 1.2V    :           :                
GND*                         : K12       :        :                   :         : 5         :                
GND                          : K13       : gnd    :                   :         :           :                
VCCIO5                       : K14       : power  :                   : 2.5V    : 5         :                
hdmi_d[0]                    : K15       : output : LVDS              :         : 5         : Y              
hdmi_d[0](n)                 : K16       : output : LVDS              :         : 5         : N              
abc_a[12]                    : L1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_inp_n[0]                 : L2        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_out_n[3]                 : L3        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_a[10]                    : L4        : input  : 3.3-V LVTTL       :         : 2         : Y              
VCCA1                        : L5        : power  :                   : 2.5V    :           :                
GND*                         : L6        :        :                   :         : 2         :                
gpio[0]                      : L7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
esp_io0                      : L8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : L9        :        :                   :         : 4         :                
abc_xoutpstb_n               : L10       : input  : 3.3-V LVTTL       :         : 4         : Y              
GND*                         : L11       :        :                   :         : 4         :                
VCCA4                        : L12       : power  :                   : 2.5V    :           :                
GND*                         : L13       :        :                   :         : 5         :                
GND*                         : L14       :        :                   :         : 5         :                
GND*                         : L15       :        :                   :         : 5         :                
GND*                         : L16       :        :                   :         : 5         :                
abc_a[13]                    : M1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_inp_n[1]                 : M2        : input  : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : M3        : power  :                   : 3.3V    : 2         :                
GND                          : M4        : gnd    :                   :         :           :                
GNDA1                        : M5        : gnd    :                   :         :           :                
abc_d[1]                     : M6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
spi_miso                     : M7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
spi_mosi                     : M8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND*                         : M9        :        :                   :         : 4         :                
sd_dat[1]                    : M10       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
hdmi_scl                     : M11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GNDA4                        : M12       : gnd    :                   :         :           :                
GND                          : M13       : gnd    :                   :         :           :                
VCCIO5                       : M14       : power  :                   : 2.5V    : 5         :                
clock_48                     : M15       : input  : 2.5 V             :         : 5         : Y              
GND+                         : M16       :        :                   :         : 5         :                
abc_a[15]                    : N1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_a[14]                    : N2        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_xmemfl_n                 : N3        : input  : 3.3-V LVTTL       :         : 3         : Y              
VCCD_PLL1                    : N4        : power  :                   : 1.2V    :           :                
abc_d[2]                     : N5        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
spi_cs_flash_n               : N6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : N7        : gnd    :                   :         :           :                
spi_cs_esp_n                 : N8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
exth_hb                      : N9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : N10       : gnd    :                   :         :           :                
exth_hg                      : N11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
exth_ha                      : N12       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCD_PLL4                    : N13       : power  :                   : 1.2V    :           :                
GND*                         : N14       :        :                   :         : 5         :                
hdmi_d[1]                    : N15       : output : LVDS              :         : 5         : Y              
hdmi_d[1](n)                 : N16       : output : LVDS              :         : 5         : N              
abc_xmemw800_n               : P1        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_rst_n                    : P2        : input  : 3.3-V LVTTL       :         : 2         : Y              
abc_d[0]                     : P3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P4        : power  :                   : 3.3V    : 3         :                
GND                          : P5        : gnd    :                   :         :           :                
spi_clk                      : P6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P7        : power  :                   : 3.3V    : 3         :                
esp_int                      : P8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
gpio[1]                      : P9        : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : P10       : power  :                   : 3.3V    : 4         :                
GND*                         : P11       :        :                   :         : 4         :                
GND                          : P12       : gnd    :                   :         :           :                
VCCIO4                       : P13       : power  :                   : 3.3V    : 4         :                
tty_dtr                      : P14       : input  : 3.3-V LVTTL       :         : 4         : Y              
GND*                         : P15       :        :                   :         : 5         :                
hdmi_d[2](n)                 : P16       : output : LVDS              :         : 5         : N              
abc_xmemw80_n                : R1        : input  : 3.3-V LVTTL       :         : 2         : Y              
GND                          : R2        : gnd    :                   :         :           :                
abc_d[4]                     : R3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_d[6]                     : R4        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_d_oe                     : R5        : output : 3.3-V LVTTL       :         : 3         : Y              
abc_resin_x                  : R6        : output : 3.3-V LVTTL       :         : 3         : Y              
gpio[5]                      : R7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
exth_hh                      : R8        : input  : 3.3-V LVTTL       :         : 3         : Y              
GND+                         : R9        :        :                   :         : 4         :                
gpio[3]                      : R10       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
exth_hd                      : R11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
exth_he                      : R12       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
hdmi_sda                     : R13       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
led[2]                       : R14       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : R15       : gnd    :                   :         :           :                
hdmi_d[2]                    : R16       : output : LVDS              :         : 5         : Y              
VCCIO3                       : T1        : power  :                   : 3.3V    : 3         :                
abc_d[3]                     : T2        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_d[5]                     : T3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_d[7]                     : T4        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_d_ce_n                   : T5        : output : 3.3-V LVTTL       :         : 3         : Y              
gpio[2]                      : T6        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
gpio[4]                      : T7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
abc_clk                      : T8        : input  : 3.3-V LVTTL       :         : 3         : Y              
exth_hc                      : T9        : input  : 3.3-V LVTTL       :         : 4         : Y              
abc_host                     : T10       : output : 3.3-V LVTTL       :         : 4         : Y              
exth_hf                      : T11       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
abc_xinpstb_n                : T12       : input  : 3.3-V LVTTL       :         : 4         : Y              
led[0]                       : T13       : output : 3.3-V LVTTL       :         : 4         : Y              
led[1]                       : T14       : output : 3.3-V LVTTL       :         : 4         : Y              
hdmi_hpd                     : T15       : bidir  : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : T16       : power  :                   : 3.3V    : 4         :                
