# -*- tcl -*-

set_global_assignment -name SOURCE_FILE v2.pins
set_global_assignment -name VERILOG_FILE ip/pll2_16.v
set_global_assignment -name QIP_FILE ip/pll2_16.qip
set_global_assignment -name VERILOG_INCLUDE_FILE v2.vh

set_global_assignment -name SOURCE_TCL_SCRIPT_FILE max80.qsf

set_instance_assignment -name IO_STANDARD "BUS LVDS" -to usb_rx
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to usb_rx
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to usb_dp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to usb_dn
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to usb_pu

set_instance_assignment -name TERMINATION OFF -to usb_rx

set_instance_assignment -name IO_STANDARD "2.5 V" -to sd_cd_n
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to sd_cd_n
