# -*- tcl -*-

set_global_assignment -name TOP_LEVEL_ENTITY v1
set_global_assignment -name SOURCE_FILE v1.pins
set_global_assignment -name SYSTEMVERILOG_FILE v1.sv
set_global_assignment -name VERILOG_FILE ip/pll2_48.v
set_global_assignment -name QIP_FILE ip/pll2_48.qip
set_global_assignment -name SOURCE_FILE "output/v1.jic.cof"

set_global_assignment -name SOURCE_TCL_SCRIPT_FILE max80.qsf

set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to gpio[1]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to gpio[3]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to gpio[5]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_clk
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_inp_n[1]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_a[13]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_a[2]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_a[6]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_a[0]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to abc_a[1]
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to tty_txd
