(footprint "QFN-80_EP_10x10_Pitch0.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "U5"
		(at 0 -6.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d431a32d-f9a5-4e15-8188-6dd0fc3aa174")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.125)
			)
		)
	)
	(property "Value" "RP235x-B"
		(at 0 0 270)
		(unlocked yes)
		(layer "Eco1.User")
		(hide yes)
		(uuid "d498eb67-0eab-429d-9f4f-946933cbb6c0")
		(effects
			(font
				(size 1 1)
				(thickness 0.12)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "64e15dcb-d66b-4e06-b7ac-056cf0028264")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9193dbb4-e8bc-4eee-ac89-c34b829a6e39")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Digikey" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d4cf195d-a4c3-4beb-9319-1ffbcbe73a12")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MOUSER" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "83813c42-4a46-4390-a9ef-83c46d9b4395")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Supplier" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aedfae49-2da3-4bd0-87b1-ee577b172003")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C42415655"
		(at 0 0 90)
		(layer "F.SilkS")
		(hide yes)
		(uuid "71725ca6-b950-4b54-b689-1ef096048b2f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(clearance 0.1)
	(attr smd)
	(fp_line
		(start -5.15 5.15)
		(end -5.149999 4.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2fe045af-a38d-4332-936a-6b6c9c6c6a6d")
	)
	(fp_line
		(start -4.2 -5.149999)
		(end -5.375 -5.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2d3f4a45-ac32-40a8-9e13-d5262b8dfe9d")
	)
	(fp_line
		(start -4.2 5.149999)
		(end -5.15 5.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3e4412ce-53f2-4a49-8c19-167802438ab0")
	)
	(fp_line
		(start 4.2 -5.149999)
		(end 5.15 -5.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "976c13a5-50a1-4a79-8b13-5fd5f11ca6a9")
	)
	(fp_line
		(start 4.2 5.149999)
		(end 5.15 5.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cc1f270b-83db-4629-8a32-1ecfcb322039")
	)
	(fp_line
		(start 5.15 -5.15)
		(end 5.149999 -4.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "af419716-2e63-4dc2-997a-9e54c3b59b7a")
	)
	(fp_line
		(start 5.15 5.15)
		(end 5.149999 4.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c65aa1f2-9c56-43ef-a0ee-0e7c567f4235")
	)
	(fp_line
		(start -5.6 -5.6)
		(end 5.6 -5.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4fa1c6ce-115a-4ec8-ac52-622be9af7910")
	)
	(fp_line
		(start -5.6 5.6)
		(end -5.6 -5.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9fcf008d-f20e-4f3f-b354-4d7a5cdd9e18")
	)
	(fp_line
		(start 5.6 -5.6)
		(end 5.6 5.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f59a08fe-af49-423f-91c5-4b2911a8f36b")
	)
	(fp_line
		(start 5.6 5.6)
		(end -5.6 5.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cd55d857-2c7b-46c0-85a8-755376df8f5b")
	)
	(fp_line
		(start -5 -4)
		(end -5 5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "13dc1204-4e1c-4fac-9a4a-eb1a18f7aff9")
	)
	(fp_line
		(start -5 5)
		(end 5 5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b12cd883-15ee-4bb5-932b-b2ed5785f579")
	)
	(fp_line
		(start -4 -5)
		(end -5 -4)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "eecf577f-fe06-44ec-9641-878bd2082f4d")
	)
	(fp_line
		(start 5 -5)
		(end -4 -5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "84be044f-7d13-4e9a-8868-36b8d395f6cc")
	)
	(fp_line
		(start 5 5)
		(end 5 -5)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f63dabdf-f47a-4219-bc71-acfd65f02678")
	)
	(pad "" smd rect
		(at 0 0)
		(size 2.8 2.8)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a0b101a6-dbe6-4344-a24f-1e1458349e5a")
	)
	(pad "1" smd rect
		(at -4.9 -3.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e57985e3-7315-411f-945d-864879d97b6a")
	)
	(pad "2" smd rect
		(at -4.9 -3.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f2222f4c-c91a-4fb5-9c74-cefd94288b10")
	)
	(pad "3" smd rect
		(at -4.9 -3 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "89fd9d94-d407-4f81-8810-c81f47950287")
	)
	(pad "4" smd rect
		(at -4.9 -2.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ed10123b-7f4c-4f62-9123-ebe07e4ce17a")
	)
	(pad "5" smd rect
		(at -4.9 -2.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "57868461-1332-4c1f-b859-df745f22731f")
	)
	(pad "6" smd rect
		(at -4.9 -1.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "20c8e942-830e-48eb-9988-e77a1972814f")
	)
	(pad "7" smd rect
		(at -4.9 -1.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b188fb51-6867-486b-bf79-ea795971e3c7")
	)
	(pad "8" smd rect
		(at -4.9 -1 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d8a825b5-205d-403a-9e3a-8106fc38c391")
	)
	(pad "9" smd rect
		(at -4.9 -0.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "56ef1ac4-e8ea-435c-a4ea-be19d69b953c")
	)
	(pad "10" smd rect
		(at -4.9 -0.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8d7dd455-e413-444b-92b5-f2095478dea9")
	)
	(pad "11" smd rect
		(at -4.9 0.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "250af62b-9f37-4b1c-a513-464cec523fb9")
	)
	(pad "12" smd rect
		(at -4.9 0.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "245a4b64-bbb3-43f3-aca5-5f89c73dcc44")
	)
	(pad "13" smd rect
		(at -4.9 1 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f6d8fc51-0a10-4b0e-a736-8575312cd438")
	)
	(pad "14" smd rect
		(at -4.9 1.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "5548dc0c-a7d9-4bdb-a1c1-54401f8b9a0b")
	)
	(pad "15" smd rect
		(at -4.9 1.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a72565ec-5670-499a-86c9-caab95ab8caa")
	)
	(pad "16" smd rect
		(at -4.9 2.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "10a68cc5-4c64-4669-81f2-7e6ad7f094bf")
	)
	(pad "17" smd rect
		(at -4.9 2.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "632d1c70-3a9d-490d-97c6-ec006910d05c")
	)
	(pad "18" smd rect
		(at -4.9 3 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ee11d3cd-a431-4df2-9a00-827f8ebc6948")
	)
	(pad "19" smd rect
		(at -4.9 3.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "88704938-353a-490c-afd3-85795a9c15af")
	)
	(pad "20" smd rect
		(at -4.9 3.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "80eadde2-293e-4ece-8ee4-f358b1ead5c0")
	)
	(pad "21" smd rect
		(at -3.8 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8a93614c-b585-4f80-b1af-253b5efe98e8")
	)
	(pad "22" smd rect
		(at -3.4 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "4ac21959-dae1-4ab8-8aec-0edd91cdfcc3")
	)
	(pad "23" smd rect
		(at -3 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e797ed48-9b39-42d2-8aa7-dadaf77b0691")
	)
	(pad "24" smd rect
		(at -2.6 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "6901f04f-7b7c-432c-8a35-3a9c80a3ec37")
	)
	(pad "25" smd rect
		(at -2.2 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f76f5402-a376-4248-ae33-f15b8e44be91")
	)
	(pad "26" smd rect
		(at -1.8 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a8e60bbe-1346-4b63-aedf-7aac86117adf")
	)
	(pad "27" smd rect
		(at -1.4 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "93bce65a-f729-4602-9054-c37c9be157d6")
	)
	(pad "28" smd rect
		(at -1 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8c64dd71-aa83-48db-8b2d-5df28db2e13f")
	)
	(pad "29" smd rect
		(at -0.6 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a4e34469-5d12-4a01-8736-205408c1cae5")
	)
	(pad "30" smd rect
		(at -0.2 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7af5af66-6bfe-4275-9bf2-5f98d838b1f4")
	)
	(pad "31" smd rect
		(at 0.2 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ccdb6dd1-ace0-4d19-918d-514fc3d88ed2")
	)
	(pad "32" smd rect
		(at 0.6 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a09e1490-6839-4fa0-89fc-496e55683ee9")
	)
	(pad "33" smd rect
		(at 1 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c2670760-e077-4110-bf97-6d3e6fa2549d")
	)
	(pad "34" smd rect
		(at 1.4 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "fd866dde-dc9a-46db-9429-18909b30c596")
	)
	(pad "35" smd rect
		(at 1.8 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "de047831-6c34-4b66-8e42-945f4a951921")
	)
	(pad "36" smd rect
		(at 2.2 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "38283879-5f1d-482b-b561-16bf78e19c99")
	)
	(pad "37" smd rect
		(at 2.6 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ec52add4-221d-4744-b4da-ffdeb5ab5e59")
	)
	(pad "38" smd rect
		(at 3 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1db227bd-bd40-49f6-9a9c-446833f7b009")
	)
	(pad "39" smd rect
		(at 3.4 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2b852432-e89c-4c85-9d8a-d8075589702c")
	)
	(pad "40" smd rect
		(at 3.8 4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "06c6abdf-20c9-4336-a785-7e194de4abb3")
	)
	(pad "41" smd rect
		(at 4.9 3.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c626c44f-bc9a-4fa7-92f4-13df2aa75761")
	)
	(pad "42" smd rect
		(at 4.9 3.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "59302f62-4b5d-41c1-9eb0-b283bb1f2284")
	)
	(pad "43" smd rect
		(at 4.9 3 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e4b9d131-4ad6-4c91-9811-e9bfcb57d6f7")
	)
	(pad "44" smd rect
		(at 4.9 2.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "82c585f6-7b71-4463-8c74-abbc6be07e7e")
	)
	(pad "45" smd rect
		(at 4.9 2.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "239727c0-b4ae-47ea-a8c1-f6a56e28365a")
	)
	(pad "46" smd rect
		(at 4.9 1.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "48608a9c-8b3a-4277-b436-4f4342f719c6")
	)
	(pad "47" smd rect
		(at 4.9 1.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f382d311-8a6c-4c58-9538-5ae9a269cd5c")
	)
	(pad "48" smd rect
		(at 4.9 1 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "90f470fa-8e43-4a2a-8e99-6fc6afcecefd")
	)
	(pad "49" smd rect
		(at 4.9 0.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2fe36a55-5f03-4c2c-b6c3-089299c23676")
	)
	(pad "50" smd rect
		(at 4.9 0.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c60730c6-2f96-4488-ae4f-845c4761faed")
	)
	(pad "51" smd rect
		(at 4.9 -0.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "79f3ae61-0762-462c-859c-78ec4b929439")
	)
	(pad "52" smd rect
		(at 4.9 -0.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9546cac6-d7ff-4b7a-acf3-2c8ab3d12cae")
	)
	(pad "53" smd rect
		(at 4.9 -1 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "55df2c32-eb0f-4eac-a8cb-7705d95cdd0f")
	)
	(pad "54" smd rect
		(at 4.9 -1.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "93ba855a-fa64-4763-841f-97e73c1c9bbf")
	)
	(pad "55" smd rect
		(at 4.9 -1.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b527e956-ae40-4836-b811-82a6771daef4")
	)
	(pad "56" smd rect
		(at 4.9 -2.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f2fd7878-d415-4453-924d-47388f06e8f6")
	)
	(pad "57" smd rect
		(at 4.9 -2.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9e7a3301-e598-474e-82ec-9d58fe18efec")
	)
	(pad "58" smd rect
		(at 4.9 -3 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "50d04c65-b5a0-4ef0-9a85-73ee1222cdc7")
	)
	(pad "59" smd rect
		(at 4.9 -3.4 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "8e1af173-f67b-4c41-9af4-f38170d085a1")
	)
	(pad "60" smd rect
		(at 4.9 -3.8 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d11cf21c-d6f6-4830-bfbf-bba216eeb42b")
	)
	(pad "61" smd rect
		(at 3.8 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "aa8a00b2-2f6f-483e-bc04-7961679faeb8")
	)
	(pad "62" smd rect
		(at 3.4 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "4c132875-1975-458d-94e4-d94067a34889")
	)
	(pad "63" smd rect
		(at 3 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3bd676be-fea6-4229-8bd0-66646c62453d")
	)
	(pad "64" smd rect
		(at 2.6 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "63b7396b-1d37-476f-aeb7-b71aa365c7f6")
	)
	(pad "65" smd rect
		(at 2.2 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "5b9bc767-b1b7-4904-9ae0-8844c73f26b3")
	)
	(pad "66" smd rect
		(at 1.8 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3688ed34-de8d-4414-bdd1-2b8e88445543")
	)
	(pad "67" smd rect
		(at 1.4 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1804e805-a1dd-4bde-b2cd-3177c0eda978")
	)
	(pad "68" smd rect
		(at 1 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "468c25d7-3415-4da8-a15f-2bccf1ec3367")
	)
	(pad "69" smd rect
		(at 0.6 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "14cd3286-7b0d-4b90-9542-041d903ad491")
	)
	(pad "70" smd rect
		(at 0.2 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d6604437-b39a-4a76-bf4a-b25d3c73d1b3")
	)
	(pad "71" smd rect
		(at -0.2 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "68ceeaa7-a1a0-4d69-9ce4-7e05e74b1ff1")
	)
	(pad "72" smd rect
		(at -0.6 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f831f4a1-f71e-4a08-8edf-f742c98852cb")
	)
	(pad "73" smd rect
		(at -1 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c81884e0-56b1-412f-b12d-2cde9fa92e51")
	)
	(pad "74" smd rect
		(at -1.4 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "62c0092d-44b0-4563-b7bb-d8ddc2bfb8bf")
	)
	(pad "75" smd rect
		(at -1.8 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2007bd4b-4070-40e5-9128-1a1df543a059")
	)
	(pad "76" smd rect
		(at -2.2 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2fadcb56-a884-4b09-81c2-2506da268e8f")
	)
	(pad "77" smd rect
		(at -2.6 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "9e16a74e-849a-4658-9212-b1a0ee8cac0c")
	)
	(pad "78" smd rect
		(at -3 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "89ae3b05-bb9e-4ee2-8147-cacb66fd55f1")
	)
	(pad "79" smd rect
		(at -3.4 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "65609248-bd3a-49db-bfea-65130d4c1102")
	)
	(pad "80" smd rect
		(at -3.8 -4.9)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ff781d74-2fc5-4140-9cfb-ae5ff5592e31")
	)
	(pad "81" smd rect
		(at 0 0)
		(size 3.4 3.4)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "1156afd5-4b27-4bd5-91b8-db95379a43a2")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3d-models/QFN-80-1EP_10x10mm_P0.4mm_EP3.4x3.4mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
