(footprint "LGA_9151_12.1x11.1mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.55 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a34b5a33-9225-497d-80a2-259eb3c194e6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LGA_9151_12.1x11.1mm"
		(at 0 6.55 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d7f09f16-9479-4e25-a74b-59460baf9dcb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "LGA_9151_12.1x11.1mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4f113327-1341-4645-80ef-86eef4224b23")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "62d2dbbd-b221-4e22-bb49-c26c250dbe19")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9bd8c925-c178-4404-8c85-e8d7c8fd70e9")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.17 -4.55)
		(end -6.17 -2.895)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d91bcf0b-d0ac-4f5f-ae5e-56664696538e")
	)
	(fp_line
		(start -6.17 5.67)
		(end -6.17 2.895)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "23ff2a68-157f-455d-aa18-8f090c5fe814")
	)
	(fp_line
		(start -3.145 -5.67)
		(end -5.05 -5.67)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "32dffab3-c8c7-432b-89b8-50ba718fc248")
	)
	(fp_line
		(start -3.145 5.67)
		(end -6.17 5.67)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c0562a8a-743e-46f2-983e-efbfcd982960")
	)
	(fp_line
		(start 3.145 -5.67)
		(end 6.17 -5.67)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "909bd79e-071b-441f-84fc-1cb9ca30ba3a")
	)
	(fp_line
		(start 3.145 5.67)
		(end 6.17 5.67)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f94db197-5623-421b-940f-7a83ceef6a65")
	)
	(fp_line
		(start 6.17 -5.67)
		(end 6.17 -2.895)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "08b10156-2a4a-4efe-aed9-1788bc4e1697")
	)
	(fp_line
		(start 6.17 5.67)
		(end 6.17 2.895)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b2e3277d-7dad-414a-9086-50e72b938e52")
	)
	(fp_circle
		(center -6.7 -5.55)
		(end -6.7 -5.45)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "83d5fcfc-bcc5-48fe-9760-62339c521401")
	)
	(fp_line
		(start -6.3 -5.8)
		(end 6.3 -5.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5b4d0b9d-8d47-4bb1-a3e0-43639244b4cc")
	)
	(fp_line
		(start -6.3 5.8)
		(end -6.3 -5.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "962f74df-4145-4207-8cc0-dea9bd624bb7")
	)
	(fp_line
		(start 6.3 -5.8)
		(end 6.3 5.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3ae7f570-8755-412d-81fb-8fc239e09a08")
	)
	(fp_line
		(start 6.3 5.8)
		(end -6.3 5.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cde3290b-5997-4154-81a3-72a7a8abafdc")
	)
	(fp_line
		(start -6.05 -4.55)
		(end -6.05 5.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "440c7312-6421-498a-b429-af8a2a27fa37")
	)
	(fp_line
		(start -6.05 5.55)
		(end 6.05 5.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d2209a90-dd20-497c-86cc-382efe7d5ca1")
	)
	(fp_line
		(start -5.05 -5.55)
		(end -6.05 -4.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "64ceee8e-3179-492a-8164-aa1b4638004f")
	)
	(fp_line
		(start 6.05 -5.55)
		(end -5.05 -5.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4e4b043b-c20f-4254-9ee8-4963b7de93b7")
	)
	(fp_line
		(start 6.05 5.55)
		(end 6.05 -5.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "01e7d52d-be3f-4c23-8214-06169ee483cc")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7c1481e4-f508-4381-a609-2199db4fc843")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -5.5 -5)
		(size 0.65 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(chamfer_ratio 0.2)
		(chamfer bottom_right)
		(thermal_bridge_angle 45)
		(uuid "e8bfcd97-d224-40dd-af15-2cdbecc1eb9e")
	)
	(pad "2" smd roundrect
		(at -5.6 -4.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "3966ab63-e5ad-4798-a709-a83f4d59aa04")
	)
	(pad "3" smd roundrect
		(at -5.6 -3.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "8339a8d9-9caf-42f8-9e7e-7a8e5876e33e")
	)
	(pad "4" smd roundrect
		(at -5.6 -3.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f71e94a2-c009-454d-9965-32f31bb1a300")
	)
	(pad "5" smd roundrect
		(at -5.6 -2.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e847e50d-7c69-43c0-aca6-7fcb5f9ff24a")
	)
	(pad "6" smd roundrect
		(at -5.6 -2.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2af32730-6fe5-408e-8b4c-97d98a10732d")
	)
	(pad "7" smd roundrect
		(at -5.6 -1.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2ab4152c-4493-4446-8f62-c0322f806988")
	)
	(pad "8" smd roundrect
		(at -5.6 -1.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "40278b18-5e4b-4ea8-8df9-0e5b3ac6cbb5")
	)
	(pad "9" smd roundrect
		(at -5.6 -0.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2f9ddf06-1161-4650-aee0-c06cb9b80bc9")
	)
	(pad "10" smd roundrect
		(at -5.6 -0.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "73ad2be8-117d-4604-8872-0ac21443bc6a")
	)
	(pad "11" smd roundrect
		(at -5.6 0.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "9a2847b2-3818-41f5-822d-6c7789a6de3e")
	)
	(pad "12" smd roundrect
		(at -5.6 0.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "172260f2-2fd5-48ba-87ea-f4032fbd503f")
	)
	(pad "13" smd roundrect
		(at -5.6 1.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a2c0b324-9457-4d6a-8d27-df2577a92ff1")
	)
	(pad "14" smd roundrect
		(at -5.6 1.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "6267dd6b-c554-4d65-aabe-883d17a51bd0")
	)
	(pad "15" smd roundrect
		(at -5.6 2.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "35fb6a53-3623-4c98-a025-dd34e4b1fd6f")
	)
	(pad "16" smd roundrect
		(at -5.6 2.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "78d4d8cc-d855-4c19-be9c-2ac55a95fbfe")
	)
	(pad "17" smd roundrect
		(at -5.6 3.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "237222c7-1e6a-401d-895d-7b40f8890b54")
	)
	(pad "18" smd roundrect
		(at -5.6 3.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "20bc3a14-ac6f-4572-8117-401117442fa7")
	)
	(pad "19" smd roundrect
		(at -5.6 4.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "4734ffbb-59bd-4558-9c39-462ef06c90ac")
	)
	(pad "20" smd roundrect
		(at -5.5 5)
		(size 0.65 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "1974be04-b22c-40dc-a2a3-3f2d819ae0ae")
	)
	(pad "21" smd roundrect
		(at -4.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "5104a586-badf-4788-a28e-3181092b063b")
	)
	(pad "22" smd roundrect
		(at -4.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "dcd2dc33-a8cf-4c96-b6d4-53a96ac57f6c")
	)
	(pad "23" smd roundrect
		(at -3.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "29b059fc-2c8d-4250-a889-6afc2fc15809")
	)
	(pad "24" smd roundrect
		(at -3.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "c1a1b9cc-22da-4bc7-acad-b40e4ad5d247")
	)
	(pad "25" smd roundrect
		(at -2.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "8ea1f69a-4145-46a4-a172-d1713f125891")
	)
	(pad "26" smd roundrect
		(at -2.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "dab419c0-fbb3-4768-a79f-bdb2442c2213")
	)
	(pad "27" smd roundrect
		(at -1.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "be4e3906-30fe-4f3f-96fc-eecd8a9359b5")
	)
	(pad "28" smd roundrect
		(at -1.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a4dc1815-a978-4f26-b0d2-37e31a0dd748")
	)
	(pad "29" smd roundrect
		(at -0.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e6e94f89-6c60-4b00-98bf-1618b805a247")
	)
	(pad "30" smd roundrect
		(at -0.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "bd22994a-f505-4ba7-88f0-91a9cf0cf2d8")
	)
	(pad "31" smd roundrect
		(at 0.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "1a1005bd-b7c7-45f2-95dc-edd21ffab327")
	)
	(pad "32" smd roundrect
		(at 0.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "3dac5429-7814-4d78-b905-a9b3d5b6d67f")
	)
	(pad "33" smd roundrect
		(at 1.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "5802ff71-b9b1-4ef6-9dfe-25ab4408d08c")
	)
	(pad "34" smd roundrect
		(at 1.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f4620d35-6d83-42b4-ba35-46067e30d93b")
	)
	(pad "35" smd roundrect
		(at 2.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a85dc75d-fc13-4d15-837e-612b3a050eb6")
	)
	(pad "36" smd roundrect
		(at 2.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "8752ee89-b1d5-451c-8d0b-20085c36cecb")
	)
	(pad "37" smd roundrect
		(at 3.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "926a126c-ee93-4ced-a153-523c0bdf746a")
	)
	(pad "38" smd roundrect
		(at 3.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "300f16b3-b300-4b44-b339-d935c4e09b39")
	)
	(pad "39" smd roundrect
		(at 4.25 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e38c1534-8ebf-44fe-b3b0-de781deaeafa")
	)
	(pad "40" smd roundrect
		(at 4.75 5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2b390cec-c359-4b7f-bc67-e32ad68f6adc")
	)
	(pad "41" smd roundrect
		(at 5.5 5)
		(size 0.65 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e9e5eb5b-eea3-4a93-ac11-675ce13b1135")
	)
	(pad "42" smd roundrect
		(at 5.6 4.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f06cefdd-7809-4d09-a294-40784c717f44")
	)
	(pad "43" smd roundrect
		(at 5.6 3.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f3e300c8-f380-44f0-8e0d-50011186e516")
	)
	(pad "44" smd roundrect
		(at 5.6 3.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "6f818563-3939-4d4f-8e2d-94ce117b6dd1")
	)
	(pad "45" smd roundrect
		(at 5.6 2.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "61114e97-3a60-4d67-ae9e-60d1e8bfa45c")
	)
	(pad "46" smd roundrect
		(at 5.6 2.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "42809765-4901-467e-b483-bf97177df9cb")
	)
	(pad "47" smd roundrect
		(at 5.6 1.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "29d71ef6-e629-4216-9e52-2672bb692d58")
	)
	(pad "48" smd roundrect
		(at 5.6 1.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f867701f-5dc9-4390-8341-849e28c9b7d4")
	)
	(pad "49" smd roundrect
		(at 5.6 0.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "0f867f2c-80ca-4012-84fd-1df5bd80528c")
	)
	(pad "50" smd roundrect
		(at 5.6 0.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "fae737e6-c5df-49ab-a1b9-6c7fdfca4059")
	)
	(pad "51" smd roundrect
		(at 5.6 -0.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "4ea37c3e-c6b5-4b8a-aba9-8bb647aaf4f4")
	)
	(pad "52" smd roundrect
		(at 5.6 -0.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "0b5c2053-961b-41d6-a08c-0edb23a33acb")
	)
	(pad "53" smd roundrect
		(at 5.6 -1.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "ce430ac7-e8ec-40b3-9d7c-25de527dc57b")
	)
	(pad "54" smd roundrect
		(at 5.6 -1.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "eb303a95-f54a-4d20-af09-85333b81b29a")
	)
	(pad "55" smd roundrect
		(at 5.6 -2.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "585a56c4-484f-407e-b379-bea0f608eca2")
	)
	(pad "56" smd roundrect
		(at 5.6 -2.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "3e414e09-0d27-4961-8a8a-a941bf933127")
	)
	(pad "57" smd roundrect
		(at 5.6 -3.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "392e1c66-3cb0-4bee-914e-d405d73a51e6")
	)
	(pad "58" smd roundrect
		(at 5.6 -3.75 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "5a77b4de-e432-4adb-a7b0-cd06f9feb21d")
	)
	(pad "59" smd roundrect
		(at 5.6 -4.25 90)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "ac25538b-6755-4d06-9f0a-b160cbb3873b")
	)
	(pad "60" smd roundrect
		(at 5.5 -5)
		(size 0.65 0.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "5b0cbb0d-f26f-40cf-b73d-7eaa475632d2")
	)
	(pad "61" smd roundrect
		(at 4.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "af5aa821-8634-4e16-a682-844408721635")
	)
	(pad "62" smd roundrect
		(at 4.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "c24b810a-1dc0-4efb-8852-7ffbd5e5b8c5")
	)
	(pad "63" smd roundrect
		(at 3.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e251f307-15a1-4dbf-b249-5a9ffc202225")
	)
	(pad "64" smd roundrect
		(at 3.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "88e13846-6f77-4f30-bd7c-085161d2cd5e")
	)
	(pad "65" smd roundrect
		(at 2.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "b5f957c9-7797-4eff-8048-546047ace25e")
	)
	(pad "66" smd roundrect
		(at 2.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "c63ce789-0c40-4c45-88e8-426e33b0f266")
	)
	(pad "67" smd roundrect
		(at 1.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2b406a47-a71e-4961-92a3-43b5693f0c7e")
	)
	(pad "68" smd roundrect
		(at 1.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "9d037f94-ecb5-4d22-9fa1-ded73a941499")
	)
	(pad "69" smd roundrect
		(at 0.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "cd286942-3a3f-4d10-a71d-73c19962d2b2")
	)
	(pad "70" smd roundrect
		(at 0.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "09064a38-adcd-40f6-b65f-58e1f6a7cf71")
	)
	(pad "71" smd roundrect
		(at -0.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "dd8bed84-1788-439a-91d2-4b142be5b083")
	)
	(pad "72" smd roundrect
		(at -0.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "681e6d36-3ef3-4069-bf7c-aff1bad84f7a")
	)
	(pad "73" smd roundrect
		(at -1.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "58562b30-b120-4f59-99b7-9416579e7812")
	)
	(pad "74" smd roundrect
		(at -1.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e1c21209-9ef8-42d3-b021-95cabe901228")
	)
	(pad "75" smd roundrect
		(at -2.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2d469631-5a81-4462-9563-64412ec4c4fb")
	)
	(pad "76" smd roundrect
		(at -2.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "83e5731f-3a28-4be9-9c4c-f690214c46af")
	)
	(pad "77" smd roundrect
		(at -3.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "61c72ea1-06de-40e7-9b6c-28b713aafd5f")
	)
	(pad "78" smd roundrect
		(at -3.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "45c99a87-f0b6-49e2-b0be-33b78f493ce9")
	)
	(pad "79" smd roundrect
		(at -4.25 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "4772b4e2-cc70-4e1a-9439-4ffef4483224")
	)
	(pad "80" smd roundrect
		(at -4.75 -5.1)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a6022d7b-bc2d-4e01-beb0-da8db9e45fbd")
	)
	(pad "81" smd roundrect
		(at -4.1 -3.4)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "1b239cbd-8453-44cc-91c4-74ccc4546da6")
	)
	(pad "82" smd roundrect
		(at -4.1 -2.85)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "92dc8888-6f19-4c94-bf46-dd1f634fcdb6")
	)
	(pad "83" smd roundrect
		(at -4.1 -2.3)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f518a2ac-6f4c-402a-b1f6-7b3cd7616c19")
	)
	(pad "84" smd roundrect
		(at -4.1 -0.55)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "8c4085c7-d18f-43af-b6d8-f8f1d2eb81f6")
	)
	(pad "85" smd roundrect
		(at -4.1 0)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "39163ea9-6e1c-4553-864e-c60916b7663c")
	)
	(pad "86" smd roundrect
		(at -4.1 0.55)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "49e3d5ea-24de-4aa5-8583-5a38a3700ada")
	)
	(pad "87" smd roundrect
		(at -4.1 2.3)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "aad8fff4-5aaf-4cca-a82c-60b55ce49b27")
	)
	(pad "88" smd roundrect
		(at -4.1 2.85)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "d3ea5e8a-89a9-4f0c-8de2-2bfea9a34628")
	)
	(pad "89" smd roundrect
		(at -4.1 3.4)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "9bbb5689-b112-4dee-b362-ae748c42ced8")
	)
	(pad "90" smd roundrect
		(at -0.55 2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "13a3e551-ecef-4af7-abf9-efccd3090c57")
	)
	(pad "91" smd roundrect
		(at 0 2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2480415f-cd75-4fcf-9c85-adffb780340d")
	)
	(pad "92" smd roundrect
		(at 0.55 2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "fd5b92b7-3077-4d94-bb78-6167a3ef0a74")
	)
	(pad "93" smd roundrect
		(at 4.1 3.4)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "f43e07e4-9c8e-43b7-9c43-5146c7bf4ac9")
	)
	(pad "94" smd roundrect
		(at 4.1 2.85)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a6c4da86-bb9a-48ef-8217-a86883e11972")
	)
	(pad "95" smd roundrect
		(at 4.1 2.3)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "cf1aadfc-2564-4c84-a19b-8e512ca72f6d")
	)
	(pad "96" smd roundrect
		(at 4.1 0.55)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "79cd601f-ffdd-484f-8778-729a261ea6c3")
	)
	(pad "97" smd roundrect
		(at 4.1 0)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "dce614d6-960f-4e69-8912-be7f119cb988")
	)
	(pad "98" smd roundrect
		(at 4.1 -0.55)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "13ae50e2-d79d-4c3c-a00c-3b275c496660")
	)
	(pad "99" smd roundrect
		(at 4.1 -2.3)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "ba249be1-55f5-4d7d-b880-411acfa91b86")
	)
	(pad "100" smd roundrect
		(at 4.1 -2.85)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "a742daab-756e-4fab-8929-5733dd841f95")
	)
	(pad "101" smd roundrect
		(at 4.1 -3.4)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "485d8aba-6a33-46ae-85da-5dc7a11fff2c")
	)
	(pad "102" smd roundrect
		(at 0.55 -2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "2e7c65d7-c17a-414e-905f-f594930e0648")
	)
	(pad "103" smd roundrect
		(at 0 -2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "3720c396-eb8a-4c8a-b9a1-85414c5a2129")
	)
	(pad "104" smd roundrect
		(at -0.55 -2.15 90)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "b29610b1-1a62-48a5-ad18-c38ac9af30c4")
	)
	(pad "105" smd roundrect
		(at -2.85 -2.85)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "9ffcc1be-eab0-497c-a400-a767f6944181")
	)
	(pad "106" smd roundrect
		(at -2.85 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "7e7ab91a-f508-49df-8e8d-cde04516a1e6")
	)
	(pad "107" smd roundrect
		(at -2.85 2.85)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "d8a4f7e1-87e8-4a10-91f0-475bbc15b2c9")
	)
	(pad "108" smd roundrect
		(at 0 3.575)
		(size 1.6 1.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "98b2c276-7f78-4742-9bca-e27507708849")
	)
	(pad "109" smd roundrect
		(at 2.85 2.85)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "1bf6376c-ed6f-4e40-8203-6e900def3337")
	)
	(pad "110" smd roundrect
		(at 2.85 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "e4b3b4e0-345f-4431-bdfd-2c740518f2e6")
	)
	(pad "111" smd roundrect
		(at 2.85 -2.85)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "61cce58d-e98a-4c76-9fce-79accd692a8c")
	)
	(pad "112" smd roundrect
		(at 0 -3.575)
		(size 1.6 1.95)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "96c41496-4eb5-42f8-ac27-b0b71baaef84")
	)
	(pad "113" smd roundrect
		(at 0 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.05)
		(thermal_bridge_angle 45)
		(uuid "cce166b5-8c4f-48d2-bc71-edd201281ee0")
	)
)
