(footprint "Fuse_2018Metric" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6212066D)
  (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
  (tags "resistor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.6) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a9ed9194-e024-4b5e-810d-ed886789888a)
  )
  (fp_text value "Fuse_2018Metric" (at 0 3.35) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a4403846-490f-4f51-a7af-a1f56bceece4)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.8 0.8) (thickness 0.12)))
    (tstamp 850a0f5b-397a-4944-9e58-f09a21de97f1)
  )
  (fp_line (start -0.602064 2.5) (end 0.602064 2.5) (layer "F.SilkS") (width 0.12) (tstamp 15644880-24f0-49ea-b8f6-32536db5cc73))
  (fp_line (start -0.602064 -2.5) (end 0.602064 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 7bfcec23-5de3-4725-80db-b86af06ee94a))
  (fp_line (start -3.5 -2.55) (end 3.5 -2.55) (layer "F.CrtYd") (width 0.05) (tstamp 0b683d2b-038d-45d6-b71b-18eb1e5b6605))
  (fp_line (start 3.5 -2.55) (end 3.5 2.55) (layer "F.CrtYd") (width 0.05) (tstamp 602c09fc-a302-4c14-ba41-2648d296ec08))
  (fp_line (start 3.5 2.55) (end -3.5 2.55) (layer "F.CrtYd") (width 0.05) (tstamp add4c559-0ac4-4850-af4a-0280d6a74903))
  (fp_line (start -3.5 2.55) (end -3.5 -2.55) (layer "F.CrtYd") (width 0.05) (tstamp e8740c43-4751-498a-8db7-c9c8369fea84))
  (fp_line (start -1.6 0.8) (end -1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 3eb2af48-db14-40c5-89b2-80d6417d5ec9))
  (fp_line (start 1.6 -0.8) (end 1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp 66d92e16-3651-4b58-92a7-e8c5f661ec8b))
  (fp_line (start -1.6 -0.8) (end 1.6 -0.8) (layer "F.Fab") (width 0.1) (tstamp 80feec60-e3dc-446f-b09a-fa6d594ec4e7))
  (fp_line (start 1.6 0.8) (end -1.6 0.8) (layer "F.Fab") (width 0.1) (tstamp d90cfad4-52a7-4d69-b6b0-d4f2a1851606))
  (pad "1" smd roundrect (at -2.45 0) (size 1.5 4.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp 599017b1-f29c-443e-9ea7-07c90719def4))
  (pad "2" smd roundrect (at 2.5 0) (size 1.5 4.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2) (tstamp b5391272-940d-4e91-ab2f-7448bcee766e))
  (model "3d_models/SMD_Polyfuse_1206.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1.8 2.4 1))
    (rotate (xyz 0 0 0))
  )
)
