(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/SWITCHED_VCC")
	(net 3 "VCC")
	(net 4 "+3V3")
	(net 5 "Net-(D1-A)")
	(net 6 "Net-(D2-K)")
	(net 7 "Net-(D3-A)")
	(net 8 "Net-(D4-A)")
	(net 9 "Net-(U1-VBUS)")
	(net 10 "/ZIF_4")
	(net 11 "/ZIF_2")
	(net 12 "/ZIF_33")
	(net 13 "/ZIF_37")
	(net 14 "/ZIF_26")
	(net 15 "/ZIF_15")
	(net 16 "/ZIF_34")
	(net 17 "/ZIF_11")
	(net 18 "/ZIF_29")
	(net 19 "/ZIF_17")
	(net 20 "/ZIF_22")
	(net 21 "/ZIF_20")
	(net 22 "/ZIF_25")
	(net 23 "/ZIF_3")
	(net 24 "/ZIF_1")
	(net 25 "/ZIF_12")
	(net 26 "/ZIF_31")
	(net 27 "/ZIF_14")
	(net 28 "/ZIF_27")
	(net 29 "/ZIF_8")
	(net 30 "/ZIF_32")
	(net 31 "/ZIF_24")
	(net 32 "/ZIF_41")
	(net 33 "/ZIF_18")
	(net 34 "/ZIF_40")
	(net 35 "/ZIF_13")
	(net 36 "/ZIF_30")
	(net 37 "/ZIF_39")
	(net 38 "/ZIF_7")
	(net 39 "/ZIF_10")
	(net 40 "/ZIF_38")
	(net 41 "/ZIF_23")
	(net 42 "/ZIF_35")
	(net 43 "/ZIF_36")
	(net 44 "/ZIF_6")
	(net 45 "/ZIF_5")
	(net 46 "/ZIF_28")
	(net 47 "/ZIF_16")
	(net 48 "/ZIF_9")
	(net 49 "/ZIF_19")
	(net 50 "Net-(J2-Pin_3)")
	(net 51 "Net-(J2-Pin_1)")
	(net 52 "Net-(JP1-B)")
	(net 53 "Net-(JP2-B)")
	(net 54 "unconnected-(K1-Pad7)")
	(net 55 "unconnected-(K1-Pad2)")
	(net 56 "Net-(Q1-B)")
	(net 57 "Net-(R1-Pad1)")
	(net 58 "Net-(U2-QA)")
	(net 59 "Net-(U2-QB)")
	(net 60 "Net-(U2-QC)")
	(net 61 "Net-(U2-QD)")
	(net 62 "Net-(U2-QE)")
	(net 63 "Net-(U2-QF)")
	(net 64 "Net-(U2-QG)")
	(net 65 "Net-(U2-QH)")
	(net 66 "Net-(U3-QA)")
	(net 67 "Net-(U3-QB)")
	(net 68 "Net-(U3-QC)")
	(net 69 "Net-(U3-QD)")
	(net 70 "Net-(U3-QE)")
	(net 71 "Net-(U3-QF)")
	(net 72 "Net-(U3-QG)")
	(net 73 "Net-(U3-QH)")
	(net 74 "Net-(U4-QA)")
	(net 75 "Net-(U4-QB)")
	(net 76 "Net-(U4-QC)")
	(net 77 "Net-(U4-QD)")
	(net 78 "Net-(U4-QE)")
	(net 79 "Net-(U4-QF)")
	(net 80 "Net-(U4-QG)")
	(net 81 "Net-(U4-QH)")
	(net 82 "Net-(U5-QA)")
	(net 83 "Net-(U5-QB)")
	(net 84 "Net-(U5-QC)")
	(net 85 "Net-(U5-QD)")
	(net 86 "Net-(U5-QE)")
	(net 87 "Net-(U5-QF)")
	(net 88 "Net-(U5-QG)")
	(net 89 "Net-(U5-QH)")
	(net 90 "Net-(U6-QA)")
	(net 91 "Net-(U6-QB)")
	(net 92 "Net-(U6-QC)")
	(net 93 "Net-(U6-QD)")
	(net 94 "Net-(U6-QE)")
	(net 95 "Net-(U6-QF)")
	(net 96 "Net-(U6-QG)")
	(net 97 "Net-(U6-QH)")
	(net 98 "/SIPO_CLK")
	(net 99 "/PISO_CLK")
	(net 100 "Net-(U1-RUN)")
	(net 101 "unconnected-(U1-3V3_EN-Pad37)")
	(net 102 "unconnected-(U1-GPIO8-Pad11)")
	(net 103 "/~{SIPO_OE}")
	(net 104 "unconnected-(U1-ADC_VREF-Pad35)")
	(net 105 "unconnected-(U1-GPIO15-Pad20)")
	(net 106 "/SIPO_SER")
	(net 107 "unconnected-(U1-GPIO11-Pad15)")
	(net 108 "unconnected-(U1-GPIO0-Pad1)")
	(net 109 "unconnected-(U1-GPIO14-Pad19)")
	(net 110 "unconnected-(U1-GPIO15-Pad20)_0")
	(net 111 "unconnected-(U1-GPIO0-Pad1)_0")
	(net 112 "/SIPO_RCLK")
	(net 113 "unconnected-(U1-GPIO10-Pad14)")
	(net 114 "unconnected-(U1-GPIO13-Pad17)")
	(net 115 "unconnected-(U1-GPIO6-Pad9)")
	(net 116 "/~{SIPO_CLR}")
	(net 117 "unconnected-(U1-GPIO7-Pad10)")
	(net 118 "unconnected-(U1-GPIO26_ADC0-Pad31)")
	(net 119 "unconnected-(U1-VSYS-Pad39)")
	(net 120 "unconnected-(U1-GPIO26_ADC0-Pad31)_0")
	(net 121 "unconnected-(U1-GPIO8-Pad11)_0")
	(net 122 "/PISO_SH")
	(net 123 "unconnected-(U1-GPIO14-Pad19)_0")
	(net 124 "unconnected-(U1-GPIO11-Pad15)_0")
	(net 125 "/~{PISO_CLR}")
	(net 126 "unconnected-(U1-GPIO22-Pad29)")
	(net 127 "unconnected-(U1-GPIO9-Pad12)")
	(net 128 "/PISO_INH")
	(net 129 "unconnected-(U1-GPIO1-Pad2)")
	(net 130 "unconnected-(U1-GPIO9-Pad12)_0")
	(net 131 "/~{RELAY_ENABLE}")
	(net 132 "/PISO_SER_3V3")
	(net 133 "unconnected-(U1-GPIO7-Pad10)_0")
	(net 134 "unconnected-(U1-GPIO13-Pad17)_0")
	(net 135 "unconnected-(U1-VSYS-Pad39)_0")
	(net 136 "unconnected-(U1-GPIO22-Pad29)_0")
	(net 137 "unconnected-(U1-GPIO16-Pad21)")
	(net 138 "unconnected-(U1-GPIO12-Pad16)")
	(net 139 "unconnected-(U1-GPIO10-Pad14)_0")
	(net 140 "unconnected-(U1-3V3_EN-Pad37)_0")
	(net 141 "unconnected-(U1-GPIO16-Pad21)_0")
	(net 142 "unconnected-(U1-GPIO12-Pad16)_0")
	(net 143 "unconnected-(U1-GPIO1-Pad2)_0")
	(net 144 "Net-(U2-QH')")
	(net 145 "Net-(U2-~{OE})")
	(net 146 "Net-(U3-QH')")
	(net 147 "Net-(U4-QH')")
	(net 148 "Net-(U5-QH')")
	(net 149 "unconnected-(U6-QH'-Pad9)")
	(net 150 "Net-(U7-Pad4)")
	(net 151 "Net-(U7-Pad1)")
	(net 152 "Net-(U8-Qh)")
	(net 153 "Net-(U10-Ds)")
	(net 154 "unconnected-(U9-CE-Pad6)")
	(net 155 "Net-(U10-Qh)")
	(net 156 "Net-(U11-Qh)")
	(net 157 "/PISO_SER")
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "003aa95f-39de-4b17-93a7-99874ff831c4")
		(at 139.093 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R29"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "c5247c33-d730-4254-b14f-aa8a9bb356b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c7a44518-b7ed-4532-9757-5addeac426c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd0b4ef2-bc82-4c16-8bee-2cca314090ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0898e6dc-cf4a-4321-9a5d-591b390e9d62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88728ea4-8bc1-4649-8ed2-a772ef5305c4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3e8e2b44-ef6d-471c-b65e-6d9baa3d89b7")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc0b58d3-8703-411d-a20e-16c90af7e55b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c637a93-ab1c-4d76-bab2-4ceb006366b0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2f9de9e-67a7-461c-832a-c9a5f8bc85b2")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d0ea3ab-2e4c-47ea-ac67-6ccd4e4d4ab8")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99649086-915a-417f-822a-04393accbb74")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cad49080-defa-4c5b-864b-ee34184d1e2b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c95ab28f-1902-468b-bae0-13428c10d3c9")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b666e2f4-fa7d-4812-806b-3c7fb5c6e89b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a56df7d-19e8-4371-8c8e-8e71458b8daf")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c264145-1c71-4c3d-a445-8f5c4aef2ef0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bc90d166-9fe8-4ce0-990f-095faf7b7ffc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 85 "Net-(U5-QD)")
			(pintype "passive")
			(uuid "c9d13553-387a-4b38-9b22-97f13e0d60bd")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 18 "/ZIF_29")
			(pintype "passive")
			(uuid "3dd038c0-816e-45c1-918e-20bbaee310f6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "0361e387-3b15-4eca-be9d-0d2811893fcc")
		(at 156.943 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R65"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f6e41a50-fca4-4b90-ac02-fe7af4ab14bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "de5b6479-83ef-4e7f-903e-cf3b0c9fc983")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa105631-267c-4252-9f27-b8001689dc89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ffd4f86-787e-459e-9f05-609660abda8b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "89422698-6adc-46a8-b6c3-c7094c82c42a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/eac08d64-7fde-475c-ad59-0df78c10b73d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "932a73cc-99d1-4056-ad76-dab1ab9652e3")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04f15e23-ed9f-43dd-8958-8d5debbe0fd0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5bfa604-6689-4581-aae3-d5cfa7cdb29b")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d249e6f-6c6f-4052-911f-f58ea0f2eba3")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e78a38f5-8826-42fd-ab85-9b0b7401b2e4")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce0f0eaa-f291-4da3-ac70-1d00059e817e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ff9ef26-3227-428d-82f3-6367450515b3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60c16c08-dcc8-4ee0-a16a-588b1eee2a0b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54ac7f28-decc-4f68-99e0-66c4e6453041")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b855a827-af85-4fdc-b222-a018dc8b638f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8dfdba54-9c88-4f2e-8732-03ec10a87a9c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 21 "/ZIF_20")
			(pintype "passive")
			(uuid "dd2a8d59-2baa-4ee7-b197-0f94e8513807")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5b4f55d7-fd1d-46a4-960e-3ee83d026ce7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "088f1257-b28e-4204-bceb-ffd63873ea53")
		(at 133.143 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "eb04699f-6078-4c72-8199-b04d42c69b27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9bb36f7a-da0f-43b3-85d3-bf0c2066f32e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "589d1360-59c4-46c0-a442-8b1b822f7143")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c6f10256-c1fc-42aa-842c-bd66bdd2b665")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "838d1f5b-44c7-41be-b802-3e99dfedbb2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c4cf15d1-a432-42cc-bdf0-22863790cb05")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f67a551c-9c95-4431-a99a-3c17e8b9754f")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b131f9a5-3d7b-42ff-ab6d-e9d6eee6d97f")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "522a8ad9-d737-4757-83d7-2ebb5a5093e4")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0ddb27c-ee90-4e70-b20b-05c6dc9745fe")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c018c992-b52e-40e7-b099-84c1a396f299")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5415802-f410-45a2-847a-b54fbd220fed")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21bed522-b02a-427c-b526-97439b7d0971")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8e59b23-f583-4e53-a27a-5c6d752d8cb1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cb7c522-1b0c-4146-8944-5c91961c60c6")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9032e25-7fad-411a-b8a9-a54fd6be9115")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "60dab81a-1f87-47b6-97a0-94fc6a9ecd26")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 73 "Net-(U3-QH)")
			(pintype "passive")
			(uuid "95947058-2e2e-402d-a191-a21a36ff3c8c")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 47 "/ZIF_16")
			(pintype "passive")
			(uuid "30289b42-2d12-4cbe-8a85-34786a41c471")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "0db49e64-5c3f-4abb-9071-e4686a98ec9c")
		(at 136.893 93.54)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U9"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "e5d0fb4d-205a-454f-9e6d-bdf85ac754ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT166"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "8cee4c55-ccb0-4814-b8c9-11a0c830b116")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7296f12e-ca96-47a5-8511-bc842e5c9585")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "77fadf63-1286-4464-9a69-bcd2eb763f0b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9111977c-d6ec-4080-99e4-bb10aa4c8edb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP?16*")
		(path "/37420c89-2df2-4aec-81db-6e18267c7ad0")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "915363dd-6b7e-4c63-87ac-70ed32312adb")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36e5ae3f-752c-4202-849f-a1a13448827c")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38d77996-7406-4230-b650-f0dca43ad557")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f50634c1-c0a9-42f2-bad7-aeb0e10a9a5e")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "18db5a2c-aa33-4e5a-8de3-640bf76b5295")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16fb987e-51d3-4bd2-9006-4cd04967a155")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea8a2b03-a8e6-49bf-9f1f-8137a3fa990c")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d487ab02-09aa-426a-958f-91acd0d48e6f")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22b09e56-56a3-4c0f-bdb4-5b7dc57304fc")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "265d355f-ad91-4bf9-823c-3be2aa97f3ab")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "957c9a2b-74fd-42c7-b71c-11ea3020517f")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c427f741-4cbc-4691-9570-0a4c120915b6")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8750338-0dd9-42a5-88c8-49b5d16a2123")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bee7e766-b563-4a66-9523-b419626e2fda")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6dfc50c4-ef43-48d0-8709-5649f4057f83")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U8-Qh)")
			(pinfunction "Ds")
			(pintype "input")
			(uuid "11cd068b-6e68-48d8-a141-7de862fb24a3")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/ZIF_9")
			(pinfunction "A")
			(pintype "input")
			(uuid "05659593-6b2d-427e-8112-d02386817ce5")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/ZIF_10")
			(pinfunction "B")
			(pintype "input")
			(uuid "f2eaf5c4-5e01-4508-83b6-9ee4fb05954b")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/ZIF_11")
			(pinfunction "C")
			(pintype "input")
			(uuid "62b91706-7e06-4505-a569-4ce30cb9eaca")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/ZIF_12")
			(pinfunction "D")
			(pintype "input")
			(uuid "ed985ca6-2457-48d0-b4af-b0867d68ab28")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "unconnected-(U9-CE-Pad6)")
			(pinfunction "CE")
			(pintype "input")
			(uuid "dbb24482-91b9-4e93-bcdb-cce78339d54c")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/PISO_CLK")
			(pinfunction "Clk")
			(pintype "input")
			(uuid "938c4714-9c5d-4b19-b553-4ea79be77d03")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "7aa3e824-af95-467e-b710-fa1958b4a1c9")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "Clr")
			(pintype "input")
			(uuid "25b4f601-1137-48c5-921b-a44c6e9f33d9")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/ZIF_13")
			(pinfunction "E")
			(pintype "input")
			(uuid "8dde07ef-9666-4853-9b3d-648f02f6fcab")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/ZIF_14")
			(pinfunction "F")
			(pintype "input")
			(uuid "d1165198-c4d5-4497-9c78-50485465d19f")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/ZIF_15")
			(pinfunction "G")
			(pintype "input")
			(uuid "2cd486ef-b28c-4175-9580-fa154cc9550a")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(U10-Ds)")
			(pinfunction "Qh")
			(pintype "output")
			(uuid "477599c6-5d2d-4127-b0e4-24cf2c07b237")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/ZIF_16")
			(pinfunction "H")
			(pintype "input")
			(uuid "a8442f67-52bb-4da0-a888-92c494bd94eb")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/PISO_SH")
			(pinfunction "PE")
			(pintype "input")
			(uuid "cf92fd42-bfa9-4085-8db6-51a4c90ec96f")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "5bb8d6f4-b9ef-4fe2-b3a2-91c0c5c2ada9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "0f98c7cf-4955-4e65-ac07-75f9670e9238")
		(at 127.193 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "43525403-7ba2-4015-b892-cf4154555eda")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "5bcd7922-a1c4-4525-b0e0-47fb2770d1e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c204c67-b03b-4522-8457-845974438cf9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c9dbd01-f8a6-4453-8974-e2abc6a5e6d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd61da8d-c871-4a70-b9c0-6a6eada3e6b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e411ec3e-101f-4585-a4af-673f91400668")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9684930d-9867-47e8-b477-f8e7f64d5e70")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c5cddde-e27a-41da-a006-d4c1537f78c7")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14337bc9-0fe8-4e7a-9a1e-11e23182485a")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7409fe8-a905-4c9b-919c-6c285fb12b6a")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c813f965-0263-404c-a437-63276547a505")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d7e1dc7-0966-4711-9d0a-62522f13c534")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "698cc622-e4f0-4a35-900b-0826d3488f3c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ffd732b-db2f-4d0e-89c1-3e0edaa9c96f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "925fa7ab-9f92-4b05-8ff8-1dbe641d806e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef3788d1-1799-4b4c-8f36-c893c0cab967")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c06c5fb9-74ee-46f5-ad18-58efbb98ba93")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 61 "Net-(U2-QD)")
			(pintype "passive")
			(uuid "bdf845b2-4ee0-4249-bcc0-29d45d340d75")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 10 "/ZIF_4")
			(pintype "passive")
			(uuid "861daf73-be21-46ce-a4b3-d156437382bb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "1736434a-f776-4639-afb7-6194deab878f")
		(at 103.143 111.87)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "99f2b275-3ad8-483a-8cf9-3a31ac41e493")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "615c9430-da13-4403-93ea-2a6c3df771f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f54e7481-ebf4-4fd9-af56-a191d3d0dea6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38772f6f-3f3b-43bf-b4ff-6c1cc4ba92a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "09fa7c96-e814-481a-a1f3-b5f26d7a927d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1c0cad2f-7b27-47d8-950c-a5357d6a4caa")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6676cb70-b232-4c22-a19f-6a03a62c318b")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00985059-8383-4a2b-b807-ab9b965daa6e")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "caaba659-84d6-44dd-be55-729da4ec5c05")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe01196d-f8d8-421f-924d-98dbc5f93662")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cab5a3c-05fa-41c0-a650-2f91f38de3b8")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba31d8ac-bef3-45ad-b0a3-e7f18751f327")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d87edc6d-fefd-4ef5-b3d2-ee9c26b269cd")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c189cf9-79c1-43df-a84a-1f758482b99c")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b0c0c0a-943a-4bbc-adea-3c017eeb5b76")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cbef018-42a5-4ab6-ba9a-22b8fef95105")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f1b802fe-805d-42f0-a0da-aaf8aea47277")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "98f46aef-8221-43d9-ab0e-59bee9071259")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e3c911fa-f158-45cd-8389-4fdc3d68c7cb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "18252e33-f98f-49d7-bd73-fd7c3c947687")
		(at 103.143 101.82)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "fb026105-476d-41ca-a169-1b7ddc51163f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "f3aa1650-d181-4786-aa8b-868a893cbbd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03f1e557-348e-469c-8b6e-b244e727b015")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abd394e5-277a-4f85-aaf7-2f0d50ef77bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "87b60bd6-df2b-45db-8f4f-08bb942d4c80")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7b0da82b-1922-4e68-bdf5-38df61aca068")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffb2c322-27cc-447e-a131-0662b2a5e8c2")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1fe36ac5-5872-432b-b065-11a41951b2e9")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54d7d4e1-107d-4623-86d5-f0f239a91e54")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc61bd98-7dfd-43c9-962c-334cac7be003")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "81a8a990-b563-477b-a27e-dbc74cd9a822")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b3b9d22-664b-45b7-8131-d724d4a13c66")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16c592c1-c1ba-4786-8aa5-ce26dd033fac")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80e4fc9b-f16f-4ff5-b3d0-380ece09875a")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f9a4ad2-b5c7-4e42-b6af-9a6af3ee8fd9")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc169fb3-e48f-4409-b2fa-4883e580bb60")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a7b77b98-37b2-4c7f-bd61-75074e85d6d8")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "418fdfe5-73c6-4b8d-8425-3b5ed90f8dc4")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9c7765ca-e69c-49d8-8286-14a9c9fe6a87")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "1873a2e0-5230-4a6d-a48a-e58b7754467a")
		(at 109.153 101.82)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "8f659ad1-1b9b-45c1-93b8-fcefe717d25c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "26ca9fc9-5f89-4bb9-b937-034c3d3503f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "beb8fc42-262a-466e-909c-9a48ccc79ff4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8dbf1973-cbc3-450c-a61d-83fc293e0ae9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15bd5fb4-c67a-405c-81d6-0e49a1529fb8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5f0778a7-6dff-40bd-8b10-4107dbbbbc21")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "206c48a2-da86-4568-8673-d2f7fa34ea2a")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b930c3d7-f581-4cb1-93e6-bff0edcefa88")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5abc6d7-52c6-4180-9e62-361fab7a2f9d")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cd8b71a-1f27-4b6b-9dc6-7f6226c122f5")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37ea5d93-aa33-4b51-9ca2-290f5bc40ae5")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd8a2787-9887-440c-9bdc-b83b4e30b9b2")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b3ef14d-1508-4189-9efc-a152a74997cf")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e76aedc0-b588-41de-b225-2ba5c51e063b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6204fe49-45e9-44f0-984a-d2968c35e8d5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5a9869e5-c349-4757-846e-2ef47b5fa85a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "47b17367-efa1-4fec-b4e5-b5d49a23ff31")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "46fc5711-938a-4b28-b4bf-5d44d59f59a5")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "50953eef-8936-4051-9a60-281608442630")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "1c233b26-2609-4aa8-9d2c-499575db6d93")
		(at 145.043 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R42"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "4060aa24-40cc-43d3-9a95-06578f53b8ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "48c7a8fb-6b9d-4cbb-8eec-43632873d402")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6551d651-9ae1-463a-b1b4-50aebe776b92")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3219818c-fc25-4cb2-89aa-32f6b4067b3e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "93030e4b-2dd2-43a5-9dbf-afc3d8de1da1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7e287319-2f81-4527-81db-11649fff42ea")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd36b073-1e9b-4c47-9637-4c9acc4abda3")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa2ce8ec-1c00-45fe-90df-f0cce3fc6be8")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a33d003f-ec18-43c1-aa62-d12fb215debe")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d632491-d22b-4e65-b92e-4f9bd81014d1")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1b184d7-27d9-46ed-8aa7-a96d9c2e35e9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3916137-d34f-4664-9cc4-28f6ade261cb")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b495960a-edeb-4d68-aa24-8de3c0832726")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa228d90-5492-4dbd-9cf9-6ff6407192e4")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a095de9d-6736-4b6c-9820-ad1228cf7a84")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "213cde38-0083-4aee-9041-121190aebd9f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b8801e18-cbb8-41ce-8903-1a6b65d4ccfa")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7e450dcb-e571-41f3-86b5-569047da5679")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 2 "/SWITCHED_VCC")
			(pintype "passive")
			(uuid "6936b6be-d7e9-4dc3-b7aa-382e2ff2bbdd")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "1ee87982-168e-4a75-9aef-ade0a962c5da")
		(at 162.893 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R71"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f2b0e5ce-0077-48bb-ae73-54562c2eca2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "b98b16ac-48c2-4449-b366-2e2f97975b43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b73e2ac4-c82f-471e-98da-d35e3694660c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb123e5a-5f05-4b88-83bf-40ca585bec71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f21ed9a-f805-4809-8966-4eed8822046b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b06cf3cc-6b0f-4dca-9ea0-c993499fdad5")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0b713334-ad36-4af9-84d1-7be0a1e90c5c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2627a49-084a-4e23-9962-be2709c4e724")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bede7e5e-d8e7-40c6-9b15-02b30289099a")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07b75c55-6205-4e72-b071-4d69b47b449d")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff97292b-01cc-4738-b4f1-6c90c589de4f")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "431ec231-b8ee-4ff1-850e-daa6bc95198d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c586fa12-09f8-4850-8877-6a46c42212a5")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff4bb138-13b4-491c-b09b-aa0d92a5fad0")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2d5e273-59ac-42e7-b2f3-c2463088c8fe")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "130b44b8-eba6-491e-ade8-85fdf338a14a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c8d6acb0-2c33-4567-b684-0b3924f8e229")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 28 "/ZIF_27")
			(pintype "passive")
			(uuid "989c426b-350b-4192-93fe-ecf63e5caadc")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "67a47b38-5af3-47a3-9cfd-d4d243e3bcba")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "1fdc7efa-0a0c-48bd-afb7-4b31ab5d344e")
		(at 109.153 111.87)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "edd05d83-f763-4f6e-95d0-ffc343bbe08d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "9d0b66ba-1715-4abe-b619-1e33b21c84b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "989044b5-2693-4463-8ca8-fd4b39837c44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e300d10-9708-4e4c-b651-3c5305edfe28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43c243b1-9567-409c-a051-433ae806138f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a8373b61-208e-4436-915d-cccf20fc433d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d04c89fb-b689-4fdc-a708-800382fa8d14")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f180d04a-fe31-4ca8-806a-2831ee9a997f")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cac4893f-ab8d-4510-b3d0-c126e7e42124")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ebe5c644-1405-4ea0-b3e9-febfd0edad13")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "559727ca-d50e-40aa-827a-d6acc942d1d5")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "baa2220e-6387-433f-b33f-3ae03e998d3e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29f07a7f-b256-46b2-8599-726fa21292ae")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c97a9679-2004-4a6d-ade8-eb4582ce47d8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62cb7a6f-3df6-4945-93fe-1ca3914a001a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d223e0e-ae23-432a-b290-a8010725a63c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5a4659ff-c9d1-469a-9425-efbcf38dea71")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "3ef51633-de76-467c-8d03-674899cb180a")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8c2b03d8-6af9-4302-b48c-3e2c6a882e79")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "21770e7c-134b-48d6-84ea-3a2bbb3c989c")
		(at 139.093 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R23"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "c7a8a716-8f80-4f2f-a4b1-0dd132826e0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "1fd64830-5fc8-49fc-a571-262c5f52c5c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "82c203fa-3a75-417b-ae35-8dd772e96090")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d1029fe2-aa48-416c-afb0-6d7b412c8f03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43593184-1489-4ba1-9a36-602f4cc1c073")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f00cfe4a-cd3e-422c-992e-774e6d96fe0c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28dacb2d-42e3-48db-985a-f28e472d8f3b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0d1c299-bf90-4c32-a531-47043e9c4433")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e68586ea-0914-4760-a055-8e57a970bd59")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37d1f123-a980-4968-a06c-3ba83b9f3343")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "172ea1ab-e202-4531-9d77-c5b17372c691")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7cbeff0f-279d-4885-9f4a-4a0e09690702")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a74320e-709d-4762-a1b1-38f6ac16361a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "640e1ea9-8504-41a8-a097-c4b9f840ac55")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e891286-3a17-47b2-b8ce-1022af206970")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48290dfe-5883-468b-8ed1-7c0466246b96")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "77251e2c-500b-4a46-bd3e-0b84be968d4d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 79 "Net-(U4-QF)")
			(pintype "passive")
			(uuid "df65e477-1d9e-4d4e-bcab-49cb97f0419a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 41 "/ZIF_23")
			(pintype "passive")
			(uuid "49402c43-aac9-474d-a246-2e4b564208f2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "224a6290-2c24-4997-8c4b-eedb5e5da9e9")
		(at 150.993 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R49"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "9bb7093b-0dfb-49a2-ac6e-9a5de94f8e3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9a13f11d-17ba-4c77-8f16-a5ad91ee4c0d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "476b8278-00ed-4684-a856-41d2f2215087")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "86f24a53-011c-4e2b-b359-2415b33c96d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a9ff401-bbc1-40b3-b270-14c7f0cffe19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3d1ce7d5-651c-4bfb-9a40-c46ad5061b39")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2797fc45-a74f-4bc2-bcf1-a09af02c5e45")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ea4a641-80c5-443c-bf58-6245415af5d1")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a97c2e42-7a7c-4dbc-9733-7c9d01a31e56")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df266308-e09e-4dac-8cff-f3bcc458b162")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c5a69b7-5435-4fd2-8c0d-1e1257883675")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1b87aa0-6ac3-4bff-ba54-68f1ef8b3f82")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab550240-5604-4d50-b662-2a6dfbc9d2ea")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f81ad77-208d-498b-83e3-aad535811a49")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d00b986b-a484-4a20-88d6-ca999e66a257")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c329af8-aca0-4364-9d38-64828fe8ae83")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c782603f-3803-4544-943c-617bd518c438")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 10 "/ZIF_4")
			(pintype "passive")
			(uuid "c1ec826b-10f8-49bb-bcd3-8650f4e6a9dc")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "48d14e0b-dd29-4570-9911-da3a7e51df55")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "25c68383-dc98-4c34-ac67-6e46832932fe")
		(at 109.153 95.12)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "8933596b-3488-4b5a-9499-cdc969a9c9a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "116baadd-2cf5-40f9-b13a-97a863a4ca23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de53957c-0f7c-43ce-9919-1a34cbac42d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d17046f8-9259-401f-93ae-21669e8c675e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "29feb508-5b40-4de8-98e4-516e98f8b586")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ef6da94f-5ed2-4d2d-b920-69a65bd9a1bc")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a461578a-d387-4834-b398-8cfc212ea24c")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d990ba6-b672-43f9-890d-043aed6052b1")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "181f0451-d0a1-4f01-bc0b-1d7c95ef90d4")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8d778c2-c694-4400-b84d-786e6921b993")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ec1918b-2d9e-45bc-911c-89aa3f19426a")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c23a631a-3c63-4c0f-86a2-4c3c74a5b3a6")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "226f3237-261a-446b-ae5d-f9f81aedb332")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06afd120-418e-49bf-84bc-aa5f010ce0c0")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "faaeb6c3-536d-4780-bc3b-4cbd5e49b6a4")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fc2fc07-7bbe-4d0f-b298-555c655a9f59")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1b2116b3-4d23-4a38-957c-d46f78b2c0cc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "8676d922-661c-434e-a24d-02ba32a4712f")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bd7cd07b-3d80-4dde-aa80-5a9dc0d6d375")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "264f4c71-77e5-48bc-acd9-7163907b9935")
		(at 168.843 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R80"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "2a6d7da4-64ff-4ae9-aa39-40c8dad3eba8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "668e1bea-3976-43d8-b3ef-cf987e3a3af0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c92c165-47e2-4b34-867e-9353294d8cdb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbb59eaa-4f98-46f5-a0ac-b9dd578f225e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f1bad162-d2ab-4d60-8305-0f0b8ab6dc64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/062434ec-f683-42e0-937c-75390438b339")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8343b530-d5aa-4910-9990-1e82fe8ce171")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f80ae22-ed1a-4576-b2df-12e7fa8c2e5e")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dff994df-6e61-4ef4-9f13-eaecd2707e97")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5418c8a-160f-4dc9-beea-202b651db378")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9845565-1056-4f74-8b54-415195a84352")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "114fd86b-b39a-40f1-9bd9-1ef8cce07c0a")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f3e5c7d-5f86-405b-b31b-ec99f7db01c4")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8420702-2b32-4798-b2ab-80de3cf67980")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a57e01ee-eb78-42c8-a724-511f63dbe14e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e5072a8-d55b-4218-8993-393784a958d8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5160ee09-e951-4598-babb-d1e04d5bcb66")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 43 "/ZIF_36")
			(pintype "passive")
			(uuid "b1e75618-9b56-4076-8b4d-714171d6cb6c")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "aa32d9bc-ee33-4a90-b28c-8c9c6802bd87")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "267f9b7e-677f-404d-b606-8c4a013aae40")
		(at 109.153 108.52)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "6f39637d-0140-4fe3-96f4-47389c34a921")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "ffac061b-7f0c-47a8-b1a2-873265204a56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8709b3ce-8b19-485f-9b20-c21985572ca5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c5fb3ef-32b3-4aad-abee-40df2e516bf0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9eaa6ca9-9e25-40e3-9739-e1335c7b0ca5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/11391350-762d-4d0a-b14d-8ab7b8065e50")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc00fbbc-5ea6-4d2f-83c2-906d6ef9f7ec")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9688c29-2c5c-4e6a-8a62-42fce5a5a572")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e411271-f0a1-40b8-bfa5-d2f9595cdfb2")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2510218e-d2d4-4b15-bdfc-a19f25a8fc09")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e048178-60ec-44d3-ba86-d7abe273ac99")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b065a949-5fac-468d-9e0a-09610f6e84b6")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77bed616-4fa9-458b-990e-5fc7602641fc")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ffdb88c-7ff1-4516-9fac-3fb5cb9b487d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78ca21eb-6058-476c-8e64-01dd16c9d7d9")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8795ab4d-6551-4580-b5c9-87e90c4f7af5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "04ce715c-dca4-4581-b6f9-8f9bfcbad2a2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "6f4a13d6-a7f2-4dee-a830-b6a712681fcd")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e47d1913-dc28-4a66-9aec-2589ddbd9bca")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "2757d3a9-aaa2-431f-8a79-c215673e8507")
		(at 103.143 98.47)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "5516760f-3733-425f-835f-587679d554b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "7c4c24cc-ff13-40f8-9a87-3f7be30c2625")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "554253a7-270f-43b9-9775-053e10c6ce88")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "293e9ec2-7e7a-421d-9d05-9733c354e980")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e4151b5-4505-4f0e-a931-c1abc4ba54d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/0eac1daa-a796-4315-bf82-df0b6113be4f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7037f277-1401-4038-b24a-159b1bf8632b")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2ad7114-2b50-45a0-9e4a-8c11be9378b2")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db0a5844-a122-4ba2-ad7c-11a011576fab")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06f8807e-7ec8-4a71-ad98-99dd6e092463")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3dd4e96c-9a37-40ae-8002-e0bbdc36234f")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2b8a1b5-edd2-4ac8-a53d-92127a895bd4")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8142ac10-3201-42b6-a6a2-fd379204e852")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3342a48b-19fd-4168-b46a-7ce91e657577")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4082459d-3eda-44c3-8e44-481b319a2fd5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e975f3cb-dc94-4990-804e-58d9f6772f41")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ee74de35-4f27-4fa0-bf90-80fe6a27e4f3")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "/SWITCHED_VCC")
			(pintype "passive")
			(uuid "9f3af213-d271-49d7-9160-7ef053484c31")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6b7987ec-8a23-4f06-b1ac-a3867b7effe9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(uuid "28b59d36-919c-4e99-b042-832c53f3718b")
		(at 126.093 101.39)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 5.08 -2.47 0)
			(layer "F.SilkS")
			(uuid "422173da-98f1-4bf1-be76-ab8fe31fedc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1N5818"
			(at 5.08 2.47 0)
			(layer "F.Fab")
			(uuid "e2cb5c87-82e4-4dc5-a96a-13f9cb7ab27f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb4bfab4-6792-4734-9d1a-ef2eebd3751f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "354e539e-ce20-4f02-94f0-01112108a652")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "30V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0de3f57-4521-43ff-94ea-1f5e0ec8d74b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "D*DO?41*")
		(path "/80aea4af-4edb-45e4-8b61-2c4f27fd940e")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.34 0)
			(end 2.36 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4261a40-2632-40d8-91db-2b53dbd59866")
		)
		(fp_line
			(start 2.36 -1.47)
			(end 2.36 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fc0cae4-d526-4edc-9769-edecb81a55b7")
		)
		(fp_line
			(start 2.36 1.47)
			(end 7.8 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73a94bad-1cce-4275-b13e-169711becfd6")
		)
		(fp_line
			(start 3.14 -1.47)
			(end 3.14 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c37c2f2c-16c0-4504-bb8d-695e3a2aa08f")
		)
		(fp_line
			(start 3.26 -1.47)
			(end 3.26 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9487be1-c99e-4edc-87a0-89b57d9d4e95")
		)
		(fp_line
			(start 3.38 -1.47)
			(end 3.38 1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abefcd1d-8488-4868-882d-b7a14da79123")
		)
		(fp_line
			(start 7.8 -1.47)
			(end 2.36 -1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5411803d-7617-4745-adcc-4b3f9d44ab93")
		)
		(fp_line
			(start 7.8 1.47)
			(end 7.8 -1.47)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d80a749-72a3-42e5-abd9-7f0f786f9646")
		)
		(fp_line
			(start 8.82 0)
			(end 7.8 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7a04aac-2058-4a84-ac1b-0f6cc3b06fd0")
		)
		(fp_line
			(start -1.35 -1.6)
			(end -1.35 1.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a75153dd-a863-4c3e-9ad0-1bb2c1d8e883")
		)
		(fp_line
			(start -1.35 1.6)
			(end 11.51 1.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49392dec-2650-41ea-b388-92ca7e4177be")
		)
		(fp_line
			(start 11.51 -1.6)
			(end -1.35 -1.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ab80dbb-b4c7-4c2c-b074-f19c2e2b09ac")
		)
		(fp_line
			(start 11.51 1.6)
			(end 11.51 -1.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7af925da-d165-4880-aeb0-940bfac9dd92")
		)
		(fp_line
			(start 0 0)
			(end 2.48 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "229b7810-1317-464e-8ad1-d9f2dfce16c9")
		)
		(fp_line
			(start 2.48 -1.35)
			(end 2.48 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2868ff58-d97a-4cb5-a396-eb06b0db9d4c")
		)
		(fp_line
			(start 2.48 1.35)
			(end 7.68 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "624174bb-fe8c-480d-a0a8-6a43469ea598")
		)
		(fp_line
			(start 3.16 -1.35)
			(end 3.16 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5f8bb3b-8b99-40b5-927b-45a60d851775")
		)
		(fp_line
			(start 3.26 -1.35)
			(end 3.26 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e711d812-51cc-4c52-8c44-2635cf03f9f9")
		)
		(fp_line
			(start 3.36 -1.35)
			(end 3.36 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab0a490b-f9e2-49b8-92a6-48a7d691a95b")
		)
		(fp_line
			(start 7.68 -1.35)
			(end 2.48 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "252befa3-e8ec-49f2-b06c-78e2fd291408")
		)
		(fp_line
			(start 7.68 1.35)
			(end 7.68 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b3e2bc8-444e-4450-9a1d-60c88ab3c4a8")
		)
		(fp_line
			(start 10.16 0)
			(end 7.68 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "540bfa43-e8e7-45d8-9995-5b011d06077e")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
			(uuid "99dc1f80-ef84-454f-9d72-78894f2f05af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
			(uuid "e98b2361-049c-4136-aa60-9d14a7fbcabb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 0)
			(layer "F.Fab")
			(uuid "ed2553ee-5f47-4a45-854c-cf8277853702")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "K")
			(pintype "passive")
			(uuid "2623a174-4e30-4de2-9345-aaec8120d155")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "875a1433-90b9-46ce-ad26-06be58e091e0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "2cc83b56-06a2-4618-ba10-2b0a78b2c141")
		(at 127.193 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "9826f82f-9b15-4aba-b4eb-e4b24af6400d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "b3984ed2-f184-42e0-a68a-be1fbde9c0a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a0284f5-72a8-4462-861d-50b042a25b55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15989b2f-5068-4683-a661-2c38a82ee9ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7ce47f3f-9ff5-43f7-b837-9f769dd1cd07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/81362b4f-83f5-40a9-9498-bf5791cca9a9")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a42adb01-b6f6-439d-8f15-19e53a0f496b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b984802e-40cd-4a09-9dc1-8b8e58ed8ed0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b87ea17-689b-4c11-a8b4-2eef75540c10")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "faa35f16-ece2-4bf4-afb0-89a590f62b17")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7fc702c-a992-4c06-8f32-6b60ad366d37")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f107943d-338e-4360-89e4-680e3f3c0ddc")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfa03f80-8929-4ee6-bec9-963bdef76d52")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "296ccdd5-0d17-4097-a726-81aaf2fb5a12")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "319b8b31-f6ab-48ac-a62d-abf9070279f7")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc85b9b2-c308-4eb8-bc80-f921a1873e9d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1eb0bf84-62c7-4f05-bb0b-d07fd5565460")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 64 "Net-(U2-QG)")
			(pintype "passive")
			(uuid "61b2b9d9-019f-416a-b54c-27820c2557fc")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 38 "/ZIF_7")
			(pintype "passive")
			(uuid "67ab1489-41cd-452f-9526-88dfb43a6246")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "2cfda113-6b88-49be-ab70-c4d663985157")
		(at 133.143 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R20"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "b326468f-b263-4e07-a8f9-f125f2b97ced")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "276eb589-f64c-4a97-8b41-62c41ed7217e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d23af8ff-50dd-43db-89ea-baef823091a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "597fe708-f7cf-4b24-b4bc-35fa2f5c3d1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dacb863c-d246-4902-8462-0cdf17cfb27f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4030e6ca-bddc-4fa0-9a9c-4202495e4c93")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "647e0a6b-7f66-407c-81bd-52cad6778700")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5c7106a-e24b-4559-afbd-e91a9e1e69ab")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd7754d6-d640-42d9-8798-aec6641c9cfc")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57da3748-3a16-429b-a130-0d561a81e05a")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3964da4-1fba-4431-b1f1-b800ee266edb")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bd89433-8a7f-491c-bc5d-7f0f2e061edf")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25a5a2bb-5383-4c59-bc4a-41f1c4f0327c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b5d8f07-f71a-440e-a522-3f67ce9480df")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11cc3e94-3162-4987-a140-cb5febad7af1")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7edafea-62bd-4445-9c10-f6a94ab1a670")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3842e6ab-b1f0-4d0e-9eb8-b94acbd009da")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 76 "Net-(U4-QC)")
			(pintype "passive")
			(uuid "b7ec924f-c53b-4eb9-8162-990b79378096")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 49 "/ZIF_19")
			(pintype "passive")
			(uuid "fbd0b4a2-a4b7-4a26-9776-e555bbf99f4c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "2e56cb18-2cd8-4e8d-a3e0-e9e5d866b303")
		(at 162.893 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R66"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f991701c-bbb9-4ec3-b2a1-b05ea2ee5134")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "bba97000-e417-4014-b0c9-6b36633f9804")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3566d308-bd39-4169-94a1-1adab1c0ee1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "167471e0-3f81-472b-821a-7da4887179b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2eb50c6b-797c-4f40-839b-7ed7f3a5b0c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2b5c342d-1866-4565-ad93-ece327281416")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b6f6ae4-29ee-4d18-af0a-e0b2fd591c4e")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c28b9d43-42bf-42a1-ab3b-0a065c3cba69")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cb51b4f-321a-4c59-8128-c9b29f77ce57")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb303118-3730-43ab-a61b-0e8037012f70")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30a8b8db-6edd-40e0-b719-3f1da1bff5f3")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e9d9326-e1e6-42ff-8f7e-d2af298c993b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b5fab64c-75a9-4236-8de9-1a7dba3f9bab")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6bb7480-9644-431f-b2e8-a7bb42527424")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c1841f1-9780-4bd3-ae5e-520040b065b5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "531ba054-0986-445d-9547-5e268dfb4e65")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bb8b7a75-de27-4fe6-b3c8-9f866c72e5e8")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 20 "/ZIF_22")
			(pintype "passive")
			(uuid "8c6c71a7-ed33-4520-9013-5916ecfeb885")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f8047789-a939-464b-8c2e-a84e682f45c6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "307756d9-8574-4af1-8bbb-d214735b2d80")
		(at 168.843 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R85"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "676c114b-a5da-43ea-8b30-0fa8339dc2d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7fa1a2bd-bd80-4453-898e-3fc43c161baa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "50d3498a-efee-4d41-9e48-9b9899f05d74")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2aac2c55-215f-41c1-b995-de95f4f781c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "016554d2-359e-4ab7-b142-681f14d5f5ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1ce34540-1dd5-4240-b637-e9a9ca4c4518")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59cb7af9-abea-438e-9baa-a97bfdd149de")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95432b17-c57c-4c24-9777-33e5609cd972")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5abf8e25-459b-4a05-b414-c8e8e2647f42")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "447c18c4-e80f-472d-a95e-9a3b3acc6b8f")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3874c2f5-7e3b-4404-97d8-6136178cd90c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e95a092-47ba-4d14-b81c-1cbd17cc04ce")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5920397c-798a-4687-9449-ad3f6d9a2bdc")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f7b976c-bfca-4f7b-bbf1-4f70b80491f8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbd9db8a-3663-4fee-b09c-ee3eadda757a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9223c83e-d24b-4e77-a11d-b828008bbed7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1d7dd704-34de-4b8d-9ef2-aad91f554885")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 32 "/ZIF_41")
			(pintype "passive")
			(uuid "005bf82a-c747-4bd4-acd0-0b521ff9bf71")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bd8d3600-2d43-4070-b8f1-15be64c954c7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(uuid "33961d86-963b-4064-ba67-29c5446bec7d")
		(at 156.843 101.04)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
			(uuid "75ff144e-ed47-4783-b0ae-6dfc527645db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Switch 1"
			(at 0 1.9 0)
			(layer "F.Fab")
			(uuid "02d8cd22-c183-4428-afea-1491f9da682a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4dabf59-7369-4d17-8931-947a0a35f9ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb00fc1c-330d-43b5-81e2-3a148eb17c26")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Jumper, 2-pole, small symbol, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fd5a8825-b349-4136-8b78-ff0d9ffa9da1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(path "/6169a5e0-4dbf-4041-97ac-48bdb3f9a8f1")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(fp_line
			(start -1.4 0.3)
			(end -1.4 -0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec61413f-1138-4835-91af-026fffb727af")
		)
		(fp_line
			(start -0.7 -1)
			(end 0.7 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c84eb563-aeb1-4081-914b-7817fd3176e4")
		)
		(fp_line
			(start 0.7 1)
			(end -0.7 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47b6f3d4-c5b0-4de5-a843-a76c3b6c779c")
		)
		(fp_line
			(start 1.4 -0.3)
			(end 1.4 0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b931411f-885c-4519-847f-07be41351728")
		)
		(fp_arc
			(start -1.4 -0.3)
			(mid -1.194975 -0.794975)
			(end -0.7 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d632bffc-7f8a-42ee-aa09-3cbf913b9acb")
		)
		(fp_arc
			(start -0.7 1)
			(mid -1.194975 0.794975)
			(end -1.4 0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42fa5417-7cf7-46fb-b0be-131d33417f4e")
		)
		(fp_arc
			(start 0.7 -1)
			(mid 1.194975 -0.794975)
			(end 1.4 -0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "677369e0-5a66-4418-a6d1-e29949aaec74")
		)
		(fp_arc
			(start 1.4 0.3)
			(mid 1.194975 0.794975)
			(end 0.7 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7d18936-6b8a-4f09-b5ac-ad9bde0ff3aa")
		)
		(fp_line
			(start -1.65 -1.25)
			(end -1.65 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a38bb10-2471-4070-bc38-ee9f8de26652")
		)
		(fp_line
			(start -1.65 -1.25)
			(end 1.65 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16201d66-33ae-4306-8fc1-3c7ca3141951")
		)
		(fp_line
			(start 1.65 1.25)
			(end -1.65 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70dcaf47-9ee4-40f0-b7cf-01e33cbd0e57")
		)
		(fp_line
			(start 1.65 1.25)
			(end 1.65 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1b79d12-cce3-439d-b3e6-3802a8d7ebc1")
		)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VCC")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(uuid "5ded1f11-d7e0-4f3b-88a2-935fcc753a74")
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 52 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(uuid "060f37b1-b1d2-4056-8758-12f88a32d9b6")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "34a53d08-7461-4c09-998a-4d8feaeb8eea")
		(at 103.143 108.52)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "4b19806f-b280-4df6-bb49-3f005c4516a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "bd4e66b2-7e71-45c6-9d5a-cada48af90e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d29c2ec2-2a64-4695-a30a-28db20476337")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0e345e0-98de-4c90-a578-c8599435c969")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ad02781-c60a-4919-80fe-aa649dd91a24")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/90271017-aeb1-40f7-9039-f7823c6e6257")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cbdb94f-8098-4719-ad13-41588cf62d02")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca011eb1-7ab1-40f2-9998-024261c14320")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5291828-3cb0-4a34-af00-66cde30ab421")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ed5d33ea-ff07-473f-b5cd-074c7b73776e")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4c1ee9b-0dbe-467c-8302-57ce299f056e")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25501d8d-ed46-4697-8299-d8a0dd535232")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a87a795-b269-4a6c-acd1-26cb130d2a71")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "308b846f-ff36-4646-872e-0eaeb861565d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0d4cc8d-33f6-427b-9bee-54b0d39cd327")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de24a4af-da6d-42d0-8cbc-7b831b3027e0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "39cb147f-3e1c-459f-a390-9706d7feb148")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "067627aa-0791-43d6-b3c8-3536f22eed59")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f01975da-0f54-450a-b212-14359a108e03")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3567b3ba-42e9-46e1-b4bb-de1d974510f0")
		(at 133.143 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R21"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "c66add02-6d0a-4ecf-9a97-07be1b6f2080")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "5e1739cc-f947-4c3a-a075-e37ba2c397eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "354a4de4-8762-4977-b501-d8f81aed3c76")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6092cbef-5130-437d-9317-35b471a6479a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "458bc202-17be-4a11-adc1-fd1aeb3e3301")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/31d53b23-bca7-41d7-9431-1f9109493610")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e462df8-bdce-4e94-bae5-b368cc08095f")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b872a255-e33c-4a6f-9e95-e061e69f2282")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecf847e0-de83-4d32-a81f-811abf690798")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f2e4de6-a4bd-466d-a586-2946e7b7bf18")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fcaf91da-4522-4c4f-88dd-55fd722c13f4")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f788e1a3-5ed5-400f-92ec-05f4ca61563b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79f2701f-0dfc-487c-afa5-0af7899627dd")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d140c9bc-8231-4b22-884a-97b92c304cf7")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "133c5145-a5d6-411a-88fe-e7ef535fc8a5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaa9feaf-472c-40b4-aeea-cd6a58842c8c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cc0f2713-be3b-4b81-a8f3-49fe5245b070")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 77 "Net-(U4-QD)")
			(pintype "passive")
			(uuid "025f0341-707e-4dcf-a43d-e91be7f1e660")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 21 "/ZIF_20")
			(pintype "passive")
			(uuid "46747127-74c0-4b74-9805-6817d95a1e1b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3607e365-8af8-41ed-86eb-51a48bf770aa")
		(at 139.093 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R26"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "d0cc6123-fc25-4242-ae09-19633fb2423d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7d5ad7f2-6abb-4566-8150-00ad902d93e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "aceecb32-5ad3-41de-8aa0-3515dbc68415")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6893d769-6837-4ff0-a28f-43edcdac650c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5287943-1953-414b-8588-24015582330c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0b067187-573e-4120-a84e-d15ec9f1f717")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a59bece-c88a-443c-a3fb-946aa518ed41")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91a2ad6f-980d-44fa-bb27-216909701bd4")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7aa458fd-ec95-4012-b2be-c1a4378d391b")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90b3517f-2a3a-4c19-b2a6-5367aec9f636")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4ce50ac-9e1c-4389-bffb-1930d5c00a88")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cfc3e1c-3d71-4682-94c5-1c705a35c2bf")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d67a9581-7e5b-45dc-9b25-ef23a020f632")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a3af2ce-0c53-468a-8ee1-8ee02eb73699")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb035c4f-f0f6-4cc4-bd26-8d48e0c995a5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88b9ace3-3138-4b93-acbf-586b84ca8e6f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "650615db-c006-468f-9a50-9920729e27ad")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 82 "Net-(U5-QA)")
			(pintype "passive")
			(uuid "03f90c51-5821-4e0d-933f-2681c284b0dc")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 14 "/ZIF_26")
			(pintype "passive")
			(uuid "9f485315-05e6-4af8-b40a-3dda7724d2d9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "36be488a-b466-4aae-b4f6-41fc725799b8")
		(at 145.043 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R34"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "92fc4802-4d4a-4d3d-89a5-af9ee99b76ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "293ffb71-ea01-49f3-aaff-33fb7f181a42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "00520013-c16a-4091-bd3c-a22da507e2c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "487266bd-8c46-462f-ba3b-22abadce6fc5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "25a584d2-3594-437e-a1e1-e1dd26310e97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a3a2eaa1-234f-4f95-8817-4fba41932d0b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "719dd3f6-4a1b-418d-84c1-326b0aaba0d3")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9994ffdd-1843-4a0d-bde3-ee78e6e4d916")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f82f564-fc33-4ce3-8f44-5bc96f991911")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01d08ab8-2649-4f1a-8e77-9779f69f7482")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3c9fc75-da85-427e-a1f2-bc55fe569750")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4bffc4ea-9b97-4dcf-9c00-0c307f68954f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac895541-1a93-478a-a410-f74992c9beeb")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "042bb482-0db6-4ba3-b08b-62bf2f1d17c4")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "771d8200-14e3-466c-acc1-93e9a551ad72")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51d2f41d-c36c-4b74-89a7-3a37c1ff3297")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3c91eafb-40bb-45cc-8eef-9c935eff8c6e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 90 "Net-(U6-QA)")
			(pintype "passive")
			(uuid "ca379e01-a500-4b88-af44-7a3dff01d3b8")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 16 "/ZIF_34")
			(pintype "passive")
			(uuid "c85fcddc-635f-4357-8b2c-4193e62a6150")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "36e2489a-1c72-460e-8405-920d6767062b")
		(at 153.793 93.54)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U11"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "645d2341-a976-45fa-b542-a1be87253d67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT166"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "8540efbc-14cd-4381-939d-cb295f7aa5c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d7b9162-3126-48de-9611-5404ad355fc3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "147d46a1-0338-4070-b08d-da885802e370")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45d5db9a-8636-4657-bd4a-055b254a29e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP?16*")
		(path "/3b6eaaa2-394d-4566-8c9f-2ba3b8b4f4c4")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62f35ee0-3baa-401d-8e5d-d4a7b3aa624f")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3184ec9d-242b-401e-a2d5-e351fe07dc9a")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bde37013-786e-40af-a2d0-3109f2313c72")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f0899ae-4322-4ca5-85ea-4e925111d52d")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "880e932a-6243-46f3-8f67-19f8dcb482fd")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ccf3c02-dc28-4e0a-802e-d26595a26963")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b53a1089-02da-459f-92e8-e8a695715bd1")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3a6605b-5022-4716-a549-cd483b920e7b")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91e6bf21-fa41-4fa9-8ea1-4e75a1ef9c5c")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99f91401-596e-4fb9-8af3-0775760f6d96")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a317da4c-8277-49a4-ab1b-88862f1a2d0a")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a73e0746-ac67-4b67-8f06-8162b33fe7f5")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c208453f-6d0a-419b-8c77-414b64934030")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ece52666-3479-4717-ae10-462b77c98211")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a0184c92-0921-4209-9c96-7e32ce73cce9")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U10-Qh)")
			(pinfunction "Ds")
			(pintype "input")
			(uuid "96ebeedf-9457-4094-8a36-c5dc055379ed")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/ZIF_26")
			(pinfunction "A")
			(pintype "input")
			(uuid "40c9d6a6-93dc-4076-bb39-0e9853f232f2")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/ZIF_27")
			(pinfunction "B")
			(pintype "input")
			(uuid "09dfa028-47d5-4672-9c5a-bac9ddfbb88f")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/ZIF_28")
			(pinfunction "C")
			(pintype "input")
			(uuid "0f008262-c91f-4546-9fa7-178e229e0277")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/ZIF_29")
			(pinfunction "D")
			(pintype "input")
			(uuid "6a77a364-a7a4-45fc-bce0-3f7c78c0d26e")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "/PISO_INH")
			(pinfunction "CE")
			(pintype "input")
			(uuid "a1192412-2471-4a52-b729-7b35ead01b06")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/PISO_CLK")
			(pinfunction "Clk")
			(pintype "input")
			(uuid "f4371e4e-05a5-4f3f-a3af-a1e3464d3fde")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "484c780b-bbad-44cc-9494-a55ff3e3fafa")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "Clr")
			(pintype "input")
			(uuid "93563463-9175-48ef-9cf7-6aae811d9073")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/ZIF_30")
			(pinfunction "E")
			(pintype "input")
			(uuid "6a0a4b5c-a8ce-4be3-89a5-1aec52d6e977")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/ZIF_31")
			(pinfunction "F")
			(pintype "input")
			(uuid "ec79dc6c-0129-4ae4-8563-f6121723ed5b")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/ZIF_32")
			(pinfunction "G")
			(pintype "input")
			(uuid "1d513647-2454-441a-91de-ee067d94ea26")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "Net-(U11-Qh)")
			(pinfunction "Qh")
			(pintype "output")
			(uuid "fa9663c4-7f70-4046-8b1f-49cb73fac106")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/ZIF_33")
			(pinfunction "H")
			(pintype "input")
			(uuid "e5191c53-a8ad-488b-908f-1cd3a87c1606")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/PISO_SH")
			(pinfunction "PE")
			(pintype "input")
			(uuid "ed7f70ba-70df-4551-a9eb-8478b23220cd")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "3101519e-316f-4759-8d9c-4d40e45e08ea")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(uuid "37b509bf-c730-48b6-9032-9652f73fbe8c")
		(at 142.353 113.075)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U7"
			(at 0 -5.28 0)
			(layer "F.SilkS")
			(uuid "744d6466-c7ec-4791-9318-11bd345e6bf3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT02"
			(at 0 5.28 0)
			(layer "F.Fab")
			(uuid "8ea744c5-0f05-43ec-9928-2961d9a73ec3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2523c249-cad2-43bf-b221-7a3c0491b455")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74hc02"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c10f311-3a84-4062-828d-3f2a50c030d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "quad 2-input NOR gate"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0482e1eb-0072-423d-b2b2-269157fc889c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SO14* DIP*W7.62mm*")
		(path "/da4d64d8-8a89-4a31-8c29-a715b37be528")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -4.435)
			(end -1.95 -4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9895e103-f073-4bca-8d0f-265e3b4860c7")
		)
		(fp_line
			(start 0 -4.435)
			(end 1.95 -4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e95e2a85-2a08-483e-a9fe-cb54cd54bca9")
		)
		(fp_line
			(start 0 4.435)
			(end -1.95 4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9aaac033-3bce-4360-ab81-20f8f3d845d4")
		)
		(fp_line
			(start 0 4.435)
			(end 1.95 4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec4d1f73-8ee2-409d-ac4d-e1c793196a30")
		)
		(fp_poly
			(pts
				(xy -2.7 -4.37) (xy -2.94 -4.7) (xy -2.46 -4.7) (xy -2.7 -4.37)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "ba99b9d7-1818-45d6-a3f5-9ea34804bb9c")
		)
		(fp_line
			(start -3.7 -4.58)
			(end -3.7 4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0edeaa54-0848-47d9-a9e5-c0b401436b1a")
		)
		(fp_line
			(start -3.7 4.58)
			(end 3.7 4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97021ca5-29e9-4c0b-a6b1-4094883a6ef6")
		)
		(fp_line
			(start 3.7 -4.58)
			(end -3.7 -4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eede1fa5-0e73-4d75-b0e9-a9501ae14bac")
		)
		(fp_line
			(start 3.7 4.58)
			(end 3.7 -4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eed28ca6-3f00-4e31-85e0-a289d44bdcdf")
		)
		(fp_line
			(start -1.95 -3.35)
			(end -0.975 -4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80fdd432-7bc2-4c21-9ec1-ef2cafe9796f")
		)
		(fp_line
			(start -1.95 4.325)
			(end -1.95 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ddff3ca-2305-42b6-939e-444e495b0457")
		)
		(fp_line
			(start -0.975 -4.325)
			(end 1.95 -4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48abd47f-0983-4d38-ad64-1a9865fa2e35")
		)
		(fp_line
			(start 1.95 -4.325)
			(end 1.95 4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6aaeee0a-3f84-4f7c-b217-b9a712ef2984")
		)
		(fp_line
			(start 1.95 4.325)
			(end -1.95 4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18490939-3658-4bc4-9ad8-cc17dce3c16b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c86d1b1a-741f-432e-a0e3-db16e540ab75")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(U7-Pad1)")
			(pintype "output")
			(uuid "c369923e-ae5f-4b9a-a3c7-8cdbbad5bc31")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SWITCHED_VCC")
			(pintype "input")
			(uuid "55a5677d-715a-4646-9457-053ae7da9679")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/SWITCHED_VCC")
			(pintype "input")
			(uuid "62c063ba-6dd9-4400-b5d6-fe1dcd546643")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "Net-(U7-Pad4)")
			(pintype "output")
			(uuid "c4bfd7e7-236b-412c-988c-a507f9df2028")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(U7-Pad1)")
			(pintype "input")
			(uuid "7c86a59b-7878-4b97-a4bd-3059b81a2b4c")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "/~{SIPO_OE}")
			(pintype "input")
			(uuid "594239bb-af0e-4af6-aa39-f76ce110f26d")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "0b2ef8ef-f983-456f-a11f-484d624ba944")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "Net-(U7-Pad4)")
			(pintype "input")
			(uuid "13306e3e-ccd4-4389-bd17-a615a1de8b52")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "Net-(U7-Pad4)")
			(pintype "input")
			(uuid "b5b454cf-af1e-4d9d-8f18-3730d55b5b95")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pintype "output")
			(uuid "1480b4f9-7593-43bb-94e1-7cc618abebb7")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "/~{RELAY_ENABLE}")
			(pintype "input")
			(uuid "99f3915d-9a28-4825-8737-657e5bb9942d")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "/~{RELAY_ENABLE}")
			(pintype "input")
			(uuid "8eb5a3e4-f31c-4f25-b594-0738bb3b52c4")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "Net-(R1-Pad1)")
			(pintype "output")
			(uuid "354041ad-bd66-47e8-b747-8d82fb94b0a3")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "a2c99338-a90a-4f36-b126-3d8b340cdc18")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "393365a2-6472-47f7-aba5-c2d57a0181c9")
		(at 127.193 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "de0cb479-ea06-43c2-978e-4dcf2b55ba5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "5702f082-79cf-405f-91ea-e577573c1e83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "39b19c5e-ea31-4ca2-bf38-25607b13f510")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0351573b-68d5-4e95-87b0-5f8c66e8cfb4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e73acfee-14c3-4cad-bb8e-26f6886a1499")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3bb84ce1-9c2b-4bff-bbbe-e6ba2f64923a")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "840c6d73-5bfa-46f9-a215-2ad737dd39a4")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87cf3561-cef3-4d50-bfe1-12841413ad64")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e60ccaa4-f7ca-4189-a214-7155be6b70df")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d253ed14-ae1e-4890-90d4-90872dc9fe9d")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e65e8747-5e4f-4763-a0a8-11e667acd9fd")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "498a2208-b5bb-4e60-ac7a-4894e048f8a1")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "316e9a22-fc2d-458a-8626-515ace56c29a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15b8b538-d953-4b2d-a001-d92ca684cf37")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc06b2af-044e-4506-8643-d0eaa28ade8a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6577af50-9165-4f67-bb29-cdfeded59d06")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c40768e9-e38c-4abb-85d6-6d9d48e3415f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 62 "Net-(U2-QE)")
			(pintype "passive")
			(uuid "d4d159d8-22ba-43d6-959e-95fde847a7a6")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 45 "/ZIF_5")
			(pintype "passive")
			(uuid "84cc0266-f140-444a-a82d-6df735c17bea")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "395feaa9-9fb1-46f8-8a3b-6d415e317d28")
		(at 156.943 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R57"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1478e6b7-b17c-4452-a5ab-7c2817abd7ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2fa82243-09d8-4145-8874-99b5ce4b3531")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eab83991-ad55-4054-b4c2-63cb3b2e31e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9654f44a-5636-4189-a718-e25a7c21f297")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b71dc11-0a15-40d6-ac47-bef14e1c224b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4d33fb62-c5ac-4ec6-a31d-b580329d01ba")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aebdd7bc-ebca-4bad-a8e0-8624740a6d44")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c551f337-c363-4c0a-93a1-37cc5cf7e591")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "114d407d-4eb0-4fd5-ae41-7deb6414f27f")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "96299fde-1a1c-4f20-81b0-f547109dc26c")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b90aa86c-c3ee-48c4-855e-3e10e22b116c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8e620f1-23e8-470e-b5fc-43fe3bafc196")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4dd9db8-1b38-4cc0-8d33-62df46dbc2b7")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "577e7402-5691-4610-ac3e-e68b3c2e8a2f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f78d9e27-c751-4eaf-a385-c0f545f31806")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53bf20e7-320a-47aa-90bb-f82b42da8228")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1ac419f4-1062-45fe-9765-d14e8b871c33")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 25 "/ZIF_12")
			(pintype "passive")
			(uuid "36a5639c-ac81-461e-bc2b-cfe5884911ff")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ed15c4c4-4945-40d7-a033-7a5bfa583067")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3a6cd422-660c-44fa-936c-a1ab2517713a")
		(at 139.093 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R25"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "5377593b-47af-4410-9b0d-6d450e3797a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "d8f03051-d182-4e28-aee4-1cab8196d500")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ce6b9013-0f74-422f-a184-f864ed43336f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "41f862da-b1ac-4e4f-9b4f-7df42fe060e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "911f067d-b243-422e-a53a-d2a7da8e82b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/66734b48-dcf2-4a29-82f8-10b615b80ca3")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4665893c-d9aa-4b29-83e3-1378121c88fc")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6e43987-4e24-42f8-921d-f7564e5e3dea")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ade2df4-db19-467a-afb8-c4a58f0d46e2")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "515cb80c-9e7c-405f-8d80-f80f04ac77d1")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e9d2858-5d4c-4d17-b40c-5b2775cbe638")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4226834c-eef4-4d72-8747-0a39e11e6864")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86bc4ca0-7327-475b-a35f-28ac37557e1e")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0504741-886e-466d-a222-ef2e7ea6755d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ebfd8ed-8162-48d7-a0c9-575ad295e0a5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "deec4b1c-e021-407d-a312-d718ba097f55")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5fa0b853-d03e-4729-ba1a-f78d3c2ec0bd")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 81 "Net-(U4-QH)")
			(pintype "passive")
			(uuid "883aee6c-193f-42d1-9dd1-db61087db29c")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 22 "/ZIF_25")
			(pintype "passive")
			(uuid "751cc22d-e511-476d-8eef-31e9667062e2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3b5e1ac1-e84d-45a7-86e3-4eb91382de75")
		(at 150.993 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R53"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "e9077c2b-b2a9-4ca5-988a-dcb3303c84da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "fcbcbd2e-559a-47ba-9b35-071515940db4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65b04edb-1720-41c2-abaf-8f8f1993eef9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "34f7502d-e216-49e7-86ff-5a6269b74f0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1fcdd149-0975-4186-b0da-5f059cf92ba5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fb9db377-6046-4698-8e45-eafa195eefdb")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e539913d-2bb4-4c72-8a23-5f7f7fc58f04")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49e06748-6ea7-4bb4-ac6b-d071f13ea1e1")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50879860-18a0-48c8-89ad-094f532b7abe")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91f33668-8817-4149-bcb0-b717653f0607")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "440f00e8-9bfe-421d-984b-8fa5563310a5")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e6fc666-1a27-4222-a531-17e0ce63231c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd8cf86c-6d71-4037-8a2a-4551f44454b0")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d6fb410-7366-4fae-97eb-1c451d8ed61b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "123adb0d-f33d-44bf-bb1e-38e135b13dc6")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9291198f-d08a-4552-af19-00dedb91d4f9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "48ad4025-1155-49e4-8fae-8935b03e83aa")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 29 "/ZIF_8")
			(pintype "passive")
			(uuid "5d4b35fc-86fd-47d4-881b-2f93a13c0935")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "cfc112e0-4f17-42f0-b3b4-f3d72df14408")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "3beb6bf7-057c-438b-a1c5-6037bd1e91e5")
		(at 109.153 105.17)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "0622df8d-e110-41cd-ad09-879660dc5428")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "9df052c2-0285-4e74-b88d-7b76b39543a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de4c4f68-fa80-49d1-842c-89d1a5bf1a84")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8fb60950-7b1e-4044-a6e6-0db6c8ed3348")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c1d9a20-0360-46ae-ad8f-82968bdc4254")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fc5d67c2-0536-4261-b843-6366cbad1a5d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cac0dbd-abc9-4f60-b9ad-1e4b1428472c")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ef57bde-c15b-4c54-90ef-3973f958b621")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56a13e93-abe5-4657-93af-97db63dd667d")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e99bc87-2408-4890-9618-7cddea111f4e")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12d8ab2c-0a2c-4cd5-afb7-7a6331ba5166")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57417dea-06c5-4ce1-b551-350614b393b0")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7967e79-46b5-443e-af07-6627c423756c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c4da428-6a9d-4685-9db5-afc151a46328")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04393bb0-bab2-4dc6-92e5-0f1aaec8118d")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1a0e2a8-6bab-4e62-b47f-6ce850658be9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "466693d0-3f8c-4991-85f5-00883dddea99")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "3cc8b426-542f-43b7-968a-51edd7e50ee0")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e3f6482c-e4c9-406e-b940-e3174d46a393")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3c536bef-154f-491a-8c7a-310f5b4594e3")
		(at 139.093 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R32"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "7793121e-3c08-465e-9694-4b8a1719c22b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "879eff6c-a3b4-446e-aad8-92dabf022a81")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88692274-bbd5-4ef8-bd8e-a8cfeef67f05")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "600beefb-1ff7-4977-ae25-a39df448e4fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "add8c186-4654-48ae-9248-574747ddc218")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5661f754-25db-4487-800d-133f1a0aea1b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68233b40-1122-4c4b-bd0e-7880b868076b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb80b2c1-7977-423a-8840-be2db2e7ae49")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb692c20-185f-4c3d-bae7-6d3f782a4273")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bf2daf9-9676-4a9c-be9b-a8c0b12e85e9")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38e1ac9b-b2b1-47bc-83b5-60b1f72ed33e")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c36c0e5-f845-47f8-a610-25f8e9ddf9af")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed856288-fcb9-418e-97b0-e25c3547abbf")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0051a0d-e879-4ef6-b224-d55a0fb0d363")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49d52962-c0b2-4592-8b63-a97050df31c5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b139ec4d-ae4d-4dfb-bfa0-e07f3ddeaa3a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dfcc2010-c993-467a-9824-5a2e10a2392a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 88 "Net-(U5-QG)")
			(pintype "passive")
			(uuid "06ae1e6e-620e-41ee-ac55-e5f353462be5")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 30 "/ZIF_32")
			(pintype "passive")
			(uuid "a3dc64bd-bec3-45fc-b1a1-5a69bee76cca")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "3e0b7144-db2b-4ebb-9cb2-44e49fd8859c")
		(at 168.843 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R84"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "ececdd6d-a257-412a-82ff-95732174ff4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "3a9db501-e397-4d71-b811-b02402e10357")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8467c7cb-af86-495c-82ff-0e255cdccb71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "53f1ecdb-a4f0-4af9-a467-e77ea7b0679c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b990d15a-08c4-4cc3-974a-136ea65eac45")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f8d2c653-7b9a-45dc-8c28-f0a16bdd284e")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4434dd6-9baa-42d9-9109-ee715ef68764")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca06aad8-1cf4-4a7e-ba2f-4d4e0de4b8a5")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e56b2760-40e9-4e8f-91d3-179c7e12dfc4")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ed996c30-b497-41f4-b943-4b6147ae19d6")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "756b82b3-ff35-4f5b-82ca-dadce3e4afc9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51763c9e-a83d-41d1-9aab-15ec544995bb")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c1cd319-c252-49ec-83f5-d3bf1e5b0ea3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2dc980b5-aa3f-4799-8215-761faca4ee61")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f8efd43-46ee-42b6-b406-b48bc2a00953")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3629d558-40f1-40cc-889b-624db721b710")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "44438441-0909-4978-9b0d-5313166953d8")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 34 "/ZIF_40")
			(pintype "passive")
			(uuid "eb5a6536-4a4e-47b6-a80c-3f089d8b4c83")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b7992437-f80e-43d2-b779-a251327300e7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "4028f271-5a54-497e-a368-dc0023110360")
		(at 139.093 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R27"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "8cbbb1ab-6c14-4d70-bbee-f10b99d74d54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "ebcede58-ddcb-49cf-99ca-69b2e35efb51")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57d4ec62-c66c-453a-ad37-bc173095d6a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fd526a74-2680-4c6a-b45a-b470cfa72ece")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e46c6823-3e4c-4f2d-a39c-bd2b957f3e8c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f6eabe23-8f99-40c7-923c-a640f051d8ef")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a15502e-f5da-4952-9b50-e8e78dec98de")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60d59f45-6542-4b3b-82d0-a238a73506b5")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9a0dbbf-fdfd-4733-bee1-437523baabeb")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e113e3b-3093-482a-9dff-ded81ed6b774")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8eafcfc-5df3-437f-971f-36b9aac57914")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14183c97-2623-4e51-80a1-66848f09375c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6c11d4b-b983-4731-8f7a-62663fb5cc26")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51ebd5a2-b6bf-4d02-b6fc-9e1ace1117d1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73d8f86f-f7e8-4fbe-8789-df5f4f7b920d")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b39847d0-4d09-491b-8092-14a5ec08b2a8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3d20a0bb-646f-4b45-9ce7-8b0908267641")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 83 "Net-(U5-QB)")
			(pintype "passive")
			(uuid "b8f785ae-2068-4685-8cac-53282abb6118")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 28 "/ZIF_27")
			(pintype "passive")
			(uuid "82106ca8-3b92-4694-818a-91aa2383fd19")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "41b09f0a-64a4-45d8-8973-fdaef5c7f70b")
		(at 145.043 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R40"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "fe146e57-8013-4ebb-97d5-bdadbd952632")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "e8b1efbe-c85e-4436-84e8-b61166092512")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d99aa14-0839-4b5d-8c06-47f3436e0dd3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb9bda3c-f282-49bd-8d6e-c7bd9e2dea21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b049a765-cd49-4821-8c46-3cb9b798db04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/49bf7fbd-09c1-4003-9845-199b498d3d90")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c70b1a22-05e9-4607-96d6-f7bcdbb3e153")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbd5983d-5d5f-495f-a053-bce5417c1201")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2122ea3-16f9-49eb-a572-9e39d5b0a359")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5364d1d-2f93-440c-8839-0fcdaefbf602")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ad33c74-18d0-4a4f-99d3-786392a5e013")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9fba1dd-1958-4ae4-bf6f-35ed342ed634")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "650d7465-5fff-428e-b87b-92ce9e93e066")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13940eee-fc79-439b-836e-9581c8dbc963")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "899d8d29-2c16-43de-ac34-aa198e82bda8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b7a21c6-1400-4d80-9c5d-eb4bcc0b41ea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a6164bd8-5e53-4083-8aab-58c69f7ede4a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 96 "Net-(U6-QG)")
			(pintype "passive")
			(uuid "f1ac1aa4-f7c7-43e7-8dfa-83abc45844fe")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 34 "/ZIF_40")
			(pintype "passive")
			(uuid "1d37d2e9-9408-428d-98c1-acccdcd14737")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "42e05d8b-581e-4dda-b898-d0373cacb613")
		(at 103.143 105.17)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "42fe8bef-c9ac-4d28-b75b-c376badced02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "0b5aa817-77da-4931-8fd9-a0963db45387")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d22819e2-2971-4301-84e2-40e7f3675ba6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ce8c396c-5fb4-4335-952e-6ad51d1fa9ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3effe2ee-4e7b-41c4-922d-b3e978613be8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/08573b9d-ce10-41f5-b8df-dac6444c4f9d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdeaa2a6-42cf-43ab-bbe4-5c2d2dcdacf1")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e00be5e-8d5c-42d1-bffb-f4d9ec1720f8")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f393739-916c-46b2-838f-8502bdc4ceec")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a834bab-d02d-41ba-8362-4bba49d8f91a")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58550e7f-13d9-45ec-b2b1-51c0cb37358d")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ce65ebf-2252-44a0-acd9-f5ae20dab278")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1c4778b-26a5-4576-b8b3-f894efdf507b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14aedcae-352e-4bb9-8a6b-70207dafce81")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0466c33d-ac44-46a7-b7e1-de55820f16a9")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fce9764-1630-466a-8ebd-357283bebe59")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3c609df4-75ee-449e-9139-d7db512ad734")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "8cfa1f65-bdda-4118-add4-4567c9fa881c")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "240a4832-6fb4-45e3-9d25-6979773d27a7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "45264b73-b55a-49f7-b7da-de276303457b")
		(at 127.193 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "775b1ef3-f7ad-487f-9bd7-f3d998d784f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "bde3f2f6-dfcb-4e6c-b82b-c3c97dc4791a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d366320c-5de7-4d44-a8f4-3ed055994c26")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ac1a5ea-3397-4ea4-b793-829a5af308ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc17771c-8e8a-4750-9046-709f2b6b88c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ecfd5daf-825e-4ead-896c-a37505b6cbde")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b446c84-93ba-4d95-a195-ac63941fb14e")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aed28aef-3754-45b5-a42c-c744f9181e8c")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5904722b-93a9-40d3-8f8d-c589c58ea2e8")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "187452cc-17d7-43a7-b35b-5d5a514a8419")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e3feb43-0705-4855-996b-ae7d84b9e22a")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "940cfab2-0593-4f34-a704-0cd36af1089d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75106554-5b77-4ab9-9fcc-3f9c92d0de3b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5f0d50e-0074-45db-8cf6-19556724a26a")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a79ab49f-e605-44d6-9e77-1050ca59b544")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "156d24f5-a23c-437d-a62c-3e46dfb3476b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7300a25c-3a67-4776-bfe6-d32842934fbf")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 65 "Net-(U2-QH)")
			(pintype "passive")
			(uuid "c3987756-ad7b-424c-a896-e3736aaa497b")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 29 "/ZIF_8")
			(pintype "passive")
			(uuid "688f812e-e6be-4cdd-bbf6-d40243ddf978")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "45e508cc-63c6-481d-bc02-2ebc6dae26fc")
		(at 162.893 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R67"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "62d9a70f-c7ce-45e3-b4d0-897f1bb7c7e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "ddc92796-12da-4b79-958c-71d5c77963e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e403894-97d7-4bde-894d-8955fccf8b6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "70125873-d4c8-4605-b9cf-d88af72853c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8899ce63-544d-490b-b4ee-a28545ca2517")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/835e7d88-e086-4146-91b1-a76808a85a4c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4db2fa92-1f68-4e38-91eb-197f8e7ce586")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "919550b6-2d59-4c83-ab69-0f75e9a88d87")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12330e6b-95cc-4541-be47-ecf197877e24")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97b81088-9c87-457e-a39e-e1e5c2116a3c")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30efe6c6-003b-47b3-b871-f4769f9727da")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4715553d-d0d5-43ac-97e4-78b76bd06256")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a481370-bf14-43b5-8cea-d6467d55f637")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb48b55d-d84e-45d1-8bf2-f70f89f903da")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d036783-b727-49c6-8b9c-d8ff746982d7")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4482ad5-b327-4e08-83b9-51094882b24e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "61b905df-7d9d-417e-bd44-07e9b3608406")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 41 "/ZIF_23")
			(pintype "passive")
			(uuid "d3f5d7a4-4487-4d41-b35a-ab715f3c0b49")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "997ffd06-1ddf-47fd-85d6-e3685a3e13fa")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "4c4e08ad-e7a6-40e8-bc5f-1c85d8c8863e")
		(at 145.043 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R43"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "2e96ae18-3dd3-4bad-8aa4-415572582b4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7089acb7-1522-408c-84e3-8539306e9791")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d3e883d-0f13-485a-b475-c30f1c703d47")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2390e696-916c-4a76-be13-07bae67a3032")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "82b6096c-500d-44dc-bb39-b8b3da44257c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c27cae58-77bb-41fb-9647-33f809f2f3eb")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a9b2cf5-67b6-425f-87d9-c82129e0ff1b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d54e213f-56d1-459b-a283-110312a62952")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6aede272-471e-412b-93ea-cf2d5f11df76")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5aca922b-9f3f-4d68-8f23-d6d5a17fdad8")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fa7c896-986d-4261-b847-70b2cb18988d")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a093c3a-952e-435f-8e5a-6434a454b817")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55f2f416-a479-4b8e-8709-01ec40b3427e")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a0b53c5-f3ec-4224-b1e9-ec23fd884104")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce6a843c-aa6c-48e5-9f1a-79f8b6a73a02")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afe0def6-a7fe-408d-a643-f8714f90ef4c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6f2bc9f5-354f-477d-a271-d3610d8437ea")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 6 "Net-(D2-K)")
			(pintype "passive")
			(uuid "5904e97d-f406-477b-90f8-669ce5759429")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "788b69fd-8b81-4655-9eb5-23902a61a5ae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "4d8c54a1-fb4b-4425-b3b7-2c7b19d9664c")
		(at 156.943 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R63"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "411a07b3-66a2-478a-a64b-e4e01e93ebbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "20beea4c-c681-4a3e-beaa-5ff2ed8de52d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2cf0cbf9-bc79-4c60-bdca-b4d3e7d9c945")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3dc71e7f-a6c6-4302-b59a-882d11140088")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4860c781-d726-41c7-acbd-e2e403bdbe1e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/75fbf002-1461-44ff-ad4c-210a0ea0590f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da1f335d-b811-4523-af73-99737e54e709")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b769ccfb-e8f2-4b6a-98ca-7060e1780e21")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eed220b8-4bba-4014-8f88-4a5ce751c7dc")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90cc5228-8015-4ccc-ac47-e7847f92e7e0")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "769d5c26-6de5-4393-9f5e-bf371c0d9048")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d9e0fe8-17bb-44eb-b105-da753b64f7ea")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83581351-01f7-4080-a2c5-5ebabe52c11a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4c54bbe-e66f-450e-a4fe-2155c582f216")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1692240b-c3b4-4ac8-9894-48b453e83304")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "073be527-988e-42de-8cd4-27f5420eab62")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d221a95e-d622-4678-9a86-3028dabb69a5")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 33 "/ZIF_18")
			(pintype "passive")
			(uuid "083cf108-6ec6-443a-97fb-e66dd9b8569f")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "2b45ad01-eb00-4cbd-bb52-af4432374a5a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "51a10655-2849-46e6-9273-2231f4ecde09")
		(at 151.698 104.35)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "b02dda21-2eb0-4cca-a4d0-8dad06447274")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SIPO ACT"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "4b5afb90-6a50-4f62-862d-b113ccccd587")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6743e1cc-c43e-472e-8585-c5652d4b857d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "476369b4-42a7-493f-a091-0e3ee699f9f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b17b4c6b-06a8-4ffa-8658-235365be54d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/eb298132-240e-4ebf-ab06-5f6c9a3e9483")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.46 -1.135)
			(end -2.46 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10a86f66-34a6-481a-810e-c1cc91ed8d8e")
		)
		(fp_line
			(start -2.46 1.135)
			(end 1.6 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "719c93e5-b65b-4e50-9bfb-3954e0d12676")
		)
		(fp_line
			(start 1.6 -1.135)
			(end -2.46 -1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e611407f-f152-4a26-8a68-69da3eb90c58")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4ee2bdb-51a4-4f70-899d-ef0ad34a613a")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39d33f7d-0638-4a19-8b40-88005d91e20c")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90f41a6b-b860-4534-92aa-cdd14c6bb4c2")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ef0c08f-c515-4f7c-95c9-e847b0c13e23")
		)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57d85995-d225-4898-9a70-0d968901333f")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7dc38f30-0b79-4ad9-a0b7-17984ef416bf")
		)
		(fp_line
			(start -1.2 -0.8)
			(end -1.6 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7fd731e-95b9-4094-86ae-2baf6f47f7c1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.2 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8507723-3d38-4c92-8bf9-d55db659017a")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14150fc4-d6bd-4e03-a611-0b0686ac1089")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b77bcf37-f935-4b18-a50f-e503d9ce9432")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "ac0fbd5c-23e0-46e2-837a-af94df00f2c1")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 7 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "66ddb363-cf7c-4500-b6a2-02e54695c44b")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "53ae2401-b8c4-46bc-9f1d-161d5abb5f85")
		(at 139.093 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R31"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "7fe85914-0cef-4a70-9794-56ef32ed5d57")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "f9fa1fe3-281a-46b1-927e-f8c9ac15c079")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6960d755-04b8-4c4a-a0d4-b80cf4f71fbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6554c171-982a-4997-946e-8d8eff571a7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5af7d96-28a6-4a0b-88b3-3048cb4b7607")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3e821693-4a8e-4df4-8930-1798a8c9574d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abe3c084-49cb-42c9-9a01-affd6c0022b4")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86d227e6-a785-40af-8fb5-fef3475921da")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3af746b4-b01c-4009-8e5a-c33580f37587")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6115d85-478a-4dec-99dc-0cd56f4ba299")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f9ac110-497b-47f0-ad8b-457387fdb8f9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a78cfdfe-208e-41bb-ac66-2fc4471bf12d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "219466a4-e0c3-4fbb-8814-af165e8f7f31")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20fade65-21b4-4be0-8036-f653a31f8cb4")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1125bc7-45eb-4573-9fd8-5a9d950f52ad")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c89de254-d9ca-49de-9490-9e66102ab4b3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "07beacc0-0527-44e3-b71c-06091bffcff7")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 87 "Net-(U5-QF)")
			(pintype "passive")
			(uuid "4b494ed0-68ec-42d0-a54b-35d0df467ef2")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 26 "/ZIF_31")
			(pintype "passive")
			(uuid "e5f25cfc-38f0-4d05-918d-465d6f531d76")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "553f51a8-06b4-422b-b071-514baca112b8")
		(at 136.893 81.92)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U3"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "e55024ee-a443-4b0f-8752-21403ff9ae17")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT595"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "bc404122-3bf8-4f5a-8ae4-46ec543ed629")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba4e5a31-2ae9-41ec-83d6-ea220b0ec267")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a932abef-6303-4617-ac30-e978aa4bb47b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e054e44-7063-4f23-8dac-079a8a6c4b78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(path "/51b564ff-812d-43d6-a0f4-48277aeb07f7")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54834dd5-d1f3-4db8-8cf8-dd3900ebd77e")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39d9ab5a-3f05-4358-948a-fd326c468a2f")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5971f481-fe04-4789-a792-acf9abe04e60")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ec906fa-c5c3-4651-9dc1-fa2efcfada85")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "d5c735f4-fd28-448a-9b95-c9750d048f49")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "640b36eb-facc-4ebb-8356-7166fe4c6d3d")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c700473a-8886-44ae-8ed8-4a1fa4736b48")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd5e7f71-aaaa-4cfa-b4ef-4729e644761a")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc9e97c3-dc96-4265-a278-507f1fead405")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa8f226e-72d8-4532-950e-e45bc0c942bd")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ee46b4a-4331-49e0-9dc3-d886fe2ecde8")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0deb0c5-a5b4-48a8-844c-4f7872d6f6f7")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81499b29-6ed3-4f84-873c-d9bd76bcf63d")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "507f5d2a-5f88-4dd9-8e3b-13834e10f87b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dabb6ef1-418d-41c7-a882-7c0ab1bfc5ad")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U3-QB)")
			(pinfunction "QB")
			(pintype "tri_state")
			(uuid "c1fd4a59-35fd-4867-9edb-e39b3df8eb1f")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(U3-QC)")
			(pinfunction "QC")
			(pintype "tri_state")
			(uuid "4eeca532-728f-4e95-830b-b30538fcf0c5")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(U3-QD)")
			(pinfunction "QD")
			(pintype "tri_state")
			(uuid "afa1e3ee-9597-42d4-a13c-313d725666be")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "Net-(U3-QE)")
			(pinfunction "QE")
			(pintype "tri_state")
			(uuid "57e634ed-55cf-4020-adf9-a2ad0e916db9")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U3-QF)")
			(pinfunction "QF")
			(pintype "tri_state")
			(uuid "cf1af855-38f8-458c-af3c-0d2ee42e3d83")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U3-QG)")
			(pinfunction "QG")
			(pintype "tri_state")
			(uuid "a00bf347-df68-4ac8-9ddf-107936e555ee")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(U3-QH)")
			(pinfunction "QH")
			(pintype "tri_state")
			(uuid "74791489-c15c-4eaa-a27b-928b825f54e0")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "34247c6c-efc4-4ba9-983b-5f6ed9fb8793")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "Net-(U3-QH')")
			(pinfunction "QH'")
			(pintype "output")
			(uuid "a067f765-0e3c-4234-85d5-cfab0b2a8063")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "~{SRCLR}")
			(pintype "input")
			(uuid "91ebdc39-dcdb-4c3d-957f-c31c90c7d803")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/SIPO_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
			(uuid "90a8cd39-71b4-444e-a72c-f15efb1d3142")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/SIPO_RCLK")
			(pinfunction "RCLK")
			(pintype "input")
			(uuid "0f95a204-bd9f-454a-979b-788880f489ab")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "5a7d3a3e-0be7-411b-9bfa-9c96531670ab")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "Net-(U2-QH')")
			(pinfunction "SER")
			(pintype "input")
			(uuid "c8cfbe68-0f4b-4729-bbf3-a79d69dbc715")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(U3-QA)")
			(pinfunction "QA")
			(pintype "tri_state")
			(uuid "926bd684-47f4-4e30-91ae-8ce1291d1332")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "c5eabbf0-e7ba-4b5b-8512-f8ac2efdc2f5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(uuid "5671f042-96c4-4fa8-96c1-98ad4e139aeb")
		(at 156.843 104.59)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 -1.8 0)
			(layer "F.SilkS")
			(uuid "8ead39ff-9458-4d53-ac52-9f0dd356fe8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Switch 2"
			(at 0 1.9 0)
			(layer "F.Fab")
			(uuid "8053b297-c5be-4332-8975-427aaebfdeca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d9af6c0-d6ac-42cb-a761-bb2980910067")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2f477b6-77d6-4556-bf98-f5394b8c9de8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Jumper, 2-pole, small symbol, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51c40704-28f3-4b4e-9906-eedef1f8454a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(path "/c598919a-ab87-4d0d-8a7b-308c35dd1ae2")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(fp_line
			(start -1.4 0.3)
			(end -1.4 -0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20cb810f-e230-4cf4-ba3f-c2bd4ba35f9c")
		)
		(fp_line
			(start -0.7 -1)
			(end 0.7 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35592a05-51e0-4552-8797-baba6c822f18")
		)
		(fp_line
			(start 0.7 1)
			(end -0.7 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57fb7440-b4db-4ec2-8f02-14e9f88600ac")
		)
		(fp_line
			(start 1.4 -0.3)
			(end 1.4 0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80bd3734-adb1-4b66-a75f-b09e13a8a4db")
		)
		(fp_arc
			(start -1.4 -0.3)
			(mid -1.194975 -0.794975)
			(end -0.7 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bcc03eac-19fc-4aef-baa4-9f0380493703")
		)
		(fp_arc
			(start -0.7 1)
			(mid -1.194975 0.794975)
			(end -1.4 0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f75f737-2d9f-45cc-9ef1-1eae9599b7fd")
		)
		(fp_arc
			(start 0.7 -1)
			(mid 1.194975 -0.794975)
			(end 1.4 -0.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad4b33ec-85fc-4c4f-870c-0807dfe674ad")
		)
		(fp_arc
			(start 1.4 0.3)
			(mid 1.194975 0.794975)
			(end 0.7 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa1a3da3-f006-4605-af07-dc5eef14d45d")
		)
		(fp_line
			(start -1.65 -1.25)
			(end -1.65 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "659c6c9e-3e43-458b-9816-c211da8bd6f5")
		)
		(fp_line
			(start -1.65 -1.25)
			(end 1.65 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f0a990a-03f6-4781-aace-fab28ee6350a")
		)
		(fp_line
			(start 1.65 1.25)
			(end -1.65 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2393dbbc-8ada-4bdc-8baf-e36ecbf722ec")
		)
		(fp_line
			(start 1.65 1.25)
			(end 1.65 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f66f0b0-8801-4955-8dfb-7ed7d6971f19")
		)
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "VCC")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(uuid "91548ca8-9e3d-4dbd-8266-a4a637e66833")
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 53 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(uuid "83c48f23-f40f-4293-bb29-9751bba88ae3")
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "56a14e68-c4af-4b89-8fb4-26170d24ee73")
		(at 151.698 100.96)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "fa6e5058-8c17-4b5d-8cdb-7c1d4fef9ed6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SOCKET VCC"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "dcc5272d-2e53-4fd7-80c6-60fcd11a7e71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef75ceb1-338b-435d-9d7d-c9ed902ed306")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "832f1c43-1791-4b80-aaed-f2bc85f0635f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef2fb95c-e626-43f4-bda2-371bbff14c71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/eeba9abe-d1e9-4e6a-8a35-081c1526aa07")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.46 -1.135)
			(end -2.46 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1423a2d3-ade7-4112-81fe-03978a12194b")
		)
		(fp_line
			(start -2.46 1.135)
			(end 1.6 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da55869b-8bdc-45a4-a3c8-3eca1c9833d6")
		)
		(fp_line
			(start 1.6 -1.135)
			(end -2.46 -1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ceb56da5-4a17-4cf2-bbd4-e228bd67f8d5")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09a09590-1e13-44b6-be38-ddf58b2d4cbc")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "356b153f-186f-474d-9887-02191e7042fb")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9a89df1-af18-4c63-9381-da7f2b91925f")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ad0ec17-7686-4da0-b6a8-4d2021b3c16e")
		)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cb18426-c67c-4d89-940b-5dc25e84affc")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b61f2de1-4505-43c4-8ca0-e4b20b216aa8")
		)
		(fp_line
			(start -1.2 -0.8)
			(end -1.6 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "182cbb9e-0708-49e7-b5e5-3cafd91d87d2")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.2 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddb87a95-2c24-4daf-98b8-39ee16cf175b")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6193ec8-d472-4ff5-9aaa-b4c6df95a69d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "44a3f5b8-0500-4de5-95fb-5ac3e074d48b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 6 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "20830d01-1b56-4bd4-9142-b6d9baa3900d")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 2 "/SWITCHED_VCC")
			(pinfunction "A")
			(pintype "passive")
			(uuid "13c290cf-1232-47fe-93ba-5fad919c8005")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "5de7019d-a61d-44ca-8d32-22224358c9e5")
		(at 156.943 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R60"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1c5deb9d-462b-4ffa-a080-ac5a6a0f956c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "ed85713e-2567-4a41-b1aa-8ee85c6951cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b65b4924-97cb-4e7b-9fef-e22d25be957b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d3d4cd3-cb52-4c74-86f0-3fd8b3a9efd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9b9f9f1-be3f-48a1-b2d6-d7bb832ce6d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/cf240e97-ba62-45a4-87d9-574a53656395")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84f5d3d2-206f-4dc6-8a10-660067265d98")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43202e62-b22c-4e3a-bc62-9c238efa7667")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc904380-7cd0-45ae-8a5c-4be75a8e621b")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93af2515-ccbc-4bb9-a471-1c4a8b5cdb28")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6d646fd-f614-42ba-8317-8599ef1efca5")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3283f2e8-73ce-4600-92c8-3ad8b39bc3b0")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc660e02-6cb5-4f8a-8a57-ee3513cbe384")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4411d7a6-2f94-4f73-87d6-6df22ad0a6d6")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f8e1d13-389e-48d2-80bc-72c3a48ad416")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a46abd6b-9307-48f6-a0b7-c123b1ca684a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8c569ba4-e8fa-4838-9564-064f44569abe")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 15 "/ZIF_15")
			(pintype "passive")
			(uuid "098b3676-aed4-48a8-bfb0-71ce4ec38b15")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a23034c3-0f3e-4cc9-96c2-dfe0b83b2e4c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "611f4cfe-2d20-495a-8f85-a3abf0152fb4")
		(at 127.193 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1802d18e-5c7b-465e-87e9-a5f19efd9ff6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "b472284f-2432-4b86-a5e9-bd144760f72e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4a4c797b-041f-43f0-b65d-05b9af9aa344")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "add59921-8242-47a2-b60e-7aa475bc4559")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db08025d-8810-4c10-9526-bb1a1ff8382a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2b01c48d-e571-4100-aeb2-e0937e98e11c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5df0684c-3e60-46f5-bbd0-8d60bad59051")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a0eec93-7250-49ac-b66e-7cacad6c3f97")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e4fae37-4ce0-4298-925e-9ab845746583")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffb1dfc2-2067-4863-957f-c9591f3874b3")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2841321b-f7c0-40c4-89dc-f61592581be9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af006b7c-a53e-4c5e-a67c-83dc0d1fc9e2")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03e3cbb5-d578-4a89-b9f4-ed9adbf1d6bf")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fffb45cc-2d61-4c29-8cb1-dfcb72f2cd40")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72cde2fc-019f-4c8a-be01-eee3accc18cc")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba3a8f5b-6891-4e15-8b8c-760f44751bb3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cb54bfea-c920-47da-a86d-793410a3033e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 66 "Net-(U3-QA)")
			(pintype "passive")
			(uuid "06fac74d-d4e0-4a9c-ac81-907f80560cf0")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 48 "/ZIF_9")
			(pintype "passive")
			(uuid "c37de310-7700-453e-9ab9-a28d62548447")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "637aa3cc-3834-4c5b-8826-f051f1f54ac1")
		(at 128.443 93.54)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U8"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "6ef153d6-53fd-4b27-8c84-f3f877e70caf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT166"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "8cec8a95-f358-4670-8be3-cc9264797276")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a243a517-b1ba-4c7e-bb72-50fb73d83b91")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4c0c313-6ebf-44bb-a1a0-81414f2fac4a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9be7707b-5e04-4153-9f04-5ee5f7fa7080")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP?16*")
		(path "/ce5335c9-0873-4757-ac36-a36fc860d47b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a08e3cc-ea45-4da9-af0f-165d52120867")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8138c7e4-9cc8-4ee4-9bec-cb37c7f72a64")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "304f95a2-b525-4993-b997-e9e96b8a6992")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a094028-3042-472a-a99e-9023df9de631")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "dd8fc7c2-47ca-4b32-87b4-67186f50e8e9")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "821f7a55-5b2b-4433-a6df-7a029463bd73")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30a798b6-1cff-481b-b539-68f1a10c2415")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d13658c1-0f13-428f-9b09-fc916e1d86ed")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "baa1ffbb-7823-413e-9c66-9c79d8e21b4f")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "599cbaa5-f37e-4296-b73c-d65f42e07aa6")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95d6c648-0b4b-4cfb-a894-f30294f40af8")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1dd0a78-82ec-482d-9075-1321fe02aa3a")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ea6dc10-684a-4e45-9691-533bf5c6ad93")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a73d35b-0ee3-4c58-b01b-81b0957563c3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1464ada4-db24-497b-9bbe-8774d94f2461")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Ds")
			(pintype "input")
			(uuid "9002b6e7-669c-43dd-8b45-ab67e6c83726")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/ZIF_1")
			(pinfunction "A")
			(pintype "input")
			(uuid "ce6e4716-c975-4cd3-8098-f88cd3f2e33b")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/ZIF_2")
			(pinfunction "B")
			(pintype "input")
			(uuid "8e5ad321-75e6-4867-96b6-6f2db874c552")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/ZIF_3")
			(pinfunction "C")
			(pintype "input")
			(uuid "028ce999-ea83-498f-b090-5aad9a563999")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/ZIF_4")
			(pinfunction "D")
			(pintype "input")
			(uuid "fb03bf56-bb5f-4f78-bb63-92c26c1348ce")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "/PISO_INH")
			(pinfunction "CE")
			(pintype "input")
			(uuid "7a8a368d-e187-4ab0-b561-c846f6e40187")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/PISO_CLK")
			(pinfunction "Clk")
			(pintype "input")
			(uuid "0f316744-1c52-4938-87c7-abddc09346bb")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "808ff256-41bb-4dce-abf5-7f23f8df7a37")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "Clr")
			(pintype "input")
			(uuid "d7a384c8-d593-42bc-8220-fbaa7e2daba8")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/ZIF_5")
			(pinfunction "E")
			(pintype "input")
			(uuid "5a477c4b-d66b-45ab-a5a0-461967f86252")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/ZIF_6")
			(pinfunction "F")
			(pintype "input")
			(uuid "3cfc4dc8-5da0-422c-a3a8-fbdbb1759f3a")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/ZIF_7")
			(pinfunction "G")
			(pintype "input")
			(uuid "f2e875b3-18ed-4184-8cb3-029238952d89")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U8-Qh)")
			(pinfunction "Qh")
			(pintype "output")
			(uuid "6554103d-c380-4b2c-bbfd-587f69670937")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/ZIF_8")
			(pinfunction "H")
			(pintype "input")
			(uuid "a7bd9842-72a7-4b64-830f-26d87c01bcf4")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/PISO_SH")
			(pinfunction "PE")
			(pintype "input")
			(uuid "ded522ed-0fd8-4766-baeb-059c19de5a9e")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "e88ad13f-e4ad-449f-9eca-626e4e3f502d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "66648e04-6fee-4bc4-a9e6-af86cd62d253")
		(at 150.993 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R50"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "ce81a989-486c-454c-ba56-ba89ad3dbe8c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "869bdb8a-bdb7-4b17-bd2f-6352083d4448")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "596df60e-1841-478e-a2c5-83fe5157bc1e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f246fbd5-6599-409c-a163-ec50b80cadb0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2aebc2a-d4ab-440c-8ee9-45f17012e865")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/dcfcd51c-4000-4fc3-a533-93b7e4f8e0f2")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "887f463d-2eee-4bce-b440-16cb0cb396b5")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "005c0c5f-d171-4212-b458-655778bb64a0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd279487-29da-4d7a-b32e-82155e082f3e")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7f35123-21ae-4c03-990e-9ccd6dca1e64")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f0d6b3f-7423-470e-b419-1eacc0e3f761")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "944d5422-d496-4591-8bf5-148c40ffa4b7")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f73afd2-3b8c-4999-b7ce-a790a6294081")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98a7eb90-25c5-41b6-8b4c-398fb1c402b8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65302a47-a70c-42f2-9f2f-47a3dbbd74c6")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec1cdb3b-7ab6-454d-90fb-a998172d9dba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a7c83fd0-0ca8-48ab-87ab-960ccc3c540e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 45 "/ZIF_5")
			(pintype "passive")
			(uuid "d09fbcc7-b03e-44ba-9c93-c2df3d9395ea")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "e3c188ef-766c-4776-a097-7d2d0cdbaba6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "692ef423-d09a-4d7c-8cf6-9912393caebd")
		(at 145.043 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R37"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "0cf15301-0afe-489f-bf0c-a4bdce4f98a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "d85111ef-ff9e-4b98-89e8-4acaf7d5fa40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cdf272e7-6d77-4e3a-bf68-9c5adc6f0ec9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6efb7f3f-2e39-43a7-9d4d-67f91de46365")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15953616-0056-44f9-acc0-c30b762a4356")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ef6bc9d5-6d1f-4ad1-a205-d0ac0bc54467")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "953936d9-495f-4e23-b61c-d133f133d81d")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7de6ada4-9fe8-4f81-ab8a-e96ccf746411")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2aaeb5ff-aaa4-4b9e-9b8e-52a5e22d90ac")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7c756cb-7d13-44db-ac61-851c872f0063")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03d6277f-4da4-4ec4-a9f6-018f4d507690")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8ba5d78-00b6-4871-905a-6cd8222a872e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2dfadd32-8735-4a68-9c13-9f8e630897b3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a107e28b-6553-4321-acfe-49934f062d10")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b1879ee-00a8-4a07-8dbd-938d5230b4c0")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a9d2d69-88e5-4f61-9e20-b5fe7c4e35aa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3e511619-d8dd-42ea-b187-a6b7ede6a308")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 93 "Net-(U6-QD)")
			(pintype "passive")
			(uuid "44bce0bf-eb4d-4d57-b702-0fd7f7c1a20e")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 13 "/ZIF_37")
			(pintype "passive")
			(uuid "e0c5f820-c46e-487f-baf8-176cebfd5630")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "6a9adc3c-025f-4511-94c8-cfb5dbdfccc6")
		(at 156.943 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R62"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f6d8f585-0285-4c90-9498-01aca29da021")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "189775e2-83c7-42c5-ac2a-73e48c9b98e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad416492-2684-4bb0-8627-1984c055237b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "08c4b6dd-03a2-449a-aac7-e5c0b3ae569b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca550e36-8e69-4be1-9ad2-1a717603620c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7dc4a592-6848-46a9-a914-ec17b2f3f5fc")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b486bfb0-9124-4e10-9227-1680dae3e44d")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af7e6ad8-72f1-4796-adaf-03f8cc1d3fd3")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06d9dabd-0f8e-49b1-a067-73779f37a807")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa6df6e9-b64d-443e-af6a-933d044a81fc")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "830491e1-eedc-44d1-9c14-0adad030c0b7")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b321756-5d5d-4824-989a-7897d1be1162")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8367b284-e4e1-4c86-88ca-8c1d0a7648ee")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fab4ea2a-5895-4390-be48-90150a1939e5")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00da8e57-66f8-4619-878c-01dd4ba2c985")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3760f291-1f7f-4657-9e99-7d58bba1a876")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b350ce69-6bc0-4ef8-8fe8-9be3ff58e08f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 19 "/ZIF_17")
			(pintype "passive")
			(uuid "9aebbd57-0873-487d-ac62-11459884c350")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0c47fd66-de67-428a-933a-9e6e30987894")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "6de81fcb-7a5b-495b-9802-4daadfa964e0")
		(at 150.993 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R52"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "518d110f-4c01-4a43-ab29-1a06e96cfd58")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "59fdf2a1-af1f-4c52-9ab6-6ce3581df84a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5af4f0c-51ef-4003-b221-c95d86d29fb0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "888beac9-9c9b-437e-965a-3cfbf27e0a57")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "632f1bc6-40a1-4e74-bebc-6c4cd435f426")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1299917e-870e-4fe7-b652-e5e0d00c2351")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "052d35ca-3c99-4f5a-b616-12a9585f5934")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "699ea0b4-7efb-4a6c-bd00-8e73ca7f3145")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6ccc1db-4318-433e-8731-025dc6dd7256")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d5c0231-b297-4183-9665-f65bd4942753")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9566ea18-404f-47a9-af1e-8c67319b011e")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee34ad51-480f-4b78-8d5a-f5c11991e54b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be7b2e48-78f0-428c-b5a9-276405b19a19")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e80a1176-ded7-4695-abd3-dfaac13fca09")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d09b32b6-af58-4d75-8d1d-febebf13d36a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a514d9c3-94d6-46d4-a46c-96afaa05c86d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "82d7b7e6-17d9-4c1c-aef6-7def2faefd0d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 38 "/ZIF_7")
			(pintype "passive")
			(uuid "16f96009-84ca-4fa0-afd4-38ff8ad2cab0")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "97679554-8a23-410e-9213-8ee26fbb1368")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "734d837d-f4c5-4bbf-8ab2-e1107b424521")
		(at 109.153 115.22)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "e818a056-877e-4a5c-9781-84f831549a98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "586acd33-b322-4e2e-ab5c-9f54b2cefa54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "12c1ffcf-e857-4ebf-8948-902f1b6640be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e1a2f6a-7d2b-4579-b4aa-a4107cc8c223")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fed0a3b3-3972-477b-9ad1-8a0be6814770")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5e441242-33d6-4fec-86a7-dd747d03ee65")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2574c9dd-b97c-4479-96ff-e849dbc52eec")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c996d6a9-652a-4400-b30a-0d1abe456419")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea8034ad-f599-4878-bafa-ca1902b4bfb0")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "963fd87a-9d65-4c9b-9cf9-3bbaac215cce")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e153648c-cfd5-468f-86e2-2abf471e2c94")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67785e66-62dd-42a9-9d59-3667022b7c74")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2c623d4-a0d3-4f1a-8146-d6090019d7b2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd51279c-ec52-40ce-b92e-989d9449c09e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80701a8e-df3f-44d1-9365-4b5cf92b7eab")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d924865-e034-4596-bebe-cea822af3e04")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d4010eba-528f-45df-8ecb-3a18322cc44e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 4 "+3V3")
			(pintype "passive")
			(uuid "beed8e27-3179-43fb-85c0-fae915c308aa")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8274672c-7591-42d2-8d7e-2f9fb091c692")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "73fd85a3-6b1f-4dea-b926-ed4b763e434e")
		(at 133.143 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "a40f1416-e682-4124-89ef-db3cea4bebb9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "0ecba902-de11-404b-9bae-a46e2bb92a8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c4c82ea-3cdc-4270-a316-e6ace2a99fcd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8f72f96-9283-48e8-b7ca-64509f0072c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "60dc0a58-8cc1-4f60-905f-278e56e7a4c4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1f288cd6-10f5-4d30-acd5-3dda12a87a6a")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16e4ac21-14b0-49c5-8bee-bc49866b69e5")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c532a01f-0c9d-4913-8e0a-1b132cda0220")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10cb87ec-60ce-4a7e-8170-d14582130c63")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "704d9b35-4585-46e1-9f79-9dbb5be332c1")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6171cfd-7fb1-41c0-a74d-aa50e614e02b")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0048b256-fe44-4850-a689-39f940522785")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf71648c-e24e-463f-85e7-58ffc476c25f")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "271584e6-ab7a-4e29-baf5-9231a09c7497")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74712025-695a-499f-8aaf-6d5435aa9b0a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58c42326-9709-420e-9db4-394d792c4f1a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "43b3a72b-a618-42d4-a1aa-93d15b3fe899")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 71 "Net-(U3-QF)")
			(pintype "passive")
			(uuid "36632069-d5d4-4052-9c4c-bf1fe81a31cd")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 27 "/ZIF_14")
			(pintype "passive")
			(uuid "b4436e16-0dd5-4905-b217-928410fadd75")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "763e0ce5-67b7-4369-93c1-bdb6fe15e5af")
		(at 128.443 81.92)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "a5184cfc-8fc3-48e9-bb5c-843aaf074122")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT595"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "d81b3fba-2271-4189-b1d8-d5c4a5c74999")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad0be940-3790-46da-8499-3a9d595cca28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68597ffb-d0ff-4c03-b6f1-86ff4f8b0f75")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e6c7b34-f0f3-41a0-85d2-20f1884198a2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(path "/4c644089-5667-4035-8f13-0ba367e1db2e")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09ba87b5-c7b0-4e30-aa5c-8b22f7310589")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80b2a821-6824-4951-9181-b8708fdaede4")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c045f15-a1a3-445f-86d2-08c8bf012787")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baf53c6e-39cd-4137-b8df-dfb4ddf18122")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "36c707cf-0472-4220-a8cc-c2e0b3e44ddc")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a775be77-f5ca-4b8c-b8f6-aa72c6dfe8f4")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a39b211-a3df-4b19-bcc8-f5a3e18f5138")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff66d3b1-e1df-4b54-a26e-f1e16be25330")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "224c8838-529d-441b-957d-291fe7357900")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccc72aa6-80e1-4185-9e56-a699556343b7")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "118cbb65-40c4-4c13-a947-7924334906cf")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8293c56c-023a-4577-9fa6-62f2b33c0d2d")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4c9d041-0dc1-4531-a2db-7b5c79cdf4a3")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e505650c-e0e3-4350-a037-0ee54c1c531e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9ffaf5c2-dd96-4b50-ab0d-2c0249efabde")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(U2-QB)")
			(pinfunction "QB")
			(pintype "tri_state")
			(uuid "7fcabd20-c53a-49ed-8fd1-b2a712c76ac4")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "Net-(U2-QC)")
			(pinfunction "QC")
			(pintype "tri_state")
			(uuid "9f162f5e-7617-46f2-b94f-164efb1ceb07")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U2-QD)")
			(pinfunction "QD")
			(pintype "tri_state")
			(uuid "ca1524e8-683e-4060-ae16-1e40377ac196")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(U2-QE)")
			(pinfunction "QE")
			(pintype "tri_state")
			(uuid "144d3c5e-ce60-4bda-8f8f-6e79e987dadb")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U2-QF)")
			(pinfunction "QF")
			(pintype "tri_state")
			(uuid "0b57d3d3-7a82-489c-a406-68be4b0d9d36")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U2-QG)")
			(pinfunction "QG")
			(pintype "tri_state")
			(uuid "c110a6ce-35eb-43c8-85a0-dfa1b8d5ce5d")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U2-QH)")
			(pinfunction "QH")
			(pintype "tri_state")
			(uuid "3fe17bf7-c2e1-4487-9d52-361be60d322c")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "7f06a6e0-7521-417c-9878-80fe44c733dd")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "Net-(U2-QH')")
			(pinfunction "QH'")
			(pintype "output")
			(uuid "4058f98b-9cf6-4ff1-84f7-cc11226f2165")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "~{SRCLR}")
			(pintype "input")
			(uuid "04d999e0-8cbb-4ee5-9ddd-8bc56ad8913a")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/SIPO_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
			(uuid "bd9b2e15-5cdc-49ad-a77a-a7a8a1997251")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/SIPO_RCLK")
			(pinfunction "RCLK")
			(pintype "input")
			(uuid "69c2582e-fd01-4527-ae74-89d65b95eed1")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "bc15e553-4c41-4769-a6ad-552a81dc2c8a")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "/SIPO_SER")
			(pinfunction "SER")
			(pintype "input")
			(uuid "3ab7a683-0555-4e4c-ac50-0ffb201e18da")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U2-QA)")
			(pinfunction "QA")
			(pintype "tri_state")
			(uuid "ad9786ab-b618-425e-96d4-cca4a2ca3e88")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "fbbd779b-28f4-4889-92e9-d919a54b31fe")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(uuid "76639528-72ab-4a92-9fba-99d179e0d22d")
		(at 161.003 102.52)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
			(uuid "4289ebc4-8bfc-49f1-ad49-23802ad7a14b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2N3904"
			(at 1.27 2.79 0)
			(layer "F.Fab")
			(uuid "f6c578ec-3caa-476e-8c0f-839921049df7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e861ee79-13a6-4236-a926-7a7d6d84bd74")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03179896-099a-4703-94f0-556ae8e7af3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "008e2eba-e8b7-4c46-9745-154047b41100")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?92*")
		(path "/0d424325-f728-48fc-aa4e-e691449d15ef")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.53 1.85)
			(end 3.07 1.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "166c9c46-9016-4540-839e-9c65390a384a")
		)
		(fp_arc
			(start -0.568478 1.838478)
			(mid -1.132087 -0.994977)
			(end 1.27 -2.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ea8e04c-b743-4a28-a618-7d6baf77527d")
		)
		(fp_arc
			(start 1.27 -2.6)
			(mid 3.672087 -0.994977)
			(end 3.108478 1.838478)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7cc54ab-6a5d-4ae1-9ec4-ebba67d4b5f0")
		)
		(fp_line
			(start -1.46 -2.73)
			(end -1.46 2.01)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f11bbe1-cb68-4128-b501-2a2296713ac7")
		)
		(fp_line
			(start -1.46 -2.73)
			(end 4 -2.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a99fada0-c68e-48f0-95b4-3882626ac074")
		)
		(fp_line
			(start 4 2.01)
			(end -1.46 2.01)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63e6d137-a89b-45ac-bc51-c0a72b87ce33")
		)
		(fp_line
			(start 4 2.01)
			(end 4 -2.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "faad8214-0ad7-4563-80d6-8dadda08b4f0")
		)
		(fp_line
			(start -0.5 1.75)
			(end 3 1.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87d49acd-5c5e-4c63-a369-a96c11b89728")
		)
		(fp_arc
			(start -0.483625 1.753625)
			(mid -1.021221 -0.949055)
			(end 1.27 -2.48)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3fa5e2ef-e41f-4c84-aa86-eb5c87c82c05")
		)
		(fp_arc
			(start 1.27 -2.48)
			(mid 3.561221 -0.949055)
			(end 3.023625 1.753625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1568d44-7847-4095-b901-43a58da163f5")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
			(uuid "a7bdcd2d-6ea3-4c9d-ab05-f5ea7a575bb0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "cb6561e3-9d7f-49e3-ae83-d8c45ef134a1")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "passive")
			(uuid "49eabc11-e270-4532-bd70-1c37014310bf")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D1-A)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "8338aba6-1f20-457e-b989-9ec4e904e306")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "76bc629f-59ea-4ddd-b48f-24050e082450")
		(at 133.143 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "b4ec1eb9-eb72-488c-8c26-7b87d735ddd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2ea74938-f693-444d-b8f4-9d8af5f6b793")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec33d458-9e74-451c-b5b5-893018d52bdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cee58dba-e894-430a-b2b0-f44513cb3791")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d8a7e74-4a05-4928-ae44-f9cb36194225")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c0b854b1-c780-48bb-823d-8d2c61d3ad01")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ce53355-6aa1-4b40-87dc-fff6763a32b9")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9cb514e7-1909-447b-8bfb-4847fddb3cb1")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a4ac099-493c-4bca-a897-3d080fca1c0e")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc2c173c-2dce-4c59-80a6-914dfdf1600d")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3c22290-16bb-4c8d-a314-435e76b0f74d")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e1179ab-f13b-4d2a-921c-e65fb34a5b81")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc1914d9-d0b3-40f3-a258-c42a6ab0050a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5656a6ee-1925-458d-8508-f6f1468c9922")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe1fa1c6-7918-4c66-9a8a-ec5848366fab")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfd9d4f9-4bf3-4e4c-8af0-f1f691a8a10c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6680eb8a-f204-4465-9af7-0fbc30be604c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 70 "Net-(U3-QE)")
			(pintype "passive")
			(uuid "29c3291a-b2de-45ef-be13-2da2628e374b")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 35 "/ZIF_13")
			(pintype "passive")
			(uuid "69dcf503-74c2-43f8-9b2e-89a141261993")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "776514d9-1662-47a0-af9b-ae441e1a775b")
		(at 168.843 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R79"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "58801552-0785-44a4-8926-379f05b3fa5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "76e78093-5528-4bde-9940-e641750b5e47")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9af46df2-c2bf-4c33-8cfc-7facf036ca08")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "23e282fb-c9ce-49c7-8a89-aa85f764251b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01faad20-12af-40ec-a188-aa0bc4dc97e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/cf64fcc6-2fce-4ec4-b8b6-57c33f27bccd")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "816e463d-473b-44d4-8211-aeace8e2427b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1222a0b0-306b-48d1-b9f8-7aeba12185c0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a63cb73-1ccc-4ce1-9f17-3020a15cd585")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "981678cc-47e9-4d3e-b50a-f91f2d339bfb")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38a18ae7-092a-4d05-9c81-639b5908def1")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8fa37c8e-9a2c-4b52-9c82-ec4ba6e4d04e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abeb7685-af77-4765-922e-5f3d0512d87a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa7879a3-f08a-4924-9f16-8aac13f8147d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "972bdbfb-06bf-4655-a088-7a4fd44568cd")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3800c795-8869-4de9-a484-acc650ad1789")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6d2864d6-14d0-44ad-8441-a6ec296d1f7d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 42 "/ZIF_35")
			(pintype "passive")
			(uuid "20f509ef-bdd2-4c05-8479-a80a126ef96c")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "83e7b28a-9fe6-4ecb-a0a8-0bb40a223bfb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "795c7092-4971-4a31-ab1e-c6fdafbe97a5")
		(at 156.943 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R59"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "27d4b987-05bf-4e7e-abea-c009d75a0b82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2ece55e6-c656-4f77-96de-3ce8a6a50918")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d9cf33a-d008-4406-a8d3-72b64dc5ea03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d07e0eac-919c-419a-ba77-623533ec7e5b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f81b47fd-8148-4cae-b1ed-9389d920afc6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3739845e-05db-41f1-8fbd-7cf4c236f9cd")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "daee1a4c-1624-46bc-9726-de7346571b2d")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09ab9377-b8e8-4139-a176-15764bdb8e88")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7e36710-955d-4c5a-a8d1-a665322afe09")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e85b727a-010e-4a4f-9479-610d5d75152e")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb772073-2e5d-481f-a719-83e453ae7d1c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72d42136-11b7-41a2-b715-c4790caffd58")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2b5cb2d-d0cc-43bd-a285-4609d215ddf0")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0e75ebb-4b09-4273-84c1-dfff34380e21")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc669c6b-4709-45b3-abfd-937ca2a3fddc")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c73be48-5d42-4542-a779-f9beb839680b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f91009ff-d7ab-4201-8b12-06b4b11edbe9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 27 "/ZIF_14")
			(pintype "passive")
			(uuid "089351ae-043a-429b-9677-4d72e55e6810")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "68bdfb93-9dcb-4a35-98f7-cf6d084a6bc9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "79a87046-94ed-4ecd-967d-632c56cabc7a")
		(at 145.043 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R41"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "8cbe4332-b15c-40d5-82ba-6b28b240244f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7bf6d1f3-05fd-4154-88c4-49c13c9008af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc965d3b-7150-485e-b747-0808226326bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de3eec0a-55c1-444c-a0e8-42a53f67487b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9410f13f-ec20-44df-87d8-864027ace813")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c2aaacee-68aa-4380-8015-8ec775f33744")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc974107-15b1-4e0a-9e6d-25623a732cfe")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c49e12c3-2e4d-401a-bbc5-8344a2d6527a")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78d65cb2-14db-4421-a86d-23b1c005b96f")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3e6ae78-5dc3-43f1-ac5f-2a2a3870b597")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35b2f9b6-2f7c-40ee-a83e-b884cee300cc")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4de57349-e959-4504-bb37-24dede0eca30")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "543fccfd-1fcc-4a6c-8048-783b8a5d657e")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc92fdbc-fac6-4e89-b3c9-69a7cf74f961")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "377bfd3d-b719-43f1-9d81-1d1883aac826")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36be4261-cd43-4300-9a2e-ab5a5e016ca6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "115d91d3-68a4-400e-af5e-ece63802c292")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 97 "Net-(U6-QH)")
			(pintype "passive")
			(uuid "5ef9d332-a782-4a97-91a8-04c10d385431")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 32 "/ZIF_41")
			(pintype "passive")
			(uuid "f684f030-d871-41f4-a378-4f80261c0280")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "7c132e05-7248-4947-8810-95429b8fa469")
		(at 150.993 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R46"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "ec652f05-0b8d-45cb-8ac3-0e99c4a4f364")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c86670da-1ba3-49f3-99a3-356f0c1cb3b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a94e1848-ac97-4d93-8019-1b9ecd02bfdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a78b77fb-c279-41a4-a9a8-7c5b637b1d8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6014ad7f-514b-4161-b252-a9a719316102")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/debbc86b-9260-439d-af30-1f13151edb2f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "561a0c4b-78ac-409d-868c-d67bd1cc2ae5")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bec9a24d-3cee-4507-9adb-ae7f4a0b8cd7")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24e2b1f1-3688-49f1-b1a3-9e93694a4cff")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f7f10ac-6a0b-43a9-a1a0-ffb5b88e656a")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a60a4f8-1e92-4db1-98d7-6d767f777283")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5451c976-ef9e-4327-a514-3622998fdb7e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b6395dc-242b-4fe4-a26f-18a08b99cf99")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "001b4590-dceb-4a0d-ae26-91e44e504e91")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6eb3497d-ad7d-430e-85c3-223e8a7c3090")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a75e19ef-0722-4284-8af6-0354e4b1a1a8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "28661ed1-3866-4e16-84a1-ff50075754d0")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 24 "/ZIF_1")
			(pintype "passive")
			(uuid "0ada1deb-d7d9-409e-8083-fbe03ee9db75")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "389c4077-3e2c-4790-b093-1f9fdfc63fd5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "808d8965-2983-4ad8-bcde-b20ae0d0c418")
		(at 145.043 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R38"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1730d2d2-32f9-4d6f-b14f-47223bdf9f3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "a6999787-b8ee-43b7-b2c0-42a4b08e7a3a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "25b22f5e-fa51-4848-82a6-26122ff5b94e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83fa46fe-5939-46b4-b5fc-34511843d283")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a464ca1f-f45e-40b0-ab53-b5518f9f01b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9a4c521b-a7d8-47c1-94fa-c616996c4ebc")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a13c806-8f03-4152-a32e-aa24fc3d6b9c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4aabf466-6730-43df-be4c-231e8fe6d55d")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "647dc9c5-2371-4ada-a6c3-b5ad378b0e19")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "578459e3-63f4-49c5-8b22-d47a7f04c82b")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce457bc3-8312-429f-adc5-adc46d6b4538")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59b7dac4-a418-46ec-a91e-c3788573e010")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49f63c36-daa3-4566-bb4e-7f9b88879111")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "089477ee-d7d2-4908-914b-5b4526658a5c")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ac808b4-8ac7-4e78-b507-8f3ef29d8db4")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1af95877-1297-43c5-aaa5-fdb47e5430ea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1ffa4f14-a035-4a8f-926c-6b1cda79db4f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 94 "Net-(U6-QE)")
			(pintype "passive")
			(uuid "cb414231-53c2-4878-8ef5-f9c849e50c11")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 40 "/ZIF_38")
			(pintype "passive")
			(uuid "ffa6e196-a5b7-4781-8ac9-fb5ed8839c97")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "832b0fab-1ea2-49ee-a144-b38c050e8f80")
		(at 127.193 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "ac5ba756-bdce-4305-865b-1661c1a164b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "eb7c7b86-c909-4773-bf69-6e8bcf4fea8c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad0093bd-c7ac-4b68-ab35-85a8a431c806")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2341faf7-da3e-484a-a81d-2dfb7955752a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "23991fbd-daaf-41f9-a388-773238791b1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/70d8678a-aaf3-458b-8d6f-67f841ff8b59")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd66e001-b0fb-4d5f-a1a5-7b2ec17852ee")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c839ba8e-606c-4456-a608-b37ee14860d9")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10d2d2de-5bff-4eca-be97-428541675f3b")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43968ea0-9c8d-45cb-a34d-a1d38e33c560")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f1b5a8d-a0ff-4d6d-9a0b-2e40c062b4c5")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26cba4c2-fefc-4a2d-bc13-8e420c61e0f8")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39bc5238-a246-4a27-bf32-31785766bbf2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "880eabcf-2aaf-46b6-be17-0a9f72ef5b26")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb9059d3-a61b-4a8e-b9b1-4c17776228e1")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e77e8df-c22f-49ff-866f-f21084926d95")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f871617b-f976-4aff-94b2-008c033c157e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 60 "Net-(U2-QC)")
			(pintype "passive")
			(uuid "4852d2e8-3b51-4d22-b369-f26fc1d8183e")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 23 "/ZIF_3")
			(pintype "passive")
			(uuid "56294ef4-85f2-4cdc-9583-1f662cbd6a2e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "838c4b5a-00be-4a0c-988c-e5085fd95c16")
		(at 162.893 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R73"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f9a2f433-1959-417c-8657-c1bf23f8c878")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c7108f89-ef36-4e43-9f95-44982bed8275")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c00ec69e-31f8-453f-ba73-14399fb27920")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "256b6915-ae99-4c0d-b9c1-902008a4961b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f83cf06-d7b6-45db-9cca-c109eafd05e6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2b7e8df3-762d-46dc-910f-de8a66b5de34")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08d1c53c-63e3-47fc-97a1-8e069126aba1")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71392dc9-0d59-4591-9e61-52411219e1ac")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d73be010-d75e-4d5e-b824-e602a69786ad")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c59c943-c335-4044-9d09-3af959ce4bed")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59231e21-e2e6-43d6-a16d-6cea3a7904dc")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b51de16d-ad5d-4e6c-bd7d-cafdfdf6663d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8697f3d4-1ac5-4541-9b41-8a93ada714d2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52c59f46-e5c0-4439-9147-de410c0cf74d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5152a2d0-0860-41cf-8a44-2e32a21d4e33")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce2e7493-cf7f-4755-86d6-0e70c69870e1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1dd89df7-8b8a-4605-8b59-1f7ae49e448d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 18 "/ZIF_29")
			(pintype "passive")
			(uuid "6d7a04f1-6817-4c91-b1c6-b41bd9e7a338")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "519b6cf2-153c-4a95-9e52-a8e73f13f119")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "8523428b-bd70-4bfe-8760-6f1d440e33c6")
		(at 127.193 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "108ab8b0-b046-47af-aa71-78f371c63e48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9de47a6d-435e-4283-8164-36dfe8000ae4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3597407-7492-4376-a6ee-3ad2b0f0502c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1928a095-b6b4-47a0-aef6-9db477d5aba2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa0ce215-8499-4b80-ab3a-9cfbfad52999")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6da23405-349c-48bb-969a-8b98a7561f6c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f8c62f8-7046-4dde-a413-d10827004709")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfb98bc2-b578-47cb-bea2-eb3b6e5cae91")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4987de2f-1fd5-4dd0-a0b4-f093f0ea6fc4")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ccb81c8-57c2-4b32-9bcc-1a794f877ccf")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec468d17-8861-4237-ba70-d0f1004e0b03")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "986289b2-cc4b-4af6-8be3-e1ab3b080a05")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54ea94ee-deae-44e8-ae66-5c723ae06dd9")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aacf7661-0390-4e0b-a115-8e33aa24d856")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54f2c9ff-cc6b-48e6-bec8-6147f68d521a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25a368a1-53e1-4c7d-9f68-ef021a1d7fe0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e0f2575b-66a4-47fc-afec-80ade7e22395")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 58 "Net-(U2-QA)")
			(pintype "passive")
			(uuid "5e25ae7a-d2a9-4baf-a785-ac5a0124cb7b")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 24 "/ZIF_1")
			(pintype "passive")
			(uuid "15392735-ec88-4867-9708-66825b89972a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "88c9ea69-7957-4657-b125-7fc988a336bf")
		(at 151.698 107.74)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D4"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "167c89c0-964d-4577-9951-83d13cec51ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PISO ACT"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "6584ea08-7a9f-4140-bb36-c8ac7bf4b1ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4bd7b449-9b50-4871-a3c4-ea99df09778f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a81de4c-0656-4ace-918a-484f16b30dbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6be4f610-b5e6-4132-aad0-b1d2120a86f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/d678529d-d8ba-4bdf-b1eb-95f84fa8114b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.46 -1.135)
			(end -2.46 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d41e1e4-7e45-4b06-a720-968a94e66625")
		)
		(fp_line
			(start -2.46 1.135)
			(end 1.6 1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "733a4746-5422-4422-8293-c5ba2375de3a")
		)
		(fp_line
			(start 1.6 -1.135)
			(end -2.46 -1.135)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31c1454e-a695-4dcc-9ec4-4cfb88d721a1")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fbf65b2-5891-4de6-9181-8dfba9b671a4")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b355555-3254-4b63-a943-cabe384d347b")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2c827a8-e4d4-49a3-b1f6-085ce39708cf")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "caa6c96c-7c78-4fb9-aecc-6eed793685ee")
		)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fad561e3-8d4d-4a28-bbbe-a58c3989a808")
		)
		(fp_line
			(start -1.6 0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a6d5cd2-3fcd-4532-ad58-15976118b4da")
		)
		(fp_line
			(start -1.2 -0.8)
			(end -1.6 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5ca16af-1fb1-4679-b7e5-c7905ab09ed5")
		)
		(fp_line
			(start 1.6 -0.8)
			(end -1.2 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20224144-6ff4-4424-9642-da4ad69f4184")
		)
		(fp_line
			(start 1.6 0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eca3acf8-0f39-4410-8399-b4bdc4129bbb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2f301098-81c8-4de6-9321-c4af373c5283")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "8397407b-db09-43d8-b650-b62a773c660d")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 8 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "7408ba2a-307f-47f7-9cf3-b249df503469")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "894ba2ab-8f12-4eaf-b694-355257a40fe2")
		(at 133.143 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "02be97c1-05f5-4d8b-99b9-1865edc87bb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2a629436-58a7-48d2-b547-39b0ea5faeab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d1c3b47-1f6c-454b-8cec-62354f8ba7dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0dd5506d-5681-4cc6-b158-113de66157a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "056bfc0e-679e-4c66-8d5a-f9d502386ec0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4e244ec2-3651-4560-ba4b-2cc09f7d42d8")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7af5cf1-3154-48c5-8086-8f0ee3934a80")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d876f405-46ed-49b0-ba6e-3e4fc23bfad0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fceb64ee-2b9e-416d-be6b-91e85c50dff6")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64c1772c-1eb8-49c4-a09e-256e23a4344f")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13a3ceae-da53-41b2-b889-7cc6a67dab72")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90bcfdb8-8e37-4efd-8268-3f03895a497f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b968c2d-6c78-4625-b778-81ca5e1246d3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b37aca95-ec27-41c7-86ec-d073915f382e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40db3d9a-1514-4805-a4de-7accf883c6b9")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96f426b5-1f4f-4a8d-acfe-60d947171341")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ace6702a-2e3c-4197-8dd7-a188c69080fb")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 69 "Net-(U3-QD)")
			(pintype "passive")
			(uuid "d239a04f-8fb9-4b2f-bbd2-0a74e06fd35a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 25 "/ZIF_12")
			(pintype "passive")
			(uuid "62890dec-897e-4b31-bf18-75f2a3a5d830")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(uuid "8d271409-8003-43f7-8b8f-2f29a51bf75a")
		(at 168.103 101.665)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U13"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "d7665057-4ddd-44c5-8c3b-eab67c6c63ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SN74LV1T125DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "b9cc910f-d020-4aa7-9e02-668571c24181")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "222a1d32-c804-4c5d-b839-9dec9dae9b10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t125.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbef4bbc-a93d-4dc1-8343-d4496ed87035")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Single Power Supply, Single Buffer Gate with 3-State Output, CMOS Logic Level Shifter Level Shifter, SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "358576e4-4d91-49a8-af65-179d7bef91c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/17968291-9572-4dfe-a5f1-508b7dfdd3b5")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "056fa70d-3ca3-4ef7-896b-931b5ca98a6a")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2627d4e6-4f2b-4580-a6d5-2d484a5c440e")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b3fb54e-d353-4afa-bacd-13a084355455")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "651812eb-2178-4313-ad20-dc5bf4f11e86")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84) (xy -1.3 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "b226df00-c18b-4f1f-bde2-59d4d51c98ac")
		)
		(fp_line
			(start -2.05 -1.7)
			(end -2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "119f5081-8cc7-4cc0-ad4e-894bf954999a")
		)
		(fp_line
			(start -2.05 1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af6eec52-ce0b-4522-8bca-7f06c47f9096")
		)
		(fp_line
			(start 2.05 -1.7)
			(end -2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54c161d6-48b2-46ab-93e3-adad98cbfd36")
		)
		(fp_line
			(start 2.05 1.7)
			(end 2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "62ac03c6-83f8-4e94-869a-da03ed271a7c")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7056dfe5-58d4-4756-9989-38fcd6638b2a")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d143692-2126-4f7b-9b1a-0d11f101e0ae")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3500af7-d1cd-4af6-b335-496c7a47e31a")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b43d6ee5-2997-4176-957a-475bd9be9147")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f04dc262-92a8-4c5e-a825-dcdd65085785")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4c31210a-a49c-4ee1-8515-ed690861567f")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "2889d150-bf91-4373-af24-53cbe6caed04")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "/PISO_SER")
			(pinfunction "A")
			(pintype "input")
			(uuid "0b3def40-da5a-472b-b207-cd242c4953c8")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "9584e847-81f6-4706-940c-1933c14cc684")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "/PISO_SER_3V3")
			(pinfunction "Y")
			(pintype "output")
			(uuid "8fe7992b-cfbd-4bac-af9c-5088f8891292")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "91af7ef8-b886-4741-88a0-53676775cfb3")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "8db9919d-214a-46ee-a6c7-cda214c2267c")
		(at 162.893 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R74"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "515c8215-e679-4ceb-83a6-d0139309a691")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9833ff9e-7b35-4dd5-aa7e-f6ce9490b7d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51c7f6be-bf8a-48a0-b216-5708ec10f1d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "31c354fe-ef5f-4704-ae3c-6d3dcdccfae0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "47eb8f1d-dc22-4bd4-879c-22e3f5a1f17e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2d1304e6-c39a-4bcd-b1d9-1bfe96b56c02")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7bd6e824-7b40-4cc0-b9b0-b3a21243893d")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ffd5ace-138a-423b-9a8f-8175f07e0dc0")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15ad5547-b365-41b6-b0ea-9534b14b402f")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d455bf81-3c28-438e-993a-bfc4cced743b")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6b4e2c1-2dfa-465e-8e16-c4b0d958d6c0")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4554b374-27f5-41ea-b394-e6e5d13a3870")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3b927ca-4dab-4aaf-9a7b-c5282d5c27e1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79da8f19-5a37-4fe8-b056-60dc08792499")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "284fe00b-59f5-454b-a254-5aaf9a9163c3")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57b07eed-fe67-4937-8e3b-4ad68410b85d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4ae296a0-42eb-4b15-832d-29cdd9f52e75")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 36 "/ZIF_30")
			(pintype "passive")
			(uuid "f24eeb00-3a83-4db2-910a-31391beaf17c")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8594636c-49db-44ae-9025-5150a6057b88")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "91cdefa2-5024-411d-babf-184ac2a40284")
		(at 168.843 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R77"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "c39cebb5-ce27-42cb-ad29-7b0742a07cb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "26c45de6-638c-43d6-8ed2-93300d30843c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a204fc5a-cdea-415d-af80-a147f3bb445e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff068a63-86b1-4600-bf4f-8145d2f3945f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e1c0391-8f03-4f77-80be-88bb5f0af2b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/17fe8f8e-c068-4c0b-a612-91b1ff6ac17b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e4dc56e-1956-4629-a430-2a026f9d95b3")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8bdbcf1-18e3-4730-87a1-985a5afc6cdc")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "327720bd-8d8f-492f-9080-23d289706872")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dadfef68-9d82-4091-b798-0b5ef05f7474")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a4de375-f01f-485a-b156-ac201e05d3e3")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a106d3a-5c8d-4104-9699-4d13e1350fce")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc03489b-04c1-40e7-9ef3-900fcece3952")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7c5b0d6-087e-4c7b-8eb3-f872af323b9e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ac19a45-b506-4d3f-8e33-16b031b6714b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da232ea9-a01a-4685-a0c8-460fbeec4685")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "40a98f6a-b0f8-4c05-8999-898cb918ba11")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 12 "/ZIF_33")
			(pintype "passive")
			(uuid "5523b812-97a4-4e61-9381-2807c0c1430a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "90bb4000-31f6-42d6-a00a-5815a7b1aed8")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "91f66c48-6a84-4106-b738-ba1af9f818c1")
		(at 168.843 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R81"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f3272aa0-0c41-4158-b4bd-9479a9c7eb00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "554fcff1-98e6-4efb-a326-f77198990a88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8439704f-96d1-493a-9a7c-144f47e8b71e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8cf0e128-604d-4f80-ab07-4101f7433446")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8fdad2ca-8737-40d0-ba02-d6fdc0e52be8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/04019959-56b8-4e58-b884-86ad3c0e6e4c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6ded737-183c-4520-8135-0679983c79ba")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e68397b4-5592-4153-bb54-8b4b67449d6f")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8d2a939-8860-44f0-ab79-4f95f66fae2f")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb0be70c-9141-4925-b946-894c83d6fea4")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aca2ed5e-132d-47cd-801e-a21c60993ff1")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "087dfb3e-7ca9-49fa-b133-e9a9cec631f7")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33930ca3-77dc-45e2-af49-add2b61b5313")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c78fe76-da44-4f0a-8416-272a76950f44")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6f69935-5322-4594-80b4-c0af8ee5241a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "813238dd-d819-4532-b306-b5edb05deca0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bc3b2af1-b738-4f97-9db3-510be3d1146a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 13 "/ZIF_37")
			(pintype "passive")
			(uuid "a2fc2c75-3686-40d2-98dc-b8fffe9aca6a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bfed9a3a-963f-4d56-951f-25f4290a0f38")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "92a4d11f-08b0-4c30-8d2d-7475c161ce41")
		(at 162.893 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R68"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "9b417685-e0bf-4fbb-a282-21e5e7015520")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "a39bb388-058b-4e23-8823-fc4367bc50a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "91c095f3-6b34-4c22-afc0-975758123cdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b922402f-1e48-48a0-ad8e-2350b8a51027")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abccc7f8-aa21-4bec-9f55-42bc87492b9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c4aff9b2-63b7-48fb-9df8-db14c4caa77b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "867a88c5-8530-4011-9017-3f9d37a9b5de")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "81fea643-7419-40dc-aeac-5ffd348e25e1")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ced4dde6-8077-4473-949b-2844881a6178")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db624a6d-3f74-41ee-8590-de04b1260a87")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a173369-e270-45e0-8139-d262c322653c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72383416-f2cd-42e9-b673-f7bb70bb989d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "041373e4-8874-46d4-8798-5711a5c5ed45")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83a0083f-e44c-48b7-bd11-69321ed71c09")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbfc3c69-2378-4579-a240-4f7b2194a296")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07100306-08a9-4211-bdd2-43c17ddd52d6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4779303f-b1e6-4b12-bc98-f9765028907d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 31 "/ZIF_24")
			(pintype "passive")
			(uuid "3d59d17c-d91e-4fcc-9d4a-ddd5d429ba81")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9745792a-da33-4a95-bd25-b7311bef435f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_DPDT_Omron_G6K-2P-Y"
		(layer "F.Cu")
		(uuid "967f9839-2aff-41a6-a318-db11f918ad5e")
		(at 125.878 105.675)
		(descr "Omron G6K-2P-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
		(tags "Omron G6K-2P-Y relay")
		(property "Reference" "K1"
			(at 2.7 -2.4 0)
			(layer "F.SilkS")
			(uuid "76008a1f-8969-4276-8160-a0d676955f53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "G6K-2"
			(at 2.5 10.1 0)
			(layer "F.Fab")
			(uuid "bc91ea4b-8ddb-41cd-b78d-2f2f1de87ae2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Relay_THT:Relay_DPDT_Omron_G6K-2P-Y"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "20430317-9b1e-4cd7-88a7-618f45a6e5ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6af876b1-1900-4197-9a48-470e0a34fd29")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Miniature 2-pole relay, Single-side Stable"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d59fef3-8792-48af-8628-d11a966ec929")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Relay*DPDT*Omron*G6K?2*")
		(path "/37c2bef2-4038-4f3a-a2d9-cc67c1c1e490")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.1 -1.6)
			(end 0.5 -1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2178e1e1-2269-4567-96e2-c12c08fe6dad")
		)
		(fp_line
			(start -1.1 0)
			(end -1.1 -1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb28287a-eb81-4eca-8791-4681f3ab3151")
		)
		(fp_line
			(start -0.8 -1.3)
			(end -0.8 -1.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83bcbacf-e82c-48a3-ad67-b0c14fbbfcfd")
		)
		(fp_line
			(start -0.8 -1.3)
			(end 5.9 -1.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5845bc78-18d5-48f6-a26b-d7a73540afb5")
		)
		(fp_line
			(start -0.8 2.2)
			(end -0.8 1.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "565f3a92-63e8-41f2-a71e-e3fb4182fa5f")
		)
		(fp_line
			(start -0.8 4.6)
			(end -0.8 3.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e627f55-da1c-48b1-bcac-2184edb79918")
		)
		(fp_line
			(start -0.8 6.8)
			(end -0.8 6.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "885e874b-594a-42f0-ae70-0615949d94a0")
		)
		(fp_line
			(start -0.8 8.9)
			(end -0.8 8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95d9ee98-40b6-418d-8c8c-237cc0f035ac")
		)
		(fp_line
			(start 5.9 -1.3)
			(end 5.9 -0.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "890379d5-4e03-4fcd-924d-64ac3768f12b")
		)
		(fp_line
			(start 5.9 0.8)
			(end 5.9 2.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f04abc8-d45e-4832-9780-3588538e253d")
		)
		(fp_line
			(start 5.9 3.8)
			(end 5.9 4.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "372dc820-4702-499b-84cd-578cf298ae17")
		)
		(fp_line
			(start 5.9 6.2)
			(end 5.9 6.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0881d9bc-7fd0-4ef3-be5c-4071ab42eb1d")
		)
		(fp_line
			(start 5.9 8.4)
			(end 5.9 8.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a86e2d00-c7e5-4f4f-933c-e004c4ed5390")
		)
		(fp_line
			(start 5.9 8.9)
			(end -0.8 8.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6e72c3a-814a-438c-baf0-1175daa9e4de")
		)
		(fp_line
			(start -1.1 -1.45)
			(end -1.1 9.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9eb678c1-7c95-4a57-8121-68388dca2695")
		)
		(fp_line
			(start -1.1 -1.45)
			(end 6.18 -1.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5823293-dcc4-448c-8ab1-cd1ffd1f6362")
		)
		(fp_line
			(start 6.18 9.05)
			(end -1.1 9.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "669324a8-741a-4a85-ade3-eae0f5d2bebc")
		)
		(fp_line
			(start 6.18 9.05)
			(end 6.18 -1.45)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f77a6cd-f3f7-432d-aa90-f14412763a88")
		)
		(fp_line
			(start -0.7 -0.2)
			(end 0.3 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95adb662-f7dd-427f-bceb-746a197f1f5f")
		)
		(fp_line
			(start -0.7 8.8)
			(end -0.7 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41f92668-cebc-4429-a82a-40ae0670f46d")
		)
		(fp_line
			(start 0.3 -1.2)
			(end 5.8 -1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c75b886e-820f-493b-b210-86d40f8586b0")
		)
		(fp_line
			(start 5.8 -1.2)
			(end 5.8 8.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "acbfae24-78bd-46a0-b7f4-a5919ed4a49d")
		)
		(fp_line
			(start 5.8 8.8)
			(end -0.7 8.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a34366c5-a6ed-412f-9af6-492a85a2e7b3")
		)
		(fp_text user "${REFERENCE}"
			(at 2.55 3.8 0)
			(layer "F.Fab")
			(uuid "014dab11-3d71-4b43-977d-7b0f970c50bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "c962b7d2-8b98-48a0-a5b0-fbdcbe6bb360")
		)
		(pad "2" thru_hole circle
			(at 0 3)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(K1-Pad2)")
			(pintype "passive+no_connect")
			(uuid "dfa95bc8-83e8-4737-a7d5-2fe4dc22f360")
		)
		(pad "3" thru_hole circle
			(at 0 5.4)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(JP1-B)")
			(pintype "passive")
			(uuid "923f8c33-e054-4f2f-a457-08c99b3ff71a")
		)
		(pad "4" thru_hole circle
			(at 0 7.6)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SWITCHED_VCC")
			(pintype "passive")
			(uuid "f96aabff-ce25-4c72-9580-0b2bce0c0d4e")
		)
		(pad "5" thru_hole circle
			(at 5.08 7.6)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SWITCHED_VCC")
			(pintype "passive")
			(uuid "f682d2c0-4659-4253-a80e-6c72b2a84fda")
		)
		(pad "6" thru_hole circle
			(at 5.08 5.4)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(JP2-B)")
			(pintype "passive")
			(uuid "df2e3573-c383-4a42-b12a-bbcf488781a1")
		)
		(pad "7" thru_hole circle
			(at 5.08 3)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(K1-Pad7)")
			(pintype "passive+no_connect")
			(uuid "96a496be-7ca9-4817-a245-91791b39c68d")
		)
		(pad "8" thru_hole circle
			(at 5.08 0)
			(size 1.7 1.7)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D1-A)")
			(pintype "passive")
			(uuid "c48f717a-8beb-44e9-9049-71c4b2f2cb2e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Omron_G6K-2P-Y.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(uuid "96d50e31-f268-4ac3-b435-777f03be392f")
		(at 140.153 101.29)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW1"
			(at 3.25 -2 0)
			(layer "F.SilkS")
			(uuid "f4846a71-ef79-479a-82ed-0ed641d39c2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RESET"
			(at 3.75 6.7 0)
			(layer "F.Fab")
			(uuid "c99aadec-45c3-4768-a090-1b6cb8e0eb07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be6801b0-74f2-4a66-ba90-3a319b75a713")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6481117a-8f27-4ac8-a205-021f6c76b447")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7fc3b47f-a47c-47e7-b870-067a5e7afd51")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/8d06aaf8-c4ff-4838-9185-e83e17b5af71")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.25 1.5)
			(end -0.25 3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ef84c58-f3dd-40e3-b15d-37f26c7b3448")
		)
		(fp_line
			(start 1 5.5)
			(end 5.5 5.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "943c8e9a-bca2-452b-9dd5-3da5479fc640")
		)
		(fp_line
			(start 5.5 -1)
			(end 1 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8792af2-e857-455a-93a4-4e175a17306d")
		)
		(fp_line
			(start 6.75 3)
			(end 6.75 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce068a45-ea6e-471e-a036-88a20cc22c6b")
		)
		(fp_line
			(start -1.5 -1.5)
			(end -1.25 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ede66387-6dd9-4fae-87d8-c14befb9d278")
		)
		(fp_line
			(start -1.5 -1.25)
			(end -1.5 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a7f4f04-0c2a-4d84-b185-90d19443a4dd")
		)
		(fp_line
			(start -1.5 5.75)
			(end -1.5 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1840f705-1eb2-4e1b-964b-717a91a61e4c")
		)
		(fp_line
			(start -1.5 5.75)
			(end -1.5 6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3d6a4382-aafc-4f31-9810-7065e021b64c")
		)
		(fp_line
			(start -1.5 6)
			(end -1.25 6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94c5cd99-37a9-4d94-92c8-5e8bd4ec05ec")
		)
		(fp_line
			(start -1.25 -1.5)
			(end 7.75 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11eb64b2-8d51-4f85-a099-e051e8dd323d")
		)
		(fp_line
			(start 7.75 -1.5)
			(end 8 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6a958f8-a609-4e2c-8957-df5084ae2c24")
		)
		(fp_line
			(start 7.75 6)
			(end -1.25 6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a42f58ac-2b6d-4ee4-be42-35ee7ff8cfe5")
		)
		(fp_line
			(start 7.75 6)
			(end 8 6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04d6e3b7-6e30-404a-b8d5-2f7663f0b1e2")
		)
		(fp_line
			(start 8 -1.5)
			(end 8 -1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b32f739e-c687-4ccc-82b3-cfd028563ec3")
		)
		(fp_line
			(start 8 -1.25)
			(end 8 5.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56bf61ff-2de9-4fe0-8a4b-0ccdb8b9189f")
		)
		(fp_line
			(start 8 6)
			(end 8 5.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49cef681-5860-489d-9234-aa2bce2af335")
		)
		(fp_line
			(start 0.25 -0.75)
			(end 3.25 -0.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75284c8e-468c-4989-982b-a76c3b77a426")
		)
		(fp_line
			(start 0.25 5.25)
			(end 0.25 -0.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41a882d9-97ff-4b21-84bd-684e0c3c776b")
		)
		(fp_line
			(start 3.25 -0.75)
			(end 6.25 -0.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cb39fc4-d2ab-42f6-995b-aff7725c40c7")
		)
		(fp_line
			(start 6.25 -0.75)
			(end 6.25 5.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1476198-6d27-4b3d-baa6-eca4397834ee")
		)
		(fp_line
			(start 6.25 5.25)
			(end 0.25 5.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "632d24fb-5f67-4fdd-9b70-c5cb1af42708")
		)
		(fp_circle
			(center 3.25 2.25)
			(end 1.25 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "4a65e4f6-8e76-4657-988e-d062aef8710a")
		)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 0)
			(layer "F.Fab")
			(uuid "a114f7b0-adeb-4992-9220-26d2961b41eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "Net-(U1-RUN)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "2264a371-6f2c-4c7d-ad3c-5bb33a982f0b")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "Net-(U1-RUN)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "742a866c-6c90-4940-b070-03e98e87e155")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8c505a49-1c1e-47ed-af48-4327cebfcf79")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "2d26ec6f-1d50-4e76-8614-7a76ee76b067")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "98b0d89a-9eb0-4c7d-bdb4-5652cdcb1240")
		(at 150.993 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R44"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f571a6e8-8858-4783-b021-38b87433e957")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "40a8a2ef-5f11-4bfc-a5ed-4538aacf9671")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "34287606-a32c-497e-b296-e156d9dc606b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9a54f2f-4af0-4e69-8c53-8350fbe4d0ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a6ac746-3445-4174-8184-eb9978394ba9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/8dbf39a6-6a00-46f9-93f9-1d6841bdc2e6")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f72ca9a2-9532-484a-81b6-8cbf4fd93c26")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fceb168c-dc0e-4a9a-83a0-6475566564af")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72bb7a54-537d-4371-9b02-6cafce3eba36")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c89bec0-39df-44b5-87ff-9d1ed209d94d")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6db5f15-ee11-4f4b-8e69-31740c00b5cd")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d208f41a-b705-4579-a736-fd851714930f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcac88b8-0261-420a-bcf8-96fb48777833")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2aabc0f8-1141-4985-baa0-14c2e046b7ac")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c0e2912-87d5-43ea-8a74-4d1380794473")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7218d52d-232b-46ea-a27a-363cbf7af770")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "56570390-6385-49af-909d-1d56e16544f3")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 98 "/SIPO_CLK")
			(pintype "passive")
			(uuid "1bd29bba-253e-4d14-bd82-1ff33336d925")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 7 "Net-(D3-A)")
			(pintype "passive")
			(uuid "b2f0e7ef-0926-4bb1-9fca-c21651a151ef")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "9964dece-115c-4975-9b4d-116228337695")
		(at 133.143 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f3165ca4-4469-4a6f-bbee-56f03c27bc3b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "325bb98f-4832-43b9-a173-7279c5aa57ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2834c9f-a211-40c2-9c8f-aa53978d07e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c29fdb70-ab56-4f2d-af53-3af50360ced4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2ba06337-7884-4bbc-bb11-b4be33bd43ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4cc89f5b-505f-4755-bf22-47348433bb14")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acc8dfaa-e1f8-420b-a13e-d97690c4238f")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7850e47-6134-4ff6-87f0-e389837c4fc3")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbc03aee-6b0a-4cee-96ba-01aa351acca7")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c383f0a3-c634-45c0-a0f7-c1a167643415")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78ab05bb-8715-4b47-a24c-32b2852fe5fc")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b43d719b-a4b4-4dd4-b718-9d600697f12d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ada59465-c0ff-44a9-8d50-8118e3c51eb3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68d3a6f0-b7e0-4b18-bf47-ec8430e37ab2")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7186e1fc-5a0e-4e9d-8982-0fca60eecd81")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ca89833-2722-4559-84ca-1af3bd4e7c1f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c70b3adf-b0e8-4f3a-8e8b-004e2bffd667")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 68 "Net-(U3-QC)")
			(pintype "passive")
			(uuid "be0c31dc-03aa-45f4-a0d9-4ac1c8a6ca1e")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 17 "/ZIF_11")
			(pintype "passive")
			(uuid "f50c7684-f511-4772-ae4f-428ac0c2507b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "997d0bf5-e480-4c1f-ac34-fd56c2bb340e")
		(at 127.193 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "b9ee8afe-73ec-439d-be7f-8fa1038237a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "39d0e9ef-471d-4f7e-9367-5cd47024b74b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57961d3f-10ee-468f-976d-7165e7d21c6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f7a94c8-8485-46ae-8f0b-f045cf46f40f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b078f71b-288e-48fa-a5a4-290d0742b3c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a4585223-896c-4cb4-ae3b-71963734aa3d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa1f5c27-7dd7-4786-a5d5-f3caaf886dd7")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e92090b0-c63d-4e5c-9a1f-e3c5bf2ab445")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "130cff64-b518-4da8-883b-3e1d49e4ad98")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "230e0ec5-07f4-43cc-beee-024beb8fe71e")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fce1bdc-443a-437a-9d9a-037f7d2b37fe")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0e3d986-fab9-4d66-a30f-515c66b00e99")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1addea0c-5b43-4551-8f9f-f9d97e66be5f")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77d14b36-dfd0-4815-a03f-6b2e78f0eaf0")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "996fd0aa-b21a-4d87-82f4-8d45c27bb3f7")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "729483fa-0c97-4b74-9870-5f96100dc23a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8236e670-984c-4218-affa-6209c0471fc9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 57 "Net-(R1-Pad1)")
			(pintype "passive")
			(uuid "6c136866-0fc8-437d-bbc6-a3ba96eec138")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 56 "Net-(Q1-B)")
			(pintype "passive")
			(uuid "9f016e80-ed05-46b3-bdcb-8f7126951869")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "9c866b80-af6a-4be7-9501-3f45e59bfd9a")
		(at 150.993 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R47"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f46757d8-2303-4a6a-a5b7-1124fa918b77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "666cb470-883f-4c41-b642-dffb693eef02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a34affa-6823-4513-b3c3-97d0219e0050")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "13909faa-3a74-4c16-8137-9870ca88c5a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0816c1d-91d7-40de-aa4a-d3d5998ddfe8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ef7c4cd8-0515-4f8a-879b-34ba029fbd6f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f73091a2-7bdb-4de9-98e7-e91d88021b72")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7839de1-8401-40f9-a204-acf5022ad79f")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ae2a3a0-04b2-4824-b80d-d6ad6a8f89c8")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c66b248f-e53d-49d1-9731-aa7106ba2744")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd874a03-5408-4b94-88dc-7f9371006978")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f74113bd-e7f8-4d29-8f67-24aa4642a458")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f99b33d-cf94-4846-82dd-f5abd0febe1d")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a60ed1d6-0f31-41fd-9c0e-25c726f22a25")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7592d6f0-51af-478e-a0e9-831647ecc200")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ba2354f-e698-4c85-a408-3d9491902c93")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0b979467-7ccb-43fa-baf1-e3315673fa5b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 11 "/ZIF_2")
			(pintype "passive")
			(uuid "6e8c6403-fd39-4835-8cc4-7f679bef4bb6")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7eec2cfc-d2b1-48f7-a15d-4e6c7f79de7d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "9d455ce4-1de9-40a4-b337-47ecb0744132")
		(at 145.343 93.54)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U10"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "36057b3a-864b-4e36-8b44-0f4dbabc8f67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT166"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "ffccdfa6-9e1d-443f-8382-0afb2e740a34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "17b7f35e-93ea-4b05-9368-68d6f92eeb66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f76fb7e-3a0d-4a87-8486-3afb091dc2c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "24afa232-edf5-4789-bddc-605c144c7387")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP?16*")
		(path "/91e15437-7fe7-441c-b5c3-27d50cd45935")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a477868e-7bba-4445-8bc8-cb49c531925c")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ef03068-1337-4b28-9a1c-9fb76f3b7e9a")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ad3c408-cf79-4a77-94fb-596504f730d3")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd485982-774d-4f25-8609-64736b0398e4")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "6e3fead9-dd80-4a4a-96fc-b7bea871c6b0")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1f64118-b356-4a30-b233-989f3cac79b9")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "083a3601-c404-4a00-a962-abcfa368db6a")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52b1e711-6134-42cd-bfc2-015c22db8e52")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85c21e0f-e6f9-47ca-a043-9018b20017a1")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4598f6c7-cd93-46f0-a98b-543758dcc62e")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf46da15-771d-4354-87c7-9d1b1730654c")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0dc5be4d-0401-4f5b-9b03-1de24e1914de")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "805e9adf-ac75-4023-aa96-63dde9c5b70d")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8aaae5b-8be7-423f-bc75-e4de64db6e67")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e1c1764a-b2bc-457a-84af-49e5dff5a8a8")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(U10-Ds)")
			(pinfunction "Ds")
			(pintype "input")
			(uuid "61bdb8d9-c959-4a51-9292-ab4cda28d3a0")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/ZIF_17")
			(pinfunction "A")
			(pintype "input")
			(uuid "82dec6c1-7115-476a-9688-8b3fb4a21f32")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/ZIF_18")
			(pinfunction "B")
			(pintype "input")
			(uuid "bef35c8a-5ef2-4461-a384-b6c184f1c1cf")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/ZIF_19")
			(pinfunction "C")
			(pintype "input")
			(uuid "2986883c-5d6f-4d58-9b59-3ad7edff0040")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/ZIF_20")
			(pinfunction "D")
			(pintype "input")
			(uuid "3730a891-ccd6-4720-ac70-492ec7ee1361")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "/PISO_INH")
			(pinfunction "CE")
			(pintype "input")
			(uuid "6995e00d-1ead-403b-be29-61be7d24bc51")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/PISO_CLK")
			(pinfunction "Clk")
			(pintype "input")
			(uuid "e63a8544-df92-4093-bf18-61966a3f50a0")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b9ab63ea-5e8e-43d8-9cb4-8221129b3891")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "Clr")
			(pintype "input")
			(uuid "d6552163-c64d-4215-971b-ab0a5db69a51")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/ZIF_22")
			(pinfunction "E")
			(pintype "input")
			(uuid "17f17087-03c4-4f9b-ba4c-afb70a0f764e")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/ZIF_23")
			(pinfunction "F")
			(pintype "input")
			(uuid "30e6f16c-0a4f-42c7-91d4-a2ed977ee9be")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/ZIF_24")
			(pinfunction "G")
			(pintype "input")
			(uuid "ad0b939e-9a1c-4544-a721-3a11bd6891d3")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U10-Qh)")
			(pinfunction "Qh")
			(pintype "output")
			(uuid "7728c5db-5ee6-4771-af08-ca9a3870fce0")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/ZIF_25")
			(pinfunction "H")
			(pintype "input")
			(uuid "8dc0978d-949f-4cc0-bae2-89ace15d6055")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/PISO_SH")
			(pinfunction "PE")
			(pintype "input")
			(uuid "4c28e21d-4374-4686-8a45-0c1c77031ede")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "97a5b7d7-9c69-4655-a503-6945d029a6bb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Socket:DIP_Socket-42_W11.9_W12.7_W15.24_W17.78_W18.5_3M_242-1281-00-0602J"
		(layer "F.Cu")
		(uuid "9d817fb1-2cc5-4595-b981-9b27f83d9395")
		(at 80.048 63.72)
		(descr "3M 42-pin zero insertion force socket, through-hole, row spacing 15.24 mm (600 mils), http://multimedia.3m.com/mws/media/494546O/3mtm-dip-sockets-100-2-54-mm-ts0365.pdf")
		(tags "THT DIP DIL ZIF 15.24mm 600mil Socket")
		(property "Reference" "J1"
			(at 7.62 -11.56 0)
			(layer "F.SilkS")
			(uuid "4fcb33bf-faf6-478c-9d0c-590eee1d5064")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "ZIF Socket"
			(at 7.62 58.64 0)
			(layer "F.Fab")
			(uuid "a5153d6a-7393-4a59-9067-d7ece0820183")
			(effects
				(font
					(size 0.6 0.6)
					(thickness 0.09)
				)
			)
		)
		(property "Footprint" "Socket:DIP_Socket-42_W11.9_W12.7_W15.24_W17.78_W18.5_3M_242-1281-00-0602J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5dea44d5-f917-48bd-8023-c0a63ac2b99d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64f3301d-b57f-4158-99ed-51d07e73dca9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, double row, 02x21, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5892944-98e3-4e63-9567-0f4fdfe6fb7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/abf5224a-1384-4d76-884c-d12f8c67f89e")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -4.95 1.27)
			(end -4.95 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f153781-eee6-489d-adbe-1f95a63304eb")
		)
		(fp_line
			(start -3.93 -10.66)
			(end -3.93 -8.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75b16e47-1ef6-476d-9a3f-13bd3cc8eb46")
		)
		(fp_line
			(start -3.93 -3.9)
			(end -3.93 57.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9216c08-12e4-45b6-976d-8f0221a5a9af")
		)
		(fp_line
			(start -3.93 57.74)
			(end 19.17 57.74)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29ed1d1d-45fb-4fac-a47a-144251e0a494")
		)
		(fp_line
			(start -1.65 -10.66)
			(end -1.65 -8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65d6ebfc-7fc2-4ef9-a3aa-f3374cb5f587")
		)
		(fp_line
			(start 19.17 -10.66)
			(end -3.93 -10.66)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b78cf28-e788-4da1-b2b1-a798b6aa2ee7")
		)
		(fp_line
			(start 19.17 57.74)
			(end 19.17 -10.66)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b882a947-8218-407b-abbe-2c2fbe3fc677")
		)
		(fp_circle
			(center -3.2 -6.35)
			(end -2.3 -6.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "25348454-a579-4e86-acf2-2da0100b2f63")
		)
		(fp_circle
			(center -3.2 -6.35)
			(end -0.65 -6.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "00094bb3-c045-4d95-816b-0d296b557d67")
		)
		(fp_line
			(start -5.5 -23.36)
			(end 0.1 -23.36)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30417072-2536-43b8-9b0e-e33f829722e2")
		)
		(fp_line
			(start -5.5 -3.4)
			(end -5.5 -23.36)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "707c7804-5df8-4b67-8cbf-523608641231")
		)
		(fp_line
			(start -4.33 -3.4)
			(end -5.5 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb228ea4-a0f8-4d95-9f4a-cf4192c4086c")
		)
		(fp_line
			(start -4.33 58.14)
			(end -4.33 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3362a272-6bbf-449a-96d5-096a06b19774")
		)
		(fp_line
			(start 0.1 -23.36)
			(end 0.1 -11.06)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b911329-c3c1-435d-b2ae-816416ff6c15")
		)
		(fp_line
			(start 0.1 -11.06)
			(end 19.57 -11.06)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1cfa0fce-84c4-4386-88a6-21a031262edd")
		)
		(fp_line
			(start 19.57 -11.06)
			(end 19.57 58.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "781218ee-f2f0-479d-94f9-a185c3b5b68d")
		)
		(fp_line
			(start 19.57 58.14)
			(end -4.33 58.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a99cd05-24fb-4b78-82e6-ccb2cf4a937d")
		)
		(fp_line
			(start -5 -21.46)
			(end -5 -17.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8625263-58dc-459e-bb99-c0b9dc8847e9")
		)
		(fp_line
			(start -5 -21.46)
			(end -3.7 -22.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0776f13e-51b6-45c8-bc70-f4fa3a13a1c5")
		)
		(fp_line
			(start -5 -17.86)
			(end -3.5 -15.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af6ed556-d46d-4ce6-a757-b14baf8f8c2f")
		)
		(fp_line
			(start -5 -17.86)
			(end -0.4 -17.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccb9bb6b-d7ca-4a66-9a40-dead8cd46267")
		)
		(fp_line
			(start -3.83 -9.4)
			(end -2.85 -10.56)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f377a8f-7bfc-4389-ac4f-ad1bfa83fb36")
		)
		(fp_line
			(start -3.83 57.64)
			(end -3.83 -9.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb24fbfc-5c8f-4349-98a4-06b0007b09ad")
		)
		(fp_line
			(start -3.7 -22.86)
			(end -1.7 -22.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ee9718b-5205-470e-adb1-81a17096e158")
		)
		(fp_line
			(start -3.5 -15.86)
			(end -1.9 -15.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a241e358-8b6b-4c56-87fe-570a947d3455")
		)
		(fp_line
			(start -3.5 -9.75)
			(end -3.5 -15.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5ce0453-b425-476a-9d96-fc6b501aa8a0")
		)
		(fp_line
			(start -2.85 -10.56)
			(end 19.07 -10.56)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48767d3a-3fd2-4910-9ef1-0d3ebeb3fe97")
		)
		(fp_line
			(start -1.9 -15.86)
			(end -1.9 -10.56)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "345f0754-b80a-475e-bf1f-9a33957e047e")
		)
		(fp_line
			(start -1.7 -22.86)
			(end -0.4 -21.46)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3e458f8-9e49-485e-87e1-a25ff4a74324")
		)
		(fp_line
			(start -0.4 -21.46)
			(end -5 -21.46)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86e50972-4956-404b-a8f4-47832c9d3496")
		)
		(fp_line
			(start -0.4 -17.86)
			(end -1.9 -15.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa67a6b4-5afb-4f3e-a11a-931f03e1a09e")
		)
		(fp_line
			(start -0.4 -17.86)
			(end -0.4 -21.46)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d51ca0d7-80ed-4c82-8adc-03275889cdbe")
		)
		(fp_line
			(start 19.07 -10.56)
			(end 19.07 57.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f55ac913-aed3-480f-b3f1-30d2e70fb8d1")
		)
		(fp_line
			(start 19.07 57.64)
			(end -3.83 57.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ed928bb-6742-4e68-882b-5e98da206ffa")
		)
		(fp_text user "${REFERENCE}"
			(at 7.62 23.54 0)
			(layer "F.Fab")
			(uuid "1421cea1-b4ae-42c6-987e-2b407c9d411d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/ZIF_1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "6060c739-fdd0-40d4-a1c0-05817584de80")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ZIF_2")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "092267dc-1348-4e09-a4bd-bfe16c1db75e")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/ZIF_3")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "5ddc0419-32a7-4bfb-b3b1-6bb13164ac52")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/ZIF_4")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "08a8d99d-8555-4eaf-91cb-60faea1609c5")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/ZIF_5")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "d9f23d33-cfa7-4d64-8efd-e448eb65e37a")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/ZIF_6")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "d8b9b5a3-f765-4a7f-b30a-04acf232f6ba")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/ZIF_7")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "ac89aeea-468b-483d-b8cf-192a70958d7f")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/ZIF_8")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "75c27beb-4ebd-40e2-89fc-85bfdc811eda")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/ZIF_9")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "fb45aafa-1dff-4f2b-8a60-16cf7232f8fa")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/ZIF_10")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "b12498c6-4a08-4b00-b356-aa9001126616")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/ZIF_11")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "30e12de4-b426-4297-bd37-9979aff053af")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/ZIF_12")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "60f1e998-9f9b-4fb5-9717-abb6d7897585")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/ZIF_13")
			(pinfunction "Pin_13")
			(pintype "passive")
			(uuid "956fc065-03f7-4820-9b13-5a8ac9136605")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/ZIF_14")
			(pinfunction "Pin_14")
			(pintype "passive")
			(uuid "6736e07d-fbbb-4e88-bf48-7b5e69fe82b8")
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ZIF_15")
			(pinfunction "Pin_15")
			(pintype "passive")
			(uuid "1db0059b-0b37-4a49-b9db-74747c6e18de")
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/ZIF_16")
			(pinfunction "Pin_16")
			(pintype "passive")
			(uuid "f6711e20-9640-4a25-939c-c21227a909ec")
		)
		(pad "17" thru_hole oval
			(at 0 40.64)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/ZIF_17")
			(pinfunction "Pin_17")
			(pintype "passive")
			(uuid "485ec3e2-060e-4fcb-bf4e-54c39f433c52")
		)
		(pad "18" thru_hole oval
			(at 0 43.18)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/ZIF_18")
			(pinfunction "Pin_18")
			(pintype "passive")
			(uuid "89cfb1b6-c7c6-4b2e-a50e-e466208097c4")
		)
		(pad "19" thru_hole oval
			(at 0 45.72)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/ZIF_19")
			(pinfunction "Pin_19")
			(pintype "passive")
			(uuid "fbce7f43-e31d-4367-a8a2-718e1bb1754d")
		)
		(pad "20" thru_hole oval
			(at 0 48.26)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/ZIF_20")
			(pinfunction "Pin_20")
			(pintype "passive")
			(uuid "565d8ad2-1aa4-41ba-889c-48152b8e5748")
		)
		(pad "21" thru_hole oval
			(at 0 50.8)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
			(uuid "dd358347-e3e7-48da-aae7-12fa50488dcb")
		)
		(pad "22" thru_hole oval
			(at 15.24 50.8)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/ZIF_22")
			(pinfunction "Pin_22")
			(pintype "passive")
			(uuid "4c281ce6-401f-4711-965e-e698d150d8ba")
		)
		(pad "23" thru_hole oval
			(at 15.24 48.26)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/ZIF_23")
			(pinfunction "Pin_23")
			(pintype "passive")
			(uuid "b37ac2df-76af-49c0-9858-e9b63c047112")
		)
		(pad "24" thru_hole oval
			(at 15.24 45.72)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/ZIF_24")
			(pinfunction "Pin_24")
			(pintype "passive")
			(uuid "7f094a7e-c1ea-40c3-8bff-e52d669b3850")
		)
		(pad "25" thru_hole oval
			(at 15.24 43.18)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/ZIF_25")
			(pinfunction "Pin_25")
			(pintype "passive")
			(uuid "57b320b7-ff5c-443d-8444-ff3c9b83e5f9")
		)
		(pad "26" thru_hole oval
			(at 15.24 40.64)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ZIF_26")
			(pinfunction "Pin_26")
			(pintype "passive")
			(uuid "148a2d2a-dbdb-4198-9a35-003f20ef86cf")
		)
		(pad "27" thru_hole oval
			(at 15.24 38.1)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/ZIF_27")
			(pinfunction "Pin_27")
			(pintype "passive")
			(uuid "7338f61a-5d67-4ae9-ba9a-0cab05d91e49")
		)
		(pad "28" thru_hole oval
			(at 15.24 35.56)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/ZIF_28")
			(pinfunction "Pin_28")
			(pintype "passive")
			(uuid "da4ce9b0-eee0-40e1-b058-67cde420b10c")
		)
		(pad "29" thru_hole oval
			(at 15.24 33.02)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/ZIF_29")
			(pinfunction "Pin_29")
			(pintype "passive")
			(uuid "3e48d005-b925-4317-8de5-763b28c4da4f")
		)
		(pad "30" thru_hole oval
			(at 15.24 30.48)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/ZIF_30")
			(pinfunction "Pin_30")
			(pintype "passive")
			(uuid "a263abc4-6ee4-4b9b-9dc1-b3d307b51af5")
		)
		(pad "31" thru_hole oval
			(at 15.24 27.94)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/ZIF_31")
			(pinfunction "Pin_31")
			(pintype "passive")
			(uuid "6449f7a3-dbd5-48a0-8893-58be087d056e")
		)
		(pad "32" thru_hole oval
			(at 15.24 25.4)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/ZIF_32")
			(pinfunction "Pin_32")
			(pintype "passive")
			(uuid "7e0e7119-5d60-4e6c-8598-5e460e433022")
		)
		(pad "33" thru_hole oval
			(at 15.24 22.86)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ZIF_33")
			(pinfunction "Pin_33")
			(pintype "passive")
			(uuid "09a32aab-75ff-4a43-bd09-0c6cd519931f")
		)
		(pad "34" thru_hole oval
			(at 15.24 20.32)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ZIF_34")
			(pinfunction "Pin_34")
			(pintype "passive")
			(uuid "2ad14370-920e-48e3-9d7a-860e2291d93a")
		)
		(pad "35" thru_hole oval
			(at 15.24 17.78)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/ZIF_35")
			(pinfunction "Pin_35")
			(pintype "passive")
			(uuid "cce240dd-1622-48ae-8c41-d2d99edbd6a4")
		)
		(pad "36" thru_hole oval
			(at 15.24 15.24)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/ZIF_36")
			(pinfunction "Pin_36")
			(pintype "passive")
			(uuid "d1d7e441-673d-409c-a361-a6fbc6fa793c")
		)
		(pad "37" thru_hole oval
			(at 15.24 12.7)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ZIF_37")
			(pinfunction "Pin_37")
			(pintype "passive")
			(uuid "0e8290c2-ba09-49c0-ae0d-ab7b15634761")
		)
		(pad "38" thru_hole oval
			(at 15.24 10.16)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/ZIF_38")
			(pinfunction "Pin_38")
			(pintype "passive")
			(uuid "b37188fc-9ad6-4b31-832b-f09008f7f381")
		)
		(pad "39" thru_hole oval
			(at 15.24 7.62)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/ZIF_39")
			(pinfunction "Pin_39")
			(pintype "passive")
			(uuid "a4234a10-7914-4ed0-8fd7-9164add11e2a")
		)
		(pad "40" thru_hole oval
			(at 15.24 5.08)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/ZIF_40")
			(pinfunction "Pin_40")
			(pintype "passive")
			(uuid "8e7b90b4-b62e-4ebe-9782-2584a04d60ef")
		)
		(pad "41" thru_hole oval
			(at 15.24 2.54)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/ZIF_41")
			(pinfunction "Pin_41")
			(pintype "passive")
			(uuid "85bfa6f2-9a49-43e0-b5c4-50fdf9c78811")
		)
		(pad "42" thru_hole oval
			(at 15.24 0)
			(size 2 1.44)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SWITCHED_VCC")
			(pinfunction "Pin_42")
			(pintype "passive")
			(uuid "95d5e92c-ffd0-408a-b37e-2b8a5642ef7f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Socket.3dshapes/DIP_Socket-42_W11.9_W12.7_W15.24_W17.78_W18.5_3M_242-1281-00-0602J.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "9e3fc658-8827-42c5-afb6-2699eae0f6f9")
		(at 156.943 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R64"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "5ef943bb-aacf-48cd-bcec-3db2ee530f80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9093c55a-3c11-4731-9f30-6a9fc7b63055")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "135394c9-6b72-427c-b96c-03080db4179c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ae68b6b6-21b0-43b0-9c81-6218149d938d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0face0b-c778-4c41-9f15-a03bcdf77b10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/19e7179e-38a1-4300-8138-0c6d13a855db")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c34e040-71a2-474a-9c62-cad073e6468b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99dffcf1-83b4-4acd-80e4-e986b97b83bb")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "662a22a5-cf3e-4b35-b0ec-1a2c656476c1")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2befd8f-b777-45f3-b2d0-71a3f75799c9")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3dde45ea-f860-4d3c-9592-15e7c6120d93")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ebec1257-5175-40f6-9567-925cf395c581")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6985e08-aeb7-4c25-a1ee-463d0eceefd3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60596beb-7e96-4375-817c-ba6340e376ad")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "045f2dad-65c1-4a57-9203-077a95357171")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6a40e6c-3511-4623-bc2b-f1475a266de0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "67b4b917-785a-43a4-804b-3e8b22b46937")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 49 "/ZIF_19")
			(pintype "passive")
			(uuid "14384221-325d-41b2-adfb-21f47940374e")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d4d9520c-1f5c-4a04-a6dc-7c05799abd0d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "9ec6becc-ba4a-4576-a4b4-a1a7ba8083e9")
		(at 156.943 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R61"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "da85be63-f97d-47fb-ae4e-f3c10123da24")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7ffb2a81-5053-472c-b956-d3fc55fd542b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "426c017a-eb3a-4f1d-9a38-3f4e293497e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed084e0c-74cf-4ece-8f13-5642be5f4683")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e81a2fd2-aebd-4655-866e-9d47292f74b3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/15f61715-89cc-4398-96e3-cce3e9897040")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "002e1d4c-0070-4f6a-b5d6-38407059d198")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bc8de81-e055-46d1-8e69-1f8e61f1809a")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8256d4aa-f0bb-4594-8e26-794d19e1ff86")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "82153ab0-0569-4a7c-b0c1-9775983fd141")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d26e58c-0d4f-4c69-8e8e-47a846823872")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4637d2d2-cf31-4ec1-9f5b-9408a55d80e5")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a77c1496-9513-444f-9f87-d4f9bb547af7")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6e44173-6e9e-4ea2-9898-603b3feb683f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cda5fdc-212e-4545-b922-f7c8fdf71e31")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74aff2ae-d74c-461a-99cd-fe825cf25338")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "08d811ef-9e25-47bc-aed8-a2c32a992cc5")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 47 "/ZIF_16")
			(pintype "passive")
			(uuid "386c2ff2-1c8a-4303-8bab-92e17a4f3795")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9b6da6e3-3a75-4f1e-9c7e-0c68e3757b72")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "9f56d743-1297-4670-9a4a-dcb9711e00bc")
		(at 145.043 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R35"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "4353b805-05c3-4c78-b893-b9139ceeeb4a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "76f1440b-5ee4-4bb9-861c-dff719a8e999")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "872f08ff-f7fe-40ad-bb27-897476b85f13")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "672ed8f0-d9fa-44ea-9f79-17111ba17b1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6656913-d6b6-49e3-939a-fd428664956f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1309f52d-8992-4db9-9daf-e027ee355b78")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76b83a1c-0b3c-4316-9183-4af982e5be83")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ffa252f-dabb-40e3-b168-59afb97c28d6")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2cc9876f-81c5-484f-8840-2131e4d3e89c")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6aa4af9d-72d8-42e5-a9b0-eda22e01ad26")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04bf3184-cc38-4b4e-a5b0-d350aecfd6cf")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a2b87d13-238a-469f-a8c2-5248787ce25b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b41f6001-8ffb-424b-ba8d-2a0f8f536696")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c05d9d5-864b-4eaa-92ed-99367a3c2b11")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d64341c4-236b-4742-b730-4ff366d2c026")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3ca8ce6-5e8a-472c-886c-9bb7228d2a5a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "12e6104a-62e4-4da1-aec3-083f0b8fe37d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 91 "Net-(U6-QB)")
			(pintype "passive")
			(uuid "94b9a788-7343-4beb-ae5e-44dacd85fdbe")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 42 "/ZIF_35")
			(pintype "passive")
			(uuid "e0c4569b-2986-45d2-a8c0-4779de84255e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "a0497ec2-99e0-444a-a8d7-c6b785ce4a96")
		(at 145.043 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R36"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "12afb832-9403-4bb2-b42f-7bcaeeeb5a05")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c8c7afe7-d5f3-430d-a21e-927ec6dfac1b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a51e545b-cad5-48c4-adfe-82875d894018")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c44d19a-e2be-467e-8949-e7f48df13ac7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "33d528f9-9aca-469a-9505-568e5f5cb5be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1187c40c-3b1d-4c52-83bd-619c14b453e9")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "101b169e-9900-4ed0-8e11-d6dfeb0ece41")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "075f1b72-d828-4142-9ddb-cee3984288af")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f87baf62-be0f-4348-b63a-223e4597bb6d")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d29aea52-a261-4034-aa56-910cb2c876ad")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "106badb7-e716-49f1-8a49-5e847f9bb1f2")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65583794-31b3-4ebc-838d-892f1df6f53a")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "604a7471-43ce-4048-8923-64b6715a8e72")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5b5ab69-d11c-4bd3-8018-7581bcb8b013")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79bb77a6-8ae0-4105-8bb1-5cf0c9b686c9")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b3e2770-fae1-4cf5-9970-8de86beec83c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "df4353d7-4051-4ebd-be53-b6b3040adf83")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 92 "Net-(U6-QC)")
			(pintype "passive")
			(uuid "cef53a45-6f58-4260-89dc-17fe0af244b5")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 43 "/ZIF_36")
			(pintype "passive")
			(uuid "f61bf9b6-c931-41ab-8ec3-b027e619c686")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "a27b6b58-4b1f-4ea8-aca1-dd79e5cd9aa3")
		(at 153.793 81.92)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "b75c4300-2875-441b-af63-50bc972c9e9e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT595"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "9f0b1826-2c98-4ce1-930b-c7a45e392178")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9aa8114b-e32a-460b-9bac-8339bee8e5af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "789bd687-1c1a-405b-8306-f3ccd7118aa3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "569198c1-5d80-4e0e-b48d-730482a6e146")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(path "/05c73778-a6e0-4942-9e7d-1052e0cbbf5d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c7ecbaf-0d6c-4e38-aacb-45816d680de3")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bafc1655-4198-4b60-aab6-3f53b7bbea02")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7460cb6f-7a44-4f47-93fe-f74779ec9cb9")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a050377a-cc7a-49e9-bebd-ebcb9e7492c5")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "277c783f-fbad-420a-b3f4-bea3c6d1bb35")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dee029bc-a80e-41d6-9d7e-bbf7ccaef71f")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b92a4cd8-ea11-4c66-b78f-c9c3bef0ff7b")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44c09734-8c0e-4d39-8d57-4f3b69bfbe9d")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a015b8fb-f30d-4dfd-a5ec-152119c36b15")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f706b65-2948-4442-868b-22b3a451a3bf")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00ab6f8e-1527-4b4d-9591-329cae224a74")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e683795-c98f-4a43-bc10-47dced8b0e29")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e9dc5ba-ceaa-4563-939a-d2ae06a4f1dd")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63664c68-4916-4df6-95e7-b675cf5c86ea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "803131c3-5aa4-4296-bf6b-84249f30aa17")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "Net-(U5-QB)")
			(pinfunction "QB")
			(pintype "tri_state")
			(uuid "62d2bf32-bb34-4b44-99dc-5ce43d7a4273")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "Net-(U5-QC)")
			(pinfunction "QC")
			(pintype "tri_state")
			(uuid "c5c26325-806e-4f17-b21c-6b5e1c7591ea")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "Net-(U5-QD)")
			(pinfunction "QD")
			(pintype "tri_state")
			(uuid "7894dd17-9f25-4c9c-a6ef-8abe8b0da710")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "Net-(U5-QE)")
			(pinfunction "QE")
			(pintype "tri_state")
			(uuid "58440fc7-4c98-4452-a412-cbfb423cf930")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "Net-(U5-QF)")
			(pinfunction "QF")
			(pintype "tri_state")
			(uuid "56a0df85-23c8-4e4e-a334-0fa059fb1bd4")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "Net-(U5-QG)")
			(pinfunction "QG")
			(pintype "tri_state")
			(uuid "d2b0d8f8-5594-4806-b4b0-1c2542e5ffab")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "Net-(U5-QH)")
			(pinfunction "QH")
			(pintype "tri_state")
			(uuid "541bec54-bb33-4a7c-bc28-45c0d97c2317")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "fc24e418-8799-47fc-b090-bd5ae46b8652")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "Net-(U5-QH')")
			(pinfunction "QH'")
			(pintype "output")
			(uuid "749325ab-97c8-48f5-86f9-9c6f663d11ae")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "~{SRCLR}")
			(pintype "input")
			(uuid "e159f4fc-5ef9-491f-ac86-fd1fc7dac93c")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/SIPO_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
			(uuid "23240628-ef6d-4156-8027-c3109bb78100")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/SIPO_RCLK")
			(pinfunction "RCLK")
			(pintype "input")
			(uuid "dda753ed-6d62-41cb-95ae-78688835ba3c")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "bb65990e-d54d-479d-ab19-57000d0199c0")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "Net-(U4-QH')")
			(pinfunction "SER")
			(pintype "input")
			(uuid "03ff659e-f527-456a-8654-88827ffacf41")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "Net-(U5-QA)")
			(pinfunction "QA")
			(pintype "tri_state")
			(uuid "3b456327-a641-4853-9603-c69a8c2875a5")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "0b23269d-b093-4bc7-875b-35acc411f742")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "a6bbe259-e4d3-4e66-abad-f6b569c29054")
		(at 103.143 95.12)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "19dea217-825c-44a5-8c5f-c67cbd408a7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "19cdcb76-3091-44ef-aa90-0f6d91270f75")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "52639f5a-930e-4910-b22d-4a5de77c4572")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5748e199-0d81-4d87-89b1-279aeea84a62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7785355-59fc-4fb0-bad2-1bd89010d54e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/1957c1a7-768d-49ca-b908-8dffc2bb10e2")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a92d019c-f0d5-4ce7-afba-f14f63dd1b07")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7c5ceb0-5e4f-4485-991b-1c7777c386f5")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3f86ae5-4d21-4a53-abf3-2de71146ddad")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "765abdab-5867-4c33-8dd6-4304afd95f59")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50108835-73d4-459b-83ca-ff1efe1bf5c6")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "053a978a-0e35-4ebd-af3a-09289f3404ef")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e5e3ae1-ae43-4e2a-875e-30c2bacabcad")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a3f49cf-d251-44a0-b9e8-c988e5e9be91")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fa76dda-54e5-4f33-a52e-0474ccdf4847")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4999a8b7-aafb-4faa-ad03-331b35458f50")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "23c4c1f8-9b2f-4e07-9113-336762d9ff05")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "/SWITCHED_VCC")
			(pintype "passive")
			(uuid "9a1907a3-cace-4020-a0a4-4013c189e499")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "15767215-4e8f-47d2-becc-6383781dd57b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "a6f7c3d8-8452-45b1-938e-0a89f5db15c0")
		(at 150.993 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R51"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "89563bf6-cf78-4935-b7bf-fc9ae58e9b1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "6a08c4a8-07f1-49f4-8fbc-29c8e72080ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "25e96ecd-d874-4ac0-a64e-09db355dd636")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e8c9688-0dfa-4242-9954-0796e9372218")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e553579d-11ff-4054-9912-f3a75281f2be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/18c67560-8b5c-45ae-baf5-c83ef385714a")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4f7572d-2576-40e3-96c3-bcec0758d9da")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6950301-440f-47ec-8e33-87d9c9064a23")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca048bff-6ccb-4588-b24a-d5825f71f8a5")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc102390-38b2-421c-a5ba-1be0fdce4219")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e98c71f8-5a1d-41a1-a170-1cbeb3badcfc")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68cdddd7-1043-4b91-acb4-84104e008742")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d85aaf35-f7fa-4204-b8f4-c2e63ac4622e")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60d9339c-c14f-42de-a3de-3b043fcaed2e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b58ad0c-ee34-4cff-b360-f699a932f9f2")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02bf8b57-de17-4ee3-94b6-0db7867d2839")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e6f70143-2757-4a4a-8588-4a867a0ff417")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 44 "/ZIF_6")
			(pintype "passive")
			(uuid "4f0f9813-6bd2-4af6-97db-a78d06dea136")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "1f38eab9-51ff-4f11-a45a-bc7da30de266")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "a94ad82e-77b8-44ad-8a56-6c3e15282e08")
		(at 168.843 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R83"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "816fd8f4-2bdb-40e8-acba-a461f08ff94e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "721525c9-3dc3-4cc3-b1dd-5e1527ef339f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "573f8013-ac5d-4960-8b1a-9a09d8059361")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7e61a34-8eee-4491-9a2b-915a8736ae63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d071d1ff-793d-4b41-ac17-86fe9310db87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/089de567-e4d6-4b4b-ab9b-c9adc18d2017")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fb523b1-df0d-4bae-9154-3d531a05053e")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3a36fed-d44e-48ca-9732-9d31209e4dc5")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ec736b8-f622-4c37-a505-d3e8f9b08884")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c0dfbf3-41b6-49d8-8110-9eb3c38a2eda")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c4c3e9a-eefc-46fb-8b81-3d3c5d3aa0e6")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07378efe-769e-41c7-8132-b33b8857d9b3")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3e16046-3fbe-497c-8971-4957bebaaf31")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52dc231b-77da-450a-8c6c-b5170cbcc50a")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72949a09-eda8-48cb-a8d4-c746bc97d54d")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1caa336f-2c7a-4d4c-b772-73560e33a914")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2d7408c3-f9a1-4ffb-8604-a43a19c62dcd")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 37 "/ZIF_39")
			(pintype "passive")
			(uuid "a4f4aa08-fffd-47fe-ae10-f0354f26566a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0b6f379d-beeb-4c29-beb3-97684f0e893c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "ab326af2-23c0-4bb2-a264-96e237fbbbe2")
		(at 151.003 111.76)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(uuid "7b7513e9-a546-472a-a120-db976a4d5447")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Debug Header"
			(at 0 7.41 0)
			(layer "F.Fab")
			(uuid "df1fd5d9-7686-4d29-b533-1aabae6cd1b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "283d1e4b-472f-45ba-8c37-233298d86af1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c317f83-7175-4788-8868-605eebd07535")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de22deeb-ea68-48d6-9634-8ac7a8383d70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/a340231f-2cd7-4f12-8a60-956f7205b55b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c325e80-6488-4b3b-80eb-0bf025dde5f3")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8acf793-fe9e-4301-a07a-e9dc51604166")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd2460a1-6549-43db-8258-ff4dbd72ec03")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8fed1f2-4380-452a-9d9b-44f838bef02a")
		)
		(fp_line
			(start -1.33 6.41)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "852b2e8f-ef4a-4576-b7f7-d3f3baa2faf8")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e52e59f3-eded-4356-b6c6-1cb68626c2a0")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b411d80f-e0b4-4a07-9257-63560cd9303a")
		)
		(fp_line
			(start -1.8 6.85)
			(end 1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24a1f24e-c079-42d9-b5f4-ebfd4b3c140b")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2559a078-eab3-4c87-8703-070ed0ee0f48")
		)
		(fp_line
			(start 1.8 6.85)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbda687d-8410-48f1-9c66-76969834aae2")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8afd3109-d4d2-4100-933a-4abd9120d53f")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdb9020d-04db-4556-88b0-74a92e06e86e")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ddbd558-060c-463b-bdf2-229b739800c6")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10b705d0-943e-4e32-bf92-d1401d892b4d")
		)
		(fp_line
			(start 1.27 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3732d055-c1e1-48dd-a40f-bd622aaf8e65")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
			(uuid "401992da-ddff-49d2-88d2-69fd65837a4a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c2dcedb2-a035-4177-ba13-7f8f209f9ae2")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "39d94d05-2ec2-46f5-9f83-54afe25b235c")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "4b93d87d-8459-427b-b006-37416df38ae1")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "ac9f838c-e3e3-4dbc-8017-c81ff589be74")
		(at 139.093 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R22"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "76caec9c-1b32-43d4-bd60-5f0cd8b09885")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "bf6fc6b1-7bce-41f7-82c6-a3dca8c775b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "59076d1b-b073-49d8-aeea-8b2594d4c2d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "915cd341-f7f8-4bc9-bfe6-83c42417549c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7570b33-ac11-449c-bdd0-c9002b37f7ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c2b30838-b390-4ac2-b9f0-04e728fd97e5")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8724ded-aedb-4dfa-b531-e2b92b4bb2c9")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "046d9385-3c16-4654-98fd-48474bf4652d")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb134c9b-1c8f-49c8-8409-5432ff14b125")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6da489a7-ed6d-4b50-a6b5-45f57e8ad177")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1a032e9-9758-49ff-9cfc-361b70d0bca1")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d92681c6-775b-4fc1-9b57-50bb1b927090")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97712ea1-4396-4ed3-a104-460e17e01c41")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59667151-5469-4ced-a247-9d5dd14e356e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37fabcc1-974c-404c-bbaf-7002f0282d81")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1ba6c14-d292-47c5-9931-f34573fbcc71")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ca9621bb-cd76-4a9b-9cf3-24b21a286e43")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 78 "Net-(U4-QE)")
			(pintype "passive")
			(uuid "8b472e0f-2c5e-463f-b15c-8e187ac8645a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 20 "/ZIF_22")
			(pintype "passive")
			(uuid "78830fc6-d6af-458d-b4ba-e82cc2d4a7df")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "aef2b93e-4a85-4d4b-a791-337df0d8b953")
		(at 145.343 81.92)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "3ef52a36-651c-4631-8898-ddab1769a2cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT595"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "eb85e90c-c24f-4b23-a537-7bbe448c3b6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9abb6ab-a0ea-4768-8ab9-db103d98ed6c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebe0a994-fc95-4db1-be8f-114eeae76a64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c59391a-16ad-41cb-b347-cde1d9dba375")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(path "/9c01c299-9341-484e-b49e-ed84224c5cc1")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "784493ab-1235-4db1-a64b-0201edd704af")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86509bb3-5e33-498f-aa5b-84935bb6eb56")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdb09a62-3aac-400d-82dc-56374df3a639")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e76f3508-08a6-493c-9818-567c3baef294")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "4f72d22d-dfc2-4b59-a2af-b95efcaed187")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbecf959-cd34-4443-bba2-2d16ad1c5e85")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afa85a51-0972-42db-8c25-6b143c3ed27d")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a848068-ca34-4b20-b717-e99da1648f1a")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8160b4b-4f57-4604-9db1-a1951e60f4f5")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9ffde71-32c0-471b-9de8-88c69b697b58")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8dc6f39-d423-4667-943b-d1e6d8d67fc3")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09909118-67a7-4641-98f1-740f8b6f11ae")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccb3ba67-5039-4c55-9e91-c682213915df")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be87da01-e7d9-48ef-948b-9a8e26219199")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b62ba349-4307-4f8d-a8a8-6dac46c1515b")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "Net-(U4-QB)")
			(pinfunction "QB")
			(pintype "tri_state")
			(uuid "c68072fa-d3ba-4efb-9191-82b0147d715c")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(U4-QC)")
			(pinfunction "QC")
			(pintype "tri_state")
			(uuid "a73cb0a8-0389-4319-a8d0-0fdc6a23bccb")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(U4-QD)")
			(pinfunction "QD")
			(pintype "tri_state")
			(uuid "92d406f8-d20a-4672-ac39-6cc03aa01453")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(U4-QE)")
			(pinfunction "QE")
			(pintype "tri_state")
			(uuid "1e504b69-7507-478d-b023-072308d09bb9")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(U4-QF)")
			(pinfunction "QF")
			(pintype "tri_state")
			(uuid "6c6a94d9-fea4-4b72-aabb-4fb4f41b2dc9")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(U4-QG)")
			(pinfunction "QG")
			(pintype "tri_state")
			(uuid "8d09a555-756e-4a11-b2bf-5ca8b62eced3")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(U4-QH)")
			(pinfunction "QH")
			(pintype "tri_state")
			(uuid "9ca6f1a6-0108-4daf-ba58-92a52844caad")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "725c2843-157a-43c6-ba34-17494b0f9a3c")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "Net-(U4-QH')")
			(pinfunction "QH'")
			(pintype "output")
			(uuid "69249f58-2be0-4b9d-9a28-143bdbb1ed4d")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "~{SRCLR}")
			(pintype "input")
			(uuid "40625b92-3cfc-4e73-a22d-faf337c809c1")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/SIPO_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
			(uuid "a3b83f21-8ff0-4ab8-8175-22eb3443e54a")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/SIPO_RCLK")
			(pinfunction "RCLK")
			(pintype "input")
			(uuid "8c978a0c-29e8-4445-9f6c-77e9e652d1e4")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "e8d9934b-8252-4a49-bdcf-bb4a40174985")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "Net-(U3-QH')")
			(pinfunction "SER")
			(pintype "input")
			(uuid "fab5041f-672a-48a8-a07a-a22201ef27e6")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(U4-QA)")
			(pinfunction "QA")
			(pintype "tri_state")
			(uuid "9d7b4863-2a3d-4521-841b-42db4ad320e4")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "7fbd2195-0cd7-4fb2-bceb-219e92821a4a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "b0a6f5db-9c7c-4906-a071-02bb904ad3a7")
		(at 162.893 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R70"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "4fc7af89-34e1-4d1e-923a-dd9ed62601fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "56450513-9d4a-4ec1-a04c-e3de108f42fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac26dec6-3a0a-43ea-ba72-7953ec10ce63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "18b6e06f-84f2-40b6-9823-8503b1870184")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "91ac43c4-51bb-422f-8b98-05848605f42b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/056f7b94-e44b-4e4c-954c-85ec04d0d9db")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e840920-9837-44c3-8c93-ba323264cb60")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4c225df-c559-439c-8408-1947b53053eb")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bcd610cb-3311-471d-a82c-c02cc41e846d")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fada7cd-a928-427d-b99d-540fd42c0085")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "794424cd-7714-4b86-918c-98d5fad779db")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50940acf-9a46-4556-84ad-56614eefc723")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70257757-4a7f-42c7-8689-845814625130")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77766752-2a33-4a74-aed1-5f7982b470a8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a033b906-db1d-4856-bf60-9aef16ef92fb")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1001cade-1dff-4f72-b7b7-dd91719610e5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a97526d0-e99f-4b30-95c4-ddafa3f9566d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 14 "/ZIF_26")
			(pintype "passive")
			(uuid "7598f405-e21b-4909-aa0f-88a848be0047")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "08d14191-5ac4-4443-9329-460763dc5dce")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "b3168098-0fdb-461e-9013-ccc555d88987")
		(at 162.243 93.54)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U12"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "c13fea39-947e-42bf-a45a-4f53258726ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT166"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "44519f87-4806-4ed0-8a06-1e7311197544")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c524c095-c8a1-4349-a0c3-c1c350e02f52")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS166"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88f1eeb8-cfbd-4f0a-be3c-41fa77c8a321")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Shift Register 8-bit, parallel load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "52d7d3ca-e9c6-4bf3-a974-b60b5a3dd0d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP?16*")
		(path "/1db94f17-0680-435d-9aff-298b63db8489")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a98ceb33-4ba1-4ffb-8a19-2cadd42f912e")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56e3c4b8-1a24-4aa4-b6e9-6f6a150ef152")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54fbb44d-5be0-4448-b4f7-693b7abfeb5e")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60db80dd-296c-4a1b-8f51-ee462e20e923")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "411fade1-9062-4b33-bce5-53cbfeaeca5a")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "caff79e8-d202-4fec-9c61-fc27a3ae9d5d")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bebffe05-a91c-4750-8829-a73a8cd7d1b3")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0274ba2a-2409-4ca5-b9e9-c80ee2cd5650")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3f2630e-66d9-4d09-b42b-4d5d85942f48")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c29655e-e18b-47db-bd16-7b2cce64fb15")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "823b6fc9-ebad-4b98-8b2f-b2efe3cf0812")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "864580f7-d5e4-45b8-a703-9444a0685d44")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdc24cfa-40d3-4427-815d-48b246bce442")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae61cfe0-6e34-44c5-a9db-2b95eed9faff")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2921cd72-7c05-42b6-8c7c-7b04ae5c0206")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "Net-(U11-Qh)")
			(pinfunction "Ds")
			(pintype "input")
			(uuid "285c2eb1-9aa0-40a8-b8ac-23ed9b1d1c76")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/ZIF_34")
			(pinfunction "A")
			(pintype "input")
			(uuid "26481c2d-896c-4028-86c4-151f794a92b0")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/ZIF_35")
			(pinfunction "B")
			(pintype "input")
			(uuid "dc395730-f510-4bd9-bf76-12af643c832b")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/ZIF_36")
			(pinfunction "C")
			(pintype "input")
			(uuid "b6669659-2900-4cc8-b831-5b5449c6656c")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/ZIF_37")
			(pinfunction "D")
			(pintype "input")
			(uuid "888adc7f-79fe-4c37-ae1c-0089f4d1971c")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "/PISO_INH")
			(pinfunction "CE")
			(pintype "input")
			(uuid "455bcca9-d546-423a-9275-9fae60203de5")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/PISO_CLK")
			(pinfunction "Clk")
			(pintype "input")
			(uuid "db99ae50-e2ec-43b3-a260-6c46f1b4fb72")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "f47f5055-3d6b-4da2-958d-cfc878e3635f")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "Clr")
			(pintype "input")
			(uuid "9db9253d-00da-4938-bd53-547d51ae490b")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/ZIF_38")
			(pinfunction "E")
			(pintype "input")
			(uuid "73abcc99-6269-4b5b-b58c-6cb80fd07f8a")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/ZIF_39")
			(pinfunction "F")
			(pintype "input")
			(uuid "63079afb-99ff-4598-8635-cb6e8eb29c93")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/ZIF_40")
			(pinfunction "G")
			(pintype "input")
			(uuid "dab131c7-b782-44d5-9ab1-aefb1f5e7492")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "/PISO_SER")
			(pinfunction "Qh")
			(pintype "output")
			(uuid "c8857193-b328-44b8-ac4f-2d4a8ed48629")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/ZIF_41")
			(pinfunction "H")
			(pintype "input")
			(uuid "edec16dc-fa31-4280-aebe-c3a34b90ad90")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/PISO_SH")
			(pinfunction "PE")
			(pintype "input")
			(uuid "95027add-85a7-465d-99e0-e03084776b49")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "cd295b96-9313-48ed-84ef-0866b8a2e685")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "b384c09d-20b1-497d-8641-06b584a81b16")
		(at 127.193 41.48)
		(descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse handsolder")
		(property "Reference" "F1"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "5890eb4e-cad6-472e-bf2e-27d588925545")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "500mA"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "451e30fc-4012-4a62-8ae2-14849a3d73b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "908f3caa-fe19-4e28-a403-7ca4bb4982ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "52629eff-7721-44e8-a9c7-34dd1b07c01e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fuse, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a0abbc7-c201-41c4-b640-5a190afb6718")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Fuse*")
		(path "/816ff385-c746-4397-916b-76d27b52005c")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.602064 -0.91)
			(end 0.602064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7401431c-d21f-46c8-b9d1-9e28cc269281")
		)
		(fp_line
			(start -0.602064 0.91)
			(end 0.602064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69da2edf-a9aa-4bff-8785-0149230046fa")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14907c3d-dcd4-4b28-9cff-35cfa63b701d")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "416f72d3-90c8-404f-a180-bb1d577db100")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb858b0a-34fa-4476-b942-1f1c8d36d710")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0bf1f3e1-cc06-42f0-9088-e7c34410466f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43d7b5a7-b51c-40f8-b251-31bbc0d55784")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30058c9b-c743-4202-98e8-8b9047c64ccd")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9088917c-e96a-46b5-bd33-29d92f265882")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d69d2bf5-1ae1-458d-896c-e67be4726095")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0d51dead-8c68-4826-91fc-cfd8daa44129")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 9 "Net-(U1-VBUS)")
			(pintype "passive")
			(uuid "7b027013-53c6-4334-9c20-8c60ac3d96f0")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "7c6c406a-9544-4139-9f88-1513045a831e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH"
		(layer "F.Cu")
		(uuid "b901dd56-2513-4f77-9225-fcc9c2bfdb57")
		(at 42.926 74.549)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "U1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "91d84924-fe93-42ce-b9a4-4e53b3e09820")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Pico"
			(at 0 2.159 0)
			(layer "F.Fab")
			(uuid "a1e6ec2c-88a9-4dbb-9184-8cd19d109ce3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b798d938-61b3-4699-9e58-9cf2a6d0c408")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "84453413-5bdb-4022-9117-97bd9e3805fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b169b8e-c55f-4ad6-840b-e4dc252ce7f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ba57a217-405a-46af-80f5-e5550badc478")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -10.5 -25.5)
			(end -10.5 -25.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44e4af57-d769-453e-89f4-2cae67025d68")
		)
		(fp_line
			(start -10.5 -25.5)
			(end 10.5 -25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a1095d5-0579-4c82-878d-3d8a0ca0b5db")
		)
		(fp_line
			(start -10.5 -23.1)
			(end -10.5 -22.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80968311-776c-4656-aed9-b147ca0a42a9")
		)
		(fp_line
			(start -10.5 -22.833)
			(end -7.493 -22.833)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6faa137b-0857-4d07-9406-a1806028e382")
		)
		(fp_line
			(start -10.5 -20.5)
			(end -10.5 -20.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9077349d-ccc2-419f-b33c-ee46ff3228ad")
		)
		(fp_line
			(start -10.5 -18)
			(end -10.5 -17.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c8e2f73-044f-477f-bcb9-0ba4ae8fa5a9")
		)
		(fp_line
			(start -10.5 -15.4)
			(end -10.5 -15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f00b2561-6a22-4f8e-8f99-204dd71ead65")
		)
		(fp_line
			(start -10.5 -12.9)
			(end -10.5 -12.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e79882fc-a0fd-4501-b1f8-a58681cffc54")
		)
		(fp_line
			(start -10.5 -10.4)
			(end -10.5 -10)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "784a1ee2-9e5e-4e6c-8469-7ff7a157e910")
		)
		(fp_line
			(start -10.5 -7.8)
			(end -10.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf418bd0-4721-4ea9-8dbe-cf50641d9b77")
		)
		(fp_line
			(start -10.5 -5.3)
			(end -10.5 -4.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d86e9dd9-d382-4c22-a1de-c12a05011254")
		)
		(fp_line
			(start -10.5 -2.7)
			(end -10.5 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83d7022d-de65-45ca-a8e1-b658b9f4184f")
		)
		(fp_line
			(start -10.5 -0.2)
			(end -10.5 0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f247bae9-23d1-45ad-b64e-50865fdc4926")
		)
		(fp_line
			(start -10.5 2.3)
			(end -10.5 2.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a11e2ecb-afd3-4d51-bed4-208d7e41d173")
		)
		(fp_line
			(start -10.5 4.9)
			(end -10.5 5.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70e4c309-1194-4278-9db6-1e9f0c1316a7")
		)
		(fp_line
			(start -10.5 7.4)
			(end -10.5 7.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39ca4304-3290-4116-946e-ae646d6a10cb")
		)
		(fp_line
			(start -10.5 10)
			(end -10.5 10.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d92235d7-fe09-4109-90f8-e8c7d5efa465")
		)
		(fp_line
			(start -10.5 12.5)
			(end -10.5 12.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "323acdf1-3dfb-46b9-85ff-bfe2d5bdc3bd")
		)
		(fp_line
			(start -10.5 15.1)
			(end -10.5 15.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd0b90c4-9075-4921-838a-d2574b73df83")
		)
		(fp_line
			(start -10.5 17.6)
			(end -10.5 18)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5bc804c5-37f4-408d-a95c-3bdb34c190ef")
		)
		(fp_line
			(start -10.5 20.1)
			(end -10.5 20.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f03fe65-d61e-4f5e-bf0e-47c451371db2")
		)
		(fp_line
			(start -10.5 22.7)
			(end -10.5 23.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b104ae2-dcae-4db3-8ffe-5da24cf006d8")
		)
		(fp_line
			(start -7.493 -22.833)
			(end -7.493 -25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1afae480-57f1-41bb-aad7-13cc96498f5e")
		)
		(fp_line
			(start -3.7 25.5)
			(end -10.5 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7524bfc1-c271-4959-8a5d-94572abd8f21")
		)
		(fp_line
			(start -1.5 25.5)
			(end -1.1 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60fde384-ad2b-4e0b-b0f5-47241e06efe9")
		)
		(fp_line
			(start 1.1 25.5)
			(end 1.5 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad1fc146-8003-4a1d-a7aa-58f54936b996")
		)
		(fp_line
			(start 10.5 -25.5)
			(end 10.5 -25.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a5ef62e-2ce4-4e39-8abd-274fe3f3df89")
		)
		(fp_line
			(start 10.5 -23.1)
			(end 10.5 -22.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b31d71fe-134a-4b38-967e-52dfcfeb87ed")
		)
		(fp_line
			(start 10.5 -20.5)
			(end 10.5 -20.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "869e458d-9f62-4887-b4c0-cb233817e356")
		)
		(fp_line
			(start 10.5 -18)
			(end 10.5 -17.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6eb3de18-102a-4663-8886-8907f5a1163d")
		)
		(fp_line
			(start 10.5 -15.4)
			(end 10.5 -15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2695e5f0-3f40-4f84-95dd-2b12ce56759e")
		)
		(fp_line
			(start 10.5 -12.9)
			(end 10.5 -12.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5eceb5d2-7bf1-4002-9936-d60c671bf676")
		)
		(fp_line
			(start 10.5 -10.4)
			(end 10.5 -10)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2d4aa34-9597-43d3-951f-59b0303e46ce")
		)
		(fp_line
			(start 10.5 -7.8)
			(end 10.5 -7.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f0de94a-99b4-42e7-ab03-d8549a40b4c0")
		)
		(fp_line
			(start 10.5 -5.3)
			(end 10.5 -4.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a3d04d9-24f2-4254-bb89-d764072b8d27")
		)
		(fp_line
			(start 10.5 -2.7)
			(end 10.5 -2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bd11b31-7bbe-4428-933d-3175ea15f5fa")
		)
		(fp_line
			(start 10.5 -0.2)
			(end 10.5 0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f954aba9-377d-47ed-afcb-97222e2dbc90")
		)
		(fp_line
			(start 10.5 2.3)
			(end 10.5 2.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be27b619-4aec-48c5-b89e-32a00f1849e8")
		)
		(fp_line
			(start 10.5 4.9)
			(end 10.5 5.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7436d91c-9f0f-4d88-908c-a81f8a15a79d")
		)
		(fp_line
			(start 10.5 7.4)
			(end 10.5 7.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10854f08-2717-4c86-8ee8-c2be933d0e84")
		)
		(fp_line
			(start 10.5 10)
			(end 10.5 10.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f34845cf-51a4-4f4b-8cff-c9127e030b25")
		)
		(fp_line
			(start 10.5 12.5)
			(end 10.5 12.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5092db9-ed64-480e-af5c-3863d40995e2")
		)
		(fp_line
			(start 10.5 15.1)
			(end 10.5 15.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee28db4a-4eba-495c-997b-9756208f11f3")
		)
		(fp_line
			(start 10.5 17.6)
			(end 10.5 18)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f0b537b-4f1c-470c-ab2d-68e2dd24647a")
		)
		(fp_line
			(start 10.5 20.1)
			(end 10.5 20.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c085359-5017-4aa0-9f99-9676e393d5c6")
		)
		(fp_line
			(start 10.5 22.7)
			(end 10.5 23.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f13b370a-352f-416e-90db-4f5abcac2077")
		)
		(fp_line
			(start 10.5 25.5)
			(end 3.7 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a6ef576-e61a-4838-b7f0-033bf6a30286")
		)
		(fp_poly
			(pts
				(xy -1.5 -16.5) (xy -3.5 -16.5) (xy -3.5 -18.5) (xy -1.5 -18.5)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill solid)
			(layer "Dwgs.User")
			(uuid "0bdaf2d3-fd19-4421-a562-50fce182f5d1")
		)
		(fp_poly
			(pts
				(xy -1.5 -14) (xy -3.5 -14) (xy -3.5 -16) (xy -1.5 -16)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill solid)
			(layer "Dwgs.User")
			(uuid "ae28914e-206f-4194-998b-1110eba3d1f8")
		)
		(fp_poly
			(pts
				(xy -1.5 -11.5) (xy -3.5 -11.5) (xy -3.5 -13.5) (xy -1.5 -13.5)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill solid)
			(layer "Dwgs.User")
			(uuid "095f3603-fa6f-4270-ad0f-ff72d5b0b14b")
		)
		(fp_poly
			(pts
				(xy 3.7 -20.2) (xy -3.7 -20.2) (xy -3.7 -24.9) (xy 3.7 -24.9)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill solid)
			(layer "Dwgs.User")
			(uuid "49b3006b-08fd-47fb-bd00-48f6c55964fd")
		)
		(fp_line
			(start -11 -26)
			(end 11 -26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bb934a5-ce70-40f5-bc31-1ed19623d786")
		)
		(fp_line
			(start -11 26)
			(end -11 -26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2658acae-8d98-42a9-8266-6a797833280c")
		)
		(fp_line
			(start 11 -26)
			(end 11 26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "073c11fa-2eb9-40b1-92b2-326fc51d806a")
		)
		(fp_line
			(start 11 26)
			(end -11 26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2b3bc1b-4e42-49e6-81a2-7886adf945cf")
		)
		(fp_line
			(start -10.5 -25.5)
			(end 10.5 -25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc49996d-a3a4-4b3f-ac8f-141c38dbe0c0")
		)
		(fp_line
			(start -10.5 -24.2)
			(end -9.2 -25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4fdfa77-a9bc-4790-b4bb-ba5e9f64a09f")
		)
		(fp_line
			(start -10.5 25.5)
			(end -10.5 -25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "795de948-8f43-4ca9-b04b-8ebedc256dae")
		)
		(fp_line
			(start 10.5 -25.5)
			(end 10.5 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a878f558-b0ad-4277-8696-6950a63671ef")
		)
		(fp_line
			(start 10.5 25.5)
			(end -10.5 25.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19c570ed-b95e-4b55-aa9a-6d0ab04ff7af")
		)
		(fp_text user "GND"
			(at 12.8 -19.05 45)
			(layer "F.SilkS")
			(uuid "0a473071-6776-4442-aea8-16ba260e799e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP4"
			(at -12.8 -11.43 45)
			(layer "F.SilkS")
			(uuid "0ca8520d-844d-4a7f-a381-c2e70371790d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "ADC_VREF"
			(at 14 -12.5 45)
			(layer "F.SilkS")
			(uuid "10d81c00-190d-4836-9a1e-de2f401eea47")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP10"
			(at -13.054 8.89 45)
			(layer "F.SilkS")
			(uuid "1d7bc02d-1cc8-4f89-865f-8143c2247c43")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP1"
			(at -12.9 -21.6 45)
			(layer "F.SilkS")
			(uuid "21647267-0770-4a04-94f1-aef7886ca867")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP3"
			(at -12.8 -13.97 45)
			(layer "F.SilkS")
			(uuid "221c453e-b6d0-47e6-a86b-5b0360cfacd4")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "SWDIO"
			(at 5.6 26.2 0)
			(layer "F.SilkS")
			(uuid "2bfb4a17-19f4-4411-847b-4fae7bdbabc7")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP28"
			(at 13.054 -9.144 45)
			(layer "F.SilkS")
			(uuid "41915081-b79d-42c4-9057-06e73f243aa0")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP19"
			(at 13.054 13.97 45)
			(layer "F.SilkS")
			(uuid "45874ddf-7954-488d-8184-a7a1281a821c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP20"
			(at 13.054 11.43 45)
			(layer "F.SilkS")
			(uuid "4842da94-4fad-4240-8841-0bd62b2fc981")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP22"
			(at 13.054 3.81 45)
			(layer "F.SilkS")
			(uuid "4927c515-49a1-4577-8582-1f1b8c4b4e76")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at -12.8 6.35 45)
			(layer "F.SilkS")
			(uuid "4dfdfd85-e6bb-4414-9004-4ca202c0f30f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "3V3"
			(at 12.9 -13.9 45)
			(layer "F.SilkS")
			(uuid "5a552838-29b3-4449-b5ca-12c08aad9f74")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at -12.8 19.05 45)
			(layer "F.SilkS")
			(uuid "5d1a1a90-5ad4-41c8-84f1-aa353663976b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP5"
			(at -12.8 -8.89 45)
			(layer "F.SilkS")
			(uuid "646ee7ea-bbdb-4322-846e-0175ed480d0c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP26"
			(at 13.054 -1.27 45)
			(layer "F.SilkS")
			(uuid "6928af39-f22a-4d1b-9f87-04f2e1102022")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP16"
			(at 13.054 24.13 45)
			(layer "F.SilkS")
			(uuid "72a38c9e-b694-4b80-a608-bdac8e4f66d2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at -12.8 -6.35 45)
			(layer "F.SilkS")
			(uuid "766226ca-5ebb-4f74-b72b-4522902ee074")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "3V3_EN"
			(at 13.7 -17.2 45)
			(layer "F.SilkS")
			(uuid "78f726e4-9626-46fe-9faa-4ab4a8ac7c60")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP27"
			(at 13.054 -3.8 45)
			(layer "F.SilkS")
			(uuid "8a738d9a-900d-42c0-8aec-98521e519cd2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP11"
			(at -13.2 11.43 45)
			(layer "F.SilkS")
			(uuid "8e405ec3-fb7f-4849-83c0-29c7abc40dbf")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP15"
			(at -13.054 24.13 45)
			(layer "F.SilkS")
			(uuid "8ee7bbbc-7e8a-4be7-8c27-16c590f26b93")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP7"
			(at -12.7 -1.3 45)
			(layer "F.SilkS")
			(uuid "ac7ef2be-368f-4d39-9e77-3dbffa0a6e2f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP17"
			(at 13.054 21.59 45)
			(layer "F.SilkS")
			(uuid "ae02c90c-4ca1-4181-9c74-1a2782ddde07")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP13"
			(at -13.054 16.51 45)
			(layer "F.SilkS")
			(uuid "b165cba2-67c0-4f21-889c-99c051824803")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "SWCLK"
			(at -5.7 26.2 0)
			(layer "F.SilkS")
			(uuid "b5c5085f-04a7-4544-9d43-f34802622249")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "VSYS"
			(at 13.2 -21.59 45)
			(layer "F.SilkS")
			(uuid "b9910c3c-6b4c-4fa8-8a48-16174f609ec7")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP8"
			(at -12.8 1.27 45)
			(layer "F.SilkS")
			(uuid "bd4756b0-a647-4542-892f-7c5a6810e087")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP18"
			(at 13.054 16.51 45)
			(layer "F.SilkS")
			(uuid "c21ba841-f846-4322-a2f8-bddef2642cd2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP14"
			(at -13.1 21.59 45)
			(layer "F.SilkS")
			(uuid "c718ed4d-20df-4eba-ae88-0afa8fb505bd")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at 12.8 6.35 45)
			(layer "F.SilkS")
			(uuid "c88fed34-1e48-4563-8105-1e7dcb372c3b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP2"
			(at -12.9 -16.51 45)
			(layer "F.SilkS")
			(uuid "cd4510da-fe50-40de-973a-951fdcaaaaa7")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at -12.8 -19.05 45)
			(layer "F.SilkS")
			(uuid "d795c156-bccc-4a40-a23e-23ac83fbec72")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GND"
			(at 12.8 19.05 45)
			(layer "F.SilkS")
			(uuid "da38aae6-f5c4-40aa-8d28-9d6a2302086c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP12"
			(at -13.2 13.97 45)
			(layer "F.SilkS")
			(uuid "dcabf6fa-98bf-4c02-95f7-577001db048a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "AGND"
			(at 13.054 -6.35 45)
			(layer "F.SilkS")
			(uuid "dcf7c2d1-577d-4ca4-a7e0-ac420f0b4de7")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "RUN"
			(at 13 1.27 45)
			(layer "F.SilkS")
			(uuid "de7c114f-4e05-4538-9649-0bff1cda92cc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP0"
			(at -12.8 -24.13 45)
			(layer "F.SilkS")
			(uuid "dedb1430-473a-4464-80de-0a414e77634f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP21"
			(at 13.054 8.9 45)
			(layer "F.SilkS")
			(uuid "ecf08aee-2f3e-4cfc-8805-b9c4d48ca2a6")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP6"
			(at -12.8 -3.81 45)
			(layer "F.SilkS")
			(uuid "f4cd4490-6841-4a92-8b41-77a6f7461e7a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "GP9"
			(at -12.8 3.81 45)
			(layer "F.SilkS")
			(uuid "f5ecc7e0-a450-4404-b45c-6af70b330fc9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "VBUS"
			(at 13.3 -24.2 45)
			(layer "F.SilkS")
			(uuid "ffec9606-e8d9-4484-909f-2382a9c22d1d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "Copper Keepouts shown on Dwgs layer"
			(at 0.1 -30.2 0)
			(layer "Cmts.User")
			(uuid "5fd73fa7-6ab7-4bc1-9190-f01baa2ba107")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "f08b41e9-8a2e-4c37-a168-2b50428dbd18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole oval
			(at -2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(uuid "7de35bf9-5fee-442c-b632-84e5d7517bbe")
		)
		(pad "" np_thru_hole oval
			(at -2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(uuid "0e0f6efe-3d02-4dc8-aff0-0428c681442a")
		)
		(pad "" np_thru_hole oval
			(at 2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(uuid "d81c7457-da04-4b56-bbe3-fe3465b3f01a")
		)
		(pad "" np_thru_hole oval
			(at 2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(uuid "9c7b6dd6-fdfc-4bea-a272-7c43f38317a0")
		)
		(pad "1" thru_hole oval
			(at -8.89 -24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "unconnected-(U1-GPIO0-Pad1)_0")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
			(uuid "282241b7-91c4-41b7-8c74-504f7f4c30d9")
		)
		(pad "1" smd rect
			(at -8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 108 "unconnected-(U1-GPIO0-Pad1)")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
			(uuid "1ba7c4db-b528-49a8-bca8-08868191ced2")
		)
		(pad "2" thru_hole oval
			(at -8.89 -21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "unconnected-(U1-GPIO1-Pad2)")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
			(uuid "7f8f6c82-b0cf-4894-bd28-a9f71061a22b")
		)
		(pad "2" smd rect
			(at -8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 143 "unconnected-(U1-GPIO1-Pad2)_0")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
			(uuid "ff78eb70-45bb-4085-95a8-058d2f4cf296")
		)
		(pad "3" thru_hole rect
			(at -8.89 -19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "5f794717-e497-43ac-97e8-853d004c47d6")
		)
		(pad "3" smd rect
			(at -8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "1152faea-cc46-4a9c-b9b1-630a3fb990cf")
		)
		(pad "4" thru_hole oval
			(at -8.89 -16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "/PISO_SH")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
			(uuid "57c040f4-424d-4cda-aa39-40a5cea323ce")
		)
		(pad "4" smd rect
			(at -8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 122 "/PISO_SH")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
			(uuid "d316119f-337e-49e8-af1d-02383e430db9")
		)
		(pad "5" thru_hole oval
			(at -8.89 -13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/PISO_CLK")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
			(uuid "ab2420c3-8773-49f4-9ea9-83827a0e6726")
		)
		(pad "5" smd rect
			(at -8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 99 "/PISO_CLK")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
			(uuid "edf49ffa-5d35-4ebc-ad35-3c5f13259ae2")
		)
		(pad "6" thru_hole oval
			(at -8.89 -11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "/PISO_INH")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
			(uuid "c045b6a8-e08b-473f-ae84-7a1526725c90")
		)
		(pad "6" smd rect
			(at -8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 128 "/PISO_INH")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
			(uuid "7edb4a2d-f517-496a-9621-7d3b07889fb9")
		)
		(pad "7" thru_hole oval
			(at -8.89 -8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "/~{PISO_CLR}")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
			(uuid "c0ce29c4-7c09-489c-85a7-dfc90dbd5cb2")
		)
		(pad "7" smd rect
			(at -8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 125 "/~{PISO_CLR}")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
			(uuid "69604088-36c3-4814-bbc3-195b842c1845")
		)
		(pad "8" thru_hole rect
			(at -8.89 -6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c108a89f-e097-4f96-9052-91e238517936")
		)
		(pad "8" smd rect
			(at -8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c56d68eb-382d-46e3-b3ae-96748c34c8db")
		)
		(pad "9" thru_hole oval
			(at -8.89 -3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "unconnected-(U1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
			(uuid "a8b262e3-d890-4c49-b2e6-1933544cb814")
		)
		(pad "9" smd rect
			(at -8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 115 "unconnected-(U1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
			(uuid "334febbd-5eff-411b-9503-5939b6bf10da")
		)
		(pad "10" thru_hole oval
			(at -8.89 -1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "unconnected-(U1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional+no_connect")
			(uuid "3f1fa375-1afa-40aa-b196-fc4aad4492d2")
		)
		(pad "10" smd rect
			(at -8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 133 "unconnected-(U1-GPIO7-Pad10)_0")
			(pinfunction "GPIO7")
			(pintype "bidirectional+no_connect")
			(uuid "9c00cc52-119b-4116-a1b2-ad1acdb753b5")
		)
		(pad "11" thru_hole oval
			(at -8.89 1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(U1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional+no_connect")
			(uuid "06f18b7c-bd36-40a8-8a7e-0798cc87dae5")
		)
		(pad "11" smd rect
			(at -8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 121 "unconnected-(U1-GPIO8-Pad11)_0")
			(pinfunction "GPIO8")
			(pintype "bidirectional+no_connect")
			(uuid "54b3c5c7-00f1-4822-88c1-aed0f19c1787")
		)
		(pad "12" thru_hole oval
			(at -8.89 3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "unconnected-(U1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
			(uuid "7d6f65b9-5d2b-4737-a197-f5054155f527")
		)
		(pad "12" smd rect
			(at -8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 130 "unconnected-(U1-GPIO9-Pad12)_0")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
			(uuid "8feff5e9-5545-44ce-86a3-ef489fa43249")
		)
		(pad "13" thru_hole rect
			(at -8.89 6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c9fd7b57-706d-4d73-af91-c9e06171d9f1")
		)
		(pad "13" smd rect
			(at -8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "122933bb-4017-4202-b2b0-1828bed8c036")
		)
		(pad "14" thru_hole oval
			(at -8.89 8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "unconnected-(U1-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
			(uuid "307f645a-1ecb-41c3-a444-048d61abd6e4")
		)
		(pad "14" smd rect
			(at -8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 139 "unconnected-(U1-GPIO10-Pad14)_0")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
			(uuid "dadbe00c-6adc-409b-90b2-c945bd8d46bb")
		)
		(pad "15" thru_hole oval
			(at -8.89 11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "unconnected-(U1-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional+no_connect")
			(uuid "185299f9-3c7f-4d13-8ad9-3c2bda2ca753")
		)
		(pad "15" smd rect
			(at -8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 124 "unconnected-(U1-GPIO11-Pad15)_0")
			(pinfunction "GPIO11")
			(pintype "bidirectional+no_connect")
			(uuid "611a58ca-a3bd-4fac-9d73-64e045fc4124")
		)
		(pad "16" thru_hole oval
			(at -8.89 13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "unconnected-(U1-GPIO12-Pad16)")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
			(uuid "d2b6426c-81bf-4a2b-830c-3d8cf9b8e84b")
		)
		(pad "16" smd rect
			(at -8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 142 "unconnected-(U1-GPIO12-Pad16)_0")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
			(uuid "fc9a21f5-a6b3-4d0a-861b-655d731f9f6b")
		)
		(pad "17" thru_hole oval
			(at -8.89 16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "unconnected-(U1-GPIO13-Pad17)_0")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
			(uuid "9d1bebab-7b4e-49a0-932e-f4ccfbf10c30")
		)
		(pad "17" smd rect
			(at -8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 114 "unconnected-(U1-GPIO13-Pad17)")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
			(uuid "3101bd98-4e89-42ca-adef-a13ffb651218")
		)
		(pad "18" thru_hole rect
			(at -8.89 19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "eddafb9e-80e9-496d-8fd1-77555df41a9e")
		)
		(pad "18" smd rect
			(at -8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "5d5cd7c9-7e99-4854-8a76-4e62a7de5b32")
		)
		(pad "19" thru_hole oval
			(at -8.89 21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "unconnected-(U1-GPIO14-Pad19)_0")
			(pinfunction "GPIO14")
			(pintype "bidirectional+no_connect")
			(uuid "5a4ceea0-afdc-4297-8c64-bbefe64d94a3")
		)
		(pad "19" smd rect
			(at -8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 109 "unconnected-(U1-GPIO14-Pad19)")
			(pinfunction "GPIO14")
			(pintype "bidirectional+no_connect")
			(uuid "1ced3156-95c9-439b-a1df-3cfd41c9dae5")
		)
		(pad "20" thru_hole oval
			(at -8.89 24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "unconnected-(U1-GPIO15-Pad20)_0")
			(pinfunction "GPIO15")
			(pintype "bidirectional+no_connect")
			(uuid "20aff0d1-5f47-4cb3-857f-cd7e7608b463")
		)
		(pad "20" smd rect
			(at -8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 105 "unconnected-(U1-GPIO15-Pad20)")
			(pinfunction "GPIO15")
			(pintype "bidirectional+no_connect")
			(uuid "0ddcde51-4da5-495f-a441-0c56484d5c20")
		)
		(pad "21" thru_hole oval
			(at 8.89 24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "unconnected-(U1-GPIO16-Pad21)_0")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
			(uuid "ea538893-36d1-40f6-a391-e3b8e17fa182")
		)
		(pad "21" smd rect
			(at 8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 137 "unconnected-(U1-GPIO16-Pad21)")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
			(uuid "d2a8a41b-ffbc-4d16-acf6-63ebf2f35fbc")
		)
		(pad "22" thru_hole oval
			(at 8.89 21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/SIPO_RCLK")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
			(uuid "3fc40bc5-3337-4695-a400-a5b57e408139")
		)
		(pad "22" smd rect
			(at 8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 112 "/SIPO_RCLK")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
			(uuid "290e5b65-4e7d-4cbe-a0d2-761990d683d2")
		)
		(pad "23" thru_hole rect
			(at 8.89 19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "850006e4-919c-4fc0-8de9-2ed305c48748")
		)
		(pad "23" smd rect
			(at 8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c8982bdf-c09c-4cb4-946e-3ea889749c74")
		)
		(pad "24" thru_hole oval
			(at 8.89 16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
			(uuid "393411f9-4056-488d-9d80-d5dca037f0df")
		)
		(pad "24" smd rect
			(at 8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
			(uuid "41e1a2f9-b9ae-4c17-9863-76328fb9afca")
		)
		(pad "25" thru_hole oval
			(at 8.89 13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/SIPO_CLK")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
			(uuid "404e9586-abde-4549-bde2-52c3efe573d7")
		)
		(pad "25" smd rect
			(at 8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 98 "/SIPO_CLK")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
			(uuid "7e5e5921-1110-489e-884d-50aad48badaf")
		)
		(pad "26" thru_hole oval
			(at 8.89 11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "/SIPO_SER")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(uuid "1720af1a-91a2-4f5f-913a-149462fe9e37")
		)
		(pad "26" smd rect
			(at 8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 106 "/SIPO_SER")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(uuid "37991d73-12a2-49fb-b1e6-8049a4368681")
		)
		(pad "27" thru_hole oval
			(at 8.89 8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/~{SIPO_OE}")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(uuid "c88ff04d-72d3-49a4-9795-731b0ab44b93")
		)
		(pad "27" smd rect
			(at 8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 103 "/~{SIPO_OE}")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(uuid "0896c98f-f227-4600-bcaa-c6950544e564")
		)
		(pad "28" thru_hole rect
			(at 8.89 6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "747af99e-139f-4b13-83d4-b6e075355818")
		)
		(pad "28" smd rect
			(at 8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "185279d0-6e35-4c3e-8bb1-74c31b15b855")
		)
		(pad "29" thru_hole oval
			(at 8.89 3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "unconnected-(U1-GPIO22-Pad29)_0")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
			(uuid "c488235c-18f9-46d7-90c3-b4070617d9b9")
		)
		(pad "29" smd rect
			(at 8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 126 "unconnected-(U1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
			(uuid "70c51cb7-a5c4-40d5-a08f-ba525028a95d")
		)
		(pad "30" thru_hole oval
			(at 8.89 1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "Net-(U1-RUN)")
			(pinfunction "RUN")
			(pintype "input")
			(uuid "884aee99-5ef6-4b4e-bbc7-019c6c3c423d")
		)
		(pad "30" smd rect
			(at 8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 100 "Net-(U1-RUN)")
			(pinfunction "RUN")
			(pintype "input")
			(uuid "6df21474-8c10-4290-a685-d4b4c65df118")
		)
		(pad "31" thru_hole oval
			(at 8.89 -1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "unconnected-(U1-GPIO26_ADC0-Pad31)_0")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
			(uuid "508ef401-699e-400b-bb3b-d26f1bb07fcc")
		)
		(pad "31" smd rect
			(at 8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 118 "unconnected-(U1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
			(uuid "42d0e72d-a442-4b3c-8a94-288957891916")
		)
		(pad "32" thru_hole oval
			(at 8.89 -3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "/PISO_SER_3V3")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
			(uuid "c76812b5-cd99-48f3-9ae3-4750af2b5124")
		)
		(pad "32" smd rect
			(at 8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 132 "/PISO_SER_3V3")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
			(uuid "94ca616f-0ae3-43e2-b60c-2578f9c52c02")
		)
		(pad "33" thru_hole rect
			(at 8.89 -6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
			(uuid "0b737d71-65ed-44ee-8f4c-a396cc7e11d3")
		)
		(pad "33" smd rect
			(at 8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
			(uuid "4f3647b8-2e4f-4faa-b08a-4522f206e951")
		)
		(pad "34" thru_hole oval
			(at 8.89 -8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "/~{RELAY_ENABLE}")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
			(uuid "9263f131-cc1e-4f79-ac51-0778718bce05")
		)
		(pad "34" smd rect
			(at 8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 131 "/~{RELAY_ENABLE}")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
			(uuid "dd0d249b-d709-404c-b194-7be250169acd")
		)
		(pad "35" thru_hole oval
			(at 8.89 -11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(U1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "unspecified")
			(uuid "63aa3fae-6489-42cb-b4e3-e8dea2a98601")
		)
		(pad "35" smd rect
			(at 8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 104 "unconnected-(U1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "unspecified")
			(uuid "0b43539d-454a-4967-a445-dcd2a34b43da")
		)
		(pad "36" thru_hole oval
			(at 8.89 -13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+3V3")
			(pinfunction "3V3")
			(pintype "unspecified")
			(uuid "1520f40b-269a-446e-b09d-dbf8cc206671")
		)
		(pad "36" smd rect
			(at 8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 4 "+3V3")
			(pinfunction "3V3")
			(pintype "unspecified")
			(uuid "74fb726a-c32c-4e5d-b81b-a3b96e936563")
		)
		(pad "37" thru_hole oval
			(at 8.89 -16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(U1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
			(uuid "069e4cc9-730f-4788-8101-155615782aa5")
		)
		(pad "37" smd rect
			(at 8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 140 "unconnected-(U1-3V3_EN-Pad37)_0")
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
			(uuid "e6ec5763-5d25-45bb-901e-1652c699cd10")
		)
		(pad "38" thru_hole rect
			(at 8.89 -19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(uuid "fae870f1-3f7e-4de8-bf14-d7bd53d361e5")
		)
		(pad "38" smd rect
			(at 8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(uuid "99695fae-43b7-46fd-87f2-e1dc0a4f70c6")
		)
		(pad "39" thru_hole oval
			(at 8.89 -21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "unconnected-(U1-VSYS-Pad39)_0")
			(pinfunction "VSYS")
			(pintype "unspecified+no_connect")
			(uuid "bfc884c0-605c-414c-b4ed-f464bfa13a88")
		)
		(pad "39" smd rect
			(at 8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 119 "unconnected-(U1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "unspecified+no_connect")
			(uuid "4a0c904a-dd67-446e-9f32-4a6b929e42da")
		)
		(pad "40" thru_hole oval
			(at 8.89 -24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(U1-VBUS)")
			(pinfunction "VBUS")
			(pintype "unspecified")
			(uuid "9f9f7cde-2199-4a01-b6eb-0006510f3aa0")
		)
		(pad "40" smd rect
			(at 8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 9 "Net-(U1-VBUS)")
			(pinfunction "VBUS")
			(pintype "unspecified")
			(uuid "b761bb10-3627-41ab-b564-c5e02c658712")
		)
		(pad "41" thru_hole oval
			(at -2.54 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J2-Pin_1)")
			(pinfunction "SWCLK")
			(pintype "input")
			(uuid "9c6cec71-03f9-4ea0-8d4b-78141d1f94a7")
		)
		(pad "41" smd rect
			(at -2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 51 "Net-(J2-Pin_1)")
			(pinfunction "SWCLK")
			(pintype "input")
			(uuid "d1eee568-6706-409a-ac76-d78d7a0a8d6a")
		)
		(pad "42" thru_hole rect
			(at 0 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b4553d56-8769-40ac-8d74-b38c3be7032b")
		)
		(pad "42" smd rect
			(at 0 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c6745353-d1f8-47e1-bcc9-43a6603c34cc")
		)
		(pad "43" thru_hole oval
			(at 2.54 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J2-Pin_3)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(uuid "32ab0470-fda6-414a-bbb0-79f6b67b0608")
		)
		(pad "43" smd rect
			(at 2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 50 "Net-(J2-Pin_3)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(uuid "e2da107e-5171-479d-8649-aa03da7b0faa")
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "b9175edd-f159-4ef9-9481-0b1fd93c4faf")
		(at 139.093 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R28"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "65e502c9-6493-490a-8df5-4399d2960d35")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "1a4eca67-1391-4b83-8283-b1be85e45ae5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a76e660c-ac9d-49fb-a4b1-256c27113a1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bacc22f5-b518-4bf7-b770-8d7e21e06a8e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "028e180d-79c0-4de3-9ce9-9bfc6770a3c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/76cb1642-f0cb-4fb4-a2cd-482e919b359b")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86113704-9b99-4a8c-bb66-c40b16d100d7")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3bfdefd-2069-48cb-8c35-1f2fca231f1d")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd790223-b3fc-4404-a85a-7c89450e8788")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fedd5f08-4b51-4676-a2c2-943208992be5")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4860cfa1-b217-45fa-a056-bf64fd85df1f")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "586c0edd-aaa7-4a98-8296-0394e53d2897")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "164ec467-56a9-449e-b58f-7c00158d8dd1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f426cc5-4647-4d1f-a5ad-d5fc59b9c3c8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac55ad26-c20c-4b90-aa1f-1a7c4bca98f7")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d714136-5c6f-43a4-aa71-5830ef8089c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "99e6ddc6-2b1f-455d-94a8-ce4775ae7c59")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 84 "Net-(U5-QC)")
			(pintype "passive")
			(uuid "0f9f9fe7-b8bd-4219-8742-98fbb006879a")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 46 "/ZIF_28")
			(pintype "passive")
			(uuid "eda1679b-b890-4800-bb48-54041f6441f9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "be584fff-8c87-4a4e-80ef-67058d997733")
		(at 103.143 115.22)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "0586b29f-e85b-47f0-8e7e-2fccbe3fbfda")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "b498c8fc-022a-44c8-a5be-9ffdafc4d23d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7cfe9f35-81d3-4abf-a1d8-1038d1854fcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e2f62ed-c785-4553-832a-5cbb979d8391")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e781380b-8618-4402-9d0a-927ef623f632")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/10d4fa70-1daf-4282-8e21-e4c4874307e4")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91712982-35b2-4321-933e-2b46aaea154f")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c07ea215-fb4d-430a-bca9-504df8f27d0f")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eee5a0e9-414e-43dc-b103-4939c36958f7")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e3d9586-5836-41d4-9117-df09f60f0e82")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7368d706-bf5c-42c6-8d15-bf4222519c8a")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc0729cf-d765-4eb8-bca2-b7d38d193bab")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e568b5a-6176-4e5f-b544-58bb21feb338")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e23abccf-16f6-4d61-b8f7-9e1ae4e11022")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6298ccb4-aef6-406e-9ba5-cd3b69ee10a1")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6a615b4-fa4c-4cf5-87e5-9c78f5ab1eed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1702e717-d4fc-46b6-ab20-a2102e127c5e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "16efd7ae-1881-4660-b046-ba88adf80e92")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0cacea93-b728-4d4f-aab2-c182b06979d3")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "be724eae-899e-4bb2-b52d-19df7d2a6c67")
		(at 133.143 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R18"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "0a4f3bd3-5fb0-4732-86ea-db9448f97efa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "f75a68c3-6039-4743-a819-7f9e2bd44b07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c8e9e3e-fce9-48de-8b6a-69be27826254")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f7fb45b-d50f-4922-be50-e0bd43359ea8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3ee2385-5ec2-485f-8931-3ca7b1c5a8ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0d70cfec-a500-4653-bb9a-3db92669b9c4")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6985a0d-26ab-4b8e-9177-b4cd7ffeae3f")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56fd9382-7a55-4bb7-8902-07a503fab95f")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1677b088-b8b3-4d3b-bb3d-f0bb114dc9d2")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9dcedc8-8647-4813-8efe-39d92f66a233")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bf1a162-13a6-40d4-9cb6-9934b14221e9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7e554d9-07cd-4690-b5e5-47b2b7a6c830")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c07b42ab-08df-4b71-bdeb-1cf59ae20624")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0301b251-6aca-49e3-8731-0d9cbf1185a3")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b80880a-e0e5-49fe-b36f-89c610c678fb")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1adf15e-f5c9-4203-9321-65622aecf1be")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e5c598eb-c937-4b20-9aef-ecc5b091d73f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 74 "Net-(U4-QA)")
			(pintype "passive")
			(uuid "68daa41d-6e2e-4049-a406-922096352e02")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 19 "/ZIF_17")
			(pintype "passive")
			(uuid "29455365-8aef-43a1-a454-27e34d8df820")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "bfcf17b6-2b06-429b-8afe-0f1ef232624d")
		(at 133.143 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "a543b251-c2d3-48b2-abe5-f78532b28127")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "b7fbf7d2-213a-4f12-bf97-850965ab9375")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ccd230ab-6424-441d-b388-f68f49478247")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2626f658-451d-4583-b80d-f705768a59e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf0166f3-95d3-41e6-9494-e1c27b19cd68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/af1e2b62-71c5-4242-a564-295817f5ba83")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "094c9699-3b37-4875-9151-40fdb7ebf463")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "653fc407-40f5-45dd-b357-5f7cf21a6397")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "672d3be2-a16f-4c7c-9021-b7552fedda83")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85459aeb-dfa8-4826-9b3b-de9bdb856028")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "542a0d45-4f95-4475-a7a8-e06a871858e4")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2914d25-391e-4e2b-8cce-95a680f1fc19")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6718925f-440a-4460-bf57-1eda59a6a4b8")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8841c1b3-3a1f-4b63-9dc6-9a7f9c25c887")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9387349a-1c3b-4153-8f3e-3521238ac6ec")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ccaef5c-47a4-4797-b72e-95b574fd2a12")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1a73ce05-2421-485c-a832-f752835ca3d4")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 67 "Net-(U3-QB)")
			(pintype "passive")
			(uuid "0eaf216a-982f-4d0a-89a9-59fd9cdcf6f9")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 39 "/ZIF_10")
			(pintype "passive")
			(uuid "f4b51634-5a11-4578-91a1-b1e4f923fc7b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "c140b6b1-9808-4212-b137-652a8a3a29ec")
		(at 133.143 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "b738a901-9d7e-47cb-bbb0-f10f559c4399")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "dc634669-3804-4251-b4bb-170424c3738c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f5b1a9e-2017-4b93-b637-f1f35724dca5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ae7e079-5d27-4646-b9fe-3ece92f73ca1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "895cad0e-d0b6-4a06-876c-cba02a5e5717")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b0ea3ff4-2157-4d63-b5b5-e500efe69baa")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab0055b5-a2ab-4bc4-af89-9ca479baf97c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f1b988c-e8f4-4c59-9802-87e4e51f9a87")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3343f25-84cf-433d-a3a7-d56891424d09")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7dc952e6-8e31-4ffc-9975-920639f8911f")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47b83d13-3bae-41e9-8082-9d5b4e335bc1")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7add16c4-3312-468a-b719-9e46ae8a2ab1")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "973d8aa2-fe1e-4af5-9665-61337768de36")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f079475-752b-4b14-8b04-40386852a657")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ccf41a5-0093-4945-b3ee-ca8d81beeee5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "081b5cc4-899d-4a9a-90ef-ea6484dfa7bf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d7bfcc25-629c-43d3-ac7e-7fa6de16627d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 72 "Net-(U3-QG)")
			(pintype "passive")
			(uuid "7e21283d-f018-4c49-8577-cb993142fa0e")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 15 "/ZIF_15")
			(pintype "passive")
			(uuid "be64d841-bd01-4cbb-99ec-a6f069fdca54")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "c3b91920-4a85-437f-a31e-01216d2095a0")
		(at 139.093 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R30"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "905fbc6b-c6fe-4639-9cf0-7693f40a7411")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "99740b0f-5061-4d81-9d90-ef98d49253e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "794476b3-1e7e-4352-af2b-fe8f82c99d17")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a284c233-5a2d-415a-aed4-eea23eb3ffc7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c759ce10-aebb-4bc1-8e7b-9239f2a60a50")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/cbfbfc79-796a-4909-86c8-5ba8e5986c08")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8be2e84-8477-447a-962c-64fb2495040f")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4541477-09f0-4dcb-a4c9-081a3b7cbe28")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "729f829a-6950-40a3-bef3-64392aba226c")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb7ba460-c512-417d-85b2-54da1b666caa")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0452141c-a3ab-4990-8c52-8dd1eeabdc89")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb4c1b56-0b4b-4b54-9b74-99fb05aafe1f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63bd45df-871b-4330-a4aa-954136bbbba8")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df7ff568-ccdf-42d2-861b-531dda919814")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "976c7599-4525-4880-831b-ab0cede352d6")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2b15a44-4fce-4eff-bb46-ce0a91aa3ace")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bc120435-2a9f-4d88-a89e-3d6e778ed004")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 86 "Net-(U5-QE)")
			(pintype "passive")
			(uuid "4c513ade-baa0-482a-8851-bfa36caf99d1")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 36 "/ZIF_30")
			(pintype "passive")
			(uuid "966a9892-64b8-4ff2-b989-85d06af99a20")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "c61960fe-548c-444f-ae7c-41b24ce80a83")
		(at 156.943 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R58"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "93d5caa6-8a8f-4652-9df0-5bbc1ca0b798")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "9705ea11-f679-41cd-9159-56f5b69c0282")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "711b09f2-9b4e-48bc-a6e3-739d7483628d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68120396-749e-4cd3-b999-177c26212fdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a130e3b-2454-44bc-be21-8ef8765fdb44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c2a44adc-4788-4834-ba2b-7dd55f0ab3e2")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1889fc5f-c9e3-490c-bcf5-070ffd8be514")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d9e31e3-9af6-4356-a47d-9f447d40a164")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbe366be-eaa6-47e7-bbdd-283d3789b9f0")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e67e9919-81b3-4e1d-b4fb-9ec87e3cee04")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ebd5e45-5602-492b-bb7f-2f8ec1f6bd0c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "599fb531-8753-4d25-b7de-238d83555a27")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54ad4b07-837b-4ff0-aafd-a63122076918")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9836ae7c-7b71-4b75-9b37-10eeb5608e38")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "391d425d-c602-447b-be11-2b3a88c232b3")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "913fde11-8318-4ea6-ad8e-983abcd5554b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "89d7c0b1-1284-488b-a09b-87d1466ec8a1")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 35 "/ZIF_13")
			(pintype "passive")
			(uuid "048a33ff-cb56-4d4b-9ce3-b6b5f2569f45")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5fd4839a-064a-4db4-a178-ab89a92d8539")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "c6a6df7e-1e1f-4007-9c94-6bdd425089b6")
		(at 168.843 57.93)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R82"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "0a2b2fb5-667c-4dca-a16e-6173dcdd5fd0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "f2d51ef4-0b01-43e9-8357-3d9280a5b9b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e2a9c23-cdf6-47b1-9473-29c4713c05c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e53fa619-01dc-484b-8c27-356c57b9781a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e750cf61-6155-430c-b8b5-9fa16d04754f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b07e065c-a326-49bc-8b31-42a76c8e4731")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f31a425-d08e-4360-976e-58f0c9f5c082")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70920674-3778-4c14-bed8-bae95453799f")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d3928f5-4b63-4585-a80f-b9f10c95d52f")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cda90a85-7e6f-405f-bf0b-4369c04e282f")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c1dd48a-225c-4f71-9832-e31a0a74e213")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4bbffc7-fd50-4aea-9e95-f8be3af8e4cf")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8b30cf3-642d-4e09-b05b-4f077ac588a2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4f1d136-b802-4565-aa1d-d206b6150d01")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d388c31a-b832-4422-b8bb-6e9b2f1702a8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd656abb-7043-4feb-8786-bea9c6e81862")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d05acc03-35bf-4c18-8346-c423d537b65a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 40 "/ZIF_38")
			(pintype "passive")
			(uuid "7efaf5c2-1be0-49b5-832d-9d60410975ef")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a027e337-9a53-45d2-a960-8cebe30980bf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "cab924b3-2538-4996-965d-58ec1ec40561")
		(at 162.893 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R76"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "3200bdab-fd2c-493a-bc8b-982173fc8b76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "b57708f2-9fa1-4e07-95ec-8eb5e162a458")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a210733-03e8-4e77-b2c0-30ec0b3ab699")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6dcbd495-7e3f-4047-8bc2-0af97444538e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa861038-194e-4105-a5ac-45c81db93b60")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f8a2bbb1-05ce-454b-a10a-d6db016adf76")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6cc919d0-762f-4229-806f-3fa9df199220")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a5f9eca-0409-4fff-a8a6-5123fa64292a")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5719b24b-c866-4cf6-8993-f3b2547126e2")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc52c410-f737-4251-8ba8-9ec84231d6a5")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fed401f-0290-4574-92cc-eae4f424de27")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9891b02b-cb16-4d46-b393-a9ff200416e3")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f0e1896-0ba0-4a6b-b3ff-6d170cd9e577")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f14a67b2-25d8-4466-9241-4c72fcc47aff")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a569a4a-fabe-438e-903e-a4a47caedb90")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "502a98e0-8234-4399-8f43-da138189e66c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "453bc382-b4a3-498a-93a4-403a95ffe8b9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 30 "/ZIF_32")
			(pintype "passive")
			(uuid "b221ff7f-a9df-4ef8-b7a2-abe6d72574c7")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d591914a-e987-4167-927f-0b2074d4e115")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "cc3a5d27-98df-432c-ad62-10e3d376d461")
		(at 162.243 81.92)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -5.9 0)
			(layer "F.SilkS")
			(uuid "d6466af3-9b6b-42dc-88c8-f9b451dc1da7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "74HCT595"
			(at 0 5.9 0)
			(layer "F.Fab")
			(uuid "e5fe32bf-6780-412e-aa22-e280cc01cf72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c463a5d-86c9-4df4-a7b3-566f7fa4eb11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74hc595.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7e485e68-0b92-4945-b35f-c338652a55e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d64ef7fb-a4df-44ea-a1c0-4d0b629a71ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(path "/36353b81-b69c-480f-beed-9408cf5843da")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -5.06)
			(end -1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7588da9-5e0b-4fee-8f7e-58a11ff99eec")
		)
		(fp_line
			(start 0 -5.06)
			(end 1.95 -5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7892ce76-53fd-46c4-9d7e-2fc46c7b10e1")
		)
		(fp_line
			(start 0 5.06)
			(end -1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21c836c7-fb5b-4fb2-a07d-2565860a2a6d")
		)
		(fp_line
			(start 0 5.06)
			(end 1.95 5.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0b7f28b-ae96-4893-b0aa-e1a2ac490331")
		)
		(fp_poly
			(pts
				(xy -2.7 -5.005) (xy -2.94 -5.335) (xy -2.46 -5.335) (xy -2.7 -5.005)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "5d86ba37-a80d-4c7c-bd32-c93901bf979f")
		)
		(fp_line
			(start -3.7 -5.2)
			(end -3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4271ddee-7509-4f3b-82a9-605878d688a1")
		)
		(fp_line
			(start -3.7 5.2)
			(end 3.7 5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f74b18c-c095-4f33-a6d2-aa3b200d2002")
		)
		(fp_line
			(start 3.7 -5.2)
			(end -3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fae50a2-3d13-440a-a830-fb858483a1db")
		)
		(fp_line
			(start 3.7 5.2)
			(end 3.7 -5.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ad2136c-6fc9-480d-8936-5dcf02bcdafa")
		)
		(fp_line
			(start -1.95 -3.975)
			(end -0.975 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "630680e8-8854-442b-8817-4ad9fc1f10b7")
		)
		(fp_line
			(start -1.95 4.95)
			(end -1.95 -3.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f0f6ca2-0429-4025-8d32-ca4c0642797b")
		)
		(fp_line
			(start -0.975 -4.95)
			(end 1.95 -4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62d60b5e-89b2-40c3-87ff-63f1087d42e1")
		)
		(fp_line
			(start 1.95 -4.95)
			(end 1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e4a5566-54ba-4345-9783-5cd57e92ac20")
		)
		(fp_line
			(start 1.95 4.95)
			(end -1.95 4.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b82f2b40-5088-4386-98c8-23567f4de04d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f4aff816-b10a-4168-8a24-9f73afe3ea1c")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "Net-(U6-QB)")
			(pinfunction "QB")
			(pintype "tri_state")
			(uuid "a7722347-e5a6-419b-affa-80b06096a1a6")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "Net-(U6-QC)")
			(pinfunction "QC")
			(pintype "tri_state")
			(uuid "8c71c627-dcab-422d-aa6e-ae8af57a884a")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "Net-(U6-QD)")
			(pinfunction "QD")
			(pintype "tri_state")
			(uuid "afaf9b12-d0db-4a88-8f64-6b832d024c42")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "Net-(U6-QE)")
			(pinfunction "QE")
			(pintype "tri_state")
			(uuid "bc0e4c52-bc34-4af4-af5d-4235aa905bc8")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 95 "Net-(U6-QF)")
			(pinfunction "QF")
			(pintype "tri_state")
			(uuid "030c6c9f-0415-45ad-92f4-f25bed6d97d3")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "Net-(U6-QG)")
			(pinfunction "QG")
			(pintype "tri_state")
			(uuid "42de3dca-f5a6-4ee0-bed6-519c025f5ab6")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "Net-(U6-QH)")
			(pinfunction "QH")
			(pintype "tri_state")
			(uuid "53c523c3-386b-459e-9d79-905fe4570f8f")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c3c82358-4b8e-4117-89f0-9e759171f826")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 149 "unconnected-(U6-QH'-Pad9)")
			(pinfunction "QH'")
			(pintype "output+no_connect")
			(uuid "12dd2267-2ad0-4b8d-9537-0d26f8969803")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/~{SIPO_CLR}")
			(pinfunction "~{SRCLR}")
			(pintype "input")
			(uuid "430000e5-85fe-403d-beea-b84187bdf7f8")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/SIPO_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
			(uuid "56c03fe9-3e85-4b29-84f6-a9e24a8fe883")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/SIPO_RCLK")
			(pinfunction "RCLK")
			(pintype "input")
			(uuid "0d104baf-c344-4325-b373-c7d2fb663561")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U2-~{OE})")
			(pinfunction "~{OE}")
			(pintype "input")
			(uuid "17c205e9-3ee6-44dd-869e-99518f24b7aa")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "Net-(U5-QH')")
			(pinfunction "SER")
			(pintype "input")
			(uuid "e7730072-7f41-4dab-a3ff-6a631fd4ceaf")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "Net-(U6-QA)")
			(pinfunction "QA")
			(pintype "tri_state")
			(uuid "cd004c34-7bbc-4dfb-8f1c-66c1403e1876")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "7c344baf-6e2b-4505-accf-5720fd3c9e9a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "cc452782-7f5e-41bb-8b68-a82b4471b05a")
		(at 145.043 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R39"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "f0b3e943-3a6c-446c-953e-e67622558a19")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "ca38b96c-2132-4ae1-a679-99f053647f2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8ffbe98-c635-4b48-afcf-288e7eec679c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a8f1229-dde4-4896-b799-cdcf38918ebb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66d47364-c272-46c5-bbf1-d98cf4052533")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/66dbc721-baf9-4dab-ad68-5f1f9ae2c892")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5dd88b9-2174-4c6e-aaad-e3805c857374")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2db33040-d36d-4c57-a2fd-389ffb9af10b")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b07c548-4a09-4f6a-9389-844e357425c7")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50824886-e9cf-487f-b03b-963f6426409e")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b1c7182f-9227-4f69-a714-107a4cebc996")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2bd2e5e-17b7-4caf-aa26-b149e56f1e9a")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d43fbe2f-d93b-47d8-ba64-59d0d2aabbdf")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d681f892-7452-4b5c-a0f8-9967765bb129")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c052b18-6bcb-46b4-94e1-618144d5602a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6d12983-a5a5-45c9-a1ac-a692fcf796de")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "afafe5b6-d5a0-43e8-aa98-597475cab42f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 95 "Net-(U6-QF)")
			(pintype "passive")
			(uuid "4edc30ef-c456-4526-bd75-bed01448e1fa")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 37 "/ZIF_39")
			(pintype "passive")
			(uuid "c96bc0b7-ca90-4620-8777-90b8bcce6760")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "cee98c05-6315-4888-9d1d-44e873ca226e")
		(at 162.893 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R69"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "20643226-08a8-4d50-a47b-2c9903166a7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "4b027072-76ad-4037-9676-7b125f0b10a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2d55b14-b6ba-42e3-8a44-eaa2d22caabb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f94699b0-d6ad-4737-975d-12c8ca570652")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f48e9f2-8e96-411b-9032-075c36569961")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/29035e43-7900-4bac-a714-823d861bd5b9")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3740a48e-07b2-4675-a731-b7cce0317212")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c477025e-99b3-4d1e-ae68-b2dc7e03a6d8")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "845ed22f-2751-4747-aaa3-bd9c53b6f038")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c8fa10a-435c-4648-a352-a10f28cdc930")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea330ca3-7805-4431-829a-7a04c14291ff")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "473ac0ab-b7ec-47cf-a95d-7ffe57bc9bd0")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27bba1d6-e923-4635-b3fa-25c603c14639")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81057409-0370-4189-8e48-c9eee15a9855")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d34aaabd-d5b3-4a40-9c76-1ed2656d8fb3")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "febcc186-7db4-4e2e-b284-ce7c926c441e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "32cd7a34-8b62-4144-af6b-fd267ae6e6a1")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 22 "/ZIF_25")
			(pintype "passive")
			(uuid "4238f557-fc89-4ed4-a13a-34f34b05ccf7")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f95febd9-c031-40f4-a745-0252d5e651ab")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "d0c7b3c8-0492-4e38-8c34-21d0589922e5")
		(at 150.993 74.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R54"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "10fe8842-cff0-4597-ab60-6ceec4c0cf1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "4c40ba86-fcd3-4fe2-964a-5a23d1a375d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d8a309f-bdb0-4e61-89ad-20fde7345047")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "20eaf178-dbec-4e5f-ab70-917b423bc1e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26de239c-9e6e-4477-a6b2-50414e0be315")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/38f0369e-30f7-464b-bf62-65ef33ebbc7f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9213661-672e-443e-a1bb-a5253e28ad3a")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9e9b7cc-ac53-4e41-8dda-1cd92c4171fb")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e83293a-8c82-44e7-84ab-dc867aeb0fbf")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a2e8ea0-1feb-4f71-8344-def90f4bf417")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3376f77-ce5a-4906-9783-87241ce9c6d9")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93b0f2d0-7693-48d6-a01e-84ef0aa7413f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96d1b538-18e6-4a9d-ab18-0400f3b91a08")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5fc17e5c-2703-42fc-85e9-748039befde0")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9f6e99a-288b-4eee-b511-082d0876cc5b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d0991cb-1d5d-4eda-a1a8-bbc97163d2ea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8d7d8bee-ee59-4fc2-a0b5-ed5d8bbc3caf")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 48 "/ZIF_9")
			(pintype "passive")
			(uuid "fce963d1-3587-4c91-855f-f3c916cdc872")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ae451c5b-13a9-4817-91b7-472ce6c47696")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "d1c89a98-ea6e-4e61-b662-48e5725b9e2c")
		(at 127.193 64.51)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "72b3d049-db4d-4670-ae9b-c4d830bb00f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "df7ee44a-7447-4109-84bf-564f20954c3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06f7b3af-b5d7-4a62-9b18-b7a825ac4e00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bebdbec1-4fe8-4152-9d71-770fd5e8a539")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bca5c759-67b7-4c80-8797-d246f9668140")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/af5878a4-2c93-4df3-b145-537c402ff259")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6600997a-c3c9-4290-9d8c-b384967fdc79")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f37956d-9ecd-41f7-bc96-08981048a8c2")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bc4abe9-f9a3-4d97-83e4-35d3a2c8fdf7")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2266f6a6-5c98-4435-a431-07911750e532")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d580668-eee5-437b-b1b3-602d4d278a33")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "744fadd2-f418-4a72-be8a-6f9351ab585d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ceee603b-704d-432c-8bf5-16b157db7c33")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f705ed1d-f14e-4622-aa32-c1fd37ae2263")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78a0d3fc-5f33-457f-b22c-a8d73d8a7f76")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "295dad1a-36a1-4e0f-ae02-0697f795de80")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7ce34f1d-47bc-4c6e-bc0f-e3ff1d70adbb")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 63 "Net-(U2-QF)")
			(pintype "passive")
			(uuid "02c272aa-3b2a-45dd-af07-14407711b360")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 44 "/ZIF_6")
			(pintype "passive")
			(uuid "5538481a-bfbf-4740-bf89-c7275b385f30")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "d40e70f3-9993-4e5a-8a20-e77c31e6fa62")
		(at 162.893 71.09)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R75"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1a748117-032b-4b42-91c2-2b6c43a18af4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "bd34f733-97d4-41f2-8542-5b72f0fd59e5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9361b6c3-4a04-4a0b-aa22-ac3782b02461")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3001abb4-2e18-440e-90a0-67821a4cb6e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc76538f-6aa9-458b-8ea2-f708dd621b65")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/dad3bf9a-3475-4281-8125-4769acc44b6d")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64e1ef04-27de-40a7-900a-a770fe6368db")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89b3ef57-9098-4954-abb9-9a8e99a0cd62")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8e0cad4-7fc6-48c5-9a9a-5db6e8fd44ed")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e35094a-abad-4752-a0e9-d2ff98aed590")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5cb2599-1263-4b56-b6f0-b4c682c25c90")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee837a26-2d80-46ab-9c76-920140ba3918")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1819e6fb-e1d5-42d4-b3ce-1b7f09866d8b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bdc7ce2-1840-4d76-a44e-b682e3b47932")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3450b558-2272-4683-9c63-ca18e852df6d")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e50b3ac5-fdf4-487c-a07e-a35f5d20cb85")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d217aef5-e041-40e8-98e9-dcd6148eec04")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 26 "/ZIF_31")
			(pintype "passive")
			(uuid "0f1327f0-cae8-4996-815e-1c6b5b21cb2b")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d0f16229-d3f2-4c8a-9020-ac588336b23d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "db7e061a-7925-4a36-a3fd-9ad39d8864f3")
		(at 150.993 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R45"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "5d11f8f3-c06f-4bfe-be65-5427da0523c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "7a31a50c-6b8f-45d2-899c-fc066bf9361d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9edf4729-78b0-4fce-97ce-9fb915289f3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d846ba03-40cd-4fcd-9f36-035d49ed76fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8653b823-857f-4d75-ac3e-cb5ff8277613")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/74214bf3-4e3c-4257-92c0-ffc2ee734d57")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f13e00c9-fd2b-47c5-92e7-0b2dbcf26dfb")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c87d3d92-8b0c-4da4-8a23-055282f501eb")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b49e7d90-bbfa-42dc-b2b6-50df0681c423")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "245f2357-2032-44fc-9df6-438ea9cab4f4")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4959c8e6-0831-4558-aded-5a48cc563115")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3202e80a-afeb-4e78-8a97-69423fe0091f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27d5046a-52c9-4301-9678-e9e51cb814de")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef224dd3-d9b8-44ef-97e6-4beca345e820")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66e4a249-3d7f-4a88-b3be-f87b306050f4")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "876afeb6-aa70-4c1f-9051-9c76a4400653")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5dda0cde-1c36-4389-90df-3df80716434a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 99 "/PISO_CLK")
			(pintype "passive")
			(uuid "410038d9-3ed2-4bf8-bc5d-dcdc46876d5b")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 8 "Net-(D4-A)")
			(pintype "passive")
			(uuid "3fc2f764-5958-45f0-8e67-0a839150b820")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "dc9e8624-2ea9-4196-85b1-80c96fb41993")
		(at 156.943 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R56"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "da54f067-45a6-4c16-8b03-020935c8d168")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "81e2d868-25c7-4f06-8fd2-c7494489b253")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6689a503-b635-406f-9403-8fa47fdc4f64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f8f90f93-7cce-4e82-baa3-50527216ef5e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8d982c9-9757-4647-b1b2-2a1bcff83383")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/11b74bc7-2d08-4b4e-91aa-2bb375b59bc5")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a588954-360e-4e58-9cc7-52827577a4ac")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c7aa894-1b38-40a0-afb6-ec82a9005201")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d7b3e20-835a-472d-97aa-7fb9f3f61708")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "919746a0-5a27-4e6c-b22a-7c03edc15f73")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63b81132-bb1a-49d4-a3ca-b56fa98ffcb2")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bfabaf3-2bd2-4c58-be0a-6a4b24d0f207")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1ca1d6b-f9d0-466a-94d9-b8447af4d965")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04cb1bbd-2d7b-4416-a0dd-5748e6e0c99c")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "102d51d2-5b27-4505-a208-d895183a3895")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f4ea86b-ee18-4456-8bc7-27905d8ea2c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3820a2f2-33c3-41d4-b459-e7cc86117b1f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 17 "/ZIF_11")
			(pintype "passive")
			(uuid "a19c97df-1714-4f66-995f-cd0e0f376261")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f50df352-5fbe-4041-b98b-11b97412e798")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "dd925bfb-07ba-4af4-a4d5-09b34d5453a7")
		(at 168.843 44.77)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R78"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "7f54abcd-8d50-4f43-94d0-1a1e3f3ea822")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c9bc4745-eaa6-4fc8-a7e0-3c47024c2f42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a23d423-32f6-42a1-a9e3-ccc8fb1773d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed363324-6c01-43f5-a73f-24c3469cc391")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61421a1f-3371-417e-ae98-af790cd7ea80")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b86e8770-20a4-49d2-b522-c1c1e712ce93")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f0b2bd8-099a-423e-89bf-966ce027b2c5")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39e4b1cb-72e0-4400-b7ac-b9f0b284b0af")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cacc59a0-9e11-4bd1-aeca-c0064930e9c7")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1dfbe68-03fa-4312-8cb2-50f4c00e43fe")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11f64d35-1b92-40b7-8abb-2423ec093932")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd4c1102-326f-4b46-88e7-9433c08f1e1b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53c75b34-3e5f-48e9-aab0-8a41e1613d3c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6709db5-40ba-4f50-864a-eb3125598e25")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fbb2146-2f26-46fd-8577-8d3acd01f067")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16604798-868f-496d-9b67-b78514a31f6f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3b8bcf6e-ac2c-4359-9387-077707b10a20")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 16 "/ZIF_34")
			(pintype "passive")
			(uuid "91b7b807-1682-4f6e-9dc9-c7eb5e96f6ba")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "801863a0-2d0e-4b45-aa43-479b2d89acd7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "e26cfd5f-8add-4bae-85ce-e69a0aa73836")
		(at 145.043 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R33"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "fe87b6e1-8f13-4cca-9c47-607ed0471eed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "10a756b0-4bdf-4a8b-b9bd-8216488a863b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "850e0398-ab3a-481d-b9e0-8e43ea2352f1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d5dd382-cb00-4a7d-b5fc-09f17797d5cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "31fea65c-54c2-46f6-a7f5-37833efe879b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f239dcff-8594-4dc9-8c85-240002544948")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8be1bf9-f4a6-45e9-b9d2-4a8683ec8f9a")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79234880-c78a-4d21-84c1-58bba42cc33a")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95237f9c-0708-408c-8877-c9e7e04a1482")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba127659-9088-4537-ac7c-8c5ecb1d6876")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01a27e5b-9463-491f-a424-ec61698c3aad")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f5ae94a-14db-4b59-8657-38ffd5ef15bc")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4553b5c1-2f99-44a4-be5a-186d45987faf")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "089e4200-3ca1-44cf-ad06-bf82138ebba1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebf61dab-2650-4cac-9d13-ad6c46efcd35")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b516d78-177d-411a-be3e-c6fec827b7a1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b1c6c5f9-e740-407b-889b-c6e5674c3079")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 89 "Net-(U5-QH)")
			(pintype "passive")
			(uuid "79821144-2bd7-4886-99fe-4fdc8dc8ef31")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 12 "/ZIF_33")
			(pintype "passive")
			(uuid "be648c45-d58d-4550-8ad3-53d253507a20")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "e5e08750-6de5-4f22-9a63-f5e153294674")
		(at 139.093 48.06)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R24"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "9baa60f8-40cb-4c06-9a06-66ac1e65c2a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "07b2dd99-56bc-4361-8311-1cbe74889906")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "63f2113e-2a9e-45e6-b92d-56361397ce9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fb0646c2-d068-4517-abd2-1a704c4a227c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f99fe13-8df9-4016-ac87-2570abb464da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/cbf2e60f-9151-46c1-98a3-b1a1bfa95e8f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b710d3ab-767b-4005-aced-6c98d3bd709c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b8f8657-f698-4463-9803-7b520a77b2e8")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76e235eb-8ee2-404c-a820-1ca9a922ee32")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f62d1fbc-5ff8-4c21-aee9-cdab25ca851a")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "349d597c-ecb1-4bef-a40c-0eb01f01d974")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c13e2cf2-fc09-48ba-b0ac-80354cc69ddd")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9754ffab-2d7d-4fb8-ae37-7a5fe701a9dd")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85a00892-9464-41c5-87a1-0cd2b9e802f0")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4385f8a8-d3af-4f2c-92df-80a2571b960f")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9548393-9ab0-4b7c-9b9a-34156901348c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2f5a448d-dbfd-4520-a0a2-60c7559d7361")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 80 "Net-(U4-QG)")
			(pintype "passive")
			(uuid "0596a11a-c6a7-42bd-9e41-3ea0e5a5b206")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 31 "/ZIF_24")
			(pintype "passive")
			(uuid "d04d5545-928e-49f6-ac44-e0de3af876ae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "e751d7dd-c851-40aa-9f31-dafe97f12c80")
		(at 127.193 51.35)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "708c4d65-c3ee-46de-9a3b-50c264a82634")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "1837bc85-e22a-4ef2-89d6-39c15e38f543")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f40765f-cc52-4f96-a0b0-b1752df4a792")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dc92b03b-4cc1-4f3b-8244-359bed463a33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e1988d5-de63-4f53-9415-ce41c6d55b51")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ce126535-bba9-4854-9781-33772ec492d6")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06f1e1c9-9a89-416e-95f2-e2f67e1ef0f9")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f73bcdeb-e17a-42c9-9d28-6cb4884e7590")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e174b3d4-870f-4f9c-ab42-c31d72891160")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bda13b8-08c7-4769-a009-9e3d4a92922c")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71cb94bc-96ec-4a1e-8aec-40e1f4255d5c")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3592567-b9b4-437a-91a6-4ed8f3b25525")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0e2006d-fe0c-4626-b13f-520049124d7c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a357732-9c28-4809-a9d7-c94f363db45d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0102f3ab-4eb4-4474-aa8d-dcf7a9bbdf1f")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07c9386b-4ba7-44fe-a03b-d9db4c344618")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "066abf1d-cc43-48bb-b9fb-bf602b28be54")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 59 "Net-(U2-QB)")
			(pintype "passive")
			(uuid "32dca367-4585-4031-bbcb-84b2475f5690")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 11 "/ZIF_2")
			(pintype "passive")
			(uuid "b1b5f7f5-af14-47ec-8f14-1b85c66347d1")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "ed98c8c7-947d-4900-a218-8544cfa0903a")
		(at 150.993 54.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R48"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "68e3d6c8-6ada-4cd3-a2f3-6793de6887d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "02a52eb1-fb46-4ccc-8dfe-c71977fb1227")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8aa03184-f97d-430e-ac96-9e506f1bf60d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61b1ad5e-07e3-4669-8cfb-efd7b29bec3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "279864d7-185d-4076-8882-d152676f17e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e200091d-5476-4756-806d-fe91a9104f96")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be9a634f-3829-489b-ab51-9df266fb0528")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f83df82-abef-4e82-bcef-21303f6a0eb9")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e68ce1df-ede7-4326-8ad4-c5b95124793e")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d454de6-8f5e-443b-b446-ce192c913b9e")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "557619c5-dcde-4da0-953b-5dec420099ee")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bab49ffe-53fa-4324-8d24-dad1d0dd1bfd")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1d0b740-fbf1-4da5-ae34-39cfb91101fa")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d69dbf55-cec3-4865-800b-e31e66d6cf54")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09b72f92-c06a-4f44-a803-a2cecc9b1749")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31763400-9713-483b-9178-c44add573588")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "30e8d3af-18bf-459c-be25-0b2f3b254e1b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 23 "/ZIF_3")
			(pintype "passive")
			(uuid "371b7e10-87e3-4e19-bdae-0dc7df66e0da")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d4628ab7-2247-4c04-9a8f-b990bb5cb0cc")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "effe0f2b-ab48-45e7-8970-9d23d340f20f")
		(at 162.893 61.22)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R72"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "ef78d1c4-7489-4607-bda7-d300acce33aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "1dc7c3ab-dfdf-4a63-b7f4-aee35ea61ab1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0fcf830-0fac-4bb7-98d1-b05fd8b09458")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f74cda8f-b731-471a-aadd-b78be28be90b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "edccb6bf-9754-42d6-aa1a-05b7102c4fe7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ee048eb2-c2f8-47e7-b00e-caa6b885e27a")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "605de71c-b363-4df7-b248-890b2ba624be")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1954da17-efb0-49e6-966d-bc4aecaa3181")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7818bdb-0641-4af3-8222-ee8d309a97e5")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fecc9437-676e-4ba3-bc39-58239c2058ab")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7f80bf6-f335-4646-8d6c-37ab6a2e6fb1")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfc929a5-68d1-4b65-bdb5-d0bcbee53b4c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "336fdcb4-8578-4e0a-a1f9-49f4b9c004de")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abdc367a-68ff-45d0-9005-0bf3fada2c02")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bdc564cf-048f-4622-82dd-7686f1b1b205")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d8adac2-751e-4e51-9dd5-1bc0c54e84c2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1b42c916-a579-49b7-838d-9354105ae1b3")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 46 "/ZIF_28")
			(pintype "passive")
			(uuid "b19150f9-35a2-4f57-88b8-350f11b38646")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9bd14cd2-9f32-4b51-8033-e2af4f0378b7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(uuid "f6e9f9ef-d36b-4377-889b-e0c704871e96")
		(at 109.153 98.47)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "e9677530-aeab-423b-892c-e5fc784212c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "751b044e-3289-460e-b7bb-27fda3ec4f28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2a2f29f-06dc-4746-9204-1762bcdfc3c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d834a801-62f3-4544-b718-746ab054605f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3783fdd6-b220-4bf4-a6da-bea2fe9f622d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f365ce21-e5c4-4cf3-a94f-5e986327d89f")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8dcdfb81-4ddd-4abb-8b9d-a84c895bdff7")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a10a1dc-eabb-48c7-b9b6-8ccee616a99d")
		)
		(fp_line
			(start -2.48 -1.15)
			(end 2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffe4157c-d738-41d0-bfe9-6ba73790a993")
		)
		(fp_line
			(start -2.48 1.15)
			(end -2.48 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b74a5471-ba15-43de-8b7a-e4b68242ff85")
		)
		(fp_line
			(start 2.48 -1.15)
			(end 2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d801eaf6-7c4d-4873-9d06-5fd35620c750")
		)
		(fp_line
			(start 2.48 1.15)
			(end -2.48 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3b11989-833b-4eea-805d-6b7e47f9a98e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a0aca14-b8d7-430c-abd6-3162825b618a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bca30e7-b722-4783-8810-39399231b64c")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8b4500c-c9c5-464e-8013-8f25e3a5f41c")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cfce426-4fe6-424d-98ff-6d62f0474c08")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fccb41c8-4a18-4191-a2fe-dcbcccae8e4b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "VCC")
			(pintype "passive")
			(uuid "a47c59d3-15be-4980-8504-ba5d7ef6b828")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
			(uuid "38922b86-31e9-40f0-bf15-7a530f256bb2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "fd2887c2-e29b-4894-a9d1-82c778397891")
		(at 133.143 67.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R19"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "a8961590-5a11-4dc5-9d72-3437eda1943d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "24f8f334-14db-40f0-983d-49cec2c51728")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed70e80f-4cf0-413b-8fd8-8be3ce8363cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3a48e2a-c928-4ec6-a536-df0cce32ee40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3fc3989-a024-473d-82aa-30c90566dcf6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/428dc844-48a9-4ff0-ba49-6580836f5b78")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "445ba8bd-33b6-43b2-bc3d-c73eb9be433a")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27741c4d-eede-4f44-93a9-b525efae87f7")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64ef6f1b-d8c9-4140-af9b-bbe312dacfe5")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3adfa3a1-4238-40fb-bf7b-f529458f626f")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1f1f75b-1f07-4a4e-8a93-7f801eb4689d")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9733ee4c-54b2-443d-8439-dd4bc7abfcd5")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0b8668e-a0bb-47be-b3f1-6d31905b2483")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "288d8cb5-6563-4ebe-b52d-d4bee64d12c8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e7494cf-ae36-4e5d-bc69-c41287863bc5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb032ccb-4bb9-499c-af21-56fcfa9255df")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2680efb5-8277-4281-a6b1-5c5e8bbf6df2")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 75 "Net-(U4-QB)")
			(pintype "passive")
			(uuid "1939892c-9135-4eb1-b962-a84dd7355c90")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 33 "/ZIF_18")
			(pintype "passive")
			(uuid "dcec3d42-990e-46e8-9c46-920b43e70c44")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(uuid "fd634c6c-835e-46cf-b09f-165dfdffb436")
		(at 156.943 41.48)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R55"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "92f34ab1-8897-40c0-9ad1-d8e50a8006d0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "8e84e0c3-535d-41bf-aded-150848682454")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9fc34c33-e76e-4c2e-ad4c-8d0ec12d80e6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f70b5ae-8676-4620-97e2-b852831cf004")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cab4fef6-910b-477c-839c-a78fa21c88f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/8c6f0947-dc60-4900-9c10-afe4cfdcc02a")
		(sheetname "Root")
		(sheetfile "DuPal_V3.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6f6f46a-2ff9-4731-970d-f108735d3a30")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05c76f5d-44bd-49f6-8334-45fa382082e8")
		)
		(fp_line
			(start -2.45 -1.12)
			(end 2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80a08c9d-54ca-444f-84a2-5ccb9ba1aba0")
		)
		(fp_line
			(start -2.45 1.12)
			(end -2.45 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc231b82-b776-4d34-92c7-b52aa8d152f1")
		)
		(fp_line
			(start 2.45 -1.12)
			(end 2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c068d402-18ec-44c1-887d-24402a17c49f")
		)
		(fp_line
			(start 2.45 1.12)
			(end -2.45 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "16a75c8b-cc2d-4f10-9dbe-841efe1e2307")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b5a67f0-ce37-42c6-9fc8-f39a8e2a4df4")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6366e0d-882e-4ee8-a0a6-d278c29d0f4d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9c59050-1ca8-442a-807d-f8ac92fa9e6e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aaa5fc7a-6743-4db9-b333-8d49839081cf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "168981d6-c6c9-4628-b4a3-bd8ac06b3aa6")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 39 "/ZIF_10")
			(pintype "passive")
			(uuid "60f3a283-ba37-4793-9645-040af8694886")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
			(uuid "2b43241e-2cc2-4318-981f-2f00dc4d6cb8")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
