(module SW_Push_1P1T_NO_CK_KSC7xxJ (layer F.Cu) (tedit 60F1AB12)
  (descr "CK components KSC7 tactile switch https://www.ckswitches.com/media/1973/ksc7.pdf")
  (tags "tactile switch ksc7")
  (attr smd)
  (fp_text reference REF** (at 0 4.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_Push_1P1T_NO_CK_KSC7xxJ (at 0 -4.23) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.21 -1.2) (end -3.21 1.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.21 -3.21) (end -3.21 -2.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.21 -3.21) (end -3.21 -3.21) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.21 -2.8) (end 3.21 -3.21) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.21 1.2) (end 3.21 -1.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.21 3.21) (end 3.21 2.93) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.21 3.21) (end 3.21 3.21) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.21 2.8) (end -3.21 3.21) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 0) (end 1.5 0) (layer F.Fab) (width 0.1))
  (fp_line (start -4.55 3.35) (end -4.55 -3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.55 3.35) (end -4.55 3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.55 -3.35) (end 4.55 3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.55 -3.35) (end 4.55 -3.35) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.1 3.1) (end -3.1 -3.1) (layer F.Fab) (width 0.1))
  (fp_line (start 3.1 3.1) (end -3.1 3.1) (layer F.Fab) (width 0.1))
  (fp_line (start 3.1 -3.1) (end 3.1 3.1) (layer F.Fab) (width 0.1))
  (fp_line (start -3.1 -3.1) (end 3.1 -3.1) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd rect (at -2.9 -2) (size 2.8 1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 2.9 -2) (size 2.8 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.9 2) (size 2.8 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.9 2) (size 2.8 1) (layers F.Cu F.Paste F.Mask))
  (model "3d_models/Tact Switch SMD 6x6mm.stp"
    (at (xyz 0 0 0))
    (scale (xyz 0.9 0.9 1))
    (rotate (xyz 0 0 0))
  )
)
