(footprint "BarrelJack_LCSC" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62057154)
  (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
  (tags "connector barrel jack")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.5) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 390189ed-8085-4137-9d9b-1376654e4513)
  )
  (fp_text value "BarrelJack_DC-005C-25A" (at 0 15.5) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1528b9b9-358c-4f0b-ad35-943f1e9ee7c4)
  )
  (fp_text user "${REFERENCE}" (at 0 7.5) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f0150cc6-81d2-42c3-b0d7-34f4f01133cb)
  )
  (fp_line (start -4.6 13.7) (end -4.6 -1) (layer "F.SilkS") (width 0.12) (tstamp 16f1451c-e720-40ce-b177-6bfe9aa1c209))
  (fp_line (start 4.6 -1) (end 4.6 0.3) (layer "F.SilkS") (width 0.12) (tstamp 22112936-a565-47d3-aec3-99f6a74a9b4a))
  (fp_line (start 4.6 4.95) (end 4.6 13.7) (layer "F.SilkS") (width 0.12) (tstamp 40c0bc9e-0e75-48b5-84fa-cac5f3466fc0))
  (fp_line (start -4.6 -1) (end -2.5 -1) (layer "F.SilkS") (width 0.12) (tstamp 530af9f1-9758-4ea7-8a28-94333e202e8d))
  (fp_line (start 4.6 13.7) (end -4.6 13.7) (layer "F.SilkS") (width 0.12) (tstamp 8c6588a3-b4ea-428f-bade-59f12759db05))
  (fp_line (start -3.2 -1.3) (end -4.9 -1.3) (layer "F.SilkS") (width 0.12) (tstamp 8c9f3be1-b8ed-43d0-aa8d-3f612835c9eb))
  (fp_line (start 2.5 -1) (end 4.6 -1) (layer "F.SilkS") (width 0.12) (tstamp d86ef0a3-2314-47cc-a618-360f238317d7))
  (fp_line (start -4.9 -1.3) (end -4.9 0.3) (layer "F.SilkS") (width 0.12) (tstamp f32b429b-dcd8-4991-98ca-5f2e2fbf9cec))
  (fp_line (start 5 -1.4) (end -5 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp 327b69a8-73ff-47ff-84c9-831925683b7e))
  (fp_line (start 5 14.1) (end 5 5.5) (layer "F.CrtYd") (width 0.05) (tstamp 760d6019-6f54-4cf2-88b9-03ac8e213095))
  (fp_line (start 6.2 -0.1) (end 6.2 5.5) (layer "F.CrtYd") (width 0.05) (tstamp 79bf1f0f-8199-4241-a1c9-31d3a0c17786))
  (fp_line (start 6.2 -0.1) (end 5 -0.1) (layer "F.CrtYd") (width 0.05) (tstamp a818a5ac-7625-4da0-96d6-db22d6412356))
  (fp_line (start 6.2 5.5) (end 5 5.5) (layer "F.CrtYd") (width 0.05) (tstamp b137aca6-8090-4326-abfb-2787ad836b53))
  (fp_line (start -5 14.1) (end 5 14.1) (layer "F.CrtYd") (width 0.05) (tstamp e48b1f79-fa99-4b87-8898-d6e6baa8af0f))
  (fp_line (start -5 -1.4) (end -5 14.1) (layer "F.CrtYd") (width 0.05) (tstamp e5d06160-047a-461e-9025-738367897b12))
  (fp_line (start 5 -0.1) (end 5 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp f737c5c8-ca04-46db-8ffc-ef7f0ffb13ef))
  (fp_line (start 4.5 -0.9) (end -3.5 -0.9) (layer "F.Fab") (width 0.1) (tstamp 2509a4b6-bbb5-4dca-845f-053db6d3d28d))
  (fp_line (start -4.5 13.55) (end -4.5 0.1) (layer "F.Fab") (width 0.1) (tstamp 544e5c38-dcb0-46c2-9307-024100a05ce0))
  (fp_line (start 4.5 -0.9) (end 4.5 13.55) (layer "F.Fab") (width 0.1) (tstamp 55caff64-b0cf-4f4c-a3e9-578f977ca94f))
  (fp_line (start 4.5 13.55) (end -4.5 13.55) (layer "F.Fab") (width 0.1) (tstamp 83cb4a29-2059-43ea-ada4-715be8f31e55))
  (fp_line (start -4.5 0.1) (end -3.5 -0.9) (layer "F.Fab") (width 0.1) (tstamp 8b6cfbed-99a0-4493-994a-7560220a57eb))
  (pad "1" thru_hole rect (at 0 0) (size 4.4 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask) (tstamp 3bf08e28-1b48-4f77-b697-e268dbb85802))
  (pad "2" thru_hole oval (at 0 6.65) (size 4 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask) (tstamp 4e78fe1d-b45f-4181-abcb-5a9bf96134de))
  (pad "3" thru_hole oval (at 4.7 2.55 90) (size 4 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask) (tstamp c1d3d69d-63c3-4969-abba-951b032bff8d))
  (model "${KIPRJMOD}/3d/Power Barrel Connector Jack 694106301002.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
