# SdFat: File Members

### - _ -

- __brkval : SdFatUtil.cpp
- __bss_end : SdFatUtil.cpp

### - e -

- EXP_LIMIT : istream.cpp

### - f -

- FAT_FILE_TYPE_CLOSED : SdBaseFile.h
- FAT_FILE_TYPE_MIN_DIR : SdBaseFile.h
- FAT_FILE_TYPE_NORMAL : SdBaseFile.h
- FAT_FILE_TYPE_ROOT32 : SdBaseFile.h
- FAT_FILE_TYPE_ROOT_FIXED : SdBaseFile.h
- FAT_FILE_TYPE_SUBDIR : SdBaseFile.h

### - m -

- MiniSerial : MinimumSerial.cpp

### - s -

- SD_CARD_ERROR_ACMD23 : Sd2Card.h
- SD_CARD_ERROR_ACMD41 : Sd2Card.h
- SD_CARD_ERROR_BAD_CSD : Sd2Card.h
- SD_CARD_ERROR_CMD0 : Sd2Card.h
- SD_CARD_ERROR_CMD12 : Sd2Card.h
- SD_CARD_ERROR_CMD17 : Sd2Card.h
- SD_CARD_ERROR_CMD18 : Sd2Card.h
- SD_CARD_ERROR_CMD24 : Sd2Card.h
- SD_CARD_ERROR_CMD25 : Sd2Card.h
- SD_CARD_ERROR_CMD58 : Sd2Card.h
- SD_CARD_ERROR_CMD59 : Sd2Card.h
- SD_CARD_ERROR_CMD8 : Sd2Card.h
- SD_CARD_ERROR_ERASE : Sd2Card.h
- SD_CARD_ERROR_ERASE_SINGLE_BLOCK : Sd2Card.h
- SD_CARD_ERROR_ERASE_TIMEOUT : Sd2Card.h
- SD_CARD_ERROR_INIT_NOT_CALLED : Sd2Card.h
- SD_CARD_ERROR_READ : Sd2Card.h
- SD_CARD_ERROR_READ_CRC : Sd2Card.h
- SD_CARD_ERROR_READ_REG : Sd2Card.h
- SD_CARD_ERROR_READ_TIMEOUT : Sd2Card.h
- SD_CARD_ERROR_SCK_RATE : Sd2Card.h
- SD_CARD_ERROR_SPI_DMA : Sd2Card.h
- SD_CARD_ERROR_STOP_TRAN : Sd2Card.h
- SD_CARD_ERROR_WRITE : Sd2Card.h
- SD_CARD_ERROR_WRITE_BLOCK_ZERO : Sd2Card.h
- SD_CARD_ERROR_WRITE_MULTIPLE : Sd2Card.h
- SD_CARD_ERROR_WRITE_PROGRAMMING : Sd2Card.h
- SD_CARD_ERROR_WRITE_TIMEOUT : Sd2Card.h
- SD_CARD_TYPE_SD1 : Sd2Card.h
- SD_CARD_TYPE_SD2 : Sd2Card.h
- SD_CARD_TYPE_SDHC : Sd2Card.h
- SD_CHIP_SELECT_PIN : SdSpi.h
- SOFT_SPI_CS_PIN : SdFatConfig.h
- SOFT_SPI_MISO_PIN : SdFatConfig.h
- SOFT_SPI_MOSI_PIN : SdFatConfig.h
- SOFT_SPI_SCK_PIN : SdFatConfig.h
- SPI_SCK_INIT_DIVISOR : SdFatConfig.h
- STREAM_BUF_SIZE : StdioStream.h

### - u -

- uint32_max : istream.cpp
- UNGETC_BUF_SIZE : StdioStream.h