(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ATF1508ASL-25AU100" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -17.78 71.12 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ATF1508ASL-25AU100" (id 1) (at -17.145 -28.575 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "Package_LCC:PLCC-84_SMD-Socket" (id 2) (at 1.905 29.21 90)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Microchip" (id 4) (at -3.81 3.175 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (symbol "ATF1508ASL-25AU100_0_0"
      (rectangle (start -17.78 71.12) (end 17.78 -26.035)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at -22.86 63.5 0) (length 5.08)
        (name "I/1/GCLR" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 45.72 0) (length 5.08)
        (name "I/O/10" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 43.18 0) (length 5.08)
        (name "I/O/11" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 40.64 0) (length 5.08)
        (name "I/O/12/PD1" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 38.1 0) (length 5.08)
        (name "I/O/14/TDI" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 35.56 0) (length 5.08)
        (name "I/O/15" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 33.02 0) (length 5.08)
        (name "I/O/16" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 30.48 0) (length 5.08)
        (name "I/O/17" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 27.94 0) (length 5.08)
        (name "I/O/18" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -6.985 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 60.96 0) (length 5.08)
        (name "I/2/OE2/GCLK2" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 25.4 0) (length 5.08)
        (name "I/O/20" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 22.86 0) (length 5.08)
        (name "I/O/21" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 20.32 0) (length 5.08)
        (name "I/O/22" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 17.78 0) (length 5.08)
        (name "I/O/23/TMS" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 15.24 0) (length 5.08)
        (name "I/O/24" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 12.7 0) (length 5.08)
        (name "I/O/25" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -7.62 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 10.16 0) (length 5.08)
        (name "I/O/27" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 7.62 0) (length 5.08)
        (name "I/O/28" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 5.08 0) (length 5.08)
        (name "I/O/29" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 8.89 76.2 270) (length 5.08)
        (name "VCCINT" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 2.54 0) (length 5.08)
        (name "I/O/30" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 0 0) (length 5.08)
        (name "I/O/31" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -5.08 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -2.54 0) (length 5.08)
        (name "I/O/33" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -5.08 0) (length 5.08)
        (name "I/O/34" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -7.62 0) (length 5.08)
        (name "I/O/35" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -10.16 0) (length 5.08)
        (name "I/O/36" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -12.7 0) (length 5.08)
        (name "I/O/37" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -5.715 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -15.24 0) (length 5.08)
        (name "I/O/39" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 58.42 0) (length 5.08)
        (name "I/O/4" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -17.78 0) (length 5.08)
        (name "I/O/40" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 -20.32 0) (length 5.08)
        (name "I/O/41" (effects (font (size 1.016 1.016))))
        (number "41" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -3.175 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "42" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 6.985 76.2 270) (length 5.08)
        (name "VCCINT" (effects (font (size 1.016 1.016))))
        (number "43" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -20.32 180) (length 5.08)
        (name "I/O/44" (effects (font (size 1.016 1.016))))
        (number "44" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -17.78 180) (length 5.08)
        (name "I/O/45/PD2" (effects (font (size 1.016 1.016))))
        (number "45" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -15.24 180) (length 5.08)
        (name "I/O/46" (effects (font (size 1.016 1.016))))
        (number "46" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 6.35 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "47" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -12.7 180) (length 5.08)
        (name "I/O/48" (effects (font (size 1.016 1.016))))
        (number "48" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -10.16 180) (length 5.08)
        (name "I/O/49" (effects (font (size 1.016 1.016))))
        (number "49" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 55.88 0) (length 5.08)
        (name "I/O/5" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -7.62 180) (length 5.08)
        (name "I/O/50" (effects (font (size 1.016 1.016))))
        (number "50" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -5.08 180) (length 5.08)
        (name "I/O/51" (effects (font (size 1.016 1.016))))
        (number "51" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 -2.54 180) (length 5.08)
        (name "I/O/52" (effects (font (size 1.016 1.016))))
        (number "52" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -3.81 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "53" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 0 180) (length 5.08)
        (name "I/O/54" (effects (font (size 1.016 1.016))))
        (number "54" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 2.54 180) (length 5.08)
        (name "I/O/55" (effects (font (size 1.016 1.016))))
        (number "55" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 5.08 180) (length 5.08)
        (name "I/O/56" (effects (font (size 1.016 1.016))))
        (number "56" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 7.62 180) (length 5.08)
        (name "I/O/57" (effects (font (size 1.016 1.016))))
        (number "57" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 10.16 180) (length 5.08)
        (name "I/O/58" (effects (font (size 1.016 1.016))))
        (number "58" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 0.635 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "59" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 53.34 0) (length 5.08)
        (name "I/O/6" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 12.7 180) (length 5.08)
        (name "I/O/60" (effects (font (size 1.016 1.016))))
        (number "60" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 15.24 180) (length 5.08)
        (name "I/O/61" (effects (font (size 1.016 1.016))))
        (number "61" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional clock (at 22.86 17.78 180) (length 5.08)
        (name "I/O/62/TCK" (effects (font (size 1.016 1.016))))
        (number "62" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 20.32 180) (length 5.08)
        (name "I/O/63" (effects (font (size 1.016 1.016))))
        (number "63" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 22.86 180) (length 5.08)
        (name "I/O/64" (effects (font (size 1.016 1.016))))
        (number "64" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 25.4 180) (length 5.08)
        (name "I/O/65" (effects (font (size 1.016 1.016))))
        (number "65" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -1.905 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "66" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 27.94 180) (length 5.08)
        (name "I/O/67" (effects (font (size 1.016 1.016))))
        (number "67" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 30.48 180) (length 5.08)
        (name "I/O/68" (effects (font (size 1.016 1.016))))
        (number "68" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 33.02 180) (length 5.08)
        (name "I/O/69" (effects (font (size 1.016 1.016))))
        (number "69" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 4.445 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 35.56 180) (length 5.08)
        (name "I/O/70" (effects (font (size 1.016 1.016))))
        (number "70" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 38.1 180) (length 5.08)
        (name "I/O/71/TDO" (effects (font (size 1.016 1.016))))
        (number "71" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "72" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 40.64 180) (length 5.08)
        (name "I/O/73" (effects (font (size 1.016 1.016))))
        (number "73" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 43.18 180) (length 5.08)
        (name "I/O/74" (effects (font (size 1.016 1.016))))
        (number "74" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 45.72 180) (length 5.08)
        (name "I/O/75" (effects (font (size 1.016 1.016))))
        (number "75" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 48.26 180) (length 5.08)
        (name "I/O/76" (effects (font (size 1.016 1.016))))
        (number "76" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 50.8 180) (length 5.08)
        (name "I/O/77" (effects (font (size 1.016 1.016))))
        (number "77" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 1.905 76.2 270) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "78" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 53.34 180) (length 5.08)
        (name "I/O/79" (effects (font (size 1.016 1.016))))
        (number "79" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 50.8 0) (length 5.08)
        (name "I/O/8" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 55.88 180) (length 5.08)
        (name "I/O/80" (effects (font (size 1.016 1.016))))
        (number "80" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 58.42 180) (length 5.08)
        (name "I/O/81/GCLK3" (effects (font (size 1.016 1.016))))
        (number "81" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -1.27 -31.115 90) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "82" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 60.96 180) (length 5.08)
        (name "I/83/GCLK1" (effects (font (size 1.016 1.016))))
        (number "83" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 22.86 63.5 180) (length 5.08)
        (name "I/84/OE1" (effects (font (size 1.016 1.016))))
        (number "84" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -22.86 48.26 0) (length 5.08)
        (name "I/O/9" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "CY7C1019D-10VXIT" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "CY7C1019D-10VXIT" (id 1) (at 12.7 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:SOJ-36_10.16x23.49mm_P1.27mm" (id 2) (at -12.7 29.21 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mouser.se/datasheet/2/196/CYPRS13494_1-3003573.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "SRAM MEMORY" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1Mb 10ns 128K x 8 Fast Async SRAM,SOJ32" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSOP*10.16x18.41mm*P0.8mm*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CY7C1019D-10VXIT_0_1"
      (rectangle (start -12.7 30.48) (end 12.7 -30.48)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "CY7C1019D-10VXIT_1_1"
      (pin input line (at -15.24 27.305 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
        (name "IO2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
        (name "IO3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -22.225 0) (length 2.54)
        (name "~{WE}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 17.145 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 14.605 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 12.065 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 9.525 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 6.985 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 4.445 0) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 1.905 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 24.765 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -0.635 0) (length 2.54)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -3.175 0) (length 2.54)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
        (name "IO4" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
        (name "IO5" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.27 33.02 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 1.27 -33.02 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
        (name "IO6" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
        (name "IO7" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -24.765 0) (length 2.54)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -5.715 0) (length 2.54)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 22.225 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -8.255 0) (length 2.54)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -10.795 0) (length 2.54)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -13.335 0) (length 2.54)
        (name "A16" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 19.685 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -27.305 0) (length 2.54)
        (name "~{CE}" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
        (name "IO0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
        (name "IO1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 1.27 33.02 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -1.905 -33.02 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "FT2232H-Interface_USB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 22.86 53.34 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "FT2232H-Interface_USB" (id 1) (at 17.78 -54.61 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.ftdichip.com/Products/ICs/FT2232H.html" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Mfr #" "FT2232HL-REEL" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "LCSC #" "C27882" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "QFN* LQFP*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "FT2232H-Interface_USB_0_1"
      (rectangle (start -26.67 -52.07) (end 26.67 52.07)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "FT2232H-Interface_USB_1_1"
      (pin power_in line (at -10.16 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -15.24 -55.88 90) (length 3.81)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 55.88 270) (length 3.81)
        (name "VCORE" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 -45.72 0) (length 3.81)
        (name "TEST" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 10.16 0) (length 3.81)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 48.26 180) (length 3.81)
        (name "ADBUS0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 45.72 180) (length 3.81)
        (name "ADBUS1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 43.18 180) (length 3.81)
        (name "ADBUS2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 40.64 180) (length 3.81)
        (name "ADBUS3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 -30.48 0) (length 3.81)
        (name "OSCI" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 55.88 270) (length 3.81)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 38.1 180) (length 3.81)
        (name "ADBUS4" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 35.56 180) (length 3.81)
        (name "ADBUS5" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 33.02 180) (length 3.81)
        (name "ADBUS6" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 30.48 180) (length 3.81)
        (name "ADBUS7" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 25.4 180) (length 3.81)
        (name "ACBUS0" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 22.86 180) (length 3.81)
        (name "ACBUS1" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 20.32 180) (length 3.81)
        (name "ACBUS2" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 17.78 180) (length 3.81)
        (name "ACBUS3" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -30.48 -40.64 0) (length 3.81)
        (name "OSCO" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 15.24 180) (length 3.81)
        (name "ACBUS4" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 55.88 270) (length 3.81)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 12.7 180) (length 3.81)
        (name "ACBUS5" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 10.16 180) (length 3.81)
        (name "ACBUS6" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 7.62 180) (length 3.81)
        (name "ACBUS7" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 30.48 -45.72 180) (length 3.81)
        (name "~{SUSPEND}" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 55.88 270) (length 3.81)
        (name "VCORE" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 2.54 180) (length 3.81)
        (name "BDBUS0" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 0 180) (length 3.81)
        (name "BDBUS1" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 55.88 270) (length 3.81)
        (name "VPHY" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -2.54 180) (length 3.81)
        (name "BDBUS2" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -5.08 180) (length 3.81)
        (name "BDBUS3" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.16 55.88 270) (length 3.81)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -7.62 180) (length 3.81)
        (name "BDBUS4" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -10.16 180) (length 3.81)
        (name "BDBUS5" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -12.7 180) (length 3.81)
        (name "BDBUS6" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -15.24 180) (length 3.81)
        (name "BDBUS7" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -20.32 180) (length 3.81)
        (name "BCBUS0" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -30.48 43.18 0) (length 3.81)
        (name "VREGOUT" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -7.62 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -30.48 48.26 0) (length 3.81)
        (name "VREGIN" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 -55.88 90) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -22.86 180) (length 3.81)
        (name "BCBUS1" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -25.4 180) (length 3.81)
        (name "BCBUS2" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -27.94 180) (length 3.81)
        (name "BCBUS3" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -30.48 180) (length 3.81)
        (name "BCBUS4" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 55.88 270) (length 3.81)
        (name "VCCIO" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -33.02 180) (length 3.81)
        (name "BCBUS5" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -35.56 180) (length 3.81)
        (name "BCBUS6" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -38.1 180) (length 3.81)
        (name "BCBUS7" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -30.48 15.24 0) (length 3.81)
        (name "REF" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 30.48 -43.18 180) (length 3.81)
        (name "~{PWREN}" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 -22.86 0) (length 3.81)
        (name "EEDATA" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -30.48 -20.32 0) (length 3.81)
        (name "EECLK" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -30.48 -17.78 0) (length 3.81)
        (name "EECS" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 55.88 270) (length 3.81)
        (name "VCORE" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 22.86 0) (length 3.81)
        (name "DM" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -30.48 20.32 0) (length 3.81)
        (name "DP" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 55.88 270) (length 3.81)
        (name "VPLL" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HRO-TYPE-C-31-M-12" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "USB1" (id 0) (at 0 30.5562 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "HRO-TYPE-C-31-M-12" (id 1) (at 0 27.8638 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "Greaseweazle:HRO-TYPE-C-31-M-12" (id 2) (at 0 25.1714 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "https://datasheet.lcsc.com/szlcsc/1811131825_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.pdf" (id 3) (at -17.78 1.27 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "LCSC" "C165948" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HRO-TYPE-C-31-M-12_0_1"
      (rectangle (start -11.43 15.24) (end -8.89 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 -17.78) (end -8.89 15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "HRO-TYPE-C-31-M-12_1_1"
      (pin input line (at 2.54 13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -8.89 180) (length 2.54)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -16.51 180) (length 2.54)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 8.89 180) (length 2.54)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 6.35 180) (length 2.54)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 3.81 180) (length 2.54)
        (name "DN2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 1.27 180) (length 2.54)
        (name "DP1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -1.27 180) (length 2.54)
        (name "DN1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -3.81 180) (length 2.54)
        (name "DP2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -6.35 180) (length 2.54)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "bead-myRF" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "FB2" (id 0) (at 1.905 -1.778 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "bead-myRF" (id 1) (at 2.54 -3.556 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Inductor_SMD:L_0805_2012Metric" (id 2) (at 0 -1.778 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/szlcsc/1810201211_Murata-Electronics-BLM21AG601SN1D_C85837.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Mfr #" "BLM21AG601SN1D" (id 4) (at 0 0 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "LCSC #" "C85837" (id 5) (at 0 0 90)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Inductor_* L_* *Ferrite*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "bead-myRF_0_1"
      (rectangle (start -0.381 1.27) (end 0.381 -1.143)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 0 -1.27)
          (xy 0 -0.7874)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 0.889)
          (xy 0 1.2954)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "bead-myRF_1_1"
      (pin passive line (at 0 2.54 270) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 90) (length 1.27)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
