(module STMicroelectronics-LQFP144-1A-0-3-IPC_A (layer F.Cu) (tedit 60EFE02F)
  (fp_text reference REF** (at -9.6031 -12.9031) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (fp_text value Val** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.15)))
  )
  (fp_line (start -10 10) (end -10 -10) (layer F.Fab) (width 0.15))
  (fp_line (start -10 -10) (end 10 -10) (layer F.Fab) (width 0.15))
  (fp_line (start 10 -10) (end 10 10) (layer F.Fab) (width 0.15))
  (fp_line (start 10 10) (end -10 10) (layer F.Fab) (width 0.15))
  (fp_line (start -9.25 9.25) (end -9.25 -9.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.25 -9.25) (end 9.25 -9.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.25 -9.25) (end 9.25 9.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.25 9.25) (end -9.25 9.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.0781 -12.078099) (end 12.0781 -12.078099) (layer F.CrtYd) (width 0.15))
  (fp_line (start 12.0781 -12.078099) (end -12.0781 -12.078099) (layer F.CrtYd) (width 0.15))
  (fp_line (start -12.0781 -12.078099) (end -12.0781 12.078101) (layer F.CrtYd) (width 0.15))
  (fp_line (start -12.0781 12.078101) (end 12.0781 12.078101) (layer F.CrtYd) (width 0.15))
  (fp_line (start 12.0781 12.078101) (end 12.0781 -12.078099) (layer F.CrtYd) (width 0.15))
  (fp_circle (center -10.675482 -9.46) (end -10.550482 -9.46) (layer F.SilkS) (width 0.25))
  (fp_circle (center -8.4 -8.4) (end -8.15 -8.4) (layer F.SilkS) (width 0.5))
  (pad 1 smd rect (at -10.675482 -8.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd roundrect (at -10.675482 -8.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 3 smd roundrect (at -10.675482 -7.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 4 smd roundrect (at -10.675482 -7.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 5 smd roundrect (at -10.675482 -6.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 6 smd roundrect (at -10.675482 -6.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 7 smd roundrect (at -10.675482 -5.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 8 smd roundrect (at -10.675482 -5.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 9 smd roundrect (at -10.675482 -4.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 10 smd roundrect (at -10.675482 -4.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 11 smd roundrect (at -10.675482 -3.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 12 smd roundrect (at -10.675482 -3.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 13 smd roundrect (at -10.675482 -2.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 14 smd roundrect (at -10.675482 -2.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 15 smd roundrect (at -10.675482 -1.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 16 smd roundrect (at -10.675482 -1.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 17 smd roundrect (at -10.675482 -0.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 18 smd roundrect (at -10.675482 -0.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 19 smd roundrect (at -10.675482 0.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 20 smd roundrect (at -10.675482 0.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 21 smd roundrect (at -10.675482 1.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 22 smd roundrect (at -10.675482 1.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 23 smd roundrect (at -10.675482 2.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 24 smd roundrect (at -10.675482 2.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 25 smd roundrect (at -10.675482 3.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 26 smd roundrect (at -10.675482 3.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 27 smd roundrect (at -10.675482 4.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 28 smd roundrect (at -10.675482 4.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 29 smd roundrect (at -10.675482 5.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 30 smd roundrect (at -10.675482 5.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 31 smd roundrect (at -10.675482 6.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 32 smd roundrect (at -10.675482 6.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 33 smd roundrect (at -10.675482 7.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 34 smd roundrect (at -10.675482 7.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 35 smd roundrect (at -10.675482 8.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 36 smd roundrect (at -10.675482 8.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 73 smd roundrect (at 10.675482 8.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 74 smd roundrect (at 10.675482 8.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 75 smd roundrect (at 10.675482 7.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 76 smd roundrect (at 10.675482 7.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 77 smd roundrect (at 10.675482 6.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 78 smd roundrect (at 10.675482 6.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 79 smd roundrect (at 10.675482 5.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 80 smd roundrect (at 10.675482 5.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 81 smd roundrect (at 10.675482 4.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 82 smd roundrect (at 10.675482 4.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 83 smd roundrect (at 10.675482 3.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 84 smd roundrect (at 10.675482 3.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 85 smd roundrect (at 10.675482 2.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 86 smd roundrect (at 10.675482 2.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 87 smd roundrect (at 10.675482 1.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 88 smd roundrect (at 10.675482 1.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 89 smd roundrect (at 10.675482 0.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 90 smd roundrect (at 10.675482 0.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 91 smd roundrect (at 10.675482 -0.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 92 smd roundrect (at 10.675482 -0.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 93 smd roundrect (at 10.675482 -1.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 94 smd roundrect (at 10.675482 -1.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 95 smd roundrect (at 10.675482 -2.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 96 smd roundrect (at 10.675482 -2.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 97 smd roundrect (at 10.675482 -3.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 98 smd roundrect (at 10.675482 -3.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 99 smd roundrect (at 10.675482 -4.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 100 smd roundrect (at 10.675482 -4.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 101 smd roundrect (at 10.675482 -5.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 102 smd roundrect (at 10.675482 -5.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 103 smd roundrect (at 10.675482 -6.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 104 smd roundrect (at 10.675482 -6.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 105 smd roundrect (at 10.675482 -7.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 106 smd roundrect (at 10.675482 -7.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 107 smd roundrect (at 10.675482 -8.25) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 108 smd roundrect (at 10.675482 -8.75) (size 1.955236 0.312474) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 37 smd roundrect (at -8.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 38 smd roundrect (at -8.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 39 smd roundrect (at -7.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 40 smd roundrect (at -7.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 41 smd roundrect (at -6.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 42 smd roundrect (at -6.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 43 smd roundrect (at -5.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 44 smd roundrect (at -5.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 45 smd roundrect (at -4.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 46 smd roundrect (at -4.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 47 smd roundrect (at -3.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 48 smd roundrect (at -3.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 49 smd roundrect (at -2.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 50 smd roundrect (at -2.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 51 smd roundrect (at -1.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 52 smd roundrect (at -1.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 53 smd roundrect (at -0.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 54 smd roundrect (at -0.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 55 smd roundrect (at 0.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 56 smd roundrect (at 0.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 57 smd roundrect (at 1.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 58 smd roundrect (at 1.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 59 smd roundrect (at 2.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 60 smd roundrect (at 2.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 61 smd roundrect (at 3.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 62 smd roundrect (at 3.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 63 smd roundrect (at 4.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 64 smd roundrect (at 4.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 65 smd roundrect (at 5.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 66 smd roundrect (at 5.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 67 smd roundrect (at 6.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 68 smd roundrect (at 6.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 69 smd roundrect (at 7.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 70 smd roundrect (at 7.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 71 smd roundrect (at 8.25 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 72 smd roundrect (at 8.75 10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 109 smd roundrect (at 8.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 110 smd roundrect (at 8.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 111 smd roundrect (at 7.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 112 smd roundrect (at 7.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 113 smd roundrect (at 6.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 114 smd roundrect (at 6.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 115 smd roundrect (at 5.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 116 smd roundrect (at 5.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 117 smd roundrect (at 4.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 118 smd roundrect (at 4.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 119 smd roundrect (at 3.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 120 smd roundrect (at 3.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 121 smd roundrect (at 2.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 122 smd roundrect (at 2.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 123 smd roundrect (at 1.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 124 smd roundrect (at 1.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 125 smd roundrect (at 0.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 126 smd roundrect (at 0.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 127 smd roundrect (at -0.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 128 smd roundrect (at -0.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 129 smd roundrect (at -1.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 130 smd roundrect (at -1.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 131 smd roundrect (at -2.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 132 smd roundrect (at -2.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 133 smd roundrect (at -3.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 134 smd roundrect (at -3.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 135 smd roundrect (at -4.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 136 smd roundrect (at -4.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 137 smd roundrect (at -5.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 138 smd roundrect (at -5.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 139 smd roundrect (at -6.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 140 smd roundrect (at -6.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 141 smd roundrect (at -7.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 142 smd roundrect (at -7.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 143 smd roundrect (at -8.25 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (pad 144 smd roundrect (at -8.75 -10.675482) (size 0.312474 1.955236) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5))
  (model 3d_models/STMicroelectronics_-_STM32F730Z8T6.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
