(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "ABC-Bus" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (at 3.81 41.91 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "ABC-Bus" (at -3.81 -46.99 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "sm6uax:MAB64B-FAB64Q" (at -20.32 -1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -10.16 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ABC-Bus_1_0"
      (pin bidirectional line (at -12.7 13.97 0) (length 5.08)
        (name "D3" (effects (font (size 0.9906 0.9906))))
        (number "A10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 11.43 0) (length 5.08)
        (name "D2" (effects (font (size 0.9906 0.9906))))
        (number "A11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 8.89 0) (length 5.08)
        (name "D1" (effects (font (size 0.9906 0.9906))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 6.35 0) (length 5.08)
        (name "D0" (effects (font (size 0.9906 0.9906))))
        (number "A13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 3.81 0) (length 5.08)
        (name "NC" (effects (font (size 0.9906 0.9906))))
        (number "A14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 1.27 0) (length 5.08)
        (name "~{RST}" (effects (font (size 0.9906 0.9906))))
        (number "A15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -1.27 0) (length 5.08)
        (name "~{STATUS}" (effects (font (size 0.9906 0.9906))))
        (number "A16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -3.81 0) (length 5.08)
        (name "~{INP}" (effects (font (size 0.9906 0.9906))))
        (number "A17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -6.35 0) (length 5.08)
        (name "~{C4}" (effects (font (size 0.9906 0.9906))))
        (number "A18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -8.89 0) (length 5.08)
        (name "~{C3}" (effects (font (size 0.9906 0.9906))))
        (number "A19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 34.29 0) (length 5.08)
        (name "0V" (effects (font (size 0.9906 0.9906))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -11.43 0) (length 5.08)
        (name "~{C2}" (effects (font (size 0.9906 0.9906))))
        (number "A20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -13.97 0) (length 5.08)
        (name "~{C1}" (effects (font (size 0.9906 0.9906))))
        (number "A21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -16.51 0) (length 5.08)
        (name "~{OUT}" (effects (font (size 0.9906 0.9906))))
        (number "A22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -19.05 0) (length 5.08)
        (name "~{CS}" (effects (font (size 0.9906 0.9906))))
        (number "A23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -21.59 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A24" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -24.13 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -26.67 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A26" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -29.21 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A27" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -31.75 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A28" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -34.29 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 31.75 0) (length 5.08)
        (name "~{RESIN}" (effects (font (size 0.9906 0.9906))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -36.83 0) (length 5.08)
        (name "READY" (effects (font (size 0.9906 0.9906))))
        (number "A30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -39.37 0) (length 5.08)
        (name "+5V" (effects (font (size 0.9906 0.9906))))
        (number "A31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -41.91 0) (length 5.08)
        (name "+12V" (effects (font (size 0.9906 0.9906))))
        (number "A32" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 29.21 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 26.67 0) (length 5.08)
        (name "~{XMEMW}" (effects (font (size 0.9906 0.9906))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 24.13 0) (length 5.08)
        (name "D7" (effects (font (size 0.9906 0.9906))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 21.59 0) (length 5.08)
        (name "D6" (effects (font (size 0.9906 0.9906))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 19.05 0) (length 5.08)
        (name "D5" (effects (font (size 0.9906 0.9906))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 16.51 0) (length 5.08)
        (name "D4" (effects (font (size 0.9906 0.9906))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ABC-Bus_1_1"
      (rectangle (start -7.62 40.64) (end 5.08 -44.45)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (pin power_out line (at -12.7 36.83 0) (length 5.08)
        (name "-12V" (effects (font (size 0.9906 0.9906))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 36.83 180) (length 5.08)
        (name "-12V" (effects (font (size 0.9906 0.9906))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 13.97 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 11.43 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 8.89 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 6.35 180) (length 5.08)
        (name "~{INT}" (effects (font (size 0.9906 0.9906))))
        (number "B13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 3.81 180) (length 5.08)
        (name "A15" (effects (font (size 0.9906 0.9906))))
        (number "B14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 1.27 180) (length 5.08)
        (name "A14" (effects (font (size 0.9906 0.9906))))
        (number "B15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -1.27 180) (length 5.08)
        (name "A13" (effects (font (size 0.9906 0.9906))))
        (number "B16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -3.81 180) (length 5.08)
        (name "A12" (effects (font (size 0.9906 0.9906))))
        (number "B17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -6.35 180) (length 5.08)
        (name "A11" (effects (font (size 0.9906 0.9906))))
        (number "B18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -8.89 180) (length 5.08)
        (name "A10" (effects (font (size 0.9906 0.9906))))
        (number "B19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 34.29 180) (length 5.08)
        (name "0V" (effects (font (size 0.9906 0.9906))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -11.43 180) (length 5.08)
        (name "A9" (effects (font (size 0.9906 0.9906))))
        (number "B20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -13.97 180) (length 5.08)
        (name "A8" (effects (font (size 0.9906 0.9906))))
        (number "B21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -16.51 180) (length 5.08)
        (name "A7" (effects (font (size 0.9906 0.9906))))
        (number "B22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -19.05 180) (length 5.08)
        (name "A6" (effects (font (size 0.9906 0.9906))))
        (number "B23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -21.59 180) (length 5.08)
        (name "A5" (effects (font (size 0.9906 0.9906))))
        (number "B24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -24.13 180) (length 5.08)
        (name "A4" (effects (font (size 0.9906 0.9906))))
        (number "B25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -26.67 180) (length 5.08)
        (name "A3" (effects (font (size 0.9906 0.9906))))
        (number "B26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -29.21 180) (length 5.08)
        (name "A2" (effects (font (size 0.9906 0.9906))))
        (number "B27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -31.75 180) (length 5.08)
        (name "A1" (effects (font (size 0.9906 0.9906))))
        (number "B28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -34.29 180) (length 5.08)
        (name "A0" (effects (font (size 0.9906 0.9906))))
        (number "B29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 31.75 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -36.83 180) (length 5.08)
        (name "NC" (effects (font (size 0.9906 0.9906))))
        (number "B30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -39.37 180) (length 5.08)
        (name "+5V" (effects (font (size 0.9906 0.9906))))
        (number "B31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -41.91 180) (length 5.08)
        (name "+12V" (effects (font (size 0.9906 0.9906))))
        (number "B32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 29.21 180) (length 5.08)
        (name "~{XMEMFL}" (effects (font (size 0.9906 0.9906))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 26.67 180) (length 5.08)
        (name "5" (effects (font (size 0.9906 0.9906))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 24.13 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 21.59 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 19.05 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 16.51 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
