19677923485869
ide-usb-pcb
Crystal_SMD_2016-4Pin_2.0x1.6mm
SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package
SMD SMT crystal
0
4
4
ide-usb-pcb
Crystal_SMD_3215-2Pin_3.2x1.5mm
SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf
SMD SMT Crystal
0
2
2
ide-usb-pcb
Fuse_1206_3216Metric
Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
ide-usb-pcb
HRO-TYPE-C-31-M-12


0
16
13
ide-usb-pcb
HRO-TYPE-C-31-M-13


0
16
13
ide-usb-pcb
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm
HTSSOP, 20 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF U20E-1), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
23
21
ide-usb-pcb
LGA-8_6x8mm_P1.25mm
LGA-8
lga land grid array
0
8
8
ide-usb-pcb
Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm
Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package
SMD SMT crystal oscillator
0
4
4
ide-usb-pcb
TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm
TSSOP, 24 Pin (https://www.st.com/resource/en/datasheet/led1642gw.pdf#page=37), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
31
25
ide-usb-pcb
TXS0108E_breakout


0
20
20
ide-usb-pcb
microSD_HC_Hirose_DM3AT-SF-PEJM5
Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)
Micro SD
0
14
11
ide-usb-pcb
microSD_TF-015
Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)
Micro SD
0
13
10
