
Add on board for ABC80/80X to make it possbile for WiFi, BLE etc.

Based on a Intel FPGA for connecting to the ABC bus and an ESP32-S2 module for WiFi and BLE connectivity  


max80 (https://git.sweproj.com/ABC80/max80) contains the design files

This design is licensed under the CERN Open Hardware License -

Permissive version 2 or later.

The source repository for this can be found at:

https://git.sweproj.com/ABC80/max80

© 2021 Per Mårtensson, H Peter Anvin - All Rights Reserved

----

This source describes Open Hardware and is licensed under the CERN-OHL-P
v2

You may redistribute and modify this documentation and make products

using it under the terms of the CERN-OHL-P v2 (https:/cern.ch/cern-ohl).

This documentation is distributed WITHOUT ANY EXPRESS OR IMPLIED

WARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY QUALITY

AND FITNESS FOR A PARTICULAR PURPOSE. Please see the CERN-OHL-P v2

for applicable conditions
