(export (version D)
  (design
    (source /home/pm/project/abc80/max80/max80.sch)
    (date "lör 20 nov 2021 13:21:30")
    (tool "Eeschema 5.99.0+really5.1.10+dfsg1-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source max80.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /abc80bus/) (tstamps /6013B380/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.02)
        (date 2021-11-07)
        (source abc80bus.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /POWER/) (tstamps /6013A59C/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source power.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /ESP32/) (tstamps /602159BB/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source esp32.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /RTC/) (tstamps /6023577B/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source rtc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /ADAPTER_CONN/) (tstamps /60B94961/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source adapter_conn.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name "/Power FPGA/") (tstamps /604B2191/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source power_fpga.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /HDMI/) (tstamps /650A9AE9/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source HDMI.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /USB/) (tstamps /601569F0/)
      (title_block
        (title MAX80)
        (company "Peter o Per")
        (rev 0.01)
        (date 2021-02-22)
        (source usb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref OSC1)
      (value "EPSON Q33310 48 MHz")
      (footprint max80:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm)
      (fields
        (field (name LCSC) C32533))
      (libsource (lib Oscillator) (part ASE-xxxMHz) (description "3.3V CMOS SMD Crystal Clock Oscillator, Abracon"))
      (sheetpath (names /) (tstamps /))
      (tstamp 57BABF34))
    (comp (ref J3)
      (value "Micro_SD_Card DM3AT-SF-PEJM5")
      (footprint max80:microSD_HC_Hirose_DM3AT-SF-PEJM5)
      (datasheet http://katalog.we-online.de/em/datasheet/693072010801.pdf)
      (fields
        (field (name LCSC) C114218))
      (libsource (lib Connector) (part Micro_SD_Card_Det_Hirose_DM3AT) (description "Micro SD Card Socket with card detection pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6022B125))
    (comp (ref C48)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602D0725))
    (comp (ref C49)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602D360C))
    (comp (ref C51)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C19666))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60B62C42))
    (comp (ref D17)
      (value LED-Y)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72038))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6068751D))
    (comp (ref R29)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6068836E))
    (comp (ref D22)
      (value LED-G)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72043))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606A9A91))
    (comp (ref R30)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606A9C22))
    (comp (ref D23)
      (value LED-B)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72041))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606B64A5))
    (comp (ref R31)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606B666A))
    (comp (ref C56)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6091A70C))
    (comp (ref C46)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60932F0E))
    (comp (ref C45)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6094CE83))
    (comp (ref C34)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6097D4FE))
    (comp (ref C33)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60997E09))
    (comp (ref U13)
      (value EP4CE15F17C8N)
      (footprint Package_BGA:BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD)
      (libsource (lib max80) (part EP4CE15F17C8N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6055A8B6))
    (comp (ref R38)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604A56EE))
    (comp (ref R14)
      (value 4.7k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25900))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60A915FC))
    (comp (ref R12)
      (value 4.7k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25900))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60A90B03))
    (comp (ref R40)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 605E3046))
    (comp (ref R39)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 605E3051))
    (comp (ref R42)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60654523))
    (comp (ref R41)
      (value 25)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 607B9EC1))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6082407C))
    (comp (ref U7)
      (value W25Q128JVS)
      (footprint max80:SOIC-8_5.23x5.23mm_P1.27mm)
      (datasheet http://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf)
      (fields
        (field (name LCSC) C97521))
      (libsource (lib Memory_Flash) (part W25Q128JVS) (description "128Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6035B91A))
    (comp (ref R37)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603DBC0D))
    (comp (ref R13)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603E59B4))
    (comp (ref U6)
      (value MT48LC16M16A2P-6A)
      (footprint Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm)
      (datasheet https://www.mouser.se/datasheet/2/671/256Mb_sdr-1282350.pdf)
      (fields
        (field (name LCSC) C41881))
      (libsource (lib max80) (part MT48LC16M16A2P-6A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 604F9283))
    (comp (ref R24)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 66F72E4D))
    (comp (ref D4)
      (value 1N5819W)
      (footprint Diode_SMD:D_SOD-123)
      (datasheet ~)
      (fields
        (field (name LCSC) C963381))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60D15E22))
    (comp (ref D7)
      (value 1N5819W)
      (footprint Diode_SMD:D_SOD-123)
      (datasheet ~)
      (fields
        (field (name LCSC) C963381))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60D4872C))
    (comp (ref D6)
      (value 1N5819W)
      (footprint Diode_SMD:D_SOD-123)
      (datasheet ~)
      (fields
        (field (name LCSC) C963381))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60D4963D))
    (comp (ref D5)
      (value 1N5819W)
      (footprint Diode_SMD:D_SOD-123)
      (datasheet ~)
      (fields
        (field (name LCSC) C963381))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60E7A93B))
    (comp (ref C83)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60FC8574))
    (comp (ref R22)
      (value 100k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25741))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 612BA053))
    (comp (ref R23)
      (value 100k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25741))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 612BA99E))
    (comp (ref Q3)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6032D111))
    (comp (ref Q2)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 603658C4))
    (comp (ref X1)
      (value ABC-Bus)
      (footprint max80:MAB64B)
      (libsource (lib max80) (part ABC-Bus) (description ""))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6011F2D2))
    (comp (ref Q4)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60285B62))
    (comp (ref J1)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 603FB6A3))
    (comp (ref D28)
      (value MBRA340T)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (fields
        (field (name LCSC) C26178))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 603612AB))
    (comp (ref C3)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60EF0ABB))
    (comp (ref U3)
      (value 74HC245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (fields
        (field (name LCSC) C126198))
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 61F93DEE))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 62149379))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 62157028))
    (comp (ref U5)
      (value 74HC245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (fields
        (field (name LCSC) C126198))
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 624CCCE1))
    (comp (ref U4)
      (value 74HC245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (fields
        (field (name LCSC) C126198))
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6208BF8B))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6270830F))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 627085BD))
    (comp (ref U14)
      (value 74HC245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (fields
        (field (name LCSC) C126198))
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6277D5D4))
    (comp (ref Q5)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 66CDB068))
    (comp (ref Q1)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 66D2EFA8))
    (comp (ref Q6)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) NM))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6042861D))
    (comp (ref R25)
      (value 5.1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25905))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6049E6B8))
    (comp (ref J7)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 609B79F6))
    (comp (ref U2)
      (value 74HC245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74HC245)
      (fields
        (field (name LCSC) C126198))
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 6202F2F5))
    (comp (ref R26)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B354D0))
    (comp (ref R27)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B36F20))
    (comp (ref R28)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B37C47))
    (comp (ref R43)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B38966))
    (comp (ref R45)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B3A85D))
    (comp (ref R44)
      (value 100)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C17408))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60B3CF12))
    (comp (ref J6)
      (value Conn_01x01_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x01_Male) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 60CC7EFE))
    (comp (ref X2)
      (value ABC-Bus)
      (footprint max80:FAB64B)
      (libsource (lib max80) (part ABC-Bus) (description ""))
      (sheetpath (names /abc80bus/) (tstamps /6013B380/))
      (tstamp 61C9828F))
    (comp (ref C61)
      (value 220uF)
      (footprint Capacitor_SMD:CP_Elec_6.3x7.7)
      (datasheet ~)
      (fields
        (field (name LCSC) C127327))
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /POWER/) (tstamps /6013A59C/))
      (tstamp 602A7E22))
    (comp (ref C60)
      (value 220uF)
      (footprint Capacitor_SMD:CP_Elec_6.3x7.7)
      (datasheet ~)
      (fields
        (field (name LCSC) C127327))
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /POWER/) (tstamps /6013A59C/))
      (tstamp 602A83A7))
    (comp (ref F2)
      (value "Polyfuse 1.8A")
      (footprint max80:Fuse_1206_3216Metric)
      (datasheet https://datasheet.lcsc.com/szlcsc/1811141110_TECHFUSE-nSMD020-30V_C69680.pdf)
      (fields
        (field (name LCSC) C70082))
      (libsource (lib Device) (part Polyfuse) (description "Resettable fuse, polymeric positive temperature coefficient"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 610EE853))
    (comp (ref USB2)
      (value HRO-TYPE-C-31-M-12)
      (footprint max80:HRO-TYPE-C-31-M-12)
      (datasheet https://datasheet.lcsc.com/szlcsc/1811131825_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.pdf)
      (fields
        (field (name LCSC) C165948))
      (libsource (lib max80) (part HRO-TYPE-C-31-M-12) (description ""))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 610EE858))
    (comp (ref R4)
      (value 5.1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25905))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 5E79F20F))
    (comp (ref C52)
      (value 1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C28323))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 5E7FEAC9))
    (comp (ref U11)
      (value ESP32-S2-WROVER-I)
      (footprint max80:ESP32-S2-WROVER)
      (datasheet https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf)
      (libsource (lib RF_Module) (part ESP32-S2-WROVER-I) (description "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 610EDBDA))
    (comp (ref R3)
      (value 5.1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25905))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 61104569))
    (comp (ref C54)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C45783))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611262EE))
    (comp (ref C55)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 61126FC2))
    (comp (ref C53)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 6112E6F3))
    (comp (ref R19)
      (value 4.7k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25900))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611AB901))
    (comp (ref R20)
      (value 4.7k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25900))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611ABCC5))
    (comp (ref D1)
      (value LED-Y)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72038))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611B5A79))
    (comp (ref R16)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611B7173))
    (comp (ref R17)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611B7E9F))
    (comp (ref R18)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611B8401))
    (comp (ref D2)
      (value LED-G)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72043))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611D1925))
    (comp (ref R21)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 613A0F9D))
    (comp (ref D27)
      (value MBRA340T)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (fields
        (field (name LCSC) C26178))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 6032D6A5))
    (comp (ref R15)
      (value 1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611331F0))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 60379925))
    (comp (ref D3)
      (value LED-B)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72041))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 611D1F01))
    (comp (ref U15)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (fields
        (field (name LCSC) C7519))
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (sheetpath (names /ESP32/) (tstamps /602159BB/))
      (tstamp 610EE85E))
    (comp (ref U12)
      (value DS3231M+)
      (footprint Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm)
      (datasheet http://datasheets.maximintegrated.com/en/ds/DS3231M.pdf)
      (fields
        (field (name LCSC) C37663))
      (libsource (lib Timer_RTC) (part DS3231M) (description "Extremely Accurate I2C-Integrated RTC/TCXO/Crystal SOIC-16"))
      (sheetpath (names /RTC/) (tstamps /6023577B/))
      (tstamp 60239074))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint max80:BatteryHolder_Keystone_103_1x20mm)
      (datasheet ~)
      (fields
        (field (name LCSC) C238065))
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /RTC/) (tstamps /6023577B/))
      (tstamp 6023A838))
    (comp (ref C47)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /RTC/) (tstamps /6023577B/))
      (tstamp 6023B210))
    (comp (ref R9)
      (value 6.2k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25915))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /RTC/) (tstamps /6023577B/))
      (tstamp 6170570B))
    (comp (ref R32)
      (value 6.2k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25915))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /RTC/) (tstamps /6023577B/))
      (tstamp 61706B6D))
    (comp (ref J4)
      (value Conn_02x20_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /ADAPTER_CONN/) (tstamps /60B94961/))
      (tstamp 60B95FED))
    (comp (ref J8)
      (value Conn_02x5_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /ADAPTER_CONN/) (tstamps /60B94961/))
      (tstamp 6100C1FE))
    (comp (ref R49)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ADAPTER_CONN/) (tstamps /60B94961/))
      (tstamp 612EA5C6))
    (comp (ref R50)
      (value 10k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /ADAPTER_CONN/) (tstamps /60B94961/))
      (tstamp 612EABC3))
    (comp (ref C8)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65761895))
    (comp (ref C10)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6576482F))
    (comp (ref C11)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6576514E))
    (comp (ref C12)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65765AAD))
    (comp (ref C13)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65766122))
    (comp (ref C14)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65768E03))
    (comp (ref C15)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65769634))
    (comp (ref C9)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6576B192))
    (comp (ref C1)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65824DAA))
    (comp (ref C17)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65825077))
    (comp (ref C18)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65825082))
    (comp (ref C19)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6582508D))
    (comp (ref C20)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65825098))
    (comp (ref C21)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6584E8B0))
    (comp (ref C22)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6584EC09))
    (comp (ref C23)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6584EC1E))
    (comp (ref C24)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6584EC29))
    (comp (ref C27)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 6584EC4A))
    (comp (ref C26)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65AC4F8F))
    (comp (ref C30)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B1E160))
    (comp (ref C29)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B1E57B))
    (comp (ref C31)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B40618))
    (comp (ref C32)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B6444F))
    (comp (ref C42)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B648D0))
    (comp (ref C41)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B648DB))
    (comp (ref C43)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65B648F2))
    (comp (ref C44)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C6F7D3))
    (comp (ref C50)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C7267E))
    (comp (ref C62)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C73D10))
    (comp (ref C63)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C7591B))
    (comp (ref C66)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C78210))
    (comp (ref C28)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C52923))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65AC4DDD))
    (comp (ref C16)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65ECAF24))
    (comp (ref C25)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65ECB133))
    (comp (ref C68)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65ECB13E))
    (comp (ref C69)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65ECB149))
    (comp (ref C59)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 65C7321F))
    (comp (ref U1)
      (value AMS1117-1.2)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (fields
        (field (name LCSC) C14529))
      (libsource (lib Regulator_Linear) (part AMS1117-1.5) (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672CD418))
    (comp (ref U16)
      (value AMS1117-2.5)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (fields
        (field (name LCSC) C347221))
      (libsource (lib Regulator_Linear) (part AMS1117-2.5) (description "1A Low Dropout regulator, positive, 2.5V fixed output, SOT-223"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672CF238))
    (comp (ref C67)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672F37BB))
    (comp (ref C72)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672F463E))
    (comp (ref C64)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672F65A1))
    (comp (ref C74)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672F7260))
    (comp (ref C70)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672FA54F))
    (comp (ref C65)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 672FAB10))
    (comp (ref C71)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 67326D2C))
    (comp (ref C73)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 67327311))
    (comp (ref U8)
      (value AMS1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.advanced-monolithic.com/pdf/ds1117.pdf)
      (fields
        (field (name LCSC) C351784))
      (libsource (lib Regulator_Linear) (part AMS1117-3.3) (description "1A Low Dropout regulator, positive, 3.3V fixed output, SOT-223"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 615F4429))
    (comp (ref C36)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 615F4910))
    (comp (ref C35)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 615F491B))
    (comp (ref C37)
      (value 47uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C140782))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 615F4926))
    (comp (ref C38)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power FPGA/") (tstamps /604B2191/))
      (tstamp 615F4931))
    (comp (ref R2)
      (value 2.2k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25879))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 655D07B0))
    (comp (ref R11)
      (value 2.2k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25879))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 655D0BC8))
    (comp (ref C80)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA18DB))
    (comp (ref C81)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA22EE))
    (comp (ref C82)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA28B1))
    (comp (ref C76)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA3BB6))
    (comp (ref C75)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA3EFB))
    (comp (ref C77)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA423E))
    (comp (ref C79)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA4621))
    (comp (ref C78)
      (value 100nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60FA49FC))
    (comp (ref Q7)
      (value AO3400A)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf)
      (fields
        (field (name LCSC) C20917))
      (libsource (lib Transistor_FET) (part AO3400A) (description "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60E31564))
    (comp (ref R47)
      (value 2.2k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25879))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60E3BB83))
    (comp (ref R46)
      (value 12.7k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25752))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 60E40DE0))
    (comp (ref J2)
      (value HDMI_A)
      (footprint sm6uax:HDMI_A_Amphenol_10029449-111)
      (datasheet https://en.wikipedia.org/wiki/HDMI)
      (libsource (lib Connector) (part HDMI_A) (description "HDMI type A connector"))
      (sheetpath (names /HDMI/) (tstamps /650A9AE9/))
      (tstamp 61917A74))
    (comp (ref R6)
      (value 5.1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25905))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 61148F19))
    (comp (ref R5)
      (value 5.1k)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25905))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 6114B27A))
    (comp (ref USB1)
      (value HRO-TYPE-C-31-M-12)
      (footprint max80:HRO-TYPE-C-31-M-12)
      (datasheet https://datasheet.lcsc.com/szlcsc/1811131825_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.pdf)
      (fields
        (field (name LCSC) C165948))
      (libsource (lib max80) (part HRO-TYPE-C-31-M-12) (description ""))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 6114CF45))
    (comp (ref U9)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (fields
        (field (name LCSC) C7519))
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 6114F91C))
    (comp (ref F1)
      (value "Polyfuse 1.8A")
      (footprint max80:Fuse_1206_3216Metric)
      (datasheet https://datasheet.lcsc.com/szlcsc/1811141110_TECHFUSE-nSMD020-30V_C69680.pdf)
      (fields
        (field (name LCSC) C70082))
      (libsource (lib Device) (part Polyfuse) (description "Resettable fuse, polymeric positive temperature coefficient"))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 611529F7))
    (comp (ref C39)
      (value 1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C28323))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 61154A99))
    (comp (ref C40)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C15850))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 61156BD2))
    (comp (ref D19)
      (value MBRA340T)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (fields
        (field (name LCSC) C26178))
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 60325B03))
    (comp (ref R7)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C22966))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 6258957D))
    (comp (ref R8)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C22966))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 62589F2A))
    (comp (ref R10)
      (value 1.5k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C22843Copy))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /601569F0/))
      (tstamp 61BA625A)))
  (libparts
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib Connector) (part Conn_01x01_Male)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part HDMI_A)
      (description "HDMI type A connector")
      (docs https://en.wikipedia.org/wiki/HDMI)
      (footprints
        (fp HDMI*A*))
      (fields
        (field (name Reference) J)
        (field (name Value) HDMI_A))
      (pins
        (pin (num 1) (name D2+) (type passive))
        (pin (num 2) (name D2S) (type power_in))
        (pin (num 3) (name D2-) (type passive))
        (pin (num 4) (name D1+) (type passive))
        (pin (num 5) (name D1S) (type power_in))
        (pin (num 6) (name D1-) (type passive))
        (pin (num 7) (name D0+) (type passive))
        (pin (num 8) (name D0S) (type power_in))
        (pin (num 9) (name D0-) (type passive))
        (pin (num 10) (name CK+) (type passive))
        (pin (num 11) (name CKS) (type power_in))
        (pin (num 12) (name CK-) (type passive))
        (pin (num 13) (name CEC) (type BiDi))
        (pin (num 14) (name UTILITY) (type passive))
        (pin (num 15) (name SCL) (type passive))
        (pin (num 16) (name SDA) (type BiDi))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name +5V) (type power_in))
        (pin (num 19) (name HPD) (type passive))
        (pin (num SH) (name SH) (type passive))))
    (libpart (lib Connector) (part Micro_SD_Card_Det)
      (aliases
        (alias Micro_SD_Card_Det_Hirose_DM3AT))
      (description "Micro SD Card Socket with card detection pins")
      (docs https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1)
      (footprints
        (fp microSD*))
      (fields
        (field (name Reference) J)
        (field (name Value) Micro_SD_Card_Det))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type input))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type BiDi))
        (pin (num 8) (name DAT1) (type BiDi))
        (pin (num 9) (name DET_B) (type passive))
        (pin (num 10) (name DET_A) (type passive))
        (pin (num 11) (name SHIELD) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP_Small)
      (description "Polarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Polyfuse)
      (description "Resettable fuse, polymeric positive temperature coefficient")
      (docs ~)
      (footprints
        (fp *polyfuse*)
        (fp *PTC*))
      (fields
        (field (name Reference) F)
        (field (name Value) Polyfuse))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Memory_Flash) (part W25Q32JVSS)
      (aliases
        (alias W25Q128JVS))
      (description "32Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8")
      (docs http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf)
      (footprints
        (fp SOIC*5.23x5.23mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) W25Q32JVSS)
        (field (name Footprint) Package_SO:SOIC-8_5.23x5.23mm_P1.27mm))
      (pins
        (pin (num 1) (name ~CS) (type input))
        (pin (num 2) (name "DO(IO1)") (type BiDi))
        (pin (num 3) (name IO2) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name "DI(IO0)") (type BiDi))
        (pin (num 6) (name CLK) (type input))
        (pin (num 7) (name IO3) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Oscillator) (part ASE-xxxMHz)
      (description "3.3V CMOS SMD Crystal Clock Oscillator, Abracon")
      (docs http://www.abracon.com/Oscillators/ASV.pdf)
      (footprints
        (fp Oscillator*SMD*Abracon*ASE*3.2x2.5mm*))
      (fields
        (field (name Reference) X)
        (field (name Value) ASE-xxxMHz)
        (field (name Footprint) Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name Vdd) (type power_in))))
    (libpart (lib Power_Protection) (part USBLC6-2SC6)
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (docs https://www.st.com/resource/en/datasheet/usblc6-2.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2SC6)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name I/O1) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name I/O2) (type passive))
        (pin (num 4) (name I/O2) (type passive))
        (pin (num 5) (name VBUS) (type passive))
        (pin (num 6) (name I/O1) (type passive))))
    (libpart (lib RF_Module) (part ESP32-S2-WROVER)
      (aliases
        (alias ESP32-S2-WROVER-I))
      (description "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, 32-bit, 2.7-3.6V, onboard antenna, SMD")
      (docs https://www.espressif.com/sites/default/files/documentation/esp32-s2-wroom_esp32-s2-wroom-i_datasheet_en.pdf)
      (footprints
        (fp ESP32?S2?WROVER*))
      (fields
        (field (name Reference) U)
        (field (name Value) ESP32-S2-WROVER)
        (field (name Footprint) RF_Module:ESP32-S2-WROVER))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name 3V3) (type power_in))
        (pin (num 3) (name IO00) (type BiDi))
        (pin (num 4) (name IO01) (type BiDi))
        (pin (num 5) (name IO02) (type BiDi))
        (pin (num 6) (name IO03) (type BiDi))
        (pin (num 7) (name IO04) (type BiDi))
        (pin (num 8) (name IO05) (type BiDi))
        (pin (num 9) (name IO06) (type BiDi))
        (pin (num 10) (name IO07) (type BiDi))
        (pin (num 11) (name IO08) (type BiDi))
        (pin (num 12) (name IO09) (type BiDi))
        (pin (num 13) (name IO10) (type BiDi))
        (pin (num 14) (name IO11) (type BiDi))
        (pin (num 15) (name IO12) (type BiDi))
        (pin (num 16) (name IO13) (type BiDi))
        (pin (num 17) (name IO14) (type BiDi))
        (pin (num 18) (name IO15) (type BiDi))
        (pin (num 19) (name IO16) (type BiDi))
        (pin (num 20) (name IO17) (type BiDi))
        (pin (num 21) (name IO18) (type BiDi))
        (pin (num 22) (name USB_D-) (type BiDi))
        (pin (num 23) (name USB_D+) (type BiDi))
        (pin (num 24) (name IO21) (type BiDi))
        (pin (num 25) (name IO26) (type BiDi))
        (pin (num 26) (name GND) (type passive))
        (pin (num 27) (name IO33) (type BiDi))
        (pin (num 28) (name IO34) (type BiDi))
        (pin (num 29) (name IO35) (type BiDi))
        (pin (num 30) (name IO36) (type BiDi))
        (pin (num 31) (name IO37) (type BiDi))
        (pin (num 32) (name IO38) (type BiDi))
        (pin (num 33) (name IO39) (type BiDi))
        (pin (num 34) (name IO40) (type BiDi))
        (pin (num 35) (name IO41) (type BiDi))
        (pin (num 36) (name IO42) (type BiDi))
        (pin (num 37) (name TXD0) (type BiDi))
        (pin (num 38) (name RXD0) (type BiDi))
        (pin (num 39) (name IO45) (type BiDi))
        (pin (num 40) (name IO46) (type input))
        (pin (num 41) (name EN) (type input))
        (pin (num 42) (name GND) (type passive))
        (pin (num 43) (name GND) (type passive))))
    (libpart (lib Regulator_Linear) (part AP1117-15)
      (aliases
        (alias AP1117-18)
        (alias AP1117-25)
        (alias AP1117-33)
        (alias AP1117-50)
        (alias LD1117S33TR_SOT223)
        (alias LD1117S12TR_SOT223)
        (alias LD1117S18TR_SOT223)
        (alias LD1117S25TR_SOT223)
        (alias LD1117S50TR_SOT223)
        (alias NCP1117-12_SOT223)
        (alias NCP1117-1.5_SOT223)
        (alias NCP1117-1.8_SOT223)
        (alias NCP1117-2.0_SOT223)
        (alias NCP1117-2.5_SOT223)
        (alias NCP1117-2.85_SOT223)
        (alias NCP1117-3.3_SOT223)
        (alias NCP1117-5.0_SOT223)
        (alias AMS1117-1.5)
        (alias AMS1117-1.8)
        (alias AMS1117-2.5)
        (alias AMS1117-2.85)
        (alias AMS1117-3.3)
        (alias AMS1117-5.0))
      (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT?223*TabPin2*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117-15)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-223-3_TabPin2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Timer_RTC) (part DS3231M)
      (description "Extremely Accurate I2C-Integrated RTC/TCXO/Crystal SOIC-16")
      (docs http://datasheets.maximintegrated.com/en/ds/DS3231.pdf)
      (footprints
        (fp SOIC*7.5x10.3mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) DS3231M)
        (field (name Footprint) Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm))
      (pins
        (pin (num 1) (name 32KHZ) (type openCol))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name ~INT~/SQW) (type openCol))
        (pin (num 4) (name ~RST) (type BiDi))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name GND) (type passive))
        (pin (num 7) (name GND) (type passive))
        (pin (num 8) (name GND) (type passive))
        (pin (num 9) (name GND) (type passive))
        (pin (num 10) (name GND) (type passive))
        (pin (num 11) (name GND) (type passive))
        (pin (num 12) (name GND) (type passive))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name VBAT) (type power_in))
        (pin (num 15) (name SDA) (type BiDi))
        (pin (num 16) (name SCL) (type input))))
    (libpart (lib Transistor_FET) (part BSS138)
      (aliases
        (alias 2N7002)
        (alias 2N7002E)
        (alias 2N7002H)
        (alias 2N7002K)
        (alias BS170F)
        (alias BS870)
        (alias BSN20)
        (alias BSS123)
        (alias BSS127S)
        (alias DMG2302U)
        (alias DMG3402L)
        (alias DMG3404L)
        (alias DMG3406L)
        (alias DMG3414U)
        (alias DMG3418L)
        (alias DMN10H220L)
        (alias DMN10H700S)
        (alias DMN13H750S)
        (alias DMN2041L)
        (alias DMN2050L)
        (alias DMN2056U)
        (alias DMN2058U)
        (alias DMN2075U)
        (alias DMN2230U)
        (alias DMN24H11DS)
        (alias DMN24H3D5L)
        (alias DMN3042L)
        (alias DMN3051L)
        (alias DMN30H4D0L)
        (alias DMN3110S)
        (alias DMN3150L)
        (alias DMN3300U)
        (alias DMN3404L)
        (alias DMN6075S)
        (alias DMN6140L)
        (alias DMN67D7L)
        (alias DMN67D8L)
        (alias MMBF170)
        (alias VN10LF)
        (alias ZVN3306F)
        (alias ZVN3310F)
        (alias ZVN3320F)
        (alias ZVN4106F)
        (alias ZXM61N02F)
        (alias ZXM61N03F)
        (alias ZXMN10A07F)
        (alias ZXMN2A01F)
        (alias ZXMN2A14F)
        (alias ZXMN2B01F)
        (alias ZXMN2B14FH)
        (alias ZXMN2F30FH)
        (alias ZXMN2F34FH)
        (alias ZXMN3A01F)
        (alias ZXMN3A14F)
        (alias ZXMN3B01F)
        (alias ZXMN3B14F)
        (alias ZXMN3F30FH)
        (alias ZXMN6A07F)
        (alias IRLML0030)
        (alias IRLML2060)
        (alias TSM2302CX)
        (alias AO3400A))
      (description "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23")
      (docs https://www.onsemi.com/pub/Collateral/BSS138-D.PDF)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BSS138)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib max80) (part ABC-Bus)
      (fields
        (field (name Reference) X)
        (field (name Value) ABC-Bus)
        (field (name Footprint) sm6uax:MAB64B-FAB64Q))
      (pins
        (pin (num A1) (name -12V) (type power_out))
        (pin (num A2) (name 0V) (type power_out))
        (pin (num A3) (name ~RESIN) (type BiDi))
        (pin (num A4) (name GND) (type power_out))
        (pin (num A5) (name ~XMEMW) (type BiDi))
        (pin (num A6) (name D7) (type BiDi))
        (pin (num A7) (name D6) (type BiDi))
        (pin (num A8) (name D5) (type BiDi))
        (pin (num A9) (name D4) (type BiDi))
        (pin (num A10) (name D3) (type BiDi))
        (pin (num A11) (name D2) (type BiDi))
        (pin (num A12) (name D1) (type BiDi))
        (pin (num A13) (name D0) (type BiDi))
        (pin (num A14) (name NC) (type passive))
        (pin (num A15) (name ~RST) (type BiDi))
        (pin (num A16) (name ~STATUS) (type BiDi))
        (pin (num A17) (name ~INP) (type BiDi))
        (pin (num A18) (name ~C4) (type BiDi))
        (pin (num A19) (name ~C3) (type BiDi))
        (pin (num A20) (name ~C2) (type BiDi))
        (pin (num A21) (name ~C1) (type BiDi))
        (pin (num A22) (name ~OUT) (type BiDi))
        (pin (num A23) (name ~CS) (type BiDi))
        (pin (num A24) (name GND) (type power_out))
        (pin (num A25) (name GND) (type power_out))
        (pin (num A26) (name GND) (type power_out))
        (pin (num A27) (name GND) (type power_out))
        (pin (num A28) (name GND) (type power_out))
        (pin (num A29) (name GND) (type power_out))
        (pin (num A30) (name READY) (type BiDi))
        (pin (num A31) (name +5V) (type power_out))
        (pin (num A32) (name +12V) (type power_out))
        (pin (num B1) (name -12V) (type power_out))
        (pin (num B2) (name 0V) (type power_out))
        (pin (num B3) (name GND) (type power_out))
        (pin (num B4) (name ~XMEMFL) (type BiDi))
        (pin (num B5) (name 5) (type passive))
        (pin (num B6) (name GND) (type power_out))
        (pin (num B7) (name GND) (type power_out))
        (pin (num B8) (name GND) (type power_out))
        (pin (num B9) (name GND) (type power_out))
        (pin (num B10) (name GND) (type power_out))
        (pin (num B11) (name GND) (type power_out))
        (pin (num B12) (name GND) (type power_out))
        (pin (num B13) (name ~INT) (type BiDi))
        (pin (num B14) (name A15) (type BiDi))
        (pin (num B15) (name A14) (type BiDi))
        (pin (num B16) (name A13) (type BiDi))
        (pin (num B17) (name A12) (type BiDi))
        (pin (num B18) (name A11) (type BiDi))
        (pin (num B19) (name A10) (type BiDi))
        (pin (num B20) (name A9) (type BiDi))
        (pin (num B21) (name A8) (type BiDi))
        (pin (num B22) (name A7) (type BiDi))
        (pin (num B23) (name A6) (type BiDi))
        (pin (num B24) (name A5) (type BiDi))
        (pin (num B25) (name A4) (type BiDi))
        (pin (num B26) (name A3) (type BiDi))
        (pin (num B27) (name A2) (type BiDi))
        (pin (num B28) (name A1) (type BiDi))
        (pin (num B29) (name A0) (type BiDi))
        (pin (num B30) (name NC) (type passive))
        (pin (num B31) (name +5V) (type power_out))
        (pin (num B32) (name +12V) (type power_out))))
    (libpart (lib max80) (part EP4CE15F17C8N)
      (fields
        (field (name Reference) U)
        (field (name Value) EP4CE15F17C8N))
      (pins
        (pin (num A1) (name VCCIO8) (type power_in))
        (pin (num A2) (name VREFB8N1_B8) (type BiDi))
        (pin (num A3) (name DIFFIO_T2n_B8) (type BiDi))
        (pin (num A4) (name DIFFIO_T3n/DATA10_B8) (type BiDi))
        (pin (num A5) (name IO/DATA7_B8) (type BiDi))
        (pin (num A6) (name DIFFIO_T9n/DATA14_B8) (type BiDi))
        (pin (num A7) (name DIFFIO_T11n/PADD18_B8) (type BiDi))
        (pin (num A8) (name DIFFCLK_4n_B8) (type BiDi))
        (pin (num A9) (name DIFFCLK_5n_B7) (type BiDi))
        (pin (num A10) (name DIFFIO_T20n/PADD5_B7) (type BiDi))
        (pin (num A11) (name DIFFIO_T25n/PADD1_B7) (type BiDi))
        (pin (num A12) (name DIFFIO_T27p/PADD0_B7) (type BiDi))
        (pin (num A13) (name VREFB7N1_B7) (type BiDi))
        (pin (num A14) (name PLL2_CLKOUTn_B7) (type BiDi))
        (pin (num A15) (name DIFFIO_T23n/PADD3_B7) (type BiDi))
        (pin (num A16) (name VCCIO7) (type power_in))
        (pin (num B1) (name DIFFIO_L3p_B1) (type BiDi))
        (pin (num B2) (name GND) (type power_in))
        (pin (num B3) (name DIFFIO_T2p/DATA12_B8) (type BiDi))
        (pin (num B4) (name DIFFIO_T3p/DATA11_B8) (type BiDi))
        (pin (num B5) (name DIFFIO_T5p/DATA8_B8) (type BiDi))
        (pin (num B6) (name DIFFIO_T9p/DATA13_B8) (type BiDi))
        (pin (num B7) (name DIFFIO_T11p/DATA4_B8) (type BiDi))
        (pin (num B8) (name DIFFCLK_4p_B8) (type BiDi))
        (pin (num B9) (name DIFFCLK_5p_B7) (type BiDi))
        (pin (num B10) (name DIFFIO_T20p/PADD6_B7) (type BiDi))
        (pin (num B11) (name DIFFIO_T25p/PADD2_B7) (type BiDi))
        (pin (num B12) (name DIFFIO_T26n_B7) (type BiDi))
        (pin (num B13) (name DIFFIO_T29n_B7) (type BiDi))
        (pin (num B14) (name PLL2_CLKOUTp_B7) (type BiDi))
        (pin (num B15) (name GND) (type power_in))
        (pin (num B16) (name DIFFIO_R15n_B6) (type BiDi))
        (pin (num C1) (name DIFFIO_L4n/DATA1,ASDO_B1) (type BiDi))
        (pin (num C2) (name DIFFIO_L4p_B1) (type BiDi))
        (pin (num C3) (name PLL3_CLKOUTn_B8) (type BiDi))
        (pin (num C4) (name VCCIO8) (type power_in))
        (pin (num C5) (name GND) (type power_in))
        (pin (num C6) (name VREFB8N0_B8) (type BiDi))
        (pin (num C7) (name VCCIO8) (type power_in))
        (pin (num C8) (name DIFFIO_T13p/PADD17_B8) (type BiDi))
        (pin (num C9) (name DIFFIO_T19n/PADD7_B7) (type BiDi))
        (pin (num C10) (name VCCIO7) (type power_in))
        (pin (num C11) (name VREFB7N0_B7) (type BiDi))
        (pin (num C12) (name GND) (type power_in))
        (pin (num C13) (name VCCIO7) (type power_in))
        (pin (num C14) (name DIFFIO_T32n_B7) (type BiDi))
        (pin (num C15) (name DIFFIO_R2p_B6) (type BiDi))
        (pin (num C16) (name DIFFIO_R2n/PADD20_B6) (type BiDi))
        (pin (num D1) (name DIFFIO_L6n_B1) (type BiDi))
        (pin (num D2) (name DIFFIO_L6p/FLASH_nCE,nCSO_B1) (type BiDi))
        (pin (num D3) (name PLL3_CLKOUTp_B8) (type BiDi))
        (pin (num D4) (name VCCD_PLL3) (type power_in))
        (pin (num D5) (name IO_B8) (type BiDi))
        (pin (num D6) (name DIFFIO_T4n/DATA9_B8) (type BiDi))
        (pin (num D7) (name GND) (type power_in))
        (pin (num D8) (name IO_B8) (type BiDi))
        (pin (num D9) (name DIFFIO_T19p/PADD8_B7) (type BiDi))
        (pin (num D10) (name GND) (type power_in))
        (pin (num D11) (name DIFFIO_T30n_B7) (type BiDi))
        (pin (num D12) (name DIFFIO_T30p_B7) (type BiDi))
        (pin (num D13) (name VCCD_PLL2) (type power_in))
        (pin (num D14) (name DIFFIO_T32p_B7) (type BiDi))
        (pin (num D15) (name DIFFIO_R7p_B6) (type BiDi))
        (pin (num D16) (name DIFFIO_R7n_B6) (type BiDi))
        (pin (num E1) (name DIFFCLK_0n_B1) (type BiDi))
        (pin (num E2) (name GND) (type power_in))
        (pin (num E3) (name VCCIO1) (type power_in))
        (pin (num E4) (name GND) (type power_in))
        (pin (num E5) (name GNDA3) (type power_in))
        (pin (num E6) (name DIFFIO_T6p/DATA6_B8) (type BiDi))
        (pin (num E7) (name IO/DATA5_B8) (type BiDi))
        (pin (num E8) (name DIFFIO_T12n/DATA2_B8) (type BiDi))
        (pin (num E9) (name DIFFIO_T17p/PADD12_B7) (type BiDi))
        (pin (num E10) (name RDN4_B7) (type BiDi))
        (pin (num E11) (name RUP4_B7) (type BiDi))
        (pin (num E12) (name GNDA2) (type power_in))
        (pin (num E13) (name GND) (type power_in))
        (pin (num E14) (name VCCIO6) (type power_in))
        (pin (num E15) (name DIFFCLK_2p_B6) (type BiDi))
        (pin (num E16) (name DIFFCLK_2n_B6) (type BiDi))
        (pin (num F1) (name DIFFIO_L10n_B1) (type BiDi))
        (pin (num F2) (name DIFFIO_L10p_B1) (type BiDi))
        (pin (num F3) (name VREFB1N0_B1) (type BiDi))
        (pin (num F4) (name nSTATUS_B1) (type BiDi))
        (pin (num F5) (name VCCA3) (type power_in))
        (pin (num F6) (name GND) (type power_in))
        (pin (num F7) (name VCCINT) (type power_in))
        (pin (num F8) (name DIFFIO_T12p/DATA3_B8) (type BiDi))
        (pin (num F9) (name DIFFIO_T21p/PADD4_B7) (type BiDi))
        (pin (num F10) (name GND) (type power_in))
        (pin (num F11) (name VCCINT) (type power_in))
        (pin (num F12) (name VCCA2) (type power_in))
        (pin (num F13) (name VREFB6N1_B6) (type BiDi))
        (pin (num F14) (name VREFB6N0_B6) (type BiDi))
        (pin (num F15) (name DIFFIO_R16p/CLKUSR_B6) (type BiDi))
        (pin (num F16) (name DIFFIO_R16n/nCEO_B6) (type BiDi))
        (pin (num G1) (name VREFB1N1_B1) (type BiDi))
        (pin (num G2) (name IO_B1) (type BiDi))
        (pin (num G3) (name VCCIO1) (type power_in))
        (pin (num G4) (name GND) (type power_in))
        (pin (num G5) (name DIFFIO_L9n_B1) (type BiDi))
        (pin (num G6) (name VCCINT) (type power_in))
        (pin (num G7) (name VCCINT) (type power_in))
        (pin (num G8) (name VCCINT) (type power_in))
        (pin (num G9) (name VCCINT) (type power_in))
        (pin (num G10) (name VCCINT) (type power_in))
        (pin (num G11) (name DIFFIO_R3p/PADD21_B6) (type BiDi))
        (pin (num G12) (name MSEL2_B6) (type BiDi))
        (pin (num G13) (name GND) (type power_in))
        (pin (num G14) (name VCCIO6) (type power_in))
        (pin (num G15) (name DIFFIO_R17p/CRC_ERROR_B6) (type BiDi))
        (pin (num G16) (name DIFFIO_R17n/INIT_DONE_B6) (type BiDi))
        (pin (num H1) (name DCLK_B1) (type BiDi))
        (pin (num H2) (name IO/DATA0_B1) (type BiDi))
        (pin (num H3) (name TCK_B1) (type input))
        (pin (num H4) (name TDI_B1) (type BiDi))
        (pin (num H5) (name nCONFIG_B1) (type BiDi))
        (pin (num H6) (name VCCINT) (type power_in))
        (pin (num H7) (name GND) (type power_in))
        (pin (num H8) (name GND) (type power_in))
        (pin (num H9) (name GND) (type power_in))
        (pin (num H10) (name GND) (type power_in))
        (pin (num H11) (name VCCINT) (type power_in))
        (pin (num H12) (name MSEL1_B6) (type BiDi))
        (pin (num H13) (name MSEL0_B6) (type BiDi))
        (pin (num H14) (name CONF_DONE_B6) (type BiDi))
        (pin (num H15) (name GND) (type power_in))
        (pin (num H16) (name GND) (type power_in))
        (pin (num J1) (name DIFFIO_L14n_B2) (type BiDi))
        (pin (num J2) (name DIFFIO_L14p_B2) (type BiDi))
        (pin (num J3) (name nCE_B1) (type BiDi))
        (pin (num J4) (name TDO_B1) (type BiDi))
        (pin (num J5) (name TMS_B1) (type BiDi))
        (pin (num J6) (name VCCINT) (type power_in))
        (pin (num J7) (name GND) (type power_in))
        (pin (num J8) (name GND) (type power_in))
        (pin (num J9) (name GND) (type power_in))
        (pin (num J10) (name GND) (type power_in))
        (pin (num J11) (name GND) (type power_in))
        (pin (num J12) (name DIFFIO_R19p_B5) (type BiDi))
        (pin (num J13) (name IO_B5) (type BiDi))
        (pin (num J14) (name DIFFIO_R19n_B5) (type BiDi))
        (pin (num J15) (name DIFFIO_R21p/DEV_CLRn_B5) (type BiDi))
        (pin (num J16) (name DIFFIO_R21n/DEV_OE_B5) (type BiDi))
        (pin (num K1) (name DIFFIO_L18n_B2) (type BiDi))
        (pin (num K2) (name VREFB2N1_B2) (type BiDi))
        (pin (num K3) (name VCCIO2) (type power_in))
        (pin (num K4) (name GND) (type power_in))
        (pin (num K5) (name RUP1_B2) (type BiDi))
        (pin (num K6) (name DIFFIO_L16p_B2) (type BiDi))
        (pin (num K7) (name VCCINT) (type power_in))
        (pin (num K8) (name GND) (type power_in))
        (pin (num K9) (name DIFFIO_B19p_B4) (type BiDi))
        (pin (num K10) (name DIFFIO_B24n_B4) (type BiDi))
        (pin (num K11) (name VCCINT) (type power_in))
        (pin (num K12) (name DIFFIO_R35p_B5) (type BiDi))
        (pin (num K13) (name GND) (type power_in))
        (pin (num K14) (name VCCIO5) (type power_in))
        (pin (num K15) (name DIFFIO_R22p_B5) (type BiDi))
        (pin (num K16) (name DIFFIO_R22n_B5) (type BiDi))
        (pin (num L1) (name DIFFIO_L19n_B2) (type BiDi))
        (pin (num L2) (name DIFFIO_L19p_B2) (type BiDi))
        (pin (num L3) (name VREFB2N0_B2) (type BiDi))
        (pin (num L4) (name RDN1_B2) (type BiDi))
        (pin (num L5) (name VCCA1) (type power_in))
        (pin (num L6) (name DIFFIO_L16n_B2) (type BiDi))
        (pin (num L7) (name IO_B3) (type BiDi))
        (pin (num L8) (name IO_B3) (type BiDi))
        (pin (num L9) (name DIFFIO_B19n_B4) (type BiDi))
        (pin (num L10) (name IO_B4) (type BiDi))
        (pin (num L11) (name DIFFIO_B31p_B4) (type BiDi))
        (pin (num L12) (name VCCA4) (type power_in))
        (pin (num L13) (name DIFFIO_R26n_B5) (type BiDi))
        (pin (num L14) (name VREFB5N1_B5) (type BiDi))
        (pin (num L15) (name VREFB5N0_B5) (type BiDi))
        (pin (num L16) (name DIFFIO_R26p_B5) (type BiDi))
        (pin (num M1) (name DIFFCLK_1n_B2) (type BiDi))
        (pin (num M2) (name DIFFCLK_1p_B2) (type BiDi))
        (pin (num M3) (name VCCIO2) (type power_in))
        (pin (num M4) (name GND) (type power_in))
        (pin (num M5) (name GNDA1) (type power_in))
        (pin (num M6) (name DIFFIO_B8p_B3) (type BiDi))
        (pin (num M7) (name IO_B3) (type BiDi))
        (pin (num M8) (name DIFFIO_B18p_B3) (type BiDi))
        (pin (num M9) (name DIFFIO_B20p_B4) (type BiDi))
        (pin (num M10) (name RUP2_B4) (type BiDi))
        (pin (num M11) (name DIFFIO_B31n_B4) (type BiDi))
        (pin (num M12) (name GNDA4) (type power_in))
        (pin (num M13) (name GND) (type power_in))
        (pin (num M14) (name VCCIO5) (type power_in))
        (pin (num M15) (name DIFFCLK_3p_B5) (type BiDi))
        (pin (num M16) (name DIFFCLK_3n_B5) (type BiDi))
        (pin (num N1) (name DIFFIO_L27n_B2) (type BiDi))
        (pin (num N2) (name DIFFIO_L27p_B2) (type BiDi))
        (pin (num N3) (name DIFFIO_B3p_B3) (type BiDi))
        (pin (num N4) (name VCCD_PLL1) (type power_in))
        (pin (num N5) (name DIFFIO_B7p_B3) (type BiDi))
        (pin (num N6) (name DIFFIO_B7n_B3) (type BiDi))
        (pin (num N7) (name GND) (type power_in))
        (pin (num N8) (name DIFFIO_B18n_B3) (type BiDi))
        (pin (num N9) (name DIFFIO_B20n_B4) (type BiDi))
        (pin (num N10) (name GND) (type power_in))
        (pin (num N11) (name RDN2_B4) (type BiDi))
        (pin (num N12) (name VREFB4N1_B4) (type BiDi))
        (pin (num N13) (name VCCD_PLL4) (type power_in))
        (pin (num N14) (name RUP3_B5) (type BiDi))
        (pin (num N15) (name DIFFIO_R31p_B5) (type BiDi))
        (pin (num N16) (name DIFFIO_R31n_B5) (type BiDi))
        (pin (num P1) (name DIFFIO_L29n_B2) (type BiDi))
        (pin (num P2) (name DIFFIO_L29p_B2) (type BiDi))
        (pin (num P3) (name DIFFIO_B3n_B3) (type BiDi))
        (pin (num P4) (name VCCIO3) (type power_in))
        (pin (num P5) (name GND) (type power_in))
        (pin (num P6) (name VREFB3N0_B3) (type BiDi))
        (pin (num P7) (name VCCIO3) (type power_in))
        (pin (num P8) (name IO_B3) (type BiDi))
        (pin (num P9) (name IO_B4) (type BiDi))
        (pin (num P10) (name VCCIO4) (type power_in))
        (pin (num P11) (name VREFB4N0_B4) (type BiDi))
        (pin (num P12) (name GND) (type power_in))
        (pin (num P13) (name VCCIO4) (type power_in))
        (pin (num P14) (name PLL4_CLKOUTp_B4) (type BiDi))
        (pin (num P15) (name RDN3_B5) (type BiDi))
        (pin (num P16) (name DIFFIO_R34n_B5) (type BiDi))
        (pin (num R1) (name IO_B2) (type BiDi))
        (pin (num R2) (name GND) (type power_in))
        (pin (num R3) (name DIFFIO_B4n_B3) (type BiDi))
        (pin (num R4) (name PLL1_CLKOUTp_B3) (type BiDi))
        (pin (num R5) (name DIFFIO_B14p_B3) (type BiDi))
        (pin (num R6) (name DIFFIO_B15p_B3) (type BiDi))
        (pin (num R7) (name DIFFIO_B16p_B3) (type BiDi))
        (pin (num R8) (name DIFFCLK_6p_B3) (type BiDi))
        (pin (num R9) (name DIFFCLK_7p_B4) (type BiDi))
        (pin (num R10) (name DIFFIO_B21p_B4) (type BiDi))
        (pin (num R11) (name DIFFIO_B22p_B4) (type BiDi))
        (pin (num R12) (name DIFFIO_B23p_B4) (type BiDi))
        (pin (num R13) (name DIFFIO_B26p_B4) (type BiDi))
        (pin (num R14) (name PLL4_CLKOUTn_B4) (type BiDi))
        (pin (num R15) (name GND) (type power_in))
        (pin (num R16) (name DIFFIO_R34p_B5) (type BiDi))
        (pin (num T1) (name VCCIO3) (type power_in))
        (pin (num T2) (name IO_B3) (type BiDi))
        (pin (num T3) (name VREFB3N1_B3) (type BiDi))
        (pin (num T4) (name PLL1_CLKOUTn_B3) (type BiDi))
        (pin (num T5) (name DIFFIO_B14n_B3) (type BiDi))
        (pin (num T6) (name DIFFIO_B15n_B3) (type BiDi))
        (pin (num T7) (name DIFFIO_B16n_B3) (type BiDi))
        (pin (num T8) (name DIFFCLK_6n_B3) (type BiDi))
        (pin (num T9) (name DIFFCLK_7n_B4) (type BiDi))
        (pin (num T10) (name DIFFIO_B21n_B4) (type BiDi))
        (pin (num T11) (name DIFFIO_B22n_B4) (type BiDi))
        (pin (num T12) (name DIFFIO_B24p_B4) (type BiDi))
        (pin (num T13) (name DIFFIO_B26n_B4) (type BiDi))
        (pin (num T14) (name DIFFIO_B29p_B4) (type BiDi))
        (pin (num T15) (name DIFFIO_B29n_B4) (type BiDi))
        (pin (num T16) (name VCCIO4) (type power_in))))
    (libpart (lib max80) (part HRO-TYPE-C-31-M-12)
      (fields
        (field (name Reference) USB)
        (field (name Value) HRO-TYPE-C-31-M-12))
      (pins
        (pin (num 1) (name GND) (type input))
        (pin (num 2) (name VBUS) (type input))
        (pin (num 3) (name SBU2) (type input))
        (pin (num 4) (name CC1) (type input))
        (pin (num 5) (name DN2) (type input))
        (pin (num 6) (name DP1) (type input))
        (pin (num 7) (name DN1) (type input))
        (pin (num 8) (name DP2) (type input))
        (pin (num 9) (name SBU1) (type input))
        (pin (num 10) (name CC2) (type input))
        (pin (num 11) (name VBUS) (type input))
        (pin (num 12) (name GND) (type input))
        (pin (num 13) (name SHIELD) (type input))))
    (libpart (lib max80) (part MT48LC16M16A2P-6A)
      (docs https://www.mouser.se/datasheet/2/671/256Mb_sdr-1282350.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) MT48LC16M16A2P-6A)
        (field (name Footprint) Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm)
        (field (name LCSC) C41881))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name IO_0) (type BiDi))
        (pin (num 3) (name VDDQ) (type power_in))
        (pin (num 4) (name IO_1) (type BiDi))
        (pin (num 5) (name IO_2) (type BiDi))
        (pin (num 6) (name VSSQ) (type power_in))
        (pin (num 7) (name IO_3) (type BiDi))
        (pin (num 8) (name IO_4) (type BiDi))
        (pin (num 9) (name VDDQ) (type power_in))
        (pin (num 10) (name IO_5) (type BiDi))
        (pin (num 11) (name IO_6) (type BiDi))
        (pin (num 12) (name VSSQ) (type power_in))
        (pin (num 13) (name IO_7) (type BiDi))
        (pin (num 14) (name VDD) (type power_in))
        (pin (num 15) (name DQML) (type BiDi))
        (pin (num 16) (name ~WE) (type BiDi))
        (pin (num 17) (name ~CAS) (type BiDi))
        (pin (num 18) (name ~RAS) (type BiDi))
        (pin (num 19) (name ~CS) (type BiDi))
        (pin (num 20) (name BA0) (type BiDi))
        (pin (num 21) (name BA1) (type BiDi))
        (pin (num 22) (name A10) (type input))
        (pin (num 23) (name A0) (type input))
        (pin (num 24) (name A1) (type input))
        (pin (num 25) (name A2) (type input))
        (pin (num 26) (name A3) (type input))
        (pin (num 27) (name VDD) (type power_in))
        (pin (num 28) (name VSS) (type power_in))
        (pin (num 29) (name A4) (type input))
        (pin (num 30) (name A5) (type input))
        (pin (num 31) (name A6) (type input))
        (pin (num 32) (name A7) (type input))
        (pin (num 33) (name A8) (type input))
        (pin (num 34) (name A9) (type input))
        (pin (num 35) (name A11) (type input))
        (pin (num 36) (name A12) (type input))
        (pin (num 37) (name CKE) (type BiDi))
        (pin (num 38) (name CLK) (type BiDi))
        (pin (num 39) (name DQMH) (type BiDi))
        (pin (num 40) (name NC) (type passive))
        (pin (num 41) (name VSS) (type power_in))
        (pin (num 42) (name IO8) (type BiDi))
        (pin (num 43) (name VDDQ) (type power_in))
        (pin (num 44) (name IO9) (type BiDi))
        (pin (num 45) (name IO10) (type BiDi))
        (pin (num 46) (name VSS) (type power_in))
        (pin (num 47) (name IO11) (type BiDi))
        (pin (num 48) (name IO12) (type BiDi))
        (pin (num 49) (name VDDQ) (type power_in))
        (pin (num 50) (name IO13) (type BiDi))
        (pin (num 51) (name IO14) (type BiDi))
        (pin (num 52) (name VSSQ) (type power_in))
        (pin (num 53) (name IO15) (type BiDi))
        (pin (num 54) (name VSS) (type power_in)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Memory_Flash)
      (uri /usr/share/kicad/library/Memory_Flash.lib))
    (library (logical Oscillator)
      (uri /usr/share/kicad/library/Oscillator.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical RF_Module)
      (uri /usr/share/kicad/library/RF_Module.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical Timer_RTC)
      (uri /usr/share/kicad/library/Timer_RTC.lib))
    (library (logical Transistor_FET)
      (uri /usr/share/kicad/library/Transistor_FET.lib))
    (library (logical max80)
      (uri /home/pm/project/abc80/max80/max80.lib)))
  (nets
    (net (code 1) (name +3V3)
      (node (ref R39) (pin 2))
      (node (ref R40) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C61) (pin 1))
      (node (ref R38) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref U7) (pin 3))
      (node (ref U7) (pin 7))
      (node (ref U7) (pin 8))
      (node (ref J4) (pin 4))
      (node (ref U2) (pin 20))
      (node (ref C6) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref U14) (pin 20))
      (node (ref C7) (pin 1))
      (node (ref J4) (pin 31))
      (node (ref J8) (pin 2))
      (node (ref J8) (pin 1))
      (node (ref C33) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C45) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref C83) (pin 1))
      (node (ref U6) (pin 14))
      (node (ref U6) (pin 1))
      (node (ref R50) (pin 1))
      (node (ref U6) (pin 3))
      (node (ref U6) (pin 27))
      (node (ref R37) (pin 1))
      (node (ref U13) (pin R9))
      (node (ref C49) (pin 1))
      (node (ref C56) (pin 1))
      (node (ref J3) (pin 4))
      (node (ref OSC1) (pin 4))
      (node (ref C51) (pin 1))
      (node (ref C48) (pin 1))
      (node (ref U6) (pin 37))
      (node (ref R11) (pin 2))
      (node (ref R49) (pin 1))
      (node (ref C68) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref U12) (pin 4))
      (node (ref R1) (pin 1))
      (node (ref U12) (pin 2))
      (node (ref C55) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref U11) (pin 2))
      (node (ref C47) (pin 1))
      (node (ref R21) (pin 1))
      (node (ref U13) (pin C7))
      (node (ref U13) (pin M3))
      (node (ref U13) (pin K3))
      (node (ref U13) (pin T1))
      (node (ref U13) (pin P7))
      (node (ref U13) (pin P4))
      (node (ref U13) (pin P13))
      (node (ref U13) (pin P10))
      (node (ref U13) (pin T16))
      (node (ref U13) (pin E3))
      (node (ref U13) (pin E14))
      (node (ref U13) (pin C4))
      (node (ref U13) (pin C13))
      (node (ref U13) (pin C10))
      (node (ref U13) (pin A16))
      (node (ref U13) (pin A1))
      (node (ref U13) (pin G3))
      (node (ref U13) (pin G14))
      (node (ref C69) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U8) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref U3) (pin 20))
      (node (ref U4) (pin 20))
      (node (ref C38) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref U5) (pin 20))
      (node (ref D5) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref Q7) (pin 1))
      (node (ref U6) (pin 43))
      (node (ref D4) (pin 1))
      (node (ref R46) (pin 2))
      (node (ref U6) (pin 9))
      (node (ref OSC1) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U13) (pin H12))
      (node (ref D6) (pin 1))
      (node (ref U6) (pin 49)))
    (net (code 2) (name "Net-(U13-PadN14)")
      (node (ref U13) (pin N14)))
    (net (code 3) (name FLASH_CS#)
      (node (ref U11) (pin 4))
      (node (ref U13) (pin N6)))
    (net (code 4) (name "Net-(U13-PadJ12)")
      (node (ref U13) (pin J12)))
    (net (code 5) (name "Net-(U13-PadK12)")
      (node (ref U13) (pin K12)))
    (net (code 6) (name "Net-(U13-PadP15)")
      (node (ref U13) (pin P15)))
    (net (code 7) (name "Net-(U13-PadK10)")
      (node (ref U13) (pin K10)))
    (net (code 8) (name "Net-(U13-PadL9)")
      (node (ref U13) (pin L9)))
    (net (code 9) (name "Net-(U13-PadK9)")
      (node (ref U13) (pin K9)))
    (net (code 10) (name DD2)
      (node (ref U5) (pin 7))
      (node (ref U13) (pin N5)))
    (net (code 11) (name DD7)
      (node (ref U13) (pin T4))
      (node (ref U5) (pin 2)))
    (net (code 12) (name DD6)
      (node (ref U13) (pin R4))
      (node (ref U5) (pin 3)))
    (net (code 13) (name DD3)
      (node (ref U5) (pin 6))
      (node (ref U13) (pin T2)))
    (net (code 14) (name DD5)
      (node (ref U5) (pin 4))
      (node (ref U13) (pin T3)))
    (net (code 15) (name FPGA_JTAGEN)
      (node (ref U13) (pin J3))
      (node (ref R24) (pin 2))
      (node (ref J4) (pin 7)))
    (net (code 16) (name GND)
      (node (ref U13) (pin E12))
      (node (ref U13) (pin J10))
      (node (ref U13) (pin D7))
      (node (ref U13) (pin E2))
      (node (ref U13) (pin E13))
      (node (ref U13) (pin H16))
      (node (ref U13) (pin C5))
      (node (ref U13) (pin C12))
      (node (ref U13) (pin B2))
      (node (ref U13) (pin B15))
      (node (ref U13) (pin D10))
      (node (ref U13) (pin H9))
      (node (ref U13) (pin H8))
      (node (ref U13) (pin H7))
      (node (ref X1) (pin A2))
      (node (ref U13) (pin R15))
      (node (ref R23) (pin 2))
      (node (ref U13) (pin P5))
      (node (ref R22) (pin 2))
      (node (ref U13) (pin R2))
      (node (ref U6) (pin 46))
      (node (ref U13) (pin E5))
      (node (ref U13) (pin N7))
      (node (ref U13) (pin E4))
      (node (ref U13) (pin P12))
      (node (ref X1) (pin A4))
      (node (ref U13) (pin F6))
      (node (ref U13) (pin G13))
      (node (ref U13) (pin G4))
      (node (ref U13) (pin F10))
      (node (ref U13) (pin H10))
      (node (ref Q2) (pin 2))
      (node (ref U13) (pin H15))
      (node (ref Q3) (pin 2))
      (node (ref Q5) (pin 2))
      (node (ref J4) (pin 35))
      (node (ref J4) (pin 33))
      (node (ref J4) (pin 2))
      (node (ref J4) (pin 10))
      (node (ref U6) (pin 6))
      (node (ref U6) (pin 54))
      (node (ref X2) (pin B2))
      (node (ref J8) (pin 11))
      (node (ref J8) (pin 12))
      (node (ref U2) (pin 10))
      (node (ref Q6) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref U14) (pin 19))
      (node (ref U14) (pin 10))
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 19))
      (node (ref J4) (pin 39))
      (node (ref C12) (pin 2))
      (node (ref U13) (pin M13))
      (node (ref U13) (pin M4))
      (node (ref U13) (pin M5))
      (node (ref U13) (pin N10))
      (node (ref U6) (pin 46))
      (node (ref C8) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref X2) (pin A4))
      (node (ref C13) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U6) (pin 41))
      (node (ref X2) (pin A2))
      (node (ref U13) (pin J11))
      (node (ref U13) (pin J7))
      (node (ref U13) (pin J8))
      (node (ref U13) (pin J9))
      (node (ref U13) (pin K13))
      (node (ref U6) (pin 52))
      (node (ref U13) (pin K4))
      (node (ref U13) (pin K8))
      (node (ref U13) (pin M12))
      (node (ref C1) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref U11) (pin 43))
      (node (ref U11) (pin 42))
      (node (ref C44) (pin 2))
      (node (ref C50) (pin 2))
      (node (ref C62) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref C52) (pin 2))
      (node (ref U15) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref U13) (pin M16))
      (node (ref U9) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref C66) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref U12) (pin 9))
      (node (ref U12) (pin 8))
      (node (ref U12) (pin 7))
      (node (ref U12) (pin 6))
      (node (ref U12) (pin 5))
      (node (ref U12) (pin 13))
      (node (ref U12) (pin 12))
      (node (ref U12) (pin 11))
      (node (ref U12) (pin 10))
      (node (ref BT1) (pin 2))
      (node (ref R24) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref C55) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref USB2) (pin 1))
      (node (ref C68) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref USB2) (pin 12))
      (node (ref C32) (pin 2))
      (node (ref C47) (pin 2))
      (node (ref U11) (pin 1))
      (node (ref C41) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref U11) (pin 26))
      (node (ref C43) (pin 2))
      (node (ref C69) (pin 2))
      (node (ref U3) (pin 19))
      (node (ref C59) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U16) (pin 1))
      (node (ref U5) (pin 10))
      (node (ref C37) (pin 2))
      (node (ref U4) (pin 10))
      (node (ref U5) (pin 19))
      (node (ref U8) (pin 1))
      (node (ref C36) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref C70) (pin 2))
      (node (ref C65) (pin 2))
      (node (ref C71) (pin 2))
      (node (ref C73) (pin 2))
      (node (ref U4) (pin 19))
      (node (ref C74) (pin 2))
      (node (ref C67) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref C64) (pin 2))
      (node (ref J2) (pin 8))
      (node (ref C3) (pin 2))
      (node (ref J2) (pin 5))
      (node (ref J2) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref USB1) (pin 12))
      (node (ref USB1) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref X1) (pin B2))
      (node (ref U3) (pin 10))
      (node (ref Q4) (pin 2))
      (node (ref U6) (pin 28))
      (node (ref C2) (pin 2))
      (node (ref C48) (pin 2))
      (node (ref D23) (pin 1))
      (node (ref C60) (pin 2))
      (node (ref C61) (pin 2))
      (node (ref D22) (pin 1))
      (node (ref U7) (pin 4))
      (node (ref U13) (pin H13))
      (node (ref U13) (pin G12))
      (node (ref R42) (pin 1))
      (node (ref C45) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref J4) (pin 37))
      (node (ref J2) (pin 11))
      (node (ref C56) (pin 2))
      (node (ref C83) (pin 2))
      (node (ref C46) (pin 2))
      (node (ref OSC1) (pin 2))
      (node (ref J3) (pin 6))
      (node (ref J3) (pin 9))
      (node (ref U6) (pin 12))
      (node (ref J3) (pin 11))
      (node (ref C51) (pin 2))
      (node (ref D17) (pin 1))
      (node (ref J2) (pin 17))
      (node (ref C49) (pin 2)))
    (net (code 17) (name HDMI_D1+)
      (node (ref C77) (pin 2))
      (node (ref U13) (pin N15)))
    (net (code 18) (name /FPGA_LED3)
      (node (ref U13) (pin P14))
      (node (ref R30) (pin 2)))
    (net (code 19) (name "Net-(U13-PadJ13)")
      (node (ref U13) (pin J13)))
    (net (code 20) (name HDMI_D1-)
      (node (ref C78) (pin 2))
      (node (ref U13) (pin N16)))
    (net (code 21) (name EXT_HB)
      (node (ref J8) (pin 5))
      (node (ref U13) (pin N9)))
    (net (code 22) (name CLK0n)
      (node (ref OSC1) (pin 3))
      (node (ref U13) (pin M15)))
    (net (code 23) (name /~SD_DETECT)
      (node (ref U13) (pin L15))
      (node (ref J3) (pin 10)))
    (net (code 24) (name "Net-(U13-PadL14)")
      (node (ref U13) (pin L14)))
    (net (code 25) (name HDMI_D0-)
      (node (ref C80) (pin 2))
      (node (ref U13) (pin K16)))
    (net (code 26) (name EXT_HC)
      (node (ref J8) (pin 7))
      (node (ref R49) (pin 2))
      (node (ref U13) (pin T9)))
    (net (code 27) (name "Net-(U13-PadL11)")
      (node (ref U13) (pin L11)))
    (net (code 28) (name ~XOUTSTB_ABC_3V3)
      (node (ref U13) (pin L10))
      (node (ref U14) (pin 9)))
    (net (code 29) (name EXT_HD)
      (node (ref J8) (pin 9))
      (node (ref U13) (pin R11)))
    (net (code 30) (name EXT_HH)
      (node (ref J8) (pin 8))
      (node (ref R50) (pin 2))
      (node (ref U13) (pin R8)))
    (net (code 31) (name HDMI_D0+)
      (node (ref U13) (pin K15))
      (node (ref C79) (pin 2)))
    (net (code 32) (name EXT_HE)
      (node (ref U13) (pin R12))
      (node (ref J8) (pin 4)))
    (net (code 33) (name FPGA_GPIO1)
      (node (ref U13) (pin P9))
      (node (ref J4) (pin 14)))
    (net (code 34) (name EXT_HG)
      (node (ref J8) (pin 6))
      (node (ref U13) (pin N11)))
    (net (code 35) (name EXT_HF)
      (node (ref J8) (pin 10))
      (node (ref U13) (pin T11)))
    (net (code 36) (name ~XINPSTB_ABC_3V3)
      (node (ref U13) (pin T12))
      (node (ref U14) (pin 8)))
    (net (code 37) (name HDMI_HPD)
      (node (ref Q7) (pin 2))
      (node (ref R46) (pin 1))
      (node (ref U13) (pin T15)))
    (net (code 38) (name FPGA_GPIO3)
      (node (ref J4) (pin 16))
      (node (ref U13) (pin R10)))
    (net (code 39) (name "Net-(U13-PadA9)")
      (node (ref U13) (pin A9))
      (node (ref U13) (pin B9)))
    (net (code 40) (name "Net-(U13-PadJ14)")
      (node (ref U13) (pin J14)))
    (net (code 41) (name DD4)
      (node (ref U5) (pin 5))
      (node (ref U13) (pin R3)))
    (net (code 42) (name HDMI_SDA)
      (node (ref J2) (pin 16))
      (node (ref U13) (pin R13))
      (node (ref R2) (pin 2)))
    (net (code 43) (name HDMI_SCL)
      (node (ref U13) (pin M11))
      (node (ref R11) (pin 1))
      (node (ref J2) (pin 15)))
    (net (code 44) (name FPGA_GPIO5)
      (node (ref U13) (pin R7))
      (node (ref J4) (pin 18)))
    (net (code 45) (name ESP32_IO0)
      (node (ref J4) (pin 30))
      (node (ref U13) (pin L8))
      (node (ref U11) (pin 3))
      (node (ref R21) (pin 2)))
    (net (code 46) (name FPGA_SPI_MOSI)
      (node (ref U13) (pin M8))
      (node (ref U11) (pin 15)))
    (net (code 47) (name FGPA_SPI_CS_ESP32)
      (node (ref U13) (pin N8))
      (node (ref U11) (pin 13)))
    (net (code 48) (name INT_ESP32)
      (node (ref U13) (pin P8))
      (node (ref U11) (pin 12)))
    (net (code 49) (name FPGA_SPI_MISO)
      (node (ref U11) (pin 16))
      (node (ref U13) (pin M7)))
    (net (code 50) (name FPGA_SPI_CLK)
      (node (ref U11) (pin 14))
      (node (ref U13) (pin P6)))
    (net (code 51) (name FPGA_RESIN)
      (node (ref Q4) (pin 1))
      (node (ref R28) (pin 2))
      (node (ref U13) (pin R6)))
    (net (code 52) (name FPGA_GPIO4)
      (node (ref U13) (pin T7))
      (node (ref J4) (pin 17)))
    (net (code 53) (name FPGA_GPIO2)
      (node (ref U13) (pin T6))
      (node (ref J4) (pin 15)))
    (net (code 54) (name FPGA_GPIO0)
      (node (ref U13) (pin L7))
      (node (ref J4) (pin 13)))
    (net (code 55) (name DD1)
      (node (ref U13) (pin M6))
      (node (ref U5) (pin 8)))
    (net (code 56) (name ~XMEMFL_ABC_3V3)
      (node (ref U13) (pin N3))
      (node (ref U14) (pin 2)))
    (net (code 57) (name "Net-(U13-PadT8)")
      (node (ref U13) (pin T8)))
    (net (code 58) (name DD0)
      (node (ref U13) (pin P3))
      (node (ref U5) (pin 9)))
    (net (code 59) (name DD8)
      (node (ref U5) (pin 1))
      (node (ref U13) (pin R5)))
    (net (code 60) (name /IO2)
      (node (ref U6) (pin 5))
      (node (ref U13) (pin D11)))
    (net (code 61) (name "Net-(U6-Pad40)")
      (node (ref U6) (pin 40)))
    (net (code 62) (name /IO1)
      (node (ref U6) (pin 4))
      (node (ref U13) (pin E11)))
    (net (code 63) (name /IO4)
      (node (ref U13) (pin B11))
      (node (ref U6) (pin 8)))
    (net (code 64) (name /IO3)
      (node (ref U13) (pin C11))
      (node (ref U6) (pin 7)))
    (net (code 65) (name DATA0)
      (node (ref D7) (pin 2))
      (node (ref R41) (pin 1))
      (node (ref U13) (pin H2)))
    (net (code 66) (name HDMI_D2+)
      (node (ref U13) (pin R16))
      (node (ref C75) (pin 2)))
    (net (code 67) (name FPGA_TCK)
      (node (ref U11) (pin 21))
      (node (ref U13) (pin H3))
      (node (ref J4) (pin 1))
      (node (ref R42) (pin 2)))
    (net (code 68) (name FPGA_TMS)
      (node (ref U13) (pin J5))
      (node (ref R40) (pin 2))
      (node (ref U11) (pin 17))
      (node (ref J4) (pin 5)))
    (net (code 69) (name FPGA_TDO)
      (node (ref U13) (pin J4))
      (node (ref U11) (pin 20))
      (node (ref J4) (pin 3)))
    (net (code 70) (name "Net-(R37-Pad2)")
      (node (ref R37) (pin 2))
      (node (ref U13) (pin H5)))
    (net (code 71) (name FPGA_TDI)
      (node (ref U13) (pin H4))
      (node (ref J4) (pin 9))
      (node (ref U11) (pin 19))
      (node (ref R39) (pin 1)))
    (net (code 72) (name HDMI_D2-)
      (node (ref U13) (pin P16))
      (node (ref C76) (pin 2)))
    (net (code 73) (name DLCK)
      (node (ref U13) (pin H1))
      (node (ref D5) (pin 2))
      (node (ref U7) (pin 6)))
    (net (code 74) (name ~OUT_ABC_3V3)
      (node (ref U13) (pin G2))
      (node (ref U2) (pin 8)))
    (net (code 75) (name "Net-(R13-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref U13) (pin F4)))
    (net (code 76) (name ~CS_ABC_3V3)
      (node (ref U3) (pin 2))
      (node (ref U13) (pin F2)))
    (net (code 77) (name HDMI_CK-)
      (node (ref C82) (pin 2))
      (node (ref U13) (pin J16)))
    (net (code 78) (name HDMI_CK+)
      (node (ref C81) (pin 2))
      (node (ref U13) (pin J15)))
    (net (code 79) (name ABC_CLK_3V3)
      (node (ref U13) (pin T5))
      (node (ref U14) (pin 6)))
    (net (code 80) (name nCE0)
      (node (ref U7) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref U13) (pin D2)))
    (net (code 81) (name ASD0)
      (node (ref U7) (pin 5))
      (node (ref D6) (pin 2))
      (node (ref U13) (pin C1)))
    (net (code 82) (name XM_ABC_3V3)
      (node (ref U13) (pin B1))
      (node (ref R44) (pin 2))
      (node (ref Q6) (pin 1)))
    (net (code 83) (name /FPGA_USB_DS_DP)
      (node (ref U13) (pin L16))
      (node (ref R10) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref U13) (pin D15)))
    (net (code 84) (name /FREEI2)
      (node (ref U13) (pin A8)))
    (net (code 85) (name /FREEI3)
      (node (ref U13) (pin B8)))
    (net (code 86) (name /FPGA_USB_DS_DN)
      (node (ref U13) (pin L13))
      (node (ref R8) (pin 1))
      (node (ref U13) (pin D16)))
    (net (code 87) (name /A0)
      (node (ref U6) (pin 23))
      (node (ref U13) (pin A14)))
    (net (code 88) (name "Net-(U13-PadF13)")
      (node (ref U13) (pin F13)))
    (net (code 89) (name /FREEI4)
      (node (ref U13) (pin E1)))
    (net (code 90) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1)))
    (net (code 91) (name "Net-(J3-Pad8)")
      (node (ref J3) (pin 8)))
    (net (code 92) (name /FPGA_USB_PU)
      (node (ref R10) (pin 1))
      (node (ref U13) (pin C16)))
    (net (code 93) (name "Net-(U13-PadE16)")
      (node (ref U13) (pin E16)))
    (net (code 95) (name /FREEI8)
      (node (ref U13) (pin M1)))
    (net (code 96) (name /FREEI9)
      (node (ref U13) (pin M2)))
    (net (code 97) (name ~STATUS_ABC_3V3)
      (node (ref U4) (pin 5))
      (node (ref U13) (pin M9)))
    (net (code 98) (name /A12)
      (node (ref U13) (pin B6))
      (node (ref U6) (pin 36)))
    (net (code 99) (name /A11)
      (node (ref U6) (pin 35))
      (node (ref U13) (pin C8)))
    (net (code 100) (name /A9)
      (node (ref U13) (pin A6))
      (node (ref U6) (pin 34)))
    (net (code 101) (name /A8)
      (node (ref U6) (pin 33))
      (node (ref U13) (pin B7)))
    (net (code 102) (name /A6)
      (node (ref U6) (pin 31))
      (node (ref U13) (pin E8)))
    (net (code 103) (name /IO15)
      (node (ref U13) (pin D5))
      (node (ref U6) (pin 53)))
    (net (code 104) (name /IO13)
      (node (ref U13) (pin D6))
      (node (ref U6) (pin 50)))
    (net (code 105) (name /IO12)
      (node (ref U6) (pin 48))
      (node (ref U13) (pin E6)))
    (net (code 106) (name /IO9)
      (node (ref U13) (pin E7))
      (node (ref U6) (pin 44)))
    (net (code 107) (name /IO14)
      (node (ref U13) (pin C6))
      (node (ref U6) (pin 51)))
    (net (code 108) (name /A7)
      (node (ref U13) (pin A7))
      (node (ref U6) (pin 32)))
    (net (code 109) (name /DQMH)
      (node (ref U13) (pin D8))
      (node (ref U6) (pin 39)))
    (net (code 110) (name "Net-(U13-PadC3)")
      (node (ref U13) (pin C3)))
    (net (code 111) (name /CLK)
      (node (ref U6) (pin 38))
      (node (ref U13) (pin D3)))
    (net (code 112) (name INT800_ABC_3V3)
      (node (ref R45) (pin 2))
      (node (ref Q5) (pin 1))
      (node (ref U13) (pin A2)))
    (net (code 113) (name INT_ABC_3V3)
      (node (ref U13) (pin B3))
      (node (ref R43) (pin 2))
      (node (ref Q1) (pin 1)))
    (net (code 114) (name /IO8)
      (node (ref U6) (pin 42))
      (node (ref U13) (pin A5)))
    (net (code 115) (name /IO10)
      (node (ref U6) (pin 45))
      (node (ref U13) (pin B5)))
    (net (code 116) (name /IO11)
      (node (ref U6) (pin 47))
      (node (ref U13) (pin A4)))
    (net (code 117) (name "Net-(U13-PadP11)")
      (node (ref U13) (pin P11)))
    (net (code 118) (name EXT_HA)
      (node (ref U13) (pin N12))
      (node (ref J8) (pin 3)))
    (net (code 119) (name ~FPGA_READY)
      (node (ref R26) (pin 2))
      (node (ref U13) (pin B4))
      (node (ref Q2) (pin 1)))
    (net (code 120) (name FPGA_NMI)
      (node (ref Q3) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref U13) (pin A3)))
    (net (code 121) (name "Net-(U13-PadL6)")
      (node (ref U13) (pin L6)))
    (net (code 122) (name "Net-(U13-PadK6)")
      (node (ref U13) (pin K6)))
    (net (code 123) (name /FPGA_LED2)
      (node (ref U13) (pin R14))
      (node (ref R31) (pin 2)))
    (net (code 125) (name /BA1)
      (node (ref U6) (pin 21))
      (node (ref U13) (pin B13)))
    (net (code 126) (name /BA0)
      (node (ref U6) (pin 20))
      (node (ref U13) (pin A13)))
    (net (code 127) (name /CS#)
      (node (ref U6) (pin 19))
      (node (ref U13) (pin D12)))
    (net (code 128) (name /RAS#)
      (node (ref U13) (pin B12))
      (node (ref U6) (pin 18)))
    (net (code 129) (name /CAS#)
      (node (ref U6) (pin 17))
      (node (ref U13) (pin E9)))
    (net (code 130) (name "Net-(D23-Pad2)")
      (node (ref D23) (pin 2))
      (node (ref R31) (pin 1)))
    (net (code 131) (name "Net-(D22-Pad2)")
      (node (ref D22) (pin 2))
      (node (ref R30) (pin 1)))
    (net (code 132) (name "Net-(D17-Pad2)")
      (node (ref R29) (pin 1))
      (node (ref D17) (pin 2)))
    (net (code 133) (name /FPGA_LED1)
      (node (ref R29) (pin 2))
      (node (ref U13) (pin T13)))
    (net (code 134) (name /FPGA_SDA)
      (node (ref U11) (pin 8))
      (node (ref U12) (pin 15))
      (node (ref J4) (pin 12))
      (node (ref R14) (pin 2))
      (node (ref U13) (pin C15)))
    (net (code 135) (name /RTC_INT)
      (node (ref U13) (pin B16))
      (node (ref R32) (pin 2))
      (node (ref U12) (pin 3)))
    (net (code 136) (name /SD_CLK)
      (node (ref J3) (pin 5))
      (node (ref U13) (pin G15)))
    (net (code 137) (name /SD_DAT0)
      (node (ref J3) (pin 7))
      (node (ref U13) (pin F15)))
    (net (code 138) (name /FPGA_SCL)
      (node (ref U13) (pin G11))
      (node (ref U12) (pin 16))
      (node (ref J4) (pin 11))
      (node (ref R12) (pin 1))
      (node (ref U11) (pin 9)))
    (net (code 139) (name /DQML)
      (node (ref U13) (pin E10))
      (node (ref U6) (pin 15)))
    (net (code 140) (name /A1)
      (node (ref U13) (pin B14))
      (node (ref U6) (pin 24)))
    (net (code 141) (name /A2)
      (node (ref U13) (pin D14))
      (node (ref U6) (pin 25)))
    (net (code 142) (name /A3)
      (node (ref U13) (pin A15))
      (node (ref U6) (pin 26)))
    (net (code 143) (name /A4)
      (node (ref U6) (pin 29))
      (node (ref U13) (pin C9)))
    (net (code 144) (name /A5)
      (node (ref U13) (pin D9))
      (node (ref U6) (pin 30)))
    (net (code 145) (name /A10)
      (node (ref U6) (pin 22))
      (node (ref U13) (pin C14)))
    (net (code 146) (name /IO0)
      (node (ref U6) (pin 2))
      (node (ref U13) (pin A12)))
    (net (code 147) (name /SD_CMD)
      (node (ref J3) (pin 3))
      (node (ref U13) (pin G16)))
    (net (code 148) (name /SD_DAT3)
      (node (ref U13) (pin F16))
      (node (ref J3) (pin 2)))
    (net (code 149) (name /IO5)
      (node (ref U6) (pin 10))
      (node (ref U13) (pin A11)))
    (net (code 150) (name /IO6)
      (node (ref U6) (pin 11))
      (node (ref U13) (pin B10)))
    (net (code 151) (name /IO7)
      (node (ref U6) (pin 13))
      (node (ref U13) (pin A10)))
    (net (code 152) (name /WE#)
      (node (ref U6) (pin 16))
      (node (ref U13) (pin F9)))
    (net (code 153) (name /32KHZ)
      (node (ref U11) (pin 18))
      (node (ref R9) (pin 2))
      (node (ref U12) (pin 1))
      (node (ref U13) (pin E15)))
    (net (code 154) (name ~XMEMW80_ABC_3V3)
      (node (ref U13) (pin R1))
      (node (ref U14) (pin 3)))
    (net (code 155) (name ~XMEMW800_ABC_3V3)
      (node (ref U14) (pin 4))
      (node (ref U13) (pin P1)))
    (net (code 156) (name ~C1_ABC_3V3)
      (node (ref U2) (pin 6))
      (node (ref U13) (pin J2)))
    (net (code 157) (name ~RST_ABC_3V3)
      (node (ref U13) (pin P2))
      (node (ref U14) (pin 7)))
    (net (code 158) (name ~C3_ABC_3V3)
      (node (ref U2) (pin 2))
      (node (ref U13) (pin L3)))
    (net (code 159) (name ~INP_ABC_3V3)
      (node (ref U4) (pin 7))
      (node (ref U13) (pin L2)))
    (net (code 160) (name ~C4_ABC_3V3)
      (node (ref U13) (pin K2))
      (node (ref U4) (pin 9)))
    (net (code 161) (name ~C2_ABC_3V3)
      (node (ref U13) (pin K5))
      (node (ref U2) (pin 4)))
    (net (code 162) (name "Net-(R38-Pad2)")
      (node (ref U13) (pin H14))
      (node (ref R38) (pin 2)))
    (net (code 163) (name "Net-(R41-Pad2)")
      (node (ref R41) (pin 2))
      (node (ref U7) (pin 2)))
    (net (code 164) (name +5V)
      (node (ref D27) (pin 1))
      (node (ref C65) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref U16) (pin 3))
      (node (ref C70) (pin 1))
      (node (ref R47) (pin 2))
      (node (ref C60) (pin 1))
      (node (ref C64) (pin 1))
      (node (ref C67) (pin 1))
      (node (ref D19) (pin 1))
      (node (ref J2) (pin 18))
      (node (ref D28) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U8) (pin 3)))
    (net (code 165) (name AD16)
      (node (ref U13) (pin C2))
      (node (ref U14) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 166) (name "Net-(R25-Pad2)")
      (node (ref R25) (pin 2))
      (node (ref U14) (pin 17)))
    (net (code 167) (name /abc80bus/ABC_12V)
      (node (ref J7) (pin 1))
      (node (ref X1) (pin B32))
      (node (ref X1) (pin A32))
      (node (ref X2) (pin A32))
      (node (ref X2) (pin B32)))
    (net (code 168) (name /abc80bus/~XMEMW80)
      (node (ref R25) (pin 1))
      (node (ref X2) (pin A5))
      (node (ref Q5) (pin 3))
      (node (ref R45) (pin 1))
      (node (ref X1) (pin A5)))
    (net (code 169) (name /abc80bus/~INT)
      (node (ref X2) (pin B13))
      (node (ref Q1) (pin 3))
      (node (ref R43) (pin 1))
      (node (ref X1) (pin B13)))
    (net (code 170) (name "Net-(U14-Pad5)")
      (node (ref U14) (pin 5)))
    (net (code 171) (name "Net-(U14-Pad15)")
      (node (ref U14) (pin 15)))
    (net (code 172) (name /abc80bus/~XM)
      (node (ref R44) (pin 1))
      (node (ref Q6) (pin 3))
      (node (ref X1) (pin A28))
      (node (ref X2) (pin A28)))
    (net (code 173) (name /abc80bus/ABC_-12V)
      (node (ref X2) (pin B1))
      (node (ref X2) (pin A1))
      (node (ref X1) (pin A1))
      (node (ref J7) (pin 2))
      (node (ref X1) (pin B1)))
    (net (code 174) (name /abc80bus/~XINPSTB)
      (node (ref X2) (pin A26))
      (node (ref U14) (pin 12))
      (node (ref X1) (pin A26))
      (node (ref R22) (pin 1)))
    (net (code 175) (name /abc80bus/~XOUTSTB)
      (node (ref U14) (pin 11))
      (node (ref X1) (pin A27))
      (node (ref X2) (pin A27))
      (node (ref R23) (pin 1)))
    (net (code 176) (name /abc80bus/~RST)
      (node (ref X1) (pin A15))
      (node (ref U14) (pin 13))
      (node (ref X2) (pin A15)))
    (net (code 177) (name /abc80bus/~XMEMW800)
      (node (ref X2) (pin B3))
      (node (ref X1) (pin B3))
      (node (ref U14) (pin 16)))
    (net (code 178) (name /abc80bus/~XMEMFL)
      (node (ref X2) (pin B4))
      (node (ref X1) (pin B4))
      (node (ref U14) (pin 18)))
    (net (code 179) (name ABC_CLK_5)
      (node (ref X1) (pin B5))
      (node (ref X2) (pin B5))
      (node (ref U14) (pin 14)))
    (net (code 180) (name /abc80bus/D6)
      (node (ref X1) (pin A7))
      (node (ref U5) (pin 17))
      (node (ref X2) (pin A7)))
    (net (code 181) (name /abc80bus/A0)
      (node (ref U3) (pin 11))
      (node (ref X1) (pin B29))
      (node (ref X2) (pin B29)))
    (net (code 182) (name /abc80bus/A6)
      (node (ref X1) (pin B23))
      (node (ref U3) (pin 17))
      (node (ref X2) (pin B23)))
    (net (code 183) (name /abc80bus/A5)
      (node (ref X2) (pin B24))
      (node (ref U3) (pin 16))
      (node (ref X1) (pin B24)))
    (net (code 184) (name /abc80bus/A4)
      (node (ref U3) (pin 15))
      (node (ref X2) (pin B25))
      (node (ref X1) (pin B25)))
    (net (code 185) (name /abc80bus/A3)
      (node (ref X2) (pin B26))
      (node (ref U3) (pin 14))
      (node (ref X1) (pin B26)))
    (net (code 186) (name /abc80bus/A2)
      (node (ref X1) (pin B27))
      (node (ref X2) (pin B27))
      (node (ref U3) (pin 13)))
    (net (code 187) (name /abc80bus/A1)
      (node (ref X2) (pin B28))
      (node (ref U3) (pin 12))
      (node (ref X1) (pin B28)))
    (net (code 188) (name "Net-(X1-PadB30)")
      (node (ref X2) (pin B30))
      (node (ref X1) (pin B30)))
    (net (code 189) (name /abc80bus/ABC5V)
      (node (ref X1) (pin A31))
      (node (ref X2) (pin B31))
      (node (ref J1) (pin 1))
      (node (ref X1) (pin B31))
      (node (ref X2) (pin A31)))
    (net (code 190) (name "Net-(X1-PadB6)")
      (node (ref X2) (pin B6))
      (node (ref X1) (pin B6)))
    (net (code 191) (name "Net-(X1-PadB7)")
      (node (ref X2) (pin B7))
      (node (ref X1) (pin B7)))
    (net (code 192) (name "Net-(X1-PadB8)")
      (node (ref X2) (pin B8))
      (node (ref X1) (pin B8)))
    (net (code 193) (name "Net-(X1-PadB9)")
      (node (ref X2) (pin B9))
      (node (ref X1) (pin B9)))
    (net (code 194) (name /abc80bus/D7)
      (node (ref X1) (pin A6))
      (node (ref U5) (pin 18))
      (node (ref X2) (pin A6)))
    (net (code 195) (name /abc80bus/~NMI)
      (node (ref R27) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref X1) (pin A24))
      (node (ref X2) (pin A24)))
    (net (code 196) (name "Net-(X1-PadA25)")
      (node (ref X2) (pin A25))
      (node (ref X1) (pin A25)))
    (net (code 197) (name "Net-(X1-PadA29)")
      (node (ref X1) (pin A29))
      (node (ref X2) (pin A29)))
    (net (code 198) (name /abc80bus/~CS)
      (node (ref X1) (pin A23))
      (node (ref U3) (pin 18))
      (node (ref X2) (pin A23)))
    (net (code 199) (name /abc80bus/D5)
      (node (ref X1) (pin A8))
      (node (ref X2) (pin A8))
      (node (ref U5) (pin 16)))
    (net (code 200) (name /abc80bus/D4)
      (node (ref X1) (pin A9))
      (node (ref X2) (pin A9))
      (node (ref U5) (pin 15)))
    (net (code 201) (name "Net-(X1-PadB10)")
      (node (ref X1) (pin B10))
      (node (ref X2) (pin B10)))
    (net (code 202) (name "Net-(X1-PadB11)")
      (node (ref X1) (pin B11))
      (node (ref X2) (pin B11)))
    (net (code 203) (name "Net-(X1-PadB12)")
      (node (ref X1) (pin B12))
      (node (ref X2) (pin B12)))
    (net (code 204) (name /abc80bus/D2)
      (node (ref U5) (pin 13))
      (node (ref X2) (pin A11))
      (node (ref X1) (pin A11)))
    (net (code 205) (name /abc80bus/D3)
      (node (ref X1) (pin A10))
      (node (ref U5) (pin 14))
      (node (ref X2) (pin A10)))
    (net (code 206) (name /abc80bus/D1)
      (node (ref X2) (pin A12))
      (node (ref U5) (pin 12))
      (node (ref X1) (pin A12)))
    (net (code 207) (name /abc80bus/D0)
      (node (ref U5) (pin 11))
      (node (ref X2) (pin A13))
      (node (ref X1) (pin A13)))
    (net (code 208) (name "Net-(X1-PadA14)")
      (node (ref X1) (pin A14))
      (node (ref X2) (pin A14)))
    (net (code 210) (name /abc80bus/~INP)
      (node (ref U4) (pin 13))
      (node (ref X2) (pin A17))
      (node (ref X1) (pin A17)))
    (net (code 211) (name /abc80bus/READY)
      (node (ref R26) (pin 1))
      (node (ref Q2) (pin 3))
      (node (ref X1) (pin A30))
      (node (ref X2) (pin A30)))
    (net (code 212) (name /abc80bus/~RESIN)
      (node (ref X1) (pin A3))
      (node (ref Q4) (pin 3))
      (node (ref X2) (pin A3))
      (node (ref R28) (pin 1)))
    (net (code 213) (name /abc80bus/A7)
      (node (ref U2) (pin 11))
      (node (ref X1) (pin B22))
      (node (ref X2) (pin B22)))
    (net (code 214) (name /abc80bus/A8)
      (node (ref X2) (pin B21))
      (node (ref X1) (pin B21))
      (node (ref U2) (pin 13)))
    (net (code 215) (name /abc80bus/A9)
      (node (ref X1) (pin B20))
      (node (ref U2) (pin 15))
      (node (ref X2) (pin B20)))
    (net (code 216) (name /abc80bus/A10)
      (node (ref U2) (pin 17))
      (node (ref X2) (pin B19))
      (node (ref X1) (pin B19)))
    (net (code 217) (name /abc80bus/A11)
      (node (ref U4) (pin 12))
      (node (ref X1) (pin B18))
      (node (ref X2) (pin B18)))
    (net (code 218) (name /abc80bus/A12)
      (node (ref U4) (pin 14))
      (node (ref X2) (pin B17))
      (node (ref X1) (pin B17)))
    (net (code 219) (name /abc80bus/A13)
      (node (ref U4) (pin 16))
      (node (ref X2) (pin B16))
      (node (ref X1) (pin B16)))
    (net (code 220) (name /abc80bus/A14)
      (node (ref X2) (pin B15))
      (node (ref U4) (pin 17))
      (node (ref X1) (pin B15)))
    (net (code 221) (name /abc80bus/A15)
      (node (ref U4) (pin 18))
      (node (ref X2) (pin B14))
      (node (ref X1) (pin B14)))
    (net (code 222) (name /abc80bus/~OUT)
      (node (ref X2) (pin A22))
      (node (ref X1) (pin A22))
      (node (ref U2) (pin 12)))
    (net (code 223) (name /abc80bus/~STATUS)
      (node (ref X2) (pin A16))
      (node (ref U4) (pin 15))
      (node (ref X1) (pin A16)))
    (net (code 224) (name /abc80bus/~C1)
      (node (ref X1) (pin A21))
      (node (ref X2) (pin A21))
      (node (ref U2) (pin 14)))
    (net (code 225) (name /abc80bus/~C2)
      (node (ref X2) (pin A20))
      (node (ref U2) (pin 16))
      (node (ref X1) (pin A20)))
    (net (code 226) (name /abc80bus/~C3)
      (node (ref U2) (pin 18))
      (node (ref X1) (pin A19))
      (node (ref X2) (pin A19)))
    (net (code 227) (name /abc80bus/~C4)
      (node (ref X1) (pin A18))
      (node (ref U4) (pin 11))
      (node (ref X2) (pin A18)))
    (net (code 228) (name "Net-(D28-Pad2)")
      (node (ref D28) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 229) (name "Net-(USB1-Pad13)")
      (node (ref USB1) (pin 13)))
    (net (code 230) (name "Net-(U9-Pad6)")
      (node (ref U9) (pin 6))
      (node (ref USB1) (pin 7)))
    (net (code 231) (name "Net-(R6-Pad2)")
      (node (ref USB1) (pin 10))
      (node (ref R6) (pin 2)))
    (net (code 232) (name "Net-(USB1-Pad3)")
      (node (ref USB1) (pin 3)))
    (net (code 233) (name "Net-(R5-Pad2)")
      (node (ref USB1) (pin 4))
      (node (ref R5) (pin 2)))
    (net (code 234) (name "Net-(USB1-Pad5)")
      (node (ref USB1) (pin 5)))
    (net (code 235) (name "Net-(U9-Pad4)")
      (node (ref U9) (pin 4))
      (node (ref USB1) (pin 6)))
    (net (code 236) (name "Net-(USB1-Pad8)")
      (node (ref USB1) (pin 8)))
    (net (code 237) (name "Net-(USB1-Pad9)")
      (node (ref USB1) (pin 9)))
    (net (code 239) (name "Net-(R8-Pad2)")
      (node (ref U9) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 240) (name "Net-(R7-Pad2)")
      (node (ref U9) (pin 3))
      (node (ref R7) (pin 2)))
    (net (code 241) (name "Net-(C39-Pad1)")
      (node (ref D19) (pin 2))
      (node (ref C39) (pin 1))
      (node (ref F1) (pin 1)))
    (net (code 242) (name "Net-(F1-Pad2)")
      (node (ref F1) (pin 2))
      (node (ref U9) (pin 5))
      (node (ref USB1) (pin 11))
      (node (ref USB1) (pin 2)))
    (net (code 243) (name "Net-(F2-Pad2)")
      (node (ref F2) (pin 2))
      (node (ref USB2) (pin 11))
      (node (ref USB2) (pin 2))
      (node (ref U15) (pin 5)))
    (net (code 244) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref USB2) (pin 4)))
    (net (code 245) (name /ESP32/USB_D-)
      (node (ref U11) (pin 22))
      (node (ref U15) (pin 1)))
    (net (code 246) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref U11) (pin 5)))
    (net (code 247) (name ESP32_TXD)
      (node (ref J4) (pin 27))
      (node (ref U11) (pin 37)))
    (net (code 248) (name ESP32_RXD)
      (node (ref U11) (pin 38))
      (node (ref J4) (pin 29)))
    (net (code 249) (name ESP32_CS1)
      (node (ref U11) (pin 39))
      (node (ref J4) (pin 23)))
    (net (code 250) (name "Net-(U11-Pad40)")
      (node (ref U11) (pin 40)))
    (net (code 251) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref U11) (pin 6)))
    (net (code 252) (name "Net-(D2-Pad2)")
      (node (ref U11) (pin 7))
      (node (ref D2) (pin 2)))
    (net (code 253) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref R18) (pin 1)))
    (net (code 254) (name ESP32_TMS)
      (node (ref J4) (pin 32))
      (node (ref U11) (pin 36)))
    (net (code 255) (name ESP32_EN)
      (node (ref R15) (pin 2))
      (node (ref J4) (pin 28))
      (node (ref U11) (pin 41)))
    (net (code 256) (name /ESP32/USB_D+)
      (node (ref U15) (pin 3))
      (node (ref U11) (pin 23)))
    (net (code 257) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref USB2) (pin 10)))
    (net (code 258) (name "Net-(USB2-Pad3)")
      (node (ref USB2) (pin 3)))
    (net (code 259) (name "Net-(USB2-Pad5)")
      (node (ref USB2) (pin 5)))
    (net (code 260) (name "Net-(USB2-Pad8)")
      (node (ref USB2) (pin 8)))
    (net (code 261) (name "Net-(USB2-Pad9)")
      (node (ref USB2) (pin 9)))
    (net (code 262) (name "Net-(U15-Pad4)")
      (node (ref USB2) (pin 6))
      (node (ref U15) (pin 4)))
    (net (code 263) (name "Net-(U15-Pad6)")
      (node (ref U15) (pin 6))
      (node (ref USB2) (pin 7)))
    (net (code 264) (name "Net-(USB2-Pad13)")
      (node (ref USB2) (pin 13)))
    (net (code 265) (name "Net-(U11-Pad25)")
      (node (ref U11) (pin 25)))
    (net (code 266) (name ESP32_TCK)
      (node (ref J4) (pin 34))
      (node (ref U11) (pin 33)))
    (net (code 267) (name ESP32_TDO)
      (node (ref U11) (pin 34))
      (node (ref J4) (pin 36)))
    (net (code 268) (name ESP32_TDI)
      (node (ref U11) (pin 35))
      (node (ref J4) (pin 38)))
    (net (code 269) (name "Net-(U11-Pad10)")
      (node (ref U11) (pin 10)))
    (net (code 270) (name "Net-(U11-Pad11)")
      (node (ref U11) (pin 11)))
    (net (code 271) (name "Net-(C53-Pad1)")
      (node (ref C53) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 272) (name "Net-(C52-Pad1)")
      (node (ref C52) (pin 1))
      (node (ref F2) (pin 1))
      (node (ref D27) (pin 2)))
    (net (code 273) (name "Net-(D2-Pad1)")
      (node (ref R17) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 274) (name ESP32_CS2)
      (node (ref U11) (pin 24))
      (node (ref J4) (pin 19)))
    (net (code 275) (name ESP32_SDA)
      (node (ref J4) (pin 20))
      (node (ref R20) (pin 2))
      (node (ref U11) (pin 27)))
    (net (code 276) (name ESP32_SCL)
      (node (ref R19) (pin 2))
      (node (ref J4) (pin 21))
      (node (ref U11) (pin 28)))
    (net (code 277) (name ESP32_MISO)
      (node (ref J4) (pin 26))
      (node (ref U11) (pin 31)))
    (net (code 278) (name ESP32_SCK)
      (node (ref U11) (pin 30))
      (node (ref J4) (pin 24)))
    (net (code 279) (name ESP32_MOSI)
      (node (ref U11) (pin 29))
      (node (ref J4) (pin 22)))
    (net (code 280) (name ESP32_CS0)
      (node (ref U11) (pin 32))
      (node (ref J4) (pin 25)))
    (net (code 281) (name "Net-(D1-Pad1)")
      (node (ref R16) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 282) (name "Net-(BT1-Pad1)")
      (node (ref BT1) (pin 1))
      (node (ref U12) (pin 14)))
    (net (code 283) (name +2V5)
      (node (ref C59) (pin 1))
      (node (ref U16) (pin 2))
      (node (ref U13) (pin L5))
      (node (ref C73) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref U13) (pin L12))
      (node (ref C15) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref U13) (pin F12))
      (node (ref U13) (pin F5))
      (node (ref C43) (pin 1))
      (node (ref U13) (pin M14))
      (node (ref U13) (pin K14))
      (node (ref C41) (pin 1))
      (node (ref C42) (pin 1))
      (node (ref C32) (pin 1)))
    (net (code 284) (name +1V2)
      (node (ref C62) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref C66) (pin 1))
      (node (ref C63) (pin 1))
      (node (ref C50) (pin 1))
      (node (ref C44) (pin 1))
      (node (ref C72) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref U13) (pin G6))
      (node (ref U13) (pin G8))
      (node (ref U13) (pin G9))
      (node (ref U13) (pin H11))
      (node (ref C18) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref U13) (pin N4))
      (node (ref C20) (pin 1))
      (node (ref U13) (pin G7))
      (node (ref U13) (pin F11))
      (node (ref C74) (pin 1))
      (node (ref U13) (pin F7))
      (node (ref U13) (pin G10))
      (node (ref U13) (pin D4))
      (node (ref U13) (pin K11))
      (node (ref U13) (pin J6))
      (node (ref U1) (pin 2))
      (node (ref U13) (pin K7))
      (node (ref C12) (pin 1))
      (node (ref U13) (pin D13))
      (node (ref U13) (pin N13))
      (node (ref U13) (pin H6)))
    (net (code 285) (name "Net-(J4-Pad6)")
      (node (ref J4) (pin 6)))
    (net (code 286) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8)))
    (net (code 287) (name "Net-(J4-Pad40)")
      (node (ref J4) (pin 40)))
    (net (code 288) (name "Net-(J2-Pad13)")
      (node (ref J2) (pin 13)))
    (net (code 289) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14)))
    (net (code 290) (name "Net-(J2-PadSH)")
      (node (ref J2) (pin SH)))
    (net (code 291) (name "Net-(C82-Pad1)")
      (node (ref C82) (pin 1))
      (node (ref J2) (pin 12)))
    (net (code 292) (name "Net-(C75-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref C75) (pin 1)))
    (net (code 293) (name "Net-(C81-Pad1)")
      (node (ref C81) (pin 1))
      (node (ref J2) (pin 10)))
    (net (code 294) (name "Net-(J2-Pad19)")
      (node (ref Q7) (pin 3))
      (node (ref R47) (pin 1))
      (node (ref J2) (pin 19)))
    (net (code 295) (name "Net-(C78-Pad1)")
      (node (ref C78) (pin 1))
      (node (ref J2) (pin 6)))
    (net (code 296) (name "Net-(C77-Pad1)")
      (node (ref J2) (pin 4))
      (node (ref C77) (pin 1)))
    (net (code 297) (name "Net-(C76-Pad1)")
      (node (ref C76) (pin 1))
      (node (ref J2) (pin 3)))
    (net (code 298) (name "Net-(C79-Pad1)")
      (node (ref C79) (pin 1))
      (node (ref J2) (pin 7)))
    (net (code 299) (name "Net-(C80-Pad1)")
      (node (ref C80) (pin 1))
      (node (ref J2) (pin 9)))
    (net (code 300) (name AD0)
      (node (ref U3) (pin 9))
      (node (ref U13) (pin F8)))
    (net (code 301) (name AD1)
      (node (ref U3) (pin 8))
      (node (ref U13) (pin T10)))
    (net (code 302) (name AD10)
      (node (ref U13) (pin L4))
      (node (ref U2) (pin 3)))
    (net (code 303) (name AD15)
      (node (ref U13) (pin N1))
      (node (ref U4) (pin 2)))
    (net (code 304) (name AD14)
      (node (ref U13) (pin N2))
      (node (ref U4) (pin 3)))
    (net (code 305) (name AD13)
      (node (ref U13) (pin T14))
      (node (ref U4) (pin 4)))
    (net (code 306) (name AD12)
      (node (ref U13) (pin L1))
      (node (ref U4) (pin 6)))
    (net (code 307) (name AD11)
      (node (ref U4) (pin 8))
      (node (ref U13) (pin K1)))
    (net (code 308) (name AD9)
      (node (ref U13) (pin J1))
      (node (ref U2) (pin 5)))
    (net (code 309) (name AD8)
      (node (ref U13) (pin G1))
      (node (ref U2) (pin 7)))
    (net (code 310) (name AD7)
      (node (ref U13) (pin F1))
      (node (ref U2) (pin 9)))
    (net (code 311) (name AD6)
      (node (ref U13) (pin M10))
      (node (ref U3) (pin 3)))
    (net (code 312) (name AD5)
      (node (ref U13) (pin F3))
      (node (ref U3) (pin 4)))
    (net (code 313) (name AD4)
      (node (ref U13) (pin G5))
      (node (ref U3) (pin 5)))
    (net (code 314) (name AD3)
      (node (ref U3) (pin 6))
      (node (ref U13) (pin D1)))
    (net (code 315) (name AD2)
      (node (ref U3) (pin 7))
      (node (ref U13) (pin F14)))))