(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "74LS260" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 4.826 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "74LS260" (at -9.652 8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0.508 1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.futurlec.com/74LS/74LS260.shtml" (at 0.508 -3.048 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_keywords" "TTL Nor5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "5-input NOR" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W7.62mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "74LS260_1_1"
      (arc (start -3.048 -6.858) (mid -1.0195 -0.0863) (end -3.302 6.604)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.302 6.604)
          (xy -0.127 6.604)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.048 -6.858)
          (xy 0.127 -6.858)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.254 6.604)
          (xy -2.032 6.604)
          (xy -3.302 6.604)
          (xy -2.032 4.318)
          (xy -1.524 3.048)
          (xy -1.016 1.27)
          (xy -1.016 -0.254)
          (xy -1.016 -1.27)
          (xy -1.524 -4.064)
          (xy -3.048 -6.858)
          (xy 0.254 -6.858)
          (xy 0.254 -6.858)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.254 6.604)
          (xy 1.27 5.842)
          (xy 2.286 5.08)
          (xy 3.048 4.318)
          (xy 3.81 3.302)
          (xy 4.318 1.524)
          (xy 4.572 0)
          (xy 4.318 -1.524)
          (xy 4.064 -2.54)
          (xy 3.302 -4.064)
          (xy 2.032 -5.588)
          (xy 0.254 -6.858)
          (xy -0.762 -6.858)
          (xy -0.508 -6.858)
          (xy -0.762 -6.858)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (arc (start 0.2084 -6.8387) (mid 3.3617 -4.0358) (end 4.5264 0.0193)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 4.572 0) (mid 3.2484 4.0981) (end -0.254 6.604)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -6.858 5.08 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 -2.54 0) (length 5.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 -5.334 0) (length 4.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 2.54 0) (length 5.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 0 0) (length 5.703)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 8.636 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS260_1_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS260_2_1"
      (arc (start -3.048 -6.858) (mid -1.0195 -0.0863) (end -3.302 6.604)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.302 6.604)
          (xy -0.127 6.604)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -3.048 -6.858)
          (xy 0.127 -6.858)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.254 6.604)
          (xy -2.032 6.604)
          (xy -3.302 6.604)
          (xy -2.032 4.318)
          (xy -1.524 3.048)
          (xy -1.016 1.27)
          (xy -1.016 -0.254)
          (xy -1.016 -1.27)
          (xy -1.524 -4.064)
          (xy -3.048 -6.858)
          (xy 0.254 -6.858)
          (xy 0.254 -6.858)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.254 6.604)
          (xy 1.27 5.842)
          (xy 2.286 5.08)
          (xy 3.048 4.318)
          (xy 3.81 3.302)
          (xy 4.318 1.524)
          (xy 4.572 0)
          (xy 4.318 -1.524)
          (xy 4.064 -2.54)
          (xy 3.302 -4.064)
          (xy 2.032 -5.588)
          (xy 0.254 -6.858)
          (xy -0.762 -6.858)
          (xy -0.508 -6.858)
          (xy -0.762 -6.858)
        )
        (stroke (width -25.4) (type default))
        (fill (type background))
      )
      (arc (start 0.2084 -6.8387) (mid 3.3617 -4.0358) (end 4.5264 0.0193)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (arc (start 4.572 0) (mid 3.2484 4.0981) (end -0.254 6.604)
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (pin input line (at -6.858 -2.54 0) (length 5.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 -5.334 0) (length 4.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 5.08 0) (length 4.318)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output inverted (at 8.636 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 2.54 0) (length 5.568)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -6.858 0 0) (length 5.703)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS260_2_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS260_3_0"
      (pin power_in line (at 0 12.446 270) (length 5.08)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -12.954 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "74LS260_3_1"
      (rectangle (start -5.08 7.366) (end 5.08 -7.874)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "74LS260_3_2"
      (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0 3.81)
          (xy -3.81 3.81)
          (xy -3.81 -3.81)
          (xy 0 -3.81)
        )
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input inverted (at -7.62 0 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 -2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 7.62 0 180) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -7.62 2.54 0) (length 3.81)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "82S131" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -7.62 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "82S131" (at 3.81 24.13 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_DIP:DIP-16_W7.62mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheetspdf.com/pdf-file/510594/NXP/82S131/1" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "2k bit bipolar PROM" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2k bit bipolar PROM" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W15.24mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "82S131_1_1"
      (rectangle (start -7.62 22.86) (end 7.62 -6.858)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 15.24 180) (length 2.54)
        (name "Q3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 17.78 180) (length 2.54)
        (name "Q2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 20.32 180) (length 2.54)
        (name "Q1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.414 -3.81 0) (length 2.54)
        (name "~{CE}" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 25.4 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 7.62 0 180) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 12.7 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 20.32 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 17.78 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0.254 -9.398 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 10.16 12.7 180) (length 2.54)
        (name "Q4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ABC-Bus" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "X" (at 3.81 41.91 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Value" "ABC-Bus" (at -3.81 -46.99 0)
      (effects (font (size 1.4986 1.4986)) (justify left bottom))
    )
    (property "Footprint" "sm6uax:MAB64B-FAB64Q" (at -20.32 -1.27 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -10.16 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ABC-Bus_1_0"
      (pin bidirectional line (at -12.7 13.97 0) (length 5.08)
        (name "D3" (effects (font (size 0.9906 0.9906))))
        (number "A10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 11.43 0) (length 5.08)
        (name "D2" (effects (font (size 0.9906 0.9906))))
        (number "A11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 8.89 0) (length 5.08)
        (name "D1" (effects (font (size 0.9906 0.9906))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 6.35 0) (length 5.08)
        (name "D0" (effects (font (size 0.9906 0.9906))))
        (number "A13" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -12.7 3.81 0) (length 5.08)
        (name "NC" (effects (font (size 0.9906 0.9906))))
        (number "A14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 1.27 0) (length 5.08)
        (name "~{RST}" (effects (font (size 0.9906 0.9906))))
        (number "A15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -1.27 0) (length 5.08)
        (name "~{STATUS}" (effects (font (size 0.9906 0.9906))))
        (number "A16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -3.81 0) (length 5.08)
        (name "~{INP}" (effects (font (size 0.9906 0.9906))))
        (number "A17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -6.35 0) (length 5.08)
        (name "~{C4}" (effects (font (size 0.9906 0.9906))))
        (number "A18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -8.89 0) (length 5.08)
        (name "~{C3}" (effects (font (size 0.9906 0.9906))))
        (number "A19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 34.29 0) (length 5.08)
        (name "0V" (effects (font (size 0.9906 0.9906))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -11.43 0) (length 5.08)
        (name "~{C2}" (effects (font (size 0.9906 0.9906))))
        (number "A20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -13.97 0) (length 5.08)
        (name "~{C1}" (effects (font (size 0.9906 0.9906))))
        (number "A21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -16.51 0) (length 5.08)
        (name "~{OUT}" (effects (font (size 0.9906 0.9906))))
        (number "A22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -19.05 0) (length 5.08)
        (name "~{CS}" (effects (font (size 0.9906 0.9906))))
        (number "A23" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -21.59 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A24" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -24.13 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A25" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -26.67 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A26" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -29.21 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A27" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -31.75 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A28" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -34.29 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 31.75 0) (length 5.08)
        (name "~{RESIN}" (effects (font (size 0.9906 0.9906))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -36.83 0) (length 5.08)
        (name "READY" (effects (font (size 0.9906 0.9906))))
        (number "A30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -39.37 0) (length 5.08)
        (name "+5V" (effects (font (size 0.9906 0.9906))))
        (number "A31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 -41.91 0) (length 5.08)
        (name "+12V" (effects (font (size 0.9906 0.9906))))
        (number "A32" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -12.7 29.21 0) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 26.67 0) (length 5.08)
        (name "~{XMEMW}" (effects (font (size 0.9906 0.9906))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 24.13 0) (length 5.08)
        (name "D7" (effects (font (size 0.9906 0.9906))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 21.59 0) (length 5.08)
        (name "D6" (effects (font (size 0.9906 0.9906))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 19.05 0) (length 5.08)
        (name "D5" (effects (font (size 0.9906 0.9906))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 16.51 0) (length 5.08)
        (name "D4" (effects (font (size 0.9906 0.9906))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "ABC-Bus_1_1"
      (rectangle (start -7.62 40.64) (end 5.08 -44.45)
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (pin power_out line (at -12.7 36.83 0) (length 5.08)
        (name "-12V" (effects (font (size 0.9906 0.9906))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 36.83 180) (length 5.08)
        (name "-12V" (effects (font (size 0.9906 0.9906))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 13.97 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 11.43 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 8.89 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 6.35 180) (length 5.08)
        (name "~{INT}" (effects (font (size 0.9906 0.9906))))
        (number "B13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 3.81 180) (length 5.08)
        (name "A15" (effects (font (size 0.9906 0.9906))))
        (number "B14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 1.27 180) (length 5.08)
        (name "A14" (effects (font (size 0.9906 0.9906))))
        (number "B15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -1.27 180) (length 5.08)
        (name "A13" (effects (font (size 0.9906 0.9906))))
        (number "B16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -3.81 180) (length 5.08)
        (name "A12" (effects (font (size 0.9906 0.9906))))
        (number "B17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -6.35 180) (length 5.08)
        (name "A11" (effects (font (size 0.9906 0.9906))))
        (number "B18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -8.89 180) (length 5.08)
        (name "A10" (effects (font (size 0.9906 0.9906))))
        (number "B19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 34.29 180) (length 5.08)
        (name "0V" (effects (font (size 0.9906 0.9906))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -11.43 180) (length 5.08)
        (name "A9" (effects (font (size 0.9906 0.9906))))
        (number "B20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -13.97 180) (length 5.08)
        (name "A8" (effects (font (size 0.9906 0.9906))))
        (number "B21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -16.51 180) (length 5.08)
        (name "A7" (effects (font (size 0.9906 0.9906))))
        (number "B22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -19.05 180) (length 5.08)
        (name "A6" (effects (font (size 0.9906 0.9906))))
        (number "B23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -21.59 180) (length 5.08)
        (name "A5" (effects (font (size 0.9906 0.9906))))
        (number "B24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -24.13 180) (length 5.08)
        (name "A4" (effects (font (size 0.9906 0.9906))))
        (number "B25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -26.67 180) (length 5.08)
        (name "A3" (effects (font (size 0.9906 0.9906))))
        (number "B26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -29.21 180) (length 5.08)
        (name "A2" (effects (font (size 0.9906 0.9906))))
        (number "B27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -31.75 180) (length 5.08)
        (name "A1" (effects (font (size 0.9906 0.9906))))
        (number "B28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -34.29 180) (length 5.08)
        (name "A0" (effects (font (size 0.9906 0.9906))))
        (number "B29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 31.75 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 -36.83 180) (length 5.08)
        (name "NC" (effects (font (size 0.9906 0.9906))))
        (number "B30" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -39.37 180) (length 5.08)
        (name "+5V" (effects (font (size 0.9906 0.9906))))
        (number "B31" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 -41.91 180) (length 5.08)
        (name "+12V" (effects (font (size 0.9906 0.9906))))
        (number "B32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 29.21 180) (length 5.08)
        (name "~{XMEMFL}" (effects (font (size 0.9906 0.9906))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 10.16 26.67 180) (length 5.08)
        (name "5" (effects (font (size 0.9906 0.9906))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 24.13 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 21.59 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 19.05 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 10.16 16.51 180) (length 5.08)
        (name "GND" (effects (font (size 0.9906 0.9906))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MB8416" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "MB8416" (at 2.54 20.955 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "Package_DIP:DIP-24_W15.24mm" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "RAM SRAM CMOS MEMORY" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "2048x8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "DIP*W15.24mm*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MB8416_0_0"
      (pin tri_state line (at 12.7 7.62 180) (length 2.54)
        (name "Q4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "MB8416_0_1"
      (rectangle (start -10.16 20.32) (end 10.16 -20.32)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
    )
    (symbol "MB8416_1_1"
      (pin input line (at -12.7 0.508 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 15.24 180) (length 2.54)
        (name "Q1" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 12.7 180) (length 2.54)
        (name "Q2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 10.16 180) (length 2.54)
        (name "Q3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 5.08 180) (length 2.54)
        (name "Q5" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 2.54 180) (length 2.54)
        (name "Q6" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 0 180) (length 2.54)
        (name "Q7" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -14.478 0) (length 2.54)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -7.112 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 2.794 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -17.018 0) (length 2.54)
        (name "~{CS}" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -11.938 0) (length 2.54)
        (name "~{WE}" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -4.572 0) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.032 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 22.86 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 5.08 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 7.62 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 10.16 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 12.7 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 15.24 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 17.78 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin tri_state line (at 12.7 17.78 180) (length 2.54)
        (name "Q0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
