(export (version D)
  (design
    (source /home/pm/project/abc80/x37/x37.sch)
    (date "tor 13 jan 2022 15:39:23")
    (tool "Eeschema 5.99.0+really5.1.10+dfsg1-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source x37.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name "/x37 Kernel/") (tstamps /61E05F96/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source x37kernel1.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U3)
      (value 68010-10)
      (datasheet https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf)
      (libsource (lib CPU_NXP_68000) (part 68010D) (description "16/32-bit Microprocessor"))
      (sheetpath (names "/x37 Kernel/") (tstamps /61E05F96/))
      (tstamp 61E0628E))
    (comp (ref U10)
      (value NS32081D-10)
      (footprint Package_DIP:DIP-24_W15.24mm_Socket_LongPads)
      (libsource (lib x37) (part NS32081D-10) (description ""))
      (sheetpath (names "/x37 Kernel/") (tstamps /61E05F96/))
      (tstamp 61E4489B))
    (comp (ref U32)
      (value 74ALS245)
      (footprint Package_DIP:DIP-20_W7.62mm)
      (datasheet http://www.ti.com/lit/gpn/sn74ALS245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names "/x37 Kernel/") (tstamps /61E05F96/))
      (tstamp 61EA38ED))
    (comp (ref U31)
      (value 74ALS245)
      (footprint Package_DIP:DIP-20_W7.62mm)
      (datasheet http://www.ti.com/lit/gpn/sn74ALS245)
      (libsource (lib 74xx) (part 74HC245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names "/x37 Kernel/") (tstamps /61E05F96/))
      (tstamp 61EA6712)))
  (libparts
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib CPU_NXP_68000) (part 68000D)
      (aliases
        (alias 68010D))
      (description "16/32-bit Microprocessor")
      (docs https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 68000D))
      (pins
        (pin (num 1) (name D4) (type BiDi))
        (pin (num 2) (name D3) (type BiDi))
        (pin (num 3) (name D2) (type BiDi))
        (pin (num 4) (name D1) (type BiDi))
        (pin (num 5) (name D0) (type BiDi))
        (pin (num 6) (name AS) (type output))
        (pin (num 7) (name UDS) (type output))
        (pin (num 8) (name LDS) (type output))
        (pin (num 9) (name R/W) (type output))
        (pin (num 10) (name DTACK) (type input))
        (pin (num 11) (name BG) (type output))
        (pin (num 12) (name BGACK) (type input))
        (pin (num 13) (name BR) (type input))
        (pin (num 14) (name VCC) (type power_in))
        (pin (num 15) (name CLK) (type input))
        (pin (num 16) (name GND) (type power_in))
        (pin (num 17) (name HALT) (type BiDi))
        (pin (num 18) (name RESET) (type BiDi))
        (pin (num 19) (name VMA) (type output))
        (pin (num 20) (name E) (type output))
        (pin (num 21) (name VPA) (type input))
        (pin (num 22) (name BERR) (type input))
        (pin (num 23) (name IPL2) (type input))
        (pin (num 24) (name IPL1) (type input))
        (pin (num 25) (name IPL0) (type input))
        (pin (num 26) (name FC2) (type output))
        (pin (num 27) (name FC1) (type output))
        (pin (num 28) (name FC0) (type output))
        (pin (num 29) (name A1) (type output))
        (pin (num 30) (name A2) (type output))
        (pin (num 31) (name A3) (type output))
        (pin (num 32) (name A4) (type output))
        (pin (num 33) (name A5) (type output))
        (pin (num 34) (name A6) (type output))
        (pin (num 35) (name A7) (type output))
        (pin (num 36) (name A8) (type output))
        (pin (num 37) (name A9) (type output))
        (pin (num 38) (name A10) (type output))
        (pin (num 39) (name A11) (type output))
        (pin (num 40) (name A12) (type output))
        (pin (num 41) (name A13) (type output))
        (pin (num 42) (name A14) (type output))
        (pin (num 43) (name A15) (type output))
        (pin (num 44) (name A16) (type output))
        (pin (num 45) (name A17) (type output))
        (pin (num 46) (name A18) (type output))
        (pin (num 47) (name A19) (type output))
        (pin (num 48) (name A20) (type output))
        (pin (num 49) (name VCC) (type power_in))
        (pin (num 50) (name A21) (type output))
        (pin (num 51) (name A22) (type output))
        (pin (num 52) (name A23) (type output))
        (pin (num 53) (name GND) (type power_in))
        (pin (num 54) (name D15) (type BiDi))
        (pin (num 55) (name D14) (type BiDi))
        (pin (num 56) (name D13) (type BiDi))
        (pin (num 57) (name D12) (type BiDi))
        (pin (num 58) (name D11) (type BiDi))
        (pin (num 59) (name D10) (type BiDi))
        (pin (num 60) (name D9) (type BiDi))
        (pin (num 61) (name D8) (type BiDi))
        (pin (num 62) (name D7) (type BiDi))
        (pin (num 63) (name D6) (type BiDi))
        (pin (num 64) (name D5) (type BiDi))))
    (libpart (lib x37) (part NS32081D-10)
      (fields
        (field (name Reference) U)
        (field (name Value) NS32081D-10)
        (field (name Footprint) Package_DIP:DIP-24_W15.24mm_Socket_LongPads))
      (pins
        (pin (num 1) (name D10) (type BiDi))
        (pin (num 2) (name D9) (type BiDi))
        (pin (num 3) (name D8) (type BiDi))
        (pin (num 4) (name D7) (type BiDi))
        (pin (num 5) (name D6) (type BiDi))
        (pin (num 6) (name D5) (type BiDi))
        (pin (num 7) (name D4) (type BiDi))
        (pin (num 8) (name D3) (type BiDi))
        (pin (num 9) (name D2) (type BiDi))
        (pin (num 10) (name D1) (type BiDi))
        (pin (num 11) (name D0) (type BiDi))
        (pin (num 12) (name GNDL) (type power_in))
        (pin (num 13) (name GNDB) (type power_in))
        (pin (num 14) (name CLK) (type input))
        (pin (num 15) (name ~RST) (type input))
        (pin (num 16) (name D15) (type BiDi))
        (pin (num 17) (name D14) (type BiDi))
        (pin (num 18) (name D13) (type BiDi))
        (pin (num 19) (name D12) (type BiDi))
        (pin (num 20) (name D11) (type BiDi))
        (pin (num 21) (name SPC) (type BiDi))
        (pin (num 22) (name ST1) (type BiDi))
        (pin (num 23) (name ST0) (type BiDi))
        (pin (num 24) (name VCC) (type power_in)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical CPU_NXP_68000)
      (uri /usr/share/kicad/library/CPU_NXP_68000.lib))
    (library (logical x37)
      (uri /home/pm/project/abc80/x37/x37.lib)))
  (nets
    (net (code 1) (name MD8)
      (node (ref U31) (pin 2)))
    (net (code 2) (name ~DIR)
      (node (ref U31) (pin 1))
      (node (ref U32) (pin 1)))
    (net (code 3) (name MD15)
      (node (ref U31) (pin 9)))
    (net (code 4) (name MD14)
      (node (ref U31) (pin 8)))
    (net (code 5) (name MD13)
      (node (ref U31) (pin 7)))
    (net (code 6) (name MD12)
      (node (ref U31) (pin 6)))
    (net (code 7) (name MD11)
      (node (ref U31) (pin 5)))
    (net (code 8) (name MD10)
      (node (ref U31) (pin 4)))
    (net (code 9) (name MD9)
      (node (ref U31) (pin 3)))
    (net (code 10) (name MD7)
      (node (ref U32) (pin 9)))
    (net (code 11) (name MD6)
      (node (ref U32) (pin 8)))
    (net (code 12) (name MD5)
      (node (ref U32) (pin 7)))
    (net (code 13) (name MD4)
      (node (ref U32) (pin 6)))
    (net (code 14) (name MD3)
      (node (ref U32) (pin 5)))
    (net (code 15) (name MD2)
      (node (ref U32) (pin 4)))
    (net (code 16) (name MD1)
      (node (ref U32) (pin 3)))
    (net (code 17) (name MD0)
      (node (ref U32) (pin 2)))
    (net (code 18) (name GND)
      (node (ref U32) (pin 10))
      (node (ref U10) (pin 13))
      (node (ref U3) (pin 16))
      (node (ref U3) (pin 53))
      (node (ref U10) (pin 12))
      (node (ref U31) (pin 10)))
    (net (code 19) (name D4)
      (node (ref U32) (pin 14))
      (node (ref U10) (pin 7))
      (node (ref U3) (pin 1)))
    (net (code 20) (name +5V)
      (node (ref U31) (pin 20))
      (node (ref U10) (pin 24))
      (node (ref U3) (pin 14))
      (node (ref U3) (pin 49))
      (node (ref U32) (pin 20)))
    (net (code 21) (name ~MDLE)
      (node (ref U32) (pin 19)))
    (net (code 22) (name ~MDHE)
      (node (ref U31) (pin 19)))
    (net (code 23) (name FC2)
      (node (ref U3) (pin 26)))
    (net (code 24) (name ~BERR)
      (node (ref U3) (pin 22)))
    (net (code 25) (name E)
      (node (ref U3) (pin 20)))
    (net (code 26) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 27) (name ~AS)
      (node (ref U3) (pin 6)))
    (net (code 28) (name ~BR)
      (node (ref U3) (pin 13)))
    (net (code 29) (name ~BG)
      (node (ref U3) (pin 11)))
    (net (code 30) (name ~BGACK)
      (node (ref U3) (pin 12)))
    (net (code 31) (name FC1)
      (node (ref U3) (pin 27)))
    (net (code 32) (name FC0)
      (node (ref U3) (pin 28)))
    (net (code 33) (name ~IPL2)
      (node (ref U3) (pin 23)))
    (net (code 34) (name ~IPL1)
      (node (ref U3) (pin 24)))
    (net (code 35) (name ~IPL0)
      (node (ref U3) (pin 25)))
    (net (code 36) (name CPUCLK)
      (node (ref U3) (pin 15)))
    (net (code 37) (name D5)
      (node (ref U3) (pin 64))
      (node (ref U32) (pin 13))
      (node (ref U10) (pin 6)))
    (net (code 38) (name ~RW)
      (node (ref U3) (pin 9)))
    (net (code 39) (name A6)
      (node (ref U3) (pin 34)))
    (net (code 40) (name A3)
      (node (ref U3) (pin 31)))
    (net (code 41) (name A2)
      (node (ref U3) (pin 30)))
    (net (code 42) (name A1)
      (node (ref U3) (pin 29)))
    (net (code 43) (name D6)
      (node (ref U32) (pin 12))
      (node (ref U10) (pin 5))
      (node (ref U3) (pin 63)))
    (net (code 44) (name ~LDS)
      (node (ref U3) (pin 8)))
    (net (code 45) (name ~UDS)
      (node (ref U3) (pin 7)))
    (net (code 46) (name ~DTACK)
      (node (ref U3) (pin 10)))
    (net (code 47) (name ~RST)
      (node (ref U10) (pin 15))
      (node (ref U3) (pin 18)))
    (net (code 48) (name ~VPA)
      (node (ref U3) (pin 21)))
    (net (code 49) (name ~HLT)
      (node (ref U3) (pin 17)))
    (net (code 50) (name A7)
      (node (ref U3) (pin 35)))
    (net (code 51) (name A5)
      (node (ref U3) (pin 33))
      (node (ref U10) (pin 22)))
    (net (code 52) (name D2)
      (node (ref U10) (pin 9))
      (node (ref U3) (pin 3))
      (node (ref U32) (pin 16)))
    (net (code 53) (name A9)
      (node (ref U3) (pin 37)))
    (net (code 54) (name D3)
      (node (ref U32) (pin 15))
      (node (ref U10) (pin 8))
      (node (ref U3) (pin 2)))
    (net (code 55) (name D7)
      (node (ref U32) (pin 11))
      (node (ref U10) (pin 4))
      (node (ref U3) (pin 62)))
    (net (code 56) (name D8)
      (node (ref U3) (pin 61))
      (node (ref U31) (pin 18))
      (node (ref U10) (pin 3)))
    (net (code 57) (name D9)
      (node (ref U3) (pin 60))
      (node (ref U10) (pin 2))
      (node (ref U31) (pin 17)))
    (net (code 58) (name D10)
      (node (ref U31) (pin 16))
      (node (ref U3) (pin 59))
      (node (ref U10) (pin 1)))
    (net (code 59) (name D11)
      (node (ref U3) (pin 58))
      (node (ref U10) (pin 20))
      (node (ref U31) (pin 15)))
    (net (code 60) (name D12)
      (node (ref U10) (pin 19))
      (node (ref U3) (pin 57))
      (node (ref U31) (pin 14)))
    (net (code 61) (name D13)
      (node (ref U10) (pin 18))
      (node (ref U3) (pin 56))
      (node (ref U31) (pin 13)))
    (net (code 62) (name D14)
      (node (ref U10) (pin 17))
      (node (ref U3) (pin 55))
      (node (ref U31) (pin 12)))
    (net (code 63) (name D15)
      (node (ref U31) (pin 11))
      (node (ref U10) (pin 16))
      (node (ref U3) (pin 54)))
    (net (code 64) (name A23)
      (node (ref U3) (pin 52)))
    (net (code 65) (name A22)
      (node (ref U3) (pin 51)))
    (net (code 66) (name A21)
      (node (ref U3) (pin 50)))
    (net (code 67) (name A20)
      (node (ref U3) (pin 48)))
    (net (code 68) (name A19)
      (node (ref U3) (pin 47)))
    (net (code 69) (name A18)
      (node (ref U3) (pin 46)))
    (net (code 70) (name A17)
      (node (ref U3) (pin 45)))
    (net (code 71) (name A16)
      (node (ref U3) (pin 44)))
    (net (code 72) (name A15)
      (node (ref U3) (pin 43)))
    (net (code 73) (name A14)
      (node (ref U3) (pin 42)))
    (net (code 74) (name A13)
      (node (ref U3) (pin 41)))
    (net (code 75) (name A12)
      (node (ref U3) (pin 40)))
    (net (code 76) (name D1)
      (node (ref U32) (pin 17))
      (node (ref U3) (pin 4))
      (node (ref U10) (pin 10)))
    (net (code 77) (name A11)
      (node (ref U3) (pin 39)))
    (net (code 78) (name A10)
      (node (ref U3) (pin 38)))
    (net (code 79) (name A4)
      (node (ref U10) (pin 23))
      (node (ref U3) (pin 32)))
    (net (code 80) (name A8)
      (node (ref U3) (pin 36)))
    (net (code 81) (name ~SPC)
      (node (ref U10) (pin 21)))
    (net (code 82) (name ECK)
      (node (ref U10) (pin 14)))
    (net (code 83) (name D0)
      (node (ref U32) (pin 18))
      (node (ref U10) (pin 11))
      (node (ref U3) (pin 5)))))