(footprint "SOP50P490X110-10N"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "MAX9924UAUB+T")
	(tags "Integrated Circuit")
	(property "Reference" "IC2"
		(at 0.07 2.83 0)
		(layer "F.SilkS")
		(uuid "0e71dc51-124d-4506-8f84-191a38cedf1e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Value" "MAX9924UAUB+T"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "97aad38c-5235-4846-9230-80527d529aee")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ff10de42-865b-4ebc-b1d7-ae4c9fe45ace")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b0365459-09ed-4882-8f32-2623ebbda636")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "MAXIM INTEGRATED PRODUCTS - MAX9924UAUB+T - Specialized Interface, Sensor Interface, Camshaft, Crankshaft & Vehicle Speed VRS Interfaces, 4.5 V"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "86ed8936-e65a-44e3-bde5-b8801d1fc53c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Height" "1.1"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "6d4654b6-3f33-45b1-bb61-e0f4faa1318e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer_Name" "Analog Devices"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "3b96e186-e31b-4d52-991e-6ddf20823815")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer_Part_Number" "MAX9924UAUB+T"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "8a514cf5-c3a1-4f92-9b30-55f74ceb7d8f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser Part Number" "700-MAX9924UAUBT"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "dd818998-ae5e-4389-832b-1b4716d21f2d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices-Maxim-Integrated/MAX9924UAUB%2bT?qs=CDqwynd4ZNrOG878jz77zA%3D%3D"
		(at 239.12 -67.66 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "b77a54af-9592-4b9c-85bf-e5bcaf8f4c92")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.9 -1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4dde9743-7eb8-4ce5-a570-8f274972d8c7")
	)
	(fp_line
		(start -1.15 -1.5)
		(end 1.15 -1.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "45b3835c-9ace-4e74-8eae-5ca8377d86a6")
	)
	(fp_line
		(start -1.15 1.5)
		(end -1.15 -1.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "79c1b090-b462-4282-b280-53bce209e92e")
	)
	(fp_line
		(start 1.15 -1.5)
		(end 1.15 1.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5055191b-4311-4eca-9dfe-2d5e94fba1fc")
	)
	(fp_line
		(start 1.15 1.5)
		(end -1.15 1.5)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7dbfe35f-eead-4867-9c89-13dfa6df3bc2")
	)
	(fp_line
		(start -3.15 -1.775)
		(end 3.15 -1.775)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c8a2269a-9dc6-48f5-b403-3314a5f10ec7")
	)
	(fp_line
		(start -3.15 1.775)
		(end -3.15 -1.775)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "4d2edb05-7b37-4c9d-a354-426400761f46")
	)
	(fp_line
		(start 3.15 -1.775)
		(end 3.15 1.775)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "55404e11-3e2e-490f-a8d5-39c1177cc0d8")
	)
	(fp_line
		(start 3.15 1.775)
		(end -3.15 1.775)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a1f47907-4ac3-41e2-9252-52c9d64a4576")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "110dcfbf-8b6e-4630-a0f8-34ae5b92d6f9")
	)
	(fp_line
		(start -1.5 -1)
		(end -1 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a371686-62d8-402d-8dc3-29e01ad185c3")
	)
	(fp_line
		(start -1.5 1.5)
		(end -1.5 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "32ca9504-b814-4b88-9f23-48d69f3ff2c8")
	)
	(fp_line
		(start 1.5 -1.5)
		(end 1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6a26dc52-3674-4255-ab20-defa12e0d667")
	)
	(fp_line
		(start 1.5 1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c3909f3e-ffcf-41ac-a481-270efd0edc93")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "32232526-7ad2-431c-b5ac-c4475b5b0eef")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.254)
			)
		)
	)
	(pad "1" smd rect
		(at -2.2 -1 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "b7bb5325-d890-4bc4-8454-98dddf9056c7")
	)
	(pad "2" smd rect
		(at -2.2 -0.5 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "73e6fc77-ce7c-4a68-8219-5e7a97f36e44")
	)
	(pad "3" smd rect
		(at -2.2 0 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "95a3668d-d892-4c5c-a966-745b9272db9b")
	)
	(pad "4" smd rect
		(at -2.2 0.5 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0700528a-20dd-4a33-acc5-d018d7715eb7")
	)
	(pad "5" smd rect
		(at -2.2 1 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f48b96b8-7201-418f-9773-33823996f4c9")
	)
	(pad "6" smd rect
		(at 2.2 1 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "4c048e05-4969-4471-953f-9f0ba32298ac")
	)
	(pad "7" smd rect
		(at 2.2 0.5 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "a2c040fb-e8ec-43fe-b2f9-d62d015354f2")
	)
	(pad "8" smd rect
		(at 2.2 0 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "65549b8e-3a35-4049-bc0a-b6c49c078a7e")
	)
	(pad "9" smd rect
		(at 2.2 -0.5 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "425d6545-962c-4111-81f6-1351e7d3796d")
	)
	(pad "10" smd rect
		(at 2.2 -1 90)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "e1507237-1a94-41da-9bc7-a2c36fa4efe0")
	)
	(model "MAX9924UAUB+T.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
