(footprint "DT13-2PA"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Molex Mini-Universal MATE-N-LOK, old mpn/engineering number: 1-770972-x, 6 Pins per row (http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=82181_SOFTSHELL_HIGH_DENSITY&DocType=CS&DocLang=EN), generated with kicad-footprint-generator")
	(tags "connector TE MATE-N-LOK horizontal")
	(property "Reference" "REF**"
		(at 11.99 -4.06 0)
		(layer "F.SilkS")
		(uuid "7abafa7b-e488-438f-92c8-3519a0c9924e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "DT13-2PA"
		(at 11.99 24.76 0)
		(layer "F.Fab")
		(uuid "eb272a7b-1a4a-406c-be3d-3c14ae28b298")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "48b04577-b2ee-4651-ae91-180d8b9f2c45")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ae9b1de5-65ae-40cf-a426-43f95b64cbe2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "aa4d0188-8fe8-4f83-8ecb-c616344eafff")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5.96 -8.5)
		(end -5.96 12.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d22eedba-ad56-4d77-af25-c7498288b14f")
	)
	(fp_line
		(start -5.96 -8.5)
		(end 15.5 -8.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "455c5286-f527-4614-9b4f-fdfd439b87dc")
	)
	(fp_line
		(start -1.78 -1.78)
		(end -1.78 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "58799c4a-4f08-474b-bcf3-3eb0ebd3ff96")
	)
	(fp_line
		(start 0 -1.78)
		(end -1.78 -1.78)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e6e1353d-bef5-452b-982b-47334f388279")
	)
	(fp_line
		(start 15.5 -8.5)
		(end 15.5 12.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1d754c91-6de3-4b36-9209-66b2b98d1d07")
	)
	(fp_line
		(start 15.5 12.95)
		(end -5.96 12.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "966e7b05-2ecf-48ad-a49b-663e46ed381a")
	)
	(fp_line
		(start -5.96 -14.975)
		(end -5.96 20.435)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2ce918cc-7eaf-43f1-b7c2-f8b20ade3f64")
	)
	(fp_line
		(start -5.96 20.435)
		(end 37.68 20.435)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ce273629-1fd0-4e8a-9d5f-5ddd71e8893b")
	)
	(fp_line
		(start 37.68 -14.975)
		(end -5.96 -14.975)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b36e8205-874d-4dfc-bea6-48bc897581c2")
	)
	(fp_line
		(start 37.68 20.435)
		(end 37.68 -14.975)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99ccca51-9362-4037-8fed-4e590e4293d9")
	)
	(fp_line
		(start -1.925 12.95)
		(end 15.5 12.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "44c603d5-5303-4736-b4fd-7f9a488a0499")
	)
	(fp_line
		(start -1.78 -1.78)
		(end -1.78 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7418bcd3-fbbb-4e73-9159-8e4c1089009a")
	)
	(fp_line
		(start 0 -1.78)
		(end -1.78 -1.78)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b6717414-c79a-453e-a90d-373108a97f76")
	)
	(fp_line
		(start 15.5 -8.5)
		(end -1.85 -8.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a69c4efb-a469-4ca9-a267-97049d1478be")
	)
	(fp_line
		(start 15.5 -8.5)
		(end 15.5 12.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4aef0477-2e67-454e-bd88-f53d05cf1b7a")
	)
	(fp_line
		(start 15.5 12.95)
		(end 15.5 -8.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "951e9ceb-ce75-44ce-ad4f-67e53eb8aae5")
	)
	(fp_text user "${REFERENCE}"
		(at 17.64 10.35 90)
		(layer "F.Fab")
		(uuid "b7ddbb7e-824a-4fbc-9872-e820b9316d9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -1.9 -6.425)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Mask")
		(uuid "c623acae-00ec-409f-9d88-c34a06426f01")
	)
	(pad "" np_thru_hole circle
		(at -1.9 11.885)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Mask")
		(uuid "fac4d1ae-71d7-453f-b705-3c8f46638079")
	)
	(pad "" np_thru_hole circle
		(at 6.1 2.73)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Mask")
		(uuid "ef5371cb-fce0-485b-8c59-8216449e3956")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.094697)
		(uuid "548adea9-f116-4cbc-80fd-51c2fefa640a")
	)
	(pad "2" thru_hole circle
		(at 0 5.46)
		(size 3 3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c0c554dd-52d7-4dc2-acbf-68b9c1ade88b")
	)
	(model "${KIPRJMOD}/3d-models/c-dt13-2p-99-3d.stp"
		(offset
			(xyz 30 -2.75 14)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 180 90)
		)
	)
)
