(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "SN74LVCC3245A" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.08 20.32 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SN74LVCC3245A" (at 13.97 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at -2.54 17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -2.54 17.78 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Direction controlled Level Shifter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SN74LVCC3245A_1_1"
      (rectangle (start -5.08 16.51) (end 5.08 -20.32)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (pin power_in line (at -2.54 19.05 270) (length 2.54)
        (name "VccA" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 -7.62 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 -22.86 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 -7.62 180) (length 2.54)
        (name "B8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 -5.08 180) (length 2.54)
        (name "B7" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
        (name "B6" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 0 180) (length 2.54)
        (name "B5" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 2.54 180) (length 2.54)
        (name "B4" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 5.08 180) (length 2.54)
        (name "B3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -11.43 0) (length 2.54)
        (name "DIR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 7.62 180) (length 2.54)
        (name "B2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 10.16 180) (length 2.54)
        (name "B1" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -13.97 0) (length 2.54)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 2.54 19.05 270) (length 2.54)
        (name "VccB" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 10.16 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 7.62 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 5.08 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 2.54 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 0 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 -2.54 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 -5.08 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
