36549366792989
Package_LCC
PLCC-20
PLCC, 20 pins, surface mount
plcc smt
0
20
20
Package_LCC
PLCC-20_SMD-Socket
PLCC, 20 pins, surface mount
plcc smt
0
20
20
Package_LCC
PLCC-20_THT-Socket
PLCC, 20 pins, through hole
plcc leaded
0
20
20
Package_LCC
PLCC-28
PLCC, 28 pins, surface mount
plcc smt
0
28
28
Package_LCC
PLCC-28_SMD-Socket
PLCC, 28 pins, surface mount
plcc smt
0
28
28
Package_LCC
PLCC-28_THT-Socket
PLCC, 28 pins, through hole
plcc leaded
0
28
28
Package_LCC
PLCC-32_11.4x14.0mm_P1.27mm
PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py
PLCC LCC
0
32
32
Package_LCC
PLCC-32_THT-Socket
PLCC, 32 pins, through hole, http://www.assmann-wsw.com/fileadmin/datasheets/ASS_0981_CO.pdf
plcc leaded
0
32
32
Package_LCC
PLCC-44
PLCC, 44 pins, surface mount
plcc smt
0
44
44
Package_LCC
PLCC-44_16.6x16.6mm_P1.27mm
PLCC, 44 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py
PLCC LCC
0
44
44
Package_LCC
PLCC-44_SMD-Socket
PLCC, 44 pins, surface mount
plcc smt
0
44
44
Package_LCC
PLCC-44_THT-Socket
PLCC, 44 pins, through hole
plcc leaded
0
44
44
Package_LCC
PLCC-52
PLCC, 52 pins, surface mount
plcc smt
0
52
52
Package_LCC
PLCC-52_SMD-Socket
PLCC, 52 pins, surface mount
plcc smt
0
52
52
Package_LCC
PLCC-52_THT-Socket
PLCC, 52 pins, through hole
plcc leaded
0
52
52
Package_LCC
PLCC-68
PLCC, 68 pins, surface mount
plcc smt
0
68
68
Package_LCC
PLCC-68_24.2x24.2mm_P1.27mm
PLCC, 68 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py
PLCC LCC
0
68
68
Package_LCC
PLCC-68_SMD-Socket
PLCC, 68 pins, surface mount
plcc smt
0
68
68
Package_LCC
PLCC-68_THT-Socket
PLCC, 68 pins, through hole
plcc leaded
0
68
68
Package_LCC
PLCC-84
PLCC, 84 pins, surface mount
plcc smt
0
84
84
Package_LCC
PLCC-84_29.3x29.3mm_P1.27mm
PLCC, 84 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py
PLCC LCC
0
84
84
Package_LCC
PLCC-84_SMD-Socket
PLCC, 84 pins, surface mount
plcc smt
0
84
84
Package_LCC
PLCC-84_THT-Socket
PLCC, 84 pins, through hole
plcc leaded
0
84
84
