(footprint "Relay_SPDT_SONGLES_SRD"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
	(tags "relay Sanyu SRD form C")
	(property "Reference" "K1"
		(at 8.1 9.2 0)
		(layer "F.SilkS")
		(uuid "02d5e12d-27f3-45ce-958d-b52e7ab61854")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Relay_SPDT"
		(at 8 -9.6 0)
		(layer "F.Fab")
		(uuid "3c7c4117-913f-463d-ae63-1f93461688ba")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f5b9b9df-4d9a-42e1-a596-7cd157470a6f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "27cfa6ff-dec7-43a2-b416-db9d27ef00c2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9ddd4d3d-d943-469f-aecd-4e0562df1df0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.4 -7.8)
		(end -1.4 -1.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "20bfddb9-7331-4e50-b412-aea129b5c926")
	)
	(fp_line
		(start -1.4 -7.8)
		(end 18.4 -7.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec1f5598-3eda-4e8c-8d32-1f45773d3d5e")
	)
	(fp_line
		(start -1.4 1.2)
		(end -1.4 7.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e243b4b4-45f8-41a7-95d7-92ab17e6bca0")
	)
	(fp_line
		(start 2.65 0.05)
		(end 1.85 0.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dad31e61-072e-4e2c-b897-7cc8e1a87f6a")
	)
	(fp_line
		(start 2.65 0.05)
		(end 2.65 3.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fb238c25-7753-4772-a4b4-69c9c83de800")
	)
	(fp_line
		(start 3.55 6.05)
		(end 6.05 6.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "00fb3ad2-60f9-4bdc-8523-6e115e4296e2")
	)
	(fp_line
		(start 4.05 -1.75)
		(end 8.05 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ba0bafe-18f2-4c73-8504-58ab5518d4d2")
	)
	(fp_line
		(start 4.05 1.85)
		(end 4.05 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e25762cd-901e-471b-8201-d832b3e8d271")
	)
	(fp_line
		(start 6.05 -5.95)
		(end 3.55 -5.95)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ac0e97d5-43ac-4ba9-87ab-0c9111cfc10f")
	)
	(fp_line
		(start 6.05 -5.95)
		(end 6.05 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec1a2c11-5e60-403d-992a-71ce0ca5fb76")
	)
	(fp_line
		(start 6.05 1.85)
		(end 6.05 6.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "054172eb-d369-4f1e-a11c-c75d8aed0d8f")
	)
	(fp_line
		(start 8.05 -1.75)
		(end 8.05 1.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f9e58e30-1426-480e-b2d2-d49d1e4754bc")
	)
	(fp_line
		(start 8.05 1.85)
		(end 4.05 -1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3a53e5a4-de94-4f58-9630-ab09695087ed")
	)
	(fp_line
		(start 8.05 1.85)
		(end 4.05 1.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8bc569af-a9a9-48c5-a713-177bd5665267")
	)
	(fp_line
		(start 9.45 0.05)
		(end 9.45 3.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3bf8c8df-586b-4462-8a02-5e23545c800c")
	)
	(fp_line
		(start 9.45 0.05)
		(end 10.95 0.05)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5061b07-9a34-4dec-ba06-c55d511a112e")
	)
	(fp_line
		(start 9.45 3.65)
		(end 2.65 3.65)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e5925cbe-40ce-4374-bd17-330b8758aaf8")
	)
	(fp_line
		(start 10.95 0.05)
		(end 15.55 -2.45)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a03737d3-4861-49b4-9a54-133c4d438fdf")
	)
	(fp_line
		(start 13.6 -4.2)
		(end 13.6 -1.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c8d0152c-4998-4121-a73e-caaa69616433")
	)
	(fp_line
		(start 13.6 4.2)
		(end 13.6 1.75)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6c249fcc-571d-43ce-9677-13b7063a33c9")
	)
	(fp_line
		(start 18.4 -7.8)
		(end 18.4 7.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ab4f3d66-3c21-4331-a466-cb14ecb2af1d")
	)
	(fp_line
		(start 18.4 7.8)
		(end -1.4 7.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "73432ca2-50c7-4513-9e7e-d68bf961fef8")
	)
	(fp_line
		(start -1.55 7.95)
		(end -1.55 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b38bdf92-2a3f-4ae1-8547-847046448e4c")
	)
	(fp_line
		(start -1.55 7.95)
		(end 18.55 7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7cebdef8-c8ea-4808-ab17-605c936188eb")
	)
	(fp_line
		(start 18.55 -7.95)
		(end -1.55 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1f153a67-9416-46c6-bfc0-8c0303fcc8a7")
	)
	(fp_line
		(start 18.55 -7.95)
		(end 18.55 7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dc92e962-c70b-4ea9-ae10-c0b06405fce7")
	)
	(fp_line
		(start -1.3 -7.7)
		(end 18.3 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "148497d4-d6ae-4eee-b8b7-acb4e6194b63")
	)
	(fp_line
		(start -1.3 7.7)
		(end -1.3 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4eac4d1c-c5ff-4caf-86e8-5e81be6a812e")
	)
	(fp_line
		(start 18.3 -7.7)
		(end 18.3 7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6c43a164-568d-4055-8cd5-95e67b5f9fd4")
	)
	(fp_line
		(start 18.3 7.7)
		(end -1.3 7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "97d5454c-9548-4801-990e-2573263002b1")
	)
	(fp_text user "${REFERENCE}"
		(at 7.1 0.025 0)
		(layer "F.Fab")
		(uuid "dcd468bb-08e3-4206-bb02-9ab8b7c7d9b5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "1"
		(at 0 -2.3 0)
		(layer "F.Fab")
		(uuid "f8e465bd-5275-436a-bd9c-ccfcb73d8e4f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0abc8250-82c8-4a52-9121-2648f68d0763")
	)
	(pad "2" thru_hole circle
		(at 1.4 6.05 90)
		(size 2.5 2.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "460ea377-a651-4c0d-b886-0bb71bbb4354")
	)
	(pad "3" thru_hole circle
		(at 13.6 6.05 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f841d250-040a-4571-8ec0-6158bfa8a3db")
	)
	(pad "4" thru_hole circle
		(at 13.6 -6 90)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b47d7254-4003-478c-bd04-3edd92f71da3")
	)
	(pad "5" thru_hole circle
		(at 1.4 -5.95 90)
		(size 2.5 2.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "235503a0-18c7-4434-bebc-f2137b171493")
	)
	(model "${KICAD8_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
