(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "AD8138-ad8138" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "IC" (id 0) (at -7.62 10.16 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "AD8138-ad8138" (id 1) (at -7.62 -10.16 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "agg:SOIC-8" (id 2) (at -7.62 -12.7 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/AD8138.pdf" (id 3) (at -7.62 -15.24 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Farnell" "2725700" (id 4) (at -7.62 -17.78 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (symbol "AD8138-ad8138_0_0"
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "-IN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "VOCM" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 7.62 0) (length 2.54)
        (name "V+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "+OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "-OUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -10.16 5.08 0) (length 2.54)
        (name "V-" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 10.16 7.62 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "+IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "AD8138-ad8138_0_1"
      (rectangle (start -7.62 8.89) (end 7.62 -8.89)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
  )
  (symbol "AD9235BCPZ-65" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -5.4356 37.8968 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "AD9235BCPZ-65" (id 1) (at -7.6962 -46.5582 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "QFN50P500X500X100-33N" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "SUPPLIER" "Analog Devices" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "OC_FARNELL" "1438559" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MPN" "AD9235BCPZ-65" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PACKAGE" "LFCSP-32" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "OC_NEWARK" "51R8668" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "AD9235BCPZ-65_0_0"
      (rectangle (start -15.24 -43.18) (end 15.24 35.56)
        (stroke (width 0.4064) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin no_connect line (at -20.32 -20.32 0) (length 5.08)
        (name "DNC_2" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 22.86 180) (length 5.08)
        (name "D3" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 20.32 180) (length 5.08)
        (name "D4" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 17.78 180) (length 5.08)
        (name "D5" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 15.24 180) (length 5.08)
        (name "D6" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 12.7 180) (length 5.08)
        (name "D7" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -38.1 0) (length 5.08)
        (name "DGND" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -20.32 25.4 0) (length 5.08)
        (name "DRVDD" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 10.16 180) (length 5.08)
        (name "D8" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 7.62 180) (length 5.08)
        (name "D9" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 5.08 180) (length 5.08)
        (name "D10" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 20.32 0) (length 5.08)
        (name "CLK" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 2.54 180) (length 5.08)
        (name "D11_MSB" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 15.24 0) (length 5.08)
        (name "OTR" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 12.7 0) (length 5.08)
        (name "MODE" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 5.08 0) (length 5.08)
        (name "SENSE" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 10.16 0) (length 5.08)
        (name "VREF" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -7.62 0) (length 5.08)
        (name "REFB" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -10.16 0) (length 5.08)
        (name "REFT" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -20.32 27.94 0) (length 5.08)
        (name "AVDD" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -33.02 0) (length 5.08)
        (name "AGND_2" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 0 0) (length 5.08)
        (name "VIN+" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin no_connect line (at -20.32 -22.86 0) (length 5.08)
        (name "DNC_3" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 -2.54 0) (length 5.08)
        (name "VIN-" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -35.56 0) (length 5.08)
        (name "AGND" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -20.32 30.48 0) (length 5.08)
        (name "AVDD_2" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 -15.24 0) (length 5.08)
        (name "EP" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at -20.32 7.62 0) (length 5.08)
        (name "PDWN" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin no_connect line (at -20.32 -25.4 0) (length 5.08)
        (name "DNC_4" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin no_connect line (at -20.32 -27.94 0) (length 5.08)
        (name "DNC" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 30.48 180) (length 5.08)
        (name "D0_LSB" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 27.94 180) (length 5.08)
        (name "D1" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 20.32 25.4 180) (length 5.08)
        (name "D2" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "AD9235BR-ad9235" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 26.67 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "AD9235BR-ad9235" (id 1) (at 6.35 24.13 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at -13.97 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at -13.97 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TSSOP28* LFCSP32*" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AD9235BR-ad9235_1_0"
      (polyline
        (pts
          (xy -12.7 -25.4)
          (xy -12.7 22.86)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -12.7 22.86)
          (xy 11.43 22.86)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 -25.4)
          (xy -12.7 -25.4)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 11.43 22.86)
          (xy 11.43 -25.4)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (text "AD9235" (at 0 6.35 0)
        (effects (font (size 2.54 2.54)))
      )
    )
    (symbol "AD9235BR-ad9235_1_1"
      (pin output line (at 13.97 11.43 180) (length 2.54)
        (name "OTR" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 7.62 0) (length 2.54)
        (name "VIN-" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 1.27 -27.94 90) (length 2.54)
        (name "AGND@2" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -10.16 25.4 270) (length 2.54)
        (name "AVDD@2" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 1.27 0) (length 2.54)
        (name "CLK" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 -3.81 0) (length 2.54)
        (name "PDWN" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -22.86 180) (length 2.54)
        (name "D0" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -20.32 180) (length 2.54)
        (name "D1" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -17.78 180) (length 2.54)
        (name "D2" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -15.24 180) (length 2.54)
        (name "D3" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -12.7 180) (length 2.54)
        (name "D4" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 3.81 0) (length 2.54)
        (name "MODE" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -10.16 180) (length 2.54)
        (name "D5" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -7.62 180) (length 2.54)
        (name "D6" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -5.08 180) (length 2.54)
        (name "D7" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 3.81 -27.94 90) (length 2.54)
        (name "DGND" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -5.08 25.4 270) (length 2.54)
        (name "DRVDD" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 -2.54 180) (length 2.54)
        (name "D8" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 0 180) (length 2.54)
        (name "D9" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 2.54 180) (length 2.54)
        (name "D10" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 5.08 180) (length 2.54)
        (name "D11" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 -20.32 0) (length 2.54)
        (name "SENSE" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 -7.62 0) (length 2.54)
        (name "VREF" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 13.97 180) (length 2.54)
        (name "REFB" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 13.97 20.32 180) (length 2.54)
        (name "REFT" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -7.62 25.4 270) (length 2.54)
        (name "AVDD@1" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -1.27 -27.94 90) (length 2.54)
        (name "AGND@1" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -15.24 12.7 0) (length 2.54)
        (name "VIN+" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "CP_Small-Device" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at 0.254 1.778 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CP_Small-Device" (id 1) (at 0.254 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "CP_*" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CP_Small-Device_0_1"
      (rectangle (start -1.524 -0.3048) (end 1.524 -0.6858)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -1.524 0.6858) (end 1.524 0.3048)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 1.524)
          (xy -0.762 1.524)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.016 1.27)
          (xy -1.016 1.778)
        )
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "CP_Small-Device_1_1"
      (pin passive line (at 0 2.54 270) (length 1.8542)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -2.54 90) (length 1.8542)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "FT601Q-B-T" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -15.24 60.9854 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "FT601Q-B-T" (id 1) (at -15.2654 -61.0362 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "QFN40P900X900X100-77N" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "IPC7351B" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "SNAPEDA_PACKAGE_ID" "11921" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "FTDI Chip" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "1.05" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "ki_locked" "" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (symbol "FT601Q-B-T_0_0"
      (rectangle (start -15.24 -58.42) (end 15.24 60.96)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 20.32 -53.34 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 35.56 0) (length 5.08)
        (name "SIWU_N" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 30.48 0) (length 5.08)
        (name "WR_N" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 27.94 0) (length 5.08)
        (name "RD_N" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 43.18 0) (length 5.08)
        (name "OE_N" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 55.88 180) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 40.64 0) (length 5.08)
        (name "RESET_N" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -40.64 0) (length 5.08)
        (name "WAKEUP_N" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -33.02 0) (length 5.08)
        (name "GPIO0" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 -35.56 0) (length 5.08)
        (name "GPIO1" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 50.8 180) (length 5.08)
        (name "AVDD" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 53.34 180) (length 5.08)
        (name "VCC33" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 -25.4 0) (length 5.08)
        (name "XI" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 -27.94 0) (length 5.08)
        (name "XO" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 17.78 0) (length 5.08)
        (name "DP" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 53.34 180) (length 5.08)
        (name "VCC33" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at -20.32 15.24 0) (length 5.08)
        (name "DM" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 -53.34 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 10.16 0) (length 5.08)
        (name "RREF" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 48.26 180) (length 5.08)
        (name "VDDA" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 -53.34 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 58.42 180) (length 5.08)
        (name "VD10" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 58.42 180) (length 5.08)
        (name "VD10" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 5.08 0) (length 5.08)
        (name "T0DN" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 2.54 0) (length 5.08)
        (name "T0DP" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 58.42 180) (length 5.08)
        (name "VD10" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 0 0) (length 5.08)
        (name "RIDN" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 -2.54 0) (length 5.08)
        (name "RIDP" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 -53.34 180) (length 5.08)
        (name "GND" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -20.32 22.86 0) (length 5.08)
        (name "VBUS" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 53.34 180) (length 5.08)
        (name "VCC33" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 -20.32 0) (length 5.08)
        (name "DV10" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -40.64 180) (length 5.08)
        (name "BE_0" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 43.18 180) (length 5.08)
        (name "DATA_0" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 40.64 180) (length 5.08)
        (name "DATA_1" (effects (font (size 1.016 1.016))))
        (number "41" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 38.1 180) (length 5.08)
        (name "DATA_2" (effects (font (size 1.016 1.016))))
        (number "42" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 35.56 180) (length 5.08)
        (name "DATA_3" (effects (font (size 1.016 1.016))))
        (number "43" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 33.02 180) (length 5.08)
        (name "DATA_4" (effects (font (size 1.016 1.016))))
        (number "44" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 30.48 180) (length 5.08)
        (name "DATA_5" (effects (font (size 1.016 1.016))))
        (number "45" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 27.94 180) (length 5.08)
        (name "DATA_6" (effects (font (size 1.016 1.016))))
        (number "46" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 25.4 180) (length 5.08)
        (name "DATA_7" (effects (font (size 1.016 1.016))))
        (number "47" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 58.42 180) (length 5.08)
        (name "VD10" (effects (font (size 1.016 1.016))))
        (number "48" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 55.88 180) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "49" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -43.18 180) (length 5.08)
        (name "BE_1" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 22.86 180) (length 5.08)
        (name "DATA_8" (effects (font (size 1.016 1.016))))
        (number "50" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 20.32 180) (length 5.08)
        (name "DATA_9" (effects (font (size 1.016 1.016))))
        (number "51" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 17.78 180) (length 5.08)
        (name "DATA_10" (effects (font (size 1.016 1.016))))
        (number "52" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 15.24 180) (length 5.08)
        (name "DATA_11" (effects (font (size 1.016 1.016))))
        (number "53" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 12.7 180) (length 5.08)
        (name "DATA_12" (effects (font (size 1.016 1.016))))
        (number "54" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 10.16 180) (length 5.08)
        (name "DATA_13" (effects (font (size 1.016 1.016))))
        (number "55" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 7.62 180) (length 5.08)
        (name "DATA_14" (effects (font (size 1.016 1.016))))
        (number "56" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 5.08 180) (length 5.08)
        (name "DATA_15" (effects (font (size 1.016 1.016))))
        (number "57" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 -7.62 0) (length 5.08)
        (name "CLK" (effects (font (size 1.016 1.016))))
        (number "58" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 55.88 180) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "59" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -45.72 180) (length 5.08)
        (name "BE_2" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 2.54 180) (length 5.08)
        (name "DATA_16" (effects (font (size 1.016 1.016))))
        (number "60" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 0 180) (length 5.08)
        (name "DATA_17" (effects (font (size 1.016 1.016))))
        (number "61" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -2.54 180) (length 5.08)
        (name "DATA_18" (effects (font (size 1.016 1.016))))
        (number "62" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -5.08 180) (length 5.08)
        (name "DATA_19" (effects (font (size 1.016 1.016))))
        (number "63" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -7.62 180) (length 5.08)
        (name "DATA_20" (effects (font (size 1.016 1.016))))
        (number "64" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -10.16 180) (length 5.08)
        (name "DATA_21" (effects (font (size 1.016 1.016))))
        (number "65" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -12.7 180) (length 5.08)
        (name "DATA_22" (effects (font (size 1.016 1.016))))
        (number "66" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -15.24 180) (length 5.08)
        (name "DATA_23" (effects (font (size 1.016 1.016))))
        (number "67" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 55.88 180) (length 5.08)
        (name "VCCIO" (effects (font (size 1.016 1.016))))
        (number "68" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -17.78 180) (length 5.08)
        (name "DATA_24" (effects (font (size 1.016 1.016))))
        (number "69" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -48.26 180) (length 5.08)
        (name "BE_3" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -20.32 180) (length 5.08)
        (name "DATA_25" (effects (font (size 1.016 1.016))))
        (number "70" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -22.86 180) (length 5.08)
        (name "DATA_26" (effects (font (size 1.016 1.016))))
        (number "71" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -25.4 180) (length 5.08)
        (name "DATA_27" (effects (font (size 1.016 1.016))))
        (number "72" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -27.94 180) (length 5.08)
        (name "DATA_28" (effects (font (size 1.016 1.016))))
        (number "73" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -30.48 180) (length 5.08)
        (name "DATA_29" (effects (font (size 1.016 1.016))))
        (number "74" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -33.02 180) (length 5.08)
        (name "DATA_30" (effects (font (size 1.016 1.016))))
        (number "75" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 20.32 -35.56 180) (length 5.08)
        (name "DATA_31" (effects (font (size 1.016 1.016))))
        (number "76" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 20.32 -55.88 180) (length 5.08)
        (name "EXP" (effects (font (size 1.016 1.016))))
        (number "77" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 -12.7 0) (length 5.08)
        (name "TXE_N" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at -20.32 -15.24 0) (length 5.08)
        (name "RXF_N" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "HRO-TYPE-C-31-M-12" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "USB" (id 0) (at -5.08 16.51 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "HRO-TYPE-C-31-M-12" (id 1) (at -10.16 -1.27 90)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.524 1.524)) hide)
    )
    (symbol "HRO-TYPE-C-31-M-12_0_1"
      (rectangle (start -11.43 15.24) (end -8.89 -17.78)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (rectangle (start 0 -17.78) (end -8.89 15.24)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "HRO-TYPE-C-31-M-12_1_1"
      (pin input line (at 2.54 13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -8.89 180) (length 2.54)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -13.97 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -16.51 180) (length 2.54)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 11.43 180) (length 2.54)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 8.89 180) (length 2.54)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 6.35 180) (length 2.54)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 3.81 180) (length 2.54)
        (name "DN2" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 1.27 180) (length 2.54)
        (name "DP1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -1.27 180) (length 2.54)
        (name "DN1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -3.81 180) (length 2.54)
        (name "DP2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 2.54 -6.35 180) (length 2.54)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LM2664-tinkerforge" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 6.35 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "LM2664-tinkerforge" (id 1) (at 0 -6.35 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "" (id 2) (at -19.05 -25.4 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Datasheet" "" (id 3) (at -19.05 -25.4 0)
      (effects (font (size 1.524 1.524)))
    )
    (symbol "LM2664-tinkerforge_0_1"
      (rectangle (start -7.62 5.08) (end 7.62 -5.08)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "LM2664-tinkerforge_1_1"
      (pin input line (at -11.43 -3.81 0) (length 3.81)
        (name "GND" (effects (font (size 1.524 1.524))))
        (number "1" (effects (font (size 1.524 1.524))))
      )
      (pin input line (at 11.43 -3.81 180) (length 3.81)
        (name "OUT" (effects (font (size 1.524 1.524))))
        (number "2" (effects (font (size 1.524 1.524))))
      )
      (pin input line (at 11.43 0 180) (length 3.81)
        (name "CAP-" (effects (font (size 1.524 1.524))))
        (number "3" (effects (font (size 1.524 1.524))))
      )
      (pin input line (at -11.43 0 0) (length 3.81)
        (name "nSD" (effects (font (size 1.524 1.524))))
        (number "4" (effects (font (size 1.524 1.524))))
      )
      (pin input line (at -11.43 3.81 0) (length 3.81)
        (name "V+" (effects (font (size 1.524 1.524))))
        (number "5" (effects (font (size 1.524 1.524))))
      )
      (pin input line (at 11.43 3.81 180) (length 3.81)
        (name "CAP+" (effects (font (size 1.524 1.524))))
        (number "6" (effects (font (size 1.524 1.524))))
      )
    )
  )
  (symbol "STM32F730Z8T6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "STM32F730Z8T6" (id 1) (at 0 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "sm6uax:STMicroelectronics-LQFP144-1A-0-3-IPC_A" (id 2) (at 0 10.16 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f730r8.pdf" (id 3) (at 0 12.7 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "ki_locked" "" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "ki_description" "STM32F730Z8T6" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM32F730Z8T6_1_1"
      (rectangle (start 5.08 2.54) (end 45.72 -71.12)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at 2.54 -40.64 0) (length 2.54)
        (name "VCAP_2" (effects (font (size 1.016 1.016))))
        (number "106" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -60.96 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "107" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -17.78 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "108" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -63.5 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "120" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -30.48 0) (length 2.54)
        (name "VDDSDMMC" (effects (font (size 1.016 1.016))))
        (number "121" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -66.04 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "130" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -20.32 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "131" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 2.54 -58.42 0) (length 2.54)
        (name "BOOT0" (effects (font (size 1.016 1.016))))
        (number "138" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -63.5 0) (length 2.54)
        (name "PDR_ON" (effects (font (size 1.016 1.016))))
        (number "143" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -22.86 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "144" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -45.72 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 0 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 2.54 -68.58 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.016 1.016))))
        (number "25" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -2.54 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "30" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -68.58 180) (length 2.54)
        (name "VSSA" (effects (font (size 1.016 1.016))))
        (number "31" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -48.26 0) (length 2.54)
        (name "VREF+" (effects (font (size 1.016 1.016))))
        (number "32" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -27.94 0) (length 2.54)
        (name "VDDA" (effects (font (size 1.016 1.016))))
        (number "33" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -48.26 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "38" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -5.08 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "39" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -50.8 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "51" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -7.62 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "52" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -45.72 0) (length 2.54)
        (name "VBAT" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -53.34 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "61" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -10.16 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "62" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -38.1 0) (length 2.54)
        (name "VCAP_1" (effects (font (size 1.016 1.016))))
        (number "71" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -12.7 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "72" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -53.34 0) (length 2.54)
        (name "OTG_HS_REXT" (effects (font (size 1.016 1.016))))
        (number "75" (effects (font (size 1.016 1.016))))
      )
      (pin passive line (at 2.54 -25.4 0) (length 2.54)
        (name "VDD12OTGHS" (effects (font (size 1.016 1.016))))
        (number "76" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -55.88 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "85" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -15.24 0) (length 2.54)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "86" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 48.26 -58.42 180) (length 2.54)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "94" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at 2.54 -33.02 0) (length 2.54)
        (name "VDDUSB" (effects (font (size 1.016 1.016))))
        (number "95" (effects (font (size 1.016 1.016))))
      )
    )
    (symbol "STM32F730Z8T6_2_1"
      (rectangle (start 5.08 2.54) (end 22.86 -83.82)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at 2.54 -20.32 0) (length 2.54)
        (name "PA8" (effects (font (size 1.016 1.016))))
        (number "100" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -22.86 0) (length 2.54)
        (name "PA9" (effects (font (size 1.016 1.016))))
        (number "101" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -25.4 0) (length 2.54)
        (name "PA10" (effects (font (size 1.016 1.016))))
        (number "102" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -27.94 0) (length 2.54)
        (name "PA11" (effects (font (size 1.016 1.016))))
        (number "103" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -30.48 0) (length 2.54)
        (name "PA12" (effects (font (size 1.016 1.016))))
        (number "104" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -33.02 0) (length 2.54)
        (name "PA13" (effects (font (size 1.016 1.016))))
        (number "105" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -35.56 0) (length 2.54)
        (name "PA14" (effects (font (size 1.016 1.016))))
        (number "109" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -38.1 0) (length 2.54)
        (name "PA15" (effects (font (size 1.016 1.016))))
        (number "110" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -25.4 180) (length 2.54)
        (name "PC10" (effects (font (size 1.016 1.016))))
        (number "111" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -27.94 180) (length 2.54)
        (name "PC11" (effects (font (size 1.016 1.016))))
        (number "112" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -30.48 180) (length 2.54)
        (name "PC12" (effects (font (size 1.016 1.016))))
        (number "113" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -43.18 180) (length 2.54)
        (name "PD0" (effects (font (size 1.016 1.016))))
        (number "114" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -45.72 180) (length 2.54)
        (name "PD1" (effects (font (size 1.016 1.016))))
        (number "115" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -48.26 180) (length 2.54)
        (name "PD2" (effects (font (size 1.016 1.016))))
        (number "116" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -50.8 180) (length 2.54)
        (name "PD3" (effects (font (size 1.016 1.016))))
        (number "117" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -53.34 180) (length 2.54)
        (name "PD4" (effects (font (size 1.016 1.016))))
        (number "118" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -55.88 180) (length 2.54)
        (name "PD5" (effects (font (size 1.016 1.016))))
        (number "119" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -58.42 180) (length 2.54)
        (name "PD6" (effects (font (size 1.016 1.016))))
        (number "122" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -60.96 180) (length 2.54)
        (name "PD7" (effects (font (size 1.016 1.016))))
        (number "123" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -50.8 0) (length 2.54)
        (name "PB3" (effects (font (size 1.016 1.016))))
        (number "133" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -53.34 0) (length 2.54)
        (name "PB4" (effects (font (size 1.016 1.016))))
        (number "134" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -55.88 0) (length 2.54)
        (name "PB5" (effects (font (size 1.016 1.016))))
        (number "135" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -58.42 0) (length 2.54)
        (name "PB6" (effects (font (size 1.016 1.016))))
        (number "136" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -60.96 0) (length 2.54)
        (name "PB7" (effects (font (size 1.016 1.016))))
        (number "137" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -63.5 0) (length 2.54)
        (name "PB8" (effects (font (size 1.016 1.016))))
        (number "139" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -66.04 0) (length 2.54)
        (name "PB9" (effects (font (size 1.016 1.016))))
        (number "140" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 0 180) (length 2.54)
        (name "PC0" (effects (font (size 1.016 1.016))))
        (number "26" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -2.54 180) (length 2.54)
        (name "PC1" (effects (font (size 1.016 1.016))))
        (number "27" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -5.08 180) (length 2.54)
        (name "PC2" (effects (font (size 1.016 1.016))))
        (number "28" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -7.62 180) (length 2.54)
        (name "PC3" (effects (font (size 1.016 1.016))))
        (number "29" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 0 0) (length 2.54)
        (name "PA0" (effects (font (size 1.016 1.016))))
        (number "34" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -2.54 0) (length 2.54)
        (name "PA1" (effects (font (size 1.016 1.016))))
        (number "35" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -5.08 0) (length 2.54)
        (name "PA2" (effects (font (size 1.016 1.016))))
        (number "36" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -7.62 0) (length 2.54)
        (name "PA3" (effects (font (size 1.016 1.016))))
        (number "37" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -10.16 0) (length 2.54)
        (name "PA4" (effects (font (size 1.016 1.016))))
        (number "40" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -12.7 0) (length 2.54)
        (name "PA5" (effects (font (size 1.016 1.016))))
        (number "41" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -15.24 0) (length 2.54)
        (name "PA6" (effects (font (size 1.016 1.016))))
        (number "42" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -17.78 0) (length 2.54)
        (name "PA7" (effects (font (size 1.016 1.016))))
        (number "43" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -10.16 180) (length 2.54)
        (name "PC4" (effects (font (size 1.016 1.016))))
        (number "44" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -12.7 180) (length 2.54)
        (name "PC5" (effects (font (size 1.016 1.016))))
        (number "45" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -43.18 0) (length 2.54)
        (name "PB0" (effects (font (size 1.016 1.016))))
        (number "46" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -45.72 0) (length 2.54)
        (name "PB1" (effects (font (size 1.016 1.016))))
        (number "47" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -48.26 0) (length 2.54)
        (name "PB2" (effects (font (size 1.016 1.016))))
        (number "48" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -68.58 0) (length 2.54)
        (name "PB10" (effects (font (size 1.016 1.016))))
        (number "69" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -33.02 180) (length 2.54)
        (name "PC13" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -71.12 0) (length 2.54)
        (name "PB11" (effects (font (size 1.016 1.016))))
        (number "70" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -73.66 0) (length 2.54)
        (name "PB12" (effects (font (size 1.016 1.016))))
        (number "73" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -76.2 0) (length 2.54)
        (name "PB13" (effects (font (size 1.016 1.016))))
        (number "74" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -78.74 0) (length 2.54)
        (name "PB14" (effects (font (size 1.016 1.016))))
        (number "77" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -81.28 0) (length 2.54)
        (name "PB15" (effects (font (size 1.016 1.016))))
        (number "78" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -63.5 180) (length 2.54)
        (name "PD8" (effects (font (size 1.016 1.016))))
        (number "79" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -35.56 180) (length 2.54)
        (name "PC14" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -66.04 180) (length 2.54)
        (name "PD9" (effects (font (size 1.016 1.016))))
        (number "80" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -68.58 180) (length 2.54)
        (name "PD10" (effects (font (size 1.016 1.016))))
        (number "81" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -71.12 180) (length 2.54)
        (name "PD11" (effects (font (size 1.016 1.016))))
        (number "82" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -73.66 180) (length 2.54)
        (name "PD12" (effects (font (size 1.016 1.016))))
        (number "83" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -76.2 180) (length 2.54)
        (name "PD13" (effects (font (size 1.016 1.016))))
        (number "84" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -78.74 180) (length 2.54)
        (name "PD14" (effects (font (size 1.016 1.016))))
        (number "87" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -81.28 180) (length 2.54)
        (name "PD15" (effects (font (size 1.016 1.016))))
        (number "88" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -38.1 180) (length 2.54)
        (name "PC15" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -15.24 180) (length 2.54)
        (name "PC6" (effects (font (size 1.016 1.016))))
        (number "96" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -17.78 180) (length 2.54)
        (name "PC7" (effects (font (size 1.016 1.016))))
        (number "97" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -20.32 180) (length 2.54)
        (name "PC8" (effects (font (size 1.016 1.016))))
        (number "98" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -22.86 180) (length 2.54)
        (name "PC9" (effects (font (size 1.016 1.016))))
        (number "99" (effects (font (size 1.016 1.016))))
      )
    )
    (symbol "STM32F730Z8T6_3_1"
      (rectangle (start 5.08 2.54) (end 22.86 -83.82)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin bidirectional line (at 2.54 -5.08 0) (length 2.54)
        (name "PE2" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -43.18 0) (length 2.54)
        (name "PF0" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -45.72 0) (length 2.54)
        (name "PF1" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -48.26 0) (length 2.54)
        (name "PF2" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -17.78 180) (length 2.54)
        (name "PG9" (effects (font (size 1.016 1.016))))
        (number "124" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -20.32 180) (length 2.54)
        (name "PG10" (effects (font (size 1.016 1.016))))
        (number "125" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -22.86 180) (length 2.54)
        (name "PG11" (effects (font (size 1.016 1.016))))
        (number "126" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -25.4 180) (length 2.54)
        (name "PG12" (effects (font (size 1.016 1.016))))
        (number "127" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -27.94 180) (length 2.54)
        (name "PG13" (effects (font (size 1.016 1.016))))
        (number "128" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -30.48 180) (length 2.54)
        (name "PG14" (effects (font (size 1.016 1.016))))
        (number "129" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -50.8 0) (length 2.54)
        (name "PF3" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -33.02 180) (length 2.54)
        (name "PG15" (effects (font (size 1.016 1.016))))
        (number "132" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -53.34 0) (length 2.54)
        (name "PF4" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 0 0) (length 2.54)
        (name "PE0" (effects (font (size 1.016 1.016))))
        (number "141" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -2.54 0) (length 2.54)
        (name "PE1" (effects (font (size 1.016 1.016))))
        (number "142" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -55.88 0) (length 2.54)
        (name "PF5" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -58.42 0) (length 2.54)
        (name "PF6" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -60.96 0) (length 2.54)
        (name "PF7" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -7.62 0) (length 2.54)
        (name "PE3" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -63.5 0) (length 2.54)
        (name "PF8" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -66.04 0) (length 2.54)
        (name "PF9" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -68.58 0) (length 2.54)
        (name "PF10" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -43.18 180) (length 2.54)
        (name "PH0" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -45.72 180) (length 2.54)
        (name "PH1" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -10.16 0) (length 2.54)
        (name "PE4" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -12.7 0) (length 2.54)
        (name "PE5" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -71.12 0) (length 2.54)
        (name "PF11" (effects (font (size 1.016 1.016))))
        (number "49" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -15.24 0) (length 2.54)
        (name "PE6" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -73.66 0) (length 2.54)
        (name "PF12" (effects (font (size 1.016 1.016))))
        (number "50" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -76.2 0) (length 2.54)
        (name "PF13" (effects (font (size 1.016 1.016))))
        (number "53" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -78.74 0) (length 2.54)
        (name "PF14" (effects (font (size 1.016 1.016))))
        (number "54" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -81.28 0) (length 2.54)
        (name "PF15" (effects (font (size 1.016 1.016))))
        (number "55" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 0 180) (length 2.54)
        (name "PG0" (effects (font (size 1.016 1.016))))
        (number "56" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -2.54 180) (length 2.54)
        (name "PG1" (effects (font (size 1.016 1.016))))
        (number "57" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -17.78 0) (length 2.54)
        (name "PE7" (effects (font (size 1.016 1.016))))
        (number "58" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -20.32 0) (length 2.54)
        (name "PE8" (effects (font (size 1.016 1.016))))
        (number "59" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -22.86 0) (length 2.54)
        (name "PE9" (effects (font (size 1.016 1.016))))
        (number "60" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -25.4 0) (length 2.54)
        (name "PE10" (effects (font (size 1.016 1.016))))
        (number "63" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -27.94 0) (length 2.54)
        (name "PE11" (effects (font (size 1.016 1.016))))
        (number "64" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -30.48 0) (length 2.54)
        (name "PE12" (effects (font (size 1.016 1.016))))
        (number "65" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -33.02 0) (length 2.54)
        (name "PE13" (effects (font (size 1.016 1.016))))
        (number "66" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -35.56 0) (length 2.54)
        (name "PE14" (effects (font (size 1.016 1.016))))
        (number "67" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 2.54 -38.1 0) (length 2.54)
        (name "PE15" (effects (font (size 1.016 1.016))))
        (number "68" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -5.08 180) (length 2.54)
        (name "PG2" (effects (font (size 1.016 1.016))))
        (number "89" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -7.62 180) (length 2.54)
        (name "PG3" (effects (font (size 1.016 1.016))))
        (number "90" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -10.16 180) (length 2.54)
        (name "PG4" (effects (font (size 1.016 1.016))))
        (number "91" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -12.7 180) (length 2.54)
        (name "PG5" (effects (font (size 1.016 1.016))))
        (number "92" (effects (font (size 1.016 1.016))))
      )
      (pin bidirectional line (at 25.4 -15.24 180) (length 2.54)
        (name "PG8" (effects (font (size 1.016 1.016))))
        (number "93" (effects (font (size 1.016 1.016))))
      )
    )
  )
  (symbol "TPS54331" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "TPS54331" (id 1) (at -1.27 8.89 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 1.27 -8.89 0)
      (effects (font (size 1.27 1.27) italic) (justify left) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps5430.pdf" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Step-Down DC-DC Switching Regulator" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "3A, Step Down Swift Converter, , PowerSOIC-8" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "TI*SO*PowerPAD*ThermalVias*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS54331_0_1"
      (rectangle (start -10.16 7.62) (end 10.16 -7.62)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TPS54331_1_1"
      (pin input line (at 12.7 5.08 180) (length 2.54)
        (name "BOOT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 2.54 0) (length 2.54) hide
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 5.08 0) (length 2.54)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -5.08 0) (length 2.54)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -2.54 0) (length 2.54)
        (name "SS" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -5.08 180) (length 2.54)
        (name "VSENSE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
        (name "COMP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -2.54 -10.16 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 2.54 180) (length 2.54)
        (name "PH" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "USB_C_Receptacle" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -10.16 29.21 0)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "USB_C_Receptacle" (id 1) (at 10.16 29.21 0)
      (effects (font (size 1.27 1.27)) (justify right))
    )
    (property "Footprint" "" (id 2) (at 3.81 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip" (id 3) (at 3.81 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "usb universal serial bus type-C full-featured" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "USB Full-Featured Type-C Receptacle connector" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "USB*C*Receptacle*" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "USB_C_Receptacle_0_0"
      (rectangle (start -0.254 -35.56) (end 0.254 -34.544)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -32.766) (end 9.144 -33.274)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -30.226) (end 9.144 -30.734)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -25.146) (end 9.144 -25.654)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -22.606) (end 9.144 -23.114)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -17.526) (end 9.144 -18.034)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -14.986) (end 9.144 -15.494)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -9.906) (end 9.144 -10.414)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -7.366) (end 9.144 -7.874)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 -2.286) (end 9.144 -2.794)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 0.254) (end 9.144 -0.254)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 5.334) (end 9.144 4.826)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 7.874) (end 9.144 7.366)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 10.414) (end 9.144 9.906)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 12.954) (end 9.144 12.446)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 18.034) (end 9.144 17.526)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 20.574) (end 9.144 20.066)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (rectangle (start 10.16 25.654) (end 9.144 25.146)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "USB_C_Receptacle_0_1"
      (rectangle (start -10.16 27.94) (end 10.16 -35.56)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (arc (start -8.89 -3.81) (mid -6.985 -5.715) (end -5.08 -3.81)
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -7.62 -3.81) (mid -6.985 -4.445) (end -6.35 -3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -7.62 -3.81) (mid -6.985 -4.445) (end -6.35 -3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start -7.62 -3.81) (end -6.35 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (arc (start -6.35 3.81) (mid -6.985 4.445) (end -7.62 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (arc (start -6.35 3.81) (mid -6.985 4.445) (end -7.62 3.81)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (arc (start -5.08 3.81) (mid -6.985 5.715) (end -8.89 3.81)
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -8.89 -3.81)
          (xy -8.89 3.81)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -5.08 3.81)
          (xy -5.08 -3.81)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
    )
    (symbol "USB_C_Receptacle_1_1"
      (circle (center -2.54 1.143) (radius 0.635)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (circle (center 0 -5.842) (radius 1.27)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 0 -5.842)
          (xy 0 4.318)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -3.302)
          (xy -2.54 -0.762)
          (xy -2.54 0.508)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -2.032)
          (xy 2.54 0.508)
          (xy 2.54 1.778)
        )
        (stroke (width 0.508) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.27 4.318)
          (xy 0 6.858)
          (xy 1.27 4.318)
          (xy -1.27 4.318)
        )
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (rectangle (start 1.905 1.778) (end 3.175 3.048)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type outline))
      )
      (pin passive line (at 0 -40.64 90) (length 5.08)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -15.24 180) (length 5.08)
        (name "RX2-" (effects (font (size 1.27 1.27))))
        (number "A10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -17.78 180) (length 5.08)
        (name "RX2+" (effects (font (size 1.27 1.27))))
        (number "A11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -10.16 180) (length 5.08)
        (name "TX1+" (effects (font (size 1.27 1.27))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -7.62 180) (length 5.08)
        (name "TX1-" (effects (font (size 1.27 1.27))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 25.4 180) (length 5.08)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 20.32 180) (length 5.08)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 7.62 180) (length 5.08)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 12.7 180) (length 5.08)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -30.48 180) (length 5.08)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 25.4 180) (length 5.08) hide
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 0 180) (length 5.08)
        (name "RX1-" (effects (font (size 1.27 1.27))))
        (number "B10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -2.54 180) (length 5.08)
        (name "RX1+" (effects (font (size 1.27 1.27))))
        (number "B11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 0 -40.64 90) (length 5.08) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -25.4 180) (length 5.08)
        (name "TX2+" (effects (font (size 1.27 1.27))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -22.86 180) (length 5.08)
        (name "TX2-" (effects (font (size 1.27 1.27))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 25.4 180) (length 5.08) hide
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 17.78 180) (length 5.08)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 5.08 180) (length 5.08)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 10.16 180) (length 5.08)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -33.02 180) (length 5.08)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 15.24 25.4 180) (length 5.08) hide
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -7.62 -40.64 90) (length 5.08)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
